LeCroy LS-140 Firmware Installation

This ZIP archive contains firmware installation files for LS-140's with various installed options.
Note that you must install the version that supports the hardware configuration of the instrument
you have.

If your firmware is corrupted and you cannot determine what version was in your instrument start
with the 2K version. If your scope has a network card load the NET version of the firmware. If
you have the L1 version load the 20K firmware. If you the have an L1 version and a network card
load the L1NET version. L1's typically will have a label on the back that says L1.

Versions in the archive:

V200_2k.zip     - Version 2.00 Firmware for LS-140's that have 2K of acquisition memory.
V200_2knet.zip  - version 2.00 Firmware for LS-140's that have 2k and the net card.
V200_20k.zip    - version 2.00 Firmware for LS-140's that have 20k (L1).
V200_L1_NET.zip - version 2.00 Firmware for LS-140's that have 20K (L1) and the net card.
V211_2k.zip     - Version 2.11 Firmware for LS-140's that have 2K of acquisition memory.
V211_20k.zip    - version 2.11 Firmware for LS-140's that have 20k (L1).

To install or update the firmware:

1. Obtain a pre-formatted 3.5 inch floppy disk or one that has been formatted in a MSDOS computer
you can try a Windows formatted floppy and see if it works.

2. Copy all of the files from the zip of the version that you want to install to the root directory
of the floppy.

3. Power the scope off, insert the floppy disk and re-power the scope. The scope should load the
firmware and boot normally.


SHR
16-MAR-2013
