sampler plugin
25 ps risetime
trigger pickoff
Sampling head 25 pS rise time, DC to 14 GHz,
50 ohms input impedance. Variable DC offset
allows signals between +1V and -1 V limits to be
displayed at 2 mV/DIV.
