Compaq 32-BitFast-SCSI-2 (53c710) Compaq Integrated 32-BitFast-SCSI-2 (53c710) Compaq Integrated 32-Bit Fast-SCSI-2/P (53c810) Compaq Integrated 32-Bit Fast-Wide SCSI-2/E (53c825) Compaq Integrated 32-Bit Fast-Wide SCSI-2/P (53c825) Compaq 32-Bit Fast-Wide SCSI-2/P (53c825)

Description

The Compaq family of PCI and EISA contr ollers based on the 53c xxx chip includes the following:

Note – The Wide SCSI option is not supported under the Solaris Operating envir onment. Some car ds include connectors for both narr ow cables (in other wor ds, 8-bit SCSI A cables) and wide cables (that is 16-bit SCSI P cables.) Y ou can connect devices to the SCSI W ide connectors using SCSI P cables, but the Solaris ncrs driver will not initiate or accept the W ide Data T ransfer option. The attached devices will function in 8-bit narr ow mode.

Device Configuration

Preparing for Configuration See the har dwar e manufactur er’s documentation for installation and cabling requir ements.

Compaq Controller Chip Available On Compaq 32-Bit Fast-SCSI-2 53c710 EISA add-in car d Compaq Integrated 32-Bit Fast-SCSI-2 53c710 ProLiant 2000, 4000 Compaq Integrated 32-Bit Fast-SCSI-2/P 53c810 ProSignia 300-PCI, 500-PCI Compaq Integrated 32-Bit Fast-W ide SCSI-2/E 53c825 ProLiant 4500-EISA Compaq Integrated 32-Bit Fast-W ide SCSI-2/P 53c825 ProLiant 1500-PCI Compaq 32-Bit Fast-W ide SCSI-2/P 53c825 PCI add-in car d

Configuring the Device 1. Consult your Device Configuration W orksheet to see if the NCR 53C710 settings need to be changed.

2. Use the Compaq EISA configuration utility V ersion 2.20 Revision B or later . This can be r un fr om the har d disk or fr om the diskettes that come with your system.

3. At the MAIN MENU, press ctrl-A to see the Advanced Mode options.

A pop-up box shows that Advanced Mode is enabled.

4. Press Enter .

5. Select System Configuration.

6. Select Configure Hardware.

The pr ogram will then ask you to insert the second diskette into the drive.

7. Press Enter after you have inserted the second diskette.

8. Select Configuration Set Up.

9. Select Step 2 Add/Remove Board.

Follow the instr uctions on the scr een to add your boar d.

10. Select Step 3 V iew or Edit Details.

Find the description of the slot with the Compaq 32-bit Fast-SCSI-2 Contr oller. Use the Page-Down key as needed.

11. Select BIOS Hard Drive Geometry under the slot description that lists the Compaq 32-bit Fast-SCSI-2 Controller .

12. Set this option to <=1 GB: 64 Heads, 32 Sectors > 1GB: 255 Heads, 63 sectors. This will work for disks with sizes gr eater and smaller than 1 Gbyte.

13. Press F10 to leave that menu.

14. Select Step 5 Save and Exit.

Save your changes and exit.

Known Problems and Limitations The SCSI Tagged Queuing option is not supported.