SunSoft, Inc. A Sun Micr osystems, Inc. Business 2550 Garcia Avenue Mountain V iew, CA 94043 U.S.A.

Solaris™2.4 x86Har dwar eCompatibilityList March1996

Part No: 801-6619-19 Revision A, Mar ch 1996

Please Recycle

Copyright 1996 Sun Micr osystems, Inc., 2550 Gar cia Avenue, Mountain V iew, California 94043-1 100 U.S.A. All rights r eserved.

This pr oduct or document is pr otected by copyright and distributed under licenses r estricting its use, copying, distribution, and decompilation. No part of this pr oduct or document may be r eproduced in any form by any means without prior written authorization of Sun and its licensors, if any .

Portions of this pr oduct may be derived fr om the UNIX^® system, licensed fr om Novell, Inc., and fr om the Berkeley 4.3 BSD system, licensed fr om the University of California. UNIX is a r egister ed trademark in the United States and other countries and is exclusively licensed by X/Open Company Ltd. Thir d-party softwar e, including font technology in this pr oduct, is pr otected by copyright and licensed fr om Sun’s suppliers.

RESTRICTED RIGHTS LEGEND: Use, duplication, or disclosur e by the government is subject to r estrictions as set forth in subparagraph (c)(1)(ii) of the Rights in T echnical Data and Computer Softwar e clause at DF ARS 252.227-7013 and FAR 52.227-19.

Sun, Sun Micr osystems, the Sun logo, Solaris ,and OpenW indows ar e trademarks or r egister ed trademarks of Sun Microsystems, Inc. in the United States and other countries. UNIX is a r egister ed trademark in the United States and other countries, exclusively licensed thr ough X/Open Company , Ltd. OPEN LOOK is a r egister ed trademark of Novell, Inc. PostScript and Display PostScript ar e trademarks of Adobe Systems, Inc. Pentium is a trademark of Intel Corporation .

The OPEN LOOK^® and Sun™ Graphical User Interfaces wer e developed by Sun Micr osystems, Inc. for its users and licensees. Sun acknowledges the pioneering ef forts of Xer ox in r esear ching and developing the concept of visual or graphical user interfaces for the computer industry . Sun holds a non-exclusive license fr om Xerox to the Xer ox Graphical User Interface, which license also covers Sun’s licensees who implement OPEN LOOK GUIs and otherwise comply with Sun’s written license agreements.

X Window System is a trademark of X Consortium, Inc.

THIS PUBLICATION IS PROVIDED “AS IS” WITHOUT W ARRANTY OF ANY KIND, EITHER EXPRESS OR IMPLIED, INCLUDING, BUT NOT LIMITED T O, THE IMPLIED W ARRANTIES OF MERCHANT ABILITY, FITNESS FOR A PARTICULAR PURPOSE, OR NON-INFRINGEMENT .

1

Solaris 2.4 x86 Hardware Compatibility List

This document pr ovides information about general x86 har dwar e requir ements, supported peripherals, and system platforms that have been tested on the Solaris™ 2.4 computing envir onment.

The har dwar e platforms and peripherals appearing in this document have been tested by the SunSoft Platform Certification Lab for compatibility with the Solaris 2.4 x86 operating envir onment. System platforms listed in this document have been tested in configurations that ar e actually shipped by the hardwar e manufactur ers.

The majority of the systems and peripherals listed in this document r equir e the curr ent Driver Update for pr oper operation in the Solaris envir onment.

Some systems appearing in this list may include devices that ar e not yet supported by the Solaris 2.4 x86 softwar e. Since it is the natur e of this industry to have unexpected and unannounced changes, SunSoft is committed to working with those customers who encounter dif ficulties installing the Solaris softwar e on certified systems.

How This Book Is Organized

This document is divided into the following thr ee major sections:

“General Requirements” lists the x86 har dwar e requir ements for installing the Solaris 2.4 operating envir onment.

“System Platforms” lists the platforms that have been tested on Solaris 2.4; not all of the peripherals listed in the “Supported Devices” section have been tested in all combinations on all of these platforms. This is not intended to be an exhaustive list of x86 machines that can r un Solaris 2.4; it is simply a list of machines that have been tested with Solaris 2.4 at the time this document was updated.

“Supported Devices” lists the supported peripherals, including those supported in Driver Updates.

2 Solaris 2.4 x86 Hardware Compatibility List— March 1996

Specific machines and classes of devices ar e shown in these tables in this document.

Single Processor Systems page 7

Multipr ocessor Systems (SMP) page 13

Notebook Computers page 15

SCSI Host Bus Adapters page 16

SCSI RAID Controllers page 17

Solid State SCSI Disk Devices page 17

CD-ROM Drives page 17

CDR CD-ROM W riters/Recorders page 19

Audio Devices page 19

Telephone Call Processing page 20

Multiport Serial Adapters page 21

Network Adapters—Ethernet page 21

Network Adapters—Fast Ethernet page 23

Network Adapters—FDDI page 23

Network Adapters—T oken Ring page 23

High-Speed Networking page 23

PC Card (PCMCIA)—Adapters page 23

PC Card (PCMCIA)—Add-On Boards page 23

PC Card (PCMCIA)—Modems page 24

PC Card (PCMCIA)—Serial Cards page 24

PC Card (PCMCIA)—SRAM Memory Cards page 24

How This Book Is Organized 3

Pointing Devices page 25

Tape Drives—SCSI page 26

SCSI RAID Tape page 27

Uninterruptable Power Supplies (UPS) page 27

Motherboards page 28

Video Display Adapters page 30

Notebook Display Video Support page 37

Notebooks With External Monitor V ideo Support page 37

4 Solaris 2.4 x86 Hardware Compatibility List— March 1996

How to Obtain Updated Hardwar e Compatibility Lists and Device Driver Information

Har dwar e Compatibility Lists and Driver Update r eleases (including r elated documentation) ar e produced periodically as support for new har dwar e becomes available. They ar e available fr om these sour ces:

• World W ide Web—Open URL http://access1.Sun.COM, and select

“x86” and then “Solaris Intel (x86).”

• FTP—Use anonymous FTP to access ftp.uu.net, then go to

/vendor/sun/solaris/x86/2.4/

• CompuServe—T ype go sunsoft and go to the Solaris x86 library .

Note that the W orld W ide Web, CompuServe, and ASK-IT (below) also point to Support-pr ovided installation and configuration information as well as answers to fr equently asked questions.

Related Documentation Only • Email Autor esponder—T o obtain a Har dwar e Compatibility List or a Driver

Update Announcement via email, send email to hcl-index@Sun.COM for a list of autor esponse aliases that r eturn har dwar e support information.

• ASK-IT^1—SunSoft’s Automated Support Fax-on-Demand Service

• In North America, call one of these numbers:

1-800-SUNSOFT and choose options 4, 1, 1 (310) 348-6219 and choose option 1 • Outside North America, call one of these numbers and choose option 1:

Australia 61-2-844-5374 Japan 03-5717-2560 Taiwan 886-2-719-8069 United Kingdom 44-1276-677131

1. Includes the curr ent Har dwar e Compatibility List, document No. 51201, which summarizes the curr ent Driver Update, and document No. 81234, which lists x86 Device Configuration Guide Device Refer ence Pages so you can r equest those not available in Driver Updates.

How to Obtain Technical Support 5

How to Obtain Technical Support

To obtain technical support:

• In North America, call 1-800-SUNSOFT and choose option 4. • Outside North America, contact your technical support pr ovider .

Related Books

For specific har dwar e configuration information necessary to install and r un Solaris on your particular har dwar e, see x86 Device Configuration Guide and Solaris 2.4 x86 Driver Update Guide.

Corrections and Additions

Vendors, OEMs, and manufactur ers: To supply corr ections or add pr oducts to this list, or to obtain information on the har dwar e certification pr ogram, send email to x86-certify@Cypress.West.Sun.COM or leave voice mail at (310) 348-6170.

6 Solaris 2.4 x86 Hardware Compatibility List— March 1996

General Requirements

1. A 486DX, 486DX2, or Pentium CPU is r ecommended for better performance.

CPU Minimum Memory Bus

Disk Interface

Distribution Media

Devices for Installing Solaris

Intel or compatible 386@33MHz (minimum^1) Intel or compatible 486DX, 486DX2, 486SL, 486SX, 486DX4 Intel Pentium Intel Pentium Pr o AMD 486DX2-66 AMD 486DX2-80 AMD 486DX4-100

16 Mbytes • ISA • EISA • MCA • PCI • VLB

• IDE • E-IDE • SCSI

CD-ROM with a single boot diskette

Diskette drive and one of the following devices: • Local SCSI or ATAPI/IDE CD-ROM drive • Remote SCSI or ATAPI/IDE CD-ROM drive available over the network • Remote har d disk available over the network

System Platforms 7

System Platforms

The Solaris 2.4 x86 system has been successfully installed and tested on the computers listed in this section configur ed as they ar e shipped by the system manufactur er.

Single Processor Systems

Acer AcerAltos 700 Acer AcerAltos 800^1 Acer AcerAltos 800/P (P-90) Acer AcerAltos 7000 (P-60) Acer AcerAltos 7000 (P-90) Acer AcerAltos 7000/P (1 CPU, P-90) Acer AcerPower 5000 (P-60)^{2,3} Acer AcerPower 5020 (P-90)^{2,3} Acer AcerPower 9000T Acer AcerPower Pentium-75 Desktop Acer AcerAltos 17000 Server (tested with 1 CPU only)^4

ALR BusinessVEISA DX2/66 ALR Evolution IV 4DX2/66 ALR Evolution Q/MP2 100 (1 CPU config) ALR Evolution V ST e/75 (P-75) ALR Evolution V ST/75 (P-75) ALR Evolution V ST/120 (P-120) ALR Evolution V ST/PCI (P-90) ALR Evolution VQ EISA (P-60) ALR Evolution VQ EISA (P-66) ALR Evolution VQ EISA (P-90) ALR Evolution X/75 (P-75) ALR Evolution X/120 (P-120) ALR FLYERvl 486 DX2/66 ALR PROVEISA DX2/66 ALR Revolution MP/100 (1 CPU config) ALR Revolution MP-120 (1 CPU config) ALR Revolution MP/133 (1 CPU config)

AMD Enhanced (486DX4-100)

American Micr o Group P90PE-SS Server American Micr o Group P90PE-WS W orkstation

AST Bravo-LC 4/100T AST Bravo-MS P/75 AST Bravo-MS P/90 AST Bravo-MS P/100 (P-100) AST Bravo-MS 4/50d AST Bravo-MS 4/50s AST Bravo-MS 4/66d AST Manhattan-G AST Manhattan P5090 (P-90) AST Manhattan P Series 5100 (P-100) AST Manhattan P5133 12003AE (1 CPU) AST Manhattan V5090 (P-90) AST PowerExec 4/33SL AST Premium SE 4/50 AST Premmia GX (P-90) E-IDE AST Premmia GX (P-90) Integrated SCSI AST Premmia GX (P-100) AST Premmia MX 4/100t 486 DX4-100 AST Premmia MX P/75 (P-75) AST Premmia MTE 4/66

AT&T GIS 3404 Server (P-90)

Austin Dir ect Affinity SE Austin Dir ect Power System 66 (Pentium 66)

C&S Vertriebs GmbH AMICUS Advanced (P-133) C&S Vertriebs GmbH AMICUS Performance (P-100) C&S Vertriebs GmbH (P5-100-ISA-PCI)

Centerprise LEO-486 (486DX33)

Single Processor Systems (Continued)

8 Solaris 2.4 x86 Hardware Compatibility List— March 1996

Compaq Deskpr o 4/33i Compaq Deskpr o XE 450 Compaq Deskpr o XE 560 (P-60) Compaq Deskpr o XL 466 (486DX2-66) Compaq Deskpr o XL 486 (486-66) Compaq Deskpr o XL 590 (P-90) Compaq Pr oLiant 1500 (P-75) Compaq Pr oLiant 1500 (P-133) Compaq Pr oLiant 2000 (1 CPU, P-90) Compaq Pr oLiant 4000 (1 CPU, P-90) Compaq Pr oLiant 4500 (P-100) Compaq Pr oLiant 5/133 Compaq Pr oLinea 4/33 Compaq Pr oLinea 575 (P-75) Compaq Pr oLinea 6150E Compaq Pr oSignia 300 (P-90) Compaq Pr oSignia 500 (P-90)

CompuAdd C4100D Low Pr ofile (486DX4-100) CompuAdd 450 CompuAdd C450D CompuAdd C450D Low Pr ofile CompuAdd C466D CompuAdd C466D Low Pr ofile (486DX2-66) CompuAdd CP90p CompuAdd CP90p-LX Low Pr ofile

CompuT rend PREMIO Model 5107-AL1 (P-66) CompuT rend PREMIO Model 5107-AL3 (P-90)

Cube Corp. A TX 466D2 Cube Corp. PowerStation P66

DEC Celebris 590 Low Pr ofile (P-90) DEC DECpc 466d2 MTE DEC DECpc LVp+ (433sx/466d2/4100d4) DEC Prioris HX 590 (P-90)^5

Single Processor Systems (Continued)

Dell 433/DE Dell 450/DE Dell 466/ME Dell 466/MX Dell 466/T Dell Dimension XPS P90 Dell Dimension XPS P100c Dell Dimension XPS P120c Dell Dimension XPS 6150 (P6-150) Dell Omniplex 466 Dell Omniplex 560 Dell Omniplex 566 Dell Omniplex 590 Dell OptiPlex 486/LE MTE Dell OptiPlex 560/L Low Pr ofile (P-60) Dell OptiPlex DGX 590 Dell OptiPlex DGX 5100 Dell OptiPlex DGX 5120 Dell OptiPlex XL 575 (P-75) Dell OptiPlex XM 575 (P-75) Dell OptiPlex XMT 575 (P-75) Dell OptiPlex XL 590 (P-90) Dell OptiPlex XM 590 (P-90) Dell OptiPlex XMT 590 (P-90) Dell OptiPlex XL 5100 (P-100) Dell OptiPlex XM 5100 (P-100) Dell OptiPlex XMT 5100 (P-100) Dell OptiPlex XL 5120 (P-120) Dell OptiPlex XM 5120 (P-120) Dell OptiPlex XMT 5120 (P-120) Dell OptiPlex XMT 5133 (P-133) Dell PowerEdge 466/XE Dell PowerEdge SP 590 Dell SP5100-2 (P-100)

Diversified T echnology DTI LBE4520 (P-90) Diversified T echnology DTI LBE4520 (P-100)

DTK FEAT-39 (DX4-100) DTK QUIN-35D PCI (P-90) DTK QUIN-35M PCI (P-90)

Single Processor Systems (Continued)

System Platforms 9

EIS Computers “The Client” (486/66 VLB) EIS Computers “The Client P60” (P5-60) EIS Computers “The Developer” (486/66 EISA/VLB) EIS Computers “The Developer P90” (P-90 PCI) EIS Computers “The Developer P90i” (P5-90 PCI) EIS Computers “The Developer P100” (P-100 PCI) EIS Computers “The Developer P100i” (P-100 PCI) EIS Computers “The Developer P120” (P-120 PCI) EIS Computers “The Developer P120i” (P-120) EIS Computers “The Developer P120s” (P-120) EIS Computers “The Developer P133” (P-133) EIS Computers “The Developer P133i” (P-133) EIS Computers “The Developer P133s” (P-133)

Elonex PC-590-I

Everex Step DP (tested with 1 CPU, P-90)

Fujitsu FMV -466D (486DX2-66) Fujitsu FMV -575D4L (P-75) Fujitsu FMV -590D3 (P-90) Fujitsu FMV -5100D4L (P-100) Fujitsu ICL Er goPro x450-90

Futur eTech 4100V (486 DX4/100) Futur eTech 462iV (i486 DX2-66) Futur eTech 5601P (P5-60) Futur eTech FTS4414 (AMD486 DX-40)

Gateway 2000 486/33E Gateway 2000 4DX2-66 (low pr ofile)^3 Gateway 2000 4DX2-66E Gateway 2000 4DX2-66V Gateway 2000 4SX-33 (low pr ofile)^3 Gateway 2000 P4D-66^3 Gateway 2000 P4D-100 (486DX4-100) Gateway 2000 P5-60 Gateway 2000 P5-66^3 Gateway 2000 P5-90 T ower Gateway 2000 P5-120 T ower Gateway 2000 P5-100 (P-100)^6 Gateway 2000 P5-100XL (P-100)^6 Gateway 2000 P5-120 (P-120)^7

Single Processor Systems (Continued)

GCH Systems EasyData 590 (P54C-90) GCH Systems Aegis 466 (i486DX2-66) GCH Systems Aegis 466ES (i486DX2-66)

GoldStar GT51P PCI (P-60)

Hitachi FLORA 1010DK (P-60) Hitachi FLORA 1010DL Hitachi FLORA 1010DM (P-100) Hitachi FLORA 1010DN Hitachi FLORA DS1 (P-75) Hitachi FLORA DS1 (P-100) Hitachi FLORA DS1 (P-133)

HP NetServer 4d/66LE (486DX2-66)^8 HP NetServer 4d/66LM^9 HP NetServer 5/66 LC (P-66) HP NetServer 5/66 LF (P-66) HP Vectra VL2 5/60 (P-60) HP Vectra VL2 5/90 (P-90) HP Vectra VL2 4100 (486DX4-100) HP Vectra VL3 (P-90) HP Vectra XM2 4/66i (486DX2-66) HP Vectra XM3 5/90 (P-90) HP Vectra XU (P-90) HP Vectra XU 5/90c (with Matr ox Video) (P-90)^{10}

Hyundai Phantom Desktop (P-90)

Single Processor Systems (Continued)

10 Solaris 2.4 x86 Hardware Compatibility List— March 1996

IBM PC Server 320 Model 8640-ONJ (486DX2-66) IBM PC Server 320 Model 8640-OPT (P-90) IBM PC Server 500 Model 8641 OYR (P-90) IBM Personal Computer 300 Series Model 6571 IBM Personal Computer 300 Series Model 6575 IBM Personal Computer 300 Series Model 6581 IBM Personal Computer 300 Series Model 6585 IBM Personal Computer 330 Model 6576 (P-75) IBM Personal Computer 350-100DX4 IBM Personal Computer 700 Series Model 6875 IBM Personal Computer 750 Model 6885 (P-75) IBM Personal Computer 750 Model 6885-35H (P-75) IBM Personal Computer 750 Model 6885-JOM (P-90) IBM PS/2 Model 76 (9576- xxx) IBM PS/2 Model 95 XP486 (9595-OL) IBM PS/2 Model 95 XP486 (9595-OM)^{11} IBM PS/2 Server 95 (9595-3QT)^5 IBM PS/2 Server 95 (9595-OPT)^5 IBM PS/V aluePoint 466DX2/D IBM PS/V aluePoint P60/D IBM PS/V aluePoint Performance Series 486 DX2/66 Dp

Industrial CPU Systems PC (P-133)

Infotel Ultra P5-75 PCI Infotel Ultra P5-90 PCI Minitower Infotel Ultra P5-100 PCI Infotel Ultra P5-120 PCI

Intel L486-Series Pr ofessional GX (486DX2-66) Intel Advanced ZE Mini-tower (P-100) Intel Advanced EV Pentium/100 Intel ALTserver Altair (P5-150) Intel ALTserver Altair (P5-666) Intel Pentium Pr o Performance-AU Intel Pentium Pr o Performance-AU A TX Intel Performance AU (P6-180) Intel Performance AU (P6-200) Intel Pr emier e/PCI LX (Plato) (P-90) Intel Xpr ess 486/DX33 Intel Xpr ess Pentium/60 Intel Xpr ess Pentium/90

Single Processor Systems (Continued)

Inter graph TD-1 (486DX266) Inter graph TD-2 (P-66) Inter graph TD-3 (P-90) Inter graph TD-30 (P-90)^{12}

Inves BS-486-VS i486 DX2-50

Leading Edge Fortiva Series 3000 (486DX2-50) Leading Edge Fortiva Series 4000 (Cyrix 486DLC-40)^1 Leading Edge Fortiva Series 5000 (486DX2-66) Leading Edge MT 6000 (P-90) Leading Edge MT 6000 T ower (P-90) Leading Edge V alience Desktop DT4000

Metrologie P60 Tower (Intel Xpr ess P-60) Metrologie Pr emier e/PCI P60 Desktop (Intel Mer cury)

Microbus Eur opean Data Systems iBOX (486DX-33)^{13}

Micron 486PCI MAGNUM (486 DX4/100) Micron Home MPC (P-90) Micron Millennia 100 (P-100) Micron Millennia PLUS (P-133) Micron P90PCI PowerStation^{14} Micron P90PCI PowerStation Mini-T ower, Plug and Play (P-90)

Midwest Micr o P5-75 PCI Midwest Micr o P5-100 PCI Midwest Micr o P5-120 PCI Midwest Micr o Minitower P5-90

NCR 3333 (486DX2/66)

Single Processor Systems (Continued)

System Platforms 11

Olivetti M4-82^{15} Olivetti M6-420 Olivetti M6-440^{16} Olivetti M6-450^{16} Olivetti M6-460^{16} Olivetti M6-640^5 Olivetti M6-750^{15,17} Olivetti M6-760^{15,17} Olivetti M6-770^{15,17} Olivetti M6-850^{1,5} Olivetti M6-860^5 Olivetti M6-880^5 Olivetti SNX-140^{1,5} Olivetti SNX-160UP (P-90)

Omegabyte SolarST ATION 4 (P-90) Omegabyte SolarST ATION 5 (P-100) Omegabyte SolarST ATION 6 (P-120) Omegabyte SolarST ATION 7 (P-133)

Packar d Bell Axcel Series^{18} Packar d Bell Executive Series^{18} Packar d Bell For ce Series^{18} Packar d Bell Legend Series^{18} Packar d Bell Pack-Mate Series^{18} Packar d Bell PRO Series^{18}

Peacock-AG A T 486 DX-40 Professional Plus Desktop Peacock-AG LAN-Station A T 486 DX-40 LN4

Resear ch Machines PC-425S (486SX/25) Resear ch Machines PC-450S Accelerator (486SX2-50) Resear ch Machines PC-560 Accelerator (P-60) Resear ch Machines PC-590 Pr ofessional (P-90)^{19}

Samsung Magic Power SPC8500 Samsung Magic Power SPC8500 (P-133) Samsung Magic Power SPC8500P A (P-133) Samsung SWS 520/90 (P-90) Samsung SWS 520/100 (P-100) Samsung SWS 520/133 (P-133)

Siemens ANL Siix Server 1 (486 DX2-50)

Single Processor Systems (Continued)

Siemens Nixdorf AG PCD-5H (P-133 Desktop) Siemens Nixdorf PCD-4H/VL (486 DX2-50) Siemens Nixdorf PCD-4H/VL (486 DX2-66) Siemens Nixdorf PCD-4H/PCI (486 DX2-66) Siemens Nixdorf PCD-5H (P-60 PCI)^{20} Siemens Nixdorf PCD-5H (P-90) Siemens Nixdorf PCD-5T Siemens Nixdorf PCE-5S

TAKAOKA Electric MiNT PC590d2 Desktop (P-90) TAKAOKA Electric MiNT PC590t2 T ower (P-90)

TAGRAM Platinum (P-66) TAGRAM ThunderBolt (P-66)

Toshiba J-3100 PV (486SX-25 ODP) Toshiba J-3100 PV2 (486DX2-66)

Tulip 4-Series DE PCI (486DX2-66) Tulip 5-Series DE PCI (P-90) Tulip 4-Series DE EISA (486DX2-66) Tulip 4-Series DS PCI (486DX2-66) Tulip 5-Series DS PCI (P-90) Tulip 4-Series DS EISA (486DX2-66) Tulip 4-Series DT ISA (486DX2-66) Tulip 4-Series DT PCI (486DX2-66) Tulip 5-Series DT PCI (P-90) Tulip 4-Series TR EISA (486DX2-66)

Unisys U6000/DT2 Unisys U6000/100 Unisys U6000/300

Viglen Contender Pr ofessional 4DX266 Viglen Genie PCI Pr ofessional 4DX266 Viglen Genie PCI P5-133 Viglen Genie PCI T ower P5-90

WellStone SWS 5090 (P-90)

Wyse Decision 486se Wyse Decision 486Gsi (DX2/66) Wyse Series 6000i Model 650 Wyse Series 6000i Model 665

Single Processor Systems (Continued)

12 Solaris 2.4 x86 Hardware Compatibility List— March 1996

1. Requir es substituting the video car d with one supported by Solaris 2.4 .

2. Requir es substituting the network car d with one supported by Solaris 2.4 .

3. Must use a CD-ROM drive supported by Solaris 2.4 .

4. This model is an MP server but has only been tested with one CPU.

5. Server System. Integrated video curr ently only works in 640x480 VGA

mode.

6. Requir es non-default BIOS settings for pr oper operation.

7. The thr ee-disk CD-ROM changer is not supported at this time.

8. Select “Trident 9000” when configuring the display adapter , and be sur e to

upgrade the video RAM on the motherboar d.

9. System must be upgraded to a minimum of 1-Mbyte video memory and a

minimum 32-Mbytes system memory .

10.Some versions may r equir e a futur e Driver Update to support integrated

video due to a manufactur er’s part change.

11.This machine r equir es a patch to work when L2 cache is enabled.

Zenith Data Systems Z-Select 100 XE Minitower (486DX2- 66) Zenith Data Systems Z-Select PT (P-60) Zenith Data Systems Z-Station 510 Minitower (486DX4-

100) Zenith Data Systems Z-Station EX Model II (P-90) Zenith Data Systems Z-Station GT (P-75) Zenith Data Systems Z-Station GT 5100 Zenith Data Systems Z-Station GT 5120 Zenith Data Systems Z-Station GT 5133 (P-133) Zenith Data Systems Z-Station VP (486DX4/100) Zenith Data Systems Z-Station VP (P-90) Zenith Data Systems Z-Station VP (P-100) Zenith Data Systems Z-Station VP (P-120) Zenith Data Systems Z-Station VP (P-133) Zenith Data Systems Z-Server EX P90E Model 1000 Zenith Data Systems Z-Server EX P90E Model 1000A Zenith Data Systems Z-Server L T 433DE Model 1000 Zenith Data Systems Z-Server L T 433DE Model 1000A Zenith Data Systems Z-Server L T 450DE Model 1000 Zenith Data Systems Z-Server L T 450DE Model 1000A Zenith Data Systems Z-Server L T 466XE Model 1000 Zenith Data Systems Z-Server L T P60E Model 1000 Zenith Data Systems Z-Server L T P60E Model 1000A Zenith Data Systems Z-Server MX (P-100) Zenith Data Systems Z-Server MX+Mylex (P-100) Zenith Data Systems Z-Server WG P90 (P-90)

Single Processor Systems (Continued)^{12.PC Car d support is planned for a futur e Driver Update.}

13.The design of the Cache contr oller r equir es that you map out the memory range used by the SCSI contr oller or the system will not work; the on-boar d hardwar e watchdog cir cuit R39 must also be disabled.

14.Warning: FLASH BIOS must be write-pr otected before attempting to install the Solaris softwar e; remove jumper JP9 on the motherboar d and use BIOS revision -10 or later .

15.Only tested with vendor ’s ATI Mach32 video option.

16.Integrated audio chip not curr ently supported.

17.Must set Adaptec SCSI BIOS to addr ess cc000.

18.This series of machines comes in various models and configurations. If the FCC ID label on the back panel of your machine contains one of the three-digit codes 430, 450, 470, 520, or 550, then it is based on a platform that was tested for compatibility and should r un Solaris 2.4 x86. However , ensur e that other optional equipment and subsystems on your specific model ar e listed in this document.

19.The newer version of this system had BIOS compatibility issues at the time of test. Also, attach the CD-ROM to the primary IDE channel.

20.Built-in ATIvideo car d curr ently only supported in 43-Hz mode.

System Platforms 13

Multiprocessor Systems (SMP)^1

Acer AcerAltos 7000/P (2 CPUs, P-90) Acer AcerFrame Model 3000MP (2 CPUs)

ALR Evolution V ST e/75 (2 CPUs P-75) ALR Evolution Q/MP2 100 (2 CPUs P-100) ALR Proveisa SMP (2 CPUs) ALR Revolution MP Pentium 90 (2 CPUs) ALR Revolution MP/100 (2 CPUs P-100) ALR Revolution Q-SMP Pentium/90 (2, 3, & 4 CPUs) ALR Revolution Q-SMP Pentium/100 (2 CPUs) ALR Revolution Q-SMP Pentium/100 (4 CPUs)

American Megatr ends T itan-II PCI EISA (2 CPUs)

AST Manhattan SMP 486/33 (4 CPUs) AST Manhattan SMP P/60 (4 CPUs) AST Manhattan P5090 (2 CPUs, P-90)^2 AST Manhattan P5100 (Dual) AST Manhattan P5133 (Dual) AST Manhattan V5090 (2 CPUs, P-90)^2 AST Manhattan V5100 (Dual) AST Premmia GX (2 CPUs, P-90) Integrated E-IDE AST Premmia GX (2 CPUs, P-90) Integrated SCSI AST Premmia GX (2 CPUs, P-100) AST Premmia GX (2 CPUs, P-133)

AT&T GIS Globalyst 540 (4 CPUs, P-100)

Austin Dir ect Affinity SE (2 CPUs, P-90)

C&S Vertriebs GmbH AMICUS Strategy (2 CPUs, P-133) C&S Vertriebs GmbH (Dual P5-90 EISA-PCI)

Compaq Pr oLiant 2000 (2 CPUs, P-90) Compaq Pr oLiant 4000 (4 CPUs, P-90)

DEC Celebris XL 590DP (2 CPUs, P-90) DEC Prioris HX 590DP (2 CPUs, P-90)

Dell OptiPlex DGX 590 (2 CPUs, P-90) Dell OptiPlex DGX 5100 (2 CPUs, P-100) Dell OptiPlex DGX 5120 (2 CPUs, P-120) Dell PowerEdge SP 5100-2 (2 CPUs, P-100) Dell PowerEdge XE 590-2 with DSA (2 CPUs, P-90)

Diversified T echnology (DTI) LBE-4520 DP (2 CPUs, P-90)

DTK QUIN-52M DP90 (2 CPUs, P-90)

EIS Computers “The Developer” (2 CPUs, P-90 MP) EIS Computers “The Developer” (2 CPUs, P-100 MP) EIS Computers “The Server” (2 CPUs, P-90 MP) EIS Computers “The Server” (2 CPUs, P-100 MP)

Elonex MT-5133-I (2 CPUs, P-133)

Everex Step DP (2 CPUs, P-90)

Hitachi FLORA 3010DV (2 CPUs, P-90) Hitachi FLORA 3100BP (2 CPUs, P-90) Hitachi FLORA 3100LP (8 CPUs, P-100) Hitachi FLORA 3100SP (2 CPUs, P-90)^3

HP NetServer 5/66 LM-2 (2 CPUs)^2 HP Vectra XU 5/90c (2 CPUs, P-90)^4

IBM PC Server 320 Model 8640-MXT (2 CPUs, P-75) IBM PC Server 320 Model 8640-OYT (2 CPUs, P-90)

Intel ALTserver (Altair) (2 CPUs, P-100) Intel OEM Extended Xpr ess (4 CPUs, P-100) Intel Xpr ess (4 CPUs, P-100) Intel Xpr ess Dual Pentium 60 (2 CPUs) Intel Xpr ess Dual Pentium 66 (2 CPUs)

Inter graph ISP32 (2 CPUs, P-90) Inter graph ISMP22 (2 CPUs, P-90) Inter graph ISMP32 (2 CPUs, P-90) Inter graph ISMP6 (6 CPUs, P-100) Inter graph TD-4 (2 CPUs, P-90) Inter graph TD-4 (2 CPUs P-100) Inter graph TD-40 (2 CPUs, P-100) Inter graph TD-5 (2 CPUs, P-90)

Micron PowerServer SMP (P-90) Micron PowerServer SMP (P-133)

Olivetti SNX-160MP (2 CPUs, P-90)

Peacock-AG LAN-Server Model SSE 8332 (Dual Pentium 66 Intel Xpr ess)

Multiprocessor Systems (SMP)^1 (Continued)

14 Solaris 2.4 x86 Hardware Compatibility List— March 1996

1. The number of CPUs following each entry indicates the number of

processors in the MP system as tested.

2. Only tested in VGA mode due to integrated video memory size.

3. Must use a CD-ROM drive supported by Solaris 2.4.

4. Some versions may r equir e a futur e Driver Update to support integrated

video due to a manufactur er’s part change.

5. Contact T ricord customer support at 1-800-TRICORD for information on

how to obtain the latest r elease notes.

6. Must upgrade the system BIOS to V3.03.

Samsung SWS 520/90 (2 CPUs, P-90) Samsung SWS 520/100 (2 CPUs, P-100) Samsung SWS 520/133 (2 CPUs, P-133) Samsung Magic Power SPC 8500-P (2 CPUs, P-90) Samsung Magic Power SPC 8500-P (2 CPUs, P-100) Samsung Magic Power SPC 8500-P (2 CPUs, P-133)

Siemens Nixdorf PCD-5T/PCI90de (2 CPUs, P-90) Siemens Nixdorf AG PCD-5T (2 CPUs, P-100) Siemens Nixdorf PCE-5Smp (4 CPUs, P-100)

Tricord PowerFrame Enterprise Server ES3000^5 (4 CPUs) Tricord PowerFrame Enterprise Server ES4000^5 (6 CPUs) Tricord PowerFrame Enterprise Server ES5000^5 (6 CPUs)

Unisys 5400 (2 CPUs, P-100) Unisys 6000/500 Model 20 (2 CPUs)^6

Wyse Series 7000i Model 760MP (4 CPUs) Wyse 7000-760MP DX2-66 (3 CPUs) Wyse 7000-765MP P66 (2 CPUs)

Zenith Data Systems Z-Server EX DP66E Model 1000 (2 CPUs) Zenith Data Systems Z-Server WG P90 (2 CPUs P-90)

Multiprocessor Systems (SMP)^1 (Continued)

System Platforms 15

Notebook Computers^1

The following notebook computers have been certified for standard Solaris operation. Although some specific portable/nomadic computing capabilities have been provided in Solaris, not all of the features and devices found on these notebooks are currently supported. For information on this support, see the online document Solaris 2.4 x86 Notebook Supplement Guide. For specific device support, refer to the tables on PC Card/PCMCIA peripherals in this Hardwar e Compatibility List. Note that installation (booting) using PCMCIA devices is not curr ently supported.

Ambra SN425C^{2,3}

AST Ascentia 800N 486SX/33^3 AST Ascentia 900N 4/50^3 AST Ascentia 900N 4/75^3 AST Ascentia 910N (486DX2/50)^4 AST Power Exec 4/33 ColorPlus^3

Compaq L TE 4/25C^3 Compaq L TE 4/33^3 Compaq L TE Elite 4/75 CX (486DX4-75)

Dell Latitude XP (DX4-100)^5

Ergo Powerbrick PN312/TFT (486DX4-100)^3

Everex StepNote (486DX4-100)^3

Fujitsu FMV -450NL/S (SL DX2-50)

Gateway 2000 ColorBook 486DX4-75^3

IBM ThinkPad 750^3 IBM ThinkPad 750C^3 IBM ThinkPad 755C DX2/50^3

NEC Versa/33 NEC Versa/50

Panasonic CF-V21P^3

SiO Technologies FT -500 DX2/66^3

Tadpole 1000

Texas Instr uments 4000E^3

1. For specific details on installing the Solaris 2.4 operating

envir onment on notebook computers, see Solaris 2.4 x86 Notebook Supplement Guide (order number ISOS-240-FP3-NBS).

2. Keyboar d contr oller pr oblem af fects installation. See Solaris 2.4 Open Issues and Late-Breaking News.

3. Not tested with PC Car d (PCMCIA).

4. The dual-scan model is only supported in 640x480 r esolution, VGA, 800x600 panning mode.. The active matrix model works with the standar d PMI file wd90c26am.pmi; the kdmconfig selection is “Toshiba 4600c or AST 4/33 SL: WD9026 256 Color TFT .”

5. To use this system, after the PC Car d (PCMCIA) portion of Solaris 2.4 x86 Driver Update 7 (or later ) is installed, you must edit the file

/kernel/drv/pcic.conf, changing the line
res-memory=0xcc000,0x24 to res-memory=0xdc000,0x24.

6. Requir es special configuration to install Solaris; only comes with a

120-Mbyte disk.

7. Some har dwar e configuration may be r equir ed to install Solaris. See Solaris 2.4 Open Issues and Late-Breaking News.

8. CAUTION: Some thir d-party memory expansion (PC Car d) has been found to fail with the Solaris system. Use actual T oshiba or high-grade thir d-party memory .

Toshiba T1950CT Toshiba 2400CT Toshiba T3400^6 Toshiba T3600 Toshiba T4400C^7 Toshiba T4600^7 Toshiba T4700C^7 Toshiba T4850CT (486DX4-100) Toshiba T4800^7 Toshiba T4900CT (P-75)^8 Toshiba DynaBook SS475 051CT (486DX4-75) Toshiba DynaBook SS475-JP Toshiba Portege 610CT Toshiba Satellite Pr o 400CDT (P-75) Toshiba Satellite Pr o T2150CDT (486DX4-75)^8 Toshiba Satellite Pr o T2450CT (486DX4-75)^8

Twinhead Slimnote II (486E)^3

Zenith Data Systems Z-Note^3 Zenith Data Systems Z-Noteflex^3

Notebook Computers^1 (Continued)

16 Solaris 2.4 x86 Hardware Compatibility List— March 1996

Supported Devices

Devices listed in this section have been successfully tested with Solaris 2.4 x86 in a varied but limited number of har dwar e configurations. While a complete system composed of the devices listed in this section should enable you to install and r un the Solaris softwar e, some combinations of devices may not be usable or may r equir e additional configuratio n.

SCSI Host Bus Adapters

Vendor Model

Acculogic PCIpport Model 20

Adaptec AHA-1510A AHA-1520A AHA-1522A AHA-1530P/1532P AHA-1540B/1542B AHA-1540C/1542C AHA-1540CF/1542CF AHA-1540CP/1542CP AHA-1640/1642 AHA-1740/1742A AHA-2740/2742 AHA-2740-T/2742-T AHA-2740A/2742A AHA-2740A-T/2742A-T AHA-2740W AHA-2840A/2842A AHA-2840VL/2842VL AHA-2940/2940W AHA-2940U/2940UW AHA-3940/3940W (PCI) AIC-6260 AIC-6360 AIC-7770, AIC-7770 Rev. E AIC-7850 AIC-7870

Adaptec, cont. The EISA SCSI Master II The PCI SCSI Master Kit The PCI Ultra W ide SCSI Master Kit The SCSI Bus Master Host

Adapter Kit The SCSI Channel The SCSI Dir ection The SCSI Master Kit The SCSI Micr o Channel Host Adapter Kit The VL SCSI Master

AMD PCscsi PCscsi II PCnet-SCSI

BusLogic BT-440C (VLB) BT-445C (VLB) BT-445S (VLB) BT-542B (ISA) BT-545C (ISA) BT-545S (ISA) BT-742A (EISA) BT-746C (EISA) BT-747C (EISA) BT-747S (EISA) BT-757S (EISA) BT-946C (PCI) BT-956C (PCI)

Compaq 32-bit Fast-SCSI-2 (NCR 53C710) 32-bit Fast-W ide SCSI-2/P Integrated 32-bit Fast-SCSI-2 (NCR 53C710) Integrated 32-bit Fast-SCSI-2/P Integrated 32-bit Fast-W ide SCSI-2/E Integrated 32-bit Fast-W ide SCSI-2/P

Creative Labs Sound Blaster 16 SCSI-2

SCSI Host Bus Adapters (Continued)

Vendor Model

Supported Devices 17

1. This adapter does not have the SDMS BIOS on boar d. It should be

used only on a system that contains the SCSI BIOS as part of its main system BIOS..

2. Wide SCSI not yet supported in Solaris driver .

DPT PM-2011 PM-2012B PM-2021 PM-2022 PM-2022 PM-2124 PM-2124

DTC DTC-3130 (PCI)^1

Hitachi PC-CS7210 (PCI)

IBM PS/2 Micr o Channel SCSI SCSI-2 Fast/W ide Adapter/A

Intel PCISCSI (NCR 53C825)^2 PCISCSINR (NCR 53C810)

P.E. Logic Corp PEL-1620

Siemens Nixdorf

PCE-5S (NCR 53C710)

Symbios Logic NCR 53C810 NCR 53C815 NCR 53C820^2 NCR 53C825^2

Trantor T348 MiniSCSI Plus Parallel

Tricord Intelligent SCSI Subsystem Contr oller

SCSI Host Bus Adapters (Continued)

Vendor Model

SCSI RAID Controllers

Vendor Model

Compaq SMART SCSI Array Contr oller

DEC Digital Storage W orks RAID Array (EISA)

Dell Dell SCSI Array (DSA)

DPT SmartRAID PM-3222 SmartRAID PM-3224

HP HP Disk Array/HP Disk System

IBM SCSI-2 RAID Adapter (MCA) SCSI-2 Fast/W ide Str eaming- RAID Adapter/A (PCI & MCA)

Mylex DAC960 DAC960P (PCI)

Solid State SCSI Disk Devices

Vendor Model

Imperial T echnology MegaRam (268 MB version)

CD-ROM Drives

Vendor Model Type

Chinon CDS-435 CDS-525 CDS-535^1

SCSI SCSI SCSI

Digital Storage 8422IDE ATAPI/IDE

Goldstar GCD-R320B GCD-R520B

SCSI ATAPI/IDE

Hitachi CDR-1900S CDR-3750 CDR-6750

SCSI SCSI SCSI

Lion Optics XC200SI SCSI

18 Solaris 2.4 x86 Hardware Compatibility List— March 1996

LMSI CM214 CM215

SCSI SCSI

Mitsumi CRMC-FX001DE CRMC-FX400

ATAPI/IDE ATAPI/IDE

NEC MultiSpin 2V i MultiSpin 3Xe^2 MultiSpin 3Xi^2 MultiSpin 4Xe^{1, 2} MultiSpin 4Xi^{1, 2} MultiSpin 6Xi MultiSpin 3Xp Plus Intersect CDR-74 Intersect CDR-84 CDR-210^2 CDR-211 CDR-250 CDR-260 CDR-260R CDR-271 CDR-272 Rev. 4.15 CDR-510

ATAPI/IDE SCSI SCSI SCSI SCSI SCSI SCSI SCSI SCSI SCSI SCSI ATAPI/IDE ATAPI/IDE ATAPI/IDE ATAPI/IDE ATAPI/IDE SCSI

Panasonic LK-MC509S LK-MC579B

SCSI ATAPI/IDE

Panasonic/

Matsushita

CR-572B ATAPI/IDE

Philips CM207 CM215 CM425A

ATAPI/IDE SCSI SCSI

Pioneer DRM-604X^{1, 3} SCSI

Plextor DM3028 PX-43CE (4.5 Plex) PX-43CH (4 Plex) PX-45CH PX-43CS PX-45CS PX-63CS (6 Plex) PX-65CS (6 Plex)

SCSI SCSI SCSI SCSI SCSI SCSI SCSI SCSI

CD-ROM Drives (Continued)

Vendor Model Type

1. Various CD-ROM players may not be fully SCSI-compliant in their

handling of the CDROMREADHEADER command. This may cause failur es from vold not mounting an eligible CD-ROM. The workar ound is to mount the CD-ROM manually .

Reveal 4X Internal ATAPI/IDE

Sanyo CRD-254P CDR-400I CDR-H93RMV

ATAPI/IDE SCSI SCSI

Sanyo-TORiSAN CDR-S1G ATAPI/IDE

Sony CDU-55E CDU-55S^4 CDU-76E CDU-76S CDU-77E CDU-561 CDU-6211 CDU-6811 CDU-7211 CDU-7811 CDU-8012

ATAPI/IDE SCSI ATAPI/IDE SCSI ATAPI/IDE SCSI SCSI SCSI SCSI SCSI SCSI

Sun Micr osystems SunCD SCSI

Texel DM3024 DM3028 DM5021 DM5024 DM5028

SCSI SCSI SCSI SCSI SCSI

Toshiba 4101-TA 5201B TXM-3201 TXM-3301 TXM-3401 TXM-3701 XM-3501B XM-3601B XM-5302B

SCSI SCSI SCSI SCSI SCSI SCSI SCSI SCSI ATAPI/IDE

Wearnes CDD-120^5 ATAPI/IDE

CD-ROM Drives (Continued)

Vendor Model Type

Supported Devices 19

2. Early versions of NEC firmwar e wer e not fully SCSI-compliant; thus these

drives may only work if synchr onous negotiation and disconnect ar e disabled on the SCSI adapter used with the CD-ROM drive, or if the drive is jumper ed to use scsi-1 commands, as appr opriate.

3. Only the first CD-ROM in the Pioneer DRM-604X CD-ROM changer is

supported by default.

4. This drive does not work with the Adaptec AHA-2940 SCSI HBA.

5. Must have BIOS 1.0 or later . 1. Vendor supplies CDR softwar e. Old version for Solaris 2.1 works correctly in command-line mode. GUI does not yet operate on Solaris 2.4 or 2.5.

CDR CD-ROM W riters/Recorders

Vendor Model

Young Minds Inc. CD STUDIO with Kodak PCD Writer 200^1

Audio Devices

Vendor Model

Creative Labs Sound Blaster 16 Sound Blaster 16 SCSI-2 Sound Blaster A WE32 Sound Blaster Pr o

20 Solaris 2.4 x86 Hardware Compatibility List— March 1996

1. Device driver softwar e and support is supplied by the vendor .

Telephone Call Processing

Vendor Model Description

Dialogic Corporation^1 D/21D D/4D D/41E D/121A D/121B D/240SC D/320SC D/240SC-T1 FAX/40 FAX/120 VR/40 VR/121 VR/160 VR/160C DTI/21 1 DTI/212 LSI/120 LSI/180 DMX MSI

2 POTS lines voice and tone r ecognition 4 POTS lines voice and tone r ecognition 4 POTS lines 12-port voice and tone r ecognition, and pr ocessing boar d 12-port voice and tone r ecognition, and pr ocessing boar d 24-channel voice stor e and forwar d 32-channel voice stor e and forwar d 32-channel voice stor e and forwar d, with T -1 Fax daughter card, 4 channel, for D/41 12-channel Fax for D/121 boar ds Multiline speech r ecognition daughterboar d, 4 port Multiline speech r ecognition daughterboar d, 12 port Multiline speech r ecognition daughterboar d, 16 port Multiline speech r ecognition daughterboar d, 16 port Digital Trunk Interface, North American T -1 Digital Trunk Interface, Eur opean E-1 Loop Start Interface boar d Loop Start Interface boar d Digital Multiplexor Expansion boar ds Modular Station Interface boar d, 24 port

Supported Devices 21

1. Solaris drivers for this vendor ’s devices ar e available dir ectly

from the vendor .

2. Solaris drivers and support for this vendor ’s devices ar e available

directly from the vendor .

Multiport Serial Adapters

Vendor Model

Aur ora^1 401A (ISA 4 Port)

CHASE^1 IOPRO (ISA 8 Port)

COMPUT ONE^1 IntelliServer SVR-16DB (16 Port)

COMTROL^1 Rocketport (16 Port)

DigiBoar d^1 PC/Xem (ISA, EISA) EPC/X (ISA, EISA) C/X2 (ISA, EISA) PC/8eV e AccelePort (ISA)

MILAN^2 FastPort 3100CX PrintServer FastPort 3200C PrintServer FastPort 3400C PrintServer

Moxa^1 MOXA-C218 (ISA 8 Port) MOXA-C320 (ISA 32 Port)

Specialix^1 SI/8 A T XIO/8 A T

Systech^1 Parallex SCS-2008I (ISA 8 Port)

Network Adapters — Ethernet

Vendor Name/Model

3Com EtherLink II, II/16 (3C503, 3C503-16) EtherLink 16, 16TP (3C507, 3C507-TP) EtherLink III (3C509, 3C509B, 3C529, 3C579) EtherLink III PCMCIA (3C589, 3C589B)

Accton EN1625 (ISA) EtherCombo-16 (ISA)^1

Allied Telesis

AT-1500AT-Plus (ISA) AT-1500BT-Plus (ISA)

Alta EtherCombo-16 T/C (ISA)^{1, 2}

AMD PCnet-ISA contr oller chip PCnet-PCI contr oller chip

Asante AsanteF AST 10/100

Cabletr on E-2210 (ISA)

CNet CN970EBT (PCI)

Cogent EM100 (PCI) EM110TX (PCI)^3 EM960C (PCI)^4 EM960TP (PCI)

Compaq Netflex-2 DualPort ENET Netflex-2 ENET -TR Contr oller

Compex ENET32-PCI

D-Link DE-510CT (VLB) DE-530CT (PCI)^4

Intel EtherExpr ess FlashC (PCLA8105) EtherExpr ess16 (PCLA8110) EtherExpr ess16 TP (PCLA8120) EtherExpr ess16C (PCLA8100) EtherExpr ess MCA (MCLA81 10) EtherExpr ess MCA TP (MCLA8120) EtherExpr ess 32 EtherExpr ess Flash32 (82596) EtherExpr ess PRO EtherExpr ess PRO/100 (82556)

22 Solaris 2.4 x86 Hardware Compatibility List— March 1996

Kingston KNE-2000T+ (ISA)^2 KNE-2002+ (ISA)^2 KNE-2031+ (ISA)^2 KNE-2121+ (ISA) KNE-2121H (ISA)

Microdyne NE2000 (ISA)

Mitron LX2100p (PCI)

National Semicond.

Infomover NE2000 Plus (ISA)^2

Novell/ Eagle Tech.

NE2000 (ISA) NE2000 Plus (ISA)^2 NE3200 (EISA)

Olicom EtherCom ISA/II^2

Racal Interlan

ES3210/ES3210 TP Ethernet^5 PCI T2-STR

Samsung SEB-3000C (PCI)

SMC Elite32C Ultra (EISA) Ether 10/100 (9232) (EISA) EtherCar d PLUS (8003) EtherCar d PLUS Elite (8013) EtherCar d PLUS Elite16 (8013) EtherCar d Elite16 Ultra (8216) EtherCar d Elite32T (8033T) EtherEZ (8416) EtherPower 8432BT/8432BT A (21040) (PCI)^4 EtherPower 8432BT/8432BT A (21041) (PCI)^4 EtherPower (9332) (PCI)^6

SVEC FD0421-P Rev. A-1 (ISA) FD0455 EtherBoar d-PCI NE2100 (ISA)

Thomas Conrad

NE2000 (ISA)

Network Adapters — Ethernet (Continued)

Vendor Name/Model

1. Card misdetects 8-bit slot.

2. Some NE2000plus clones may only work in I/O or shar ed memory mode, depending on the system or configuration, while r unning Solaris softwar e.

3. 100 Mbps only: 10 Mbps operation is not supported on the EM1 10TX under the curr ent Driver Update.

4. AUI medium is not supported curr ently. BNC medium is not available during initial network installation. Refer to the “DEC 21040, 21041, 21 140 Ethernet” device configuration page in the curr ent Solaris 2.4 x86 Driver Update Guide for additional information .

5. Only the newer versions of these car ds ar e supported. The versions successfully tested have stickers with the numbers 625-0367-00 and 625-0369-00; older versions of the car d, for example, those with the number 625-0136-00, do not work.

6. 10 Mbps operation is not available during initial network installation. Refer to the “DEC 21040, 21041, 21 140 Ethernet” device configuration page in the curr ent Solaris 2.4 x86 Driver Update Guide for additional information .

Unisys EISA Ethernet contr oller (Intel 82596) U6000/DT2 integrated Ethernet contr oller (Intel 82596)

Xircom Pocket Ethernet Adapter III (PE3)

Znyx EtherAction ZX312 (PCI)^4 EtherXtend ZX342 10/100 (PCI)^6

Network Adapters — Ethernet (Continued)

Vendor Name/Model

Supported Devices 23

1. 100 Mbps only: 10 Mbps operation is not supported on the EM1 10TX

under the curr ent Driver Update.

2. 10 Mbps operation is not available during initial network

installation. Refer to the “DEC 21040, 21041, 21 140 Ethernet” device configuration page in the curr ent Solaris 2.4 x86 Driver Update Guide for additional information.

3. AUI medium is not supported curr ently. BNC medium is not

available during initial network installation. Refer to the “DEC 21040, 21041, 21140 Ethernet” device configuration page in the curr ent Solaris 2.4 x86 Driver Update Guide for additional information.

Network Adapters — Fast Ethernet

Vendor Name/Model

Asante AsanteF AST 10/100

Cogent EM100 (PCI) EM110TX (PCI)^1

Intel EtherExpr ess PRO/100 (82556)

SMC Ether 10/100 (9232) (EISA) EtherPower 10/100 (9332) (PCI)^2

Znyx EtherAction ZX312 (PCI)^3 EtherXtend ZX342 10/100 (PCI)^2

Network Adapters — FDDI

Vendor Name/Model

Cabletr on F-7069

Network Adapters — Token Ring

Vendor Name/Model

3Com TokenLink III (3C619, 3C629, 3C679)

IBM Token Ring 16/4 Adapter/A

1. Driver softwar e and support for this device ar e available

directly from the vendor .

High-Speed Networking

Vendor Name/Model

ADAX^1 APC-EIX T-1 Network Interface Boar d (EISA)

PC Card (PCMCIA) — Adapters

Vendor Name/Model

Cirrus Logic

PD6710/PD6720

Intel 82365SL

Ricoh RF5C366

Toshiba

Vadem VG365/VG465/VG468/ VG469

PC Card (PCMCIA) — Add-On Boards

Vendor Name/Model

Hytec HCD 22 SCM Microsys.

SwapBox Classic SwapBox Pr emium

24 Solaris 2.4 x86 Hardware Compatibility List— March 1996

PC Card (PCMCIA) — Modems

Vendor Name/Model

APEX Data

PCA-1414 (Data/Fax)

AT&T Paradyne

371-B1-001 (14.4 Data/Fax)

Boca- Modem m144pa (14.4bps V32bis Data/Fax)

DataRace RediCar d Version 1 (V.32bis/V .42/V.42bis Fax/Data) RediCar d Version 2 (V.32bis/V .42/V.42bis Fax/Data)

Hayes Optima 144

IBM 24TTMOD-W14 (14.4 Data/Fax) 87G9800 (V.32bis/V .42/V.42bis Fax/Data)

Intel 110-US (2400 Data)

Kingston DataRex 87G9851 (V.32bis/V .42/V.42bis Fax/Data)

Megahertz CC3144 (V.32bis/V .42/V.42bis Fax/Data) XJ114 (V.32bis/V .42/V.42bis Fax/Data) XJ124FM (V.32bis/V .42/V.42bis Fax/Data) XJ214 (V.32bis/V .42/V.42bis Fax/Data) XJ2288 (V.32bis/V .42/V.42bis Fax/Data)

SMART Modular Tech.

SmartExchange 9624 Fax/Modem

Supra COMcar d 144 (V.32bis/V .42/V.42bis Fax/Data) US Robotics

Sun/USR W orldPort (V .32bis/V .42/V.42bis Fax/Data/V oice)

PC Card (PCMCIA) — Serial Cards

Vendor Name/Model

IBM IBM RS-332 Serial Car d

Socket Communication

SL0700 (RS-332)

PC Card (PCMCIA) — SRAM Memory Cards

Vendor Name/Model

Epson NB70-004268 NB70-004269 NB70-004270

IBM 0.5 MB SRAM Car d 1 MB SRAM Car d 0933155 (2 MB SRAM)

Magic Ram SR1MBP100 SR2MBP100

Mitsubishi MF3513-L5DAT MF31M1-L5DAT MF32M1-L5DAT

SMART Modular Technologies

SM9SRD512KP3 SM9SRD1MP3 SM9SED2MP3 SM9SRDA1MP3 SM9SRDA2MP3

Supported Devices 25

1. Select “Micr osoft 2-button mouse” during installation of Solaris

softwar e.

Pointing Devices

Vendor Model

Alps Electric Glidepoint, version 100797-00

Appoint Thumbelina^1 MousePen Pr o^1

CH Pr oducts RollerMouse

Dyna Point DynaTrak^1

IBM PS/2 2-button Easy Options Mouse^1

Interlink PortaPoint^1

Kraft Systems MicroTrack^1

Logitech C7 serial and bus mouse devices C9 serial and bus mouse

devices 2-Button^1 MouseMan serial and bus

mouse devices MouseMan cor dless TrackMan serial and bus

mouse devices

Microsoft Serial, bus, and PS/2 mouse devices

MicroSpeed MicroTRAC trackball

Mouse Systems Mouse! New Mouse PC Mouse II

26 Solaris 2.4 x86 Hardware Compatibility List— March 1996

Tape Drives — SCSI^1

Vendor Model

Archive 2150S 150 MB 2525 QIC-525 Python 28454 4mm Viper

Exabyte EXB-4200 4mm EXB-8200 EXB-8500 EXB-8505 8mm

HP Colorado Memory Systems PowerT ape 1100 QIC Colorado Memory Systems

PowerT ape 2400 QIC Colorado Memory Systems

PowerT ape 4000 QIC Colorado Memory Systems

PowerDA T 6000 4mm 35470A DDS 4mm 35480A DDS/Data

Compr ession 4mm C1533-00100 DDS2/Data

Compr ession 4mm C1534A DDS Tape Drive 4mm C1536A DDS/Data

Compr ession 4mm C1520E JetStore 2000e 4mm C1520E JetStore 2000i 4mm JetStore 5000e 4mm C1526E JetStore 5000i 4mm C1529A JetStor e 5000i 4mm C1528E 4mm

1. The tape drives in this table have been tested with the st tape driver softwar e. The tape drives wer e tested using the Legato Tape Exer ciser pr ogram to verify basic functionality and general compatibility with Solaris 2.4 x86.

HP, cont C1520F SureStore Tape 2000e 4mm C1525F SureStore Tape

2000i 4mm C1521F SureStore Tape

5000e 4mm C1526F SureStore Tape

5000i 4mm C1551A Sur eStore Tape

5000eU 4mm C1529F SureStore Tape

6000e 4mm C1528F SureStore Tape

6000i 4mm C1552A Sur eStore Tape

6000eU 4mm

Sony SDT-5000 4mm SDT-5200 4mm Sun Microsystems x660A 150 MB QIC x814A 5.0 GB 8mm x822A 4mm x6101A 2.5 GB QIC SCSI x6102A 2.5 GB QIC SCSI x6103A 2.5 GB QIC SCSI

Tandber g Panther 525S TDC 3820 TDC 4120 TDC 4220 TDC 4222

WangDA T 3400DX DDS-2 4mm

Wangtek 51000 QIC 5525ES QIC 9500DC QIC

Tape Drives — SCSI^1 (Continued)

Vendor Model

Supported Devices 27

SCSI RAID T ape

Vendor Model

ANDATACO Rapid Tape Array

Uninterruptable Power Supplies (UPS)

The following UPS products have been tested in the vendor’s labs. SunSoft has tested the software on selected models to ensure basic operation under Solaris 2.4 x86.

APC Back-UPS 200 APC Back-UPS 280 APC Back-UPS 400 APC Back-UPS 450 APC Back-UPS 600 APC Back-UPS 900 APC Back-UPS 1250

APC Back-UPS Pr o 280 APC Back-UPS Pr o 420 APC Back-UPS Pr o 650 APC Back-UPS Pr o 1000 APC Back-UPS Pr o 1400

APC Smart-UPS 250 APC Smart-UPS 400 APC Smart-UPS 600 APC Smart-UPS 900 APC Smart-UPS 1250 APC Smart-UPS 2000

28 Solaris 2.4 x86 Hardware Compatibility List— March 1996

Motherboards

These are individual motherboards that have been tested as components; see page7 for a list of System Platforms.

AIR 486ET VESA/EISA (Sis chipset) AIR 54CEP (P-90/100) AIR 54CDP (2 x P-90/100)

American Megatr ends T itan-II PCI EISA (2 CPUs)

AMI Atlas PCI (P-100) AMI Voyager with 486DX2-66 CPU AMI Super V oyager PCI AMI Super V oyager II VLB AMI Titan II (2 CPUs, P-90) AMI Enterprise III with 486DX2-66 CPU AMI Enterprise IV

ASUS PCI/E-P54NP4 (2 CPUs P-90) ASUS PCI/I-486SP3G (DX33, SX, DX2-66, OverDrives) ASUS PCI/I-P54NP4 (Dual 2 x P-90) ASUS PCI/I-P54SP4 (P-75, 90, 100) ASUS PCI/I-P54TP4 (P-100) ASUS PCI/I-P55TP4 (T riton) (P-90) ASUS PCI/I-P5SP4 (P-60) ASUS PCI/I-P55TP4XE (P-90) ASUS PVI-486AP4 (486SX/DX/DX2)^1 ASUS PVI-486SP3 (DX33, SX, DX2-66, OverDrives)^1 ASUS VL/EISA-486SV1 (DX33, SX, DX2-66,

OverDrives) ASUS VL/I-486SV2G (486SX/DX/DX2)

DFI G586-VPM (P-90)

DTK FEAT-39 (DX4-100) DTK PKM0038e

GenoaTurbo Expr ess 486VL GenoaTurbo Expr ess 586 PCI-4 GenoaTurbo Expr ess 586VL

Intel Advanced/AL (Aladdin-T riton) (P-90) Intel Advanced/A TX Intel Advanced/EV (Endeavor) (P-100) Intel Advanced/ZE Minitower (P-100) Intel Advanced/ZP (Zappa-T riton) (P-90) Intel Altair (2 CPUs, P-100) Intel ALTserver Altair ( P5-150) Intel ALTserver Altair ( P5-666) Intel ALTserver Altair (2 CPUs, P-100) Intel Extended Expr ess (2 CPUs, P-100) Intel Extended Expr ess (4 CPUs, P-100) Intel Performance AU (P6-180) Intel Performance AU (P6 -200) Intel Pr emier e PCI II Baby A T Board (P-90) (sometimes referred to as Plato)^2 Intel Pr emier e PCI II (P-100) Intel Xpr ess (2 CPUs, P-60) Intel Xpr ess (2 CPUs, P-66) Intel Xpr ess (2 CPUs, P-90)

Motherboards (Continued)

Supported Devices 29

Micronics EISA 486DX (30, 50, 66 CPU) Micronics EISA VLB 486DX (30, 50, 66 CPU) Micronics EISA VLB 486DX2 (30, 50, 66 CPU) Micronics ISA VLB 486DX2 Micronics JX30-WB (486DX4-100) Micronics LPH54 (P-75) Micronics LPH54 (P-90) Micronics LPH54 (P-100) Micronics LPH54 (P-120) Micronics LPH54 (P-133) Micronics LX30-WB (486SX33) Micronics M5PE (P-66) Micronics M5PI (P-66) Micronics M54HI Plus (P-90) Micronics M54HI Plus (P-100) Micronics M54HI Plus (P-120) Micronics M54HI Plus (P-133) Micronics M54HI Plus (P-150) Micronics M54HI Plus (P-166) Micronics M54HI T riton (P-100) Micronics M54PE (1 CPU, P-90)^3 Micronics M54PE (1 CPU, P-100) Micronics M54PE (1 CPU, P-133) Micronics M54PE (2 CPUs, P-90) Micronics M54PE (2 CPUs, P-100) Micronics M54PI (P-90 or P-75) Micronics M54SI (P-75) Micronics M54SI (P-90) Micronics M54SI (P-100) Micronics M54LI-1B (P-90) Micronics M54LI-1B (P-133) Micronics Mpower 4 plus (486DX2-66)

SuperMicr o P55CMS

Tulip TC32 (486DX2-66) Tulip TC40 (486DX2-66) Tulip TC42 (P-90) Tulip TC43 (P-90)

VEGA 486F-3VL with Symphony SL1287, SL82C461,

SL82C362 chipset and 486DX2-66 CPU

Motherboards (Continued)^{1. This boar d does not work pr operly with various PCI SCSI contr ollers, such}

as the Adaptec 2940. It is not r ecommended for use with a SCSI contr oller.

2. Only the version that uses Neptune-2 stepping of the PCI chipset has been tested and certified.

3. This is a dual pr ocessor system, but only works as a single pr ocessor system at this time.

30 Solaris 2.4 x86 Hardware Compatibility List— March 1996

Video Display Adapters

Vendor Model Bus Chipset^{21}

Resolution and Color Depth 800x600 1024x768 1152x900 1280x1024 1600x1200 8 24 8 24 8 24 8 24 8 24 Acer ET4000/W32^1 ISA ET4000/W32 ALR Flyer VL WD90C33 AST Manhattan 5090P^2 — Cirrus Logic 5424 ATI 8514 Ultra ISA ATI Mach8 Graphics Xpr ession PCI ATI Mach64 Graphics Xpr ession VLB ATI Mach64 Graphics Pr o Turbo PCI ATI Mach64 Graphics Pr o Turbo VLB ATI Mach64 Winturbo^3 PCI ATI Mach64 Graphics Ultra ISA ATI Mach8 Graphics Ultra+ ISA ATI Mach32 Graphics Ultra Pr o ISA ATI Mach32 Graphics Ultra Pr o PCI ATI Mach32 Graphics Ultra Pr o VLB ATI Mach32 Mach64 — ATI Mach64 Mach64CT — ATI Mach64CT Mach64CT Rev .2 — ATI Mach64CT VGA Wonder XL ISA ATI Mach8 VGA Wonder XL 24 ISA ATI Mach8 Boca Voyager 64^4 PCI S3 Trio64 Cirrus Logic 5420 chipset w/512Kbyte DRAM 5424 chipset w/512Kbyte DRAM^2 5428 chipset w/512Kbyte VRAM 5430 chipset 5434 chipset 542x chipset Compaq QVision 1024/E EISA TRITON

Supported Devices 31

Compaq, cont QVision 1024/I ISA TRITON QVision 1280 chipset^5 EISA ORION QVision 2000 PCI Matr ox MGA-2 QVision 2000 (Rev. G) PCI Matr ox MGA-3 ProLiant — Cirrus Logic 5420 ProSignia^6 — Cirrus Logic 5420 ProSignia 300 — Cirrus Logic 8424 CompuAdd Hi-Res VGA ISA ET-4000 DEC DECpc XL 590 — Cirrus Logic 5428 Dell DE Series ISA ET-4000 M/ME Series S3 805 L Series ET4000/W32 L Series ET4000/W32i OptiPlex DGX 590 — ATI Mach64 OptiPlex XMT 590 — S3 864 PowerEdge SP5 xx ATI Mach32 Diamond SpeedStar Plus ISA ET4000 SpeedStar 24x ISA WD90C31 SpeedStar Pr o/ SpeedStar Pr o 1100

ISA Cirrus Logic 5426

SpeedStar 64/ SpeedStar 64 Graphics 2000XL Series

ISA/ PCI Cirrus Logic 5434

Stealth VRAM ISA S3 911 Stealth Pr o ISA S3 928 Stealth 24 ISA S3 801 Stealth 32 PCI ET4000/W32p Stealth 32 VLB ET4000/W32p

Video Display Adapters (Continued)

Vendor Model Bus Chipset^{21}

Resolution and Color Depth 800x600 1024x768 1152x900 1280x1024 1600x1200 8 24 8 24 8 24 8 24 8 24

32 Solaris 2.4 x86 Hardware Compatibility List— March 1996

Diamond, cont Stealth 64 DRAM/ Stealth 64 Graphics 2000 Series

PCI/ VLB S3 Vision 864

Stealth 64 DRAM PCI S3 Trio64 Stealth 64 VRAM PCI S3 Vision 964 Stealth 64 VRAM VLB S3 Vision 964 Stealth Video DRAM Stealth 64 Video 2000 Series

PCI/ VLB S3 Vision 868

Stealth64 Video 2001 PCI S3 Vision 765 Stealth Video VRAM/ Stealth 64 Video 3000^7 Series: TI RAMDAC only

PCI S3 Vision 968

Viper PCI PCI Weitek Power 9000 Viper VLB VLB Weitek Power 9000 Viper Pr o PCI Weitek Power 9100 Viper Pr o VLB Weitek Power 9100 Viper SE^8 PCI Weitek Power 9100 ELSA Winner 1000 VLB S3 928 Winner 2000 VLB S3 928 Winner 1000Pr o-VL^9 VLB S3 Vision 864 Winner 2000Pr o-PCI PCI S3 Vision 964 Winner 2000Pr o-VL VLB S3 Vision 964 Everex FIC 864P PCI S3 Vision 864 VGA Trio 64P PCI S3 Trio64 ViewPoint 64P PCI S3 Vision 864 Genoa SuperVGA 7000 Hewlett- Packar d

HP NetServer LC/LE/LF TVGA 9000i

HP Vectra VL2 Cirrus Logic 5428 HP Vectra XM2i S3 Vision 864

Video Display Adapters (Continued)

Vendor Model Bus Chipset^{21}

Resolution and Color Depth 800x600 1024x768 1152x900 1280x1024 1600x1200 8 24 8 24 8 24 8 24 8 24

Supported Devices 33

Hewlett- Packar d, cont.

HP Vectra XU^{10} — S3 Vision 864

IBM Easy Options (VC550)^{11} ISA Cirrus Logic 5428 PC Series 300-486 Cirrus Logic 5430 PC Series 300 S3 Vision 864 PC Series 700 S3 Vision 864 PS/V aluepoint S3 805 PS/V aluePoint Performance Series

S3 Vision 864

VGA^{12} ISA IBM VGA XGA MCA XGA XGA-2 MCA XGA-2 Intel Professional/GX High Resolution

ATI Mach32

Xpress VGA WD90C31 Inter graph TD-1^{13} S3 928 TD-2, TD-3; (G90)^{14} PCI Weitek Power 9000 G91^{15} PCI Weitek Power 9100 G95^{16} PCI STORM ISMP (SMP 224)^{17} Cirrus Logic 5434 Matr ox MGA Impr ession VLB Matr ox MGA-1 MGA Impr ession Plus PCI Matr ox MGA-3 MGA Millenium PCI STORM MGA Ultima VLB Matr ox MGA-2 MGA Ultima Plus PCI Matr ox MGA-2 MGA Ultima Plus 200 PCI Matr ox MGA-2 Micronics Mpower 4 plus — ATI Mach64 Miro miroCRYSTAL 20SD PCI S3 864, S3 SDAC miroCRYSTAL 20SD PCI S3 Vision 864 miroCRYSTAL 40SV PCI S3 Vision 964

Video Display Adapters (Continued)

Vendor Model Bus Chipset^{21}

Resolution and Color Depth 800x600 1024x768 1152x900 1280x1024 1600x1200 8 24 8 24 8 24 8 24 8 24

34 Solaris 2.4 x86 Hardware Compatibility List— March 1996

Miro, cont. miroMagic ISA S3 86C805 Nanao EizoAccel AA51 ISA CHIPS F82C480 Nanao HA50/HL50 ISA S3 928 Nanao HA60 ISA S3 928 Number Nine #9GXE^{18} ISA S3 928 #9GXE^{18} VLB S3 928 #9GXE64 PCI S3 Vision 864 #9GXE64 Pro PCI S3 Vision 964 9FX Motion 531 PCI S3 Vision 868 9FX Motion 771 PCI S3 Vision 968 Imagine 128 PCI Imagine128 Vision330^{19} PCI S3 Trio64 Oak Technology OTI107 PCI OTI107 Orchid Fahrenheit 1280 ISA S3 924 Fahrenheit 1280 Plus ISA S3 801 Fahrenheit 1280 Plus VLB S3 801 Fahrenheit VA ISA S3 801 Kelvin 64 PCI Cirrus Logic 5434 Kelvin 64^{20} VLB Cirrus Logic 5434 Prodesigner IIs ISA ET4000 S3 Trio64 chipset — S3 Trio64 Trio64V+ chipset — S3 Trio64V+ Vision 864+SDAC chipset Vision 868 — S3 Vision 868 SPEA V7-Mirage P-64 PCI S3 868 STB LIGHTSPEED VL VLB ET4000/W32p NITRO PCI PCI Cirrus Logic 5434 PowerGraph 64 PCI S3 Trio64 STB, cont. Power graph 64 V ideo PCI S3 Trio64V+

Video Display Adapters (Continued)

Vendor Model Bus Chipset^{21}

Resolution and Color Depth 800x600 1024x768 1152x900 1280x1024 1600x1200 8 24 8 24 8 24 8 24 8 24

Supported Devices 35

1. The ET4000/W32 video car ds that ar e shipped with Acer machines ar e not all the same; if you encounter any display pr oblems when the OpenW indows envir onment is r unning, try using a dif ferent add-on boar d that is compatible with the Solaris operating envir onment.

2. Video adapters based on the Cirr us Logic 5424 chipset with 512-Kbyte DRAM may not perform well in 800x600x256 mode, particularly if the selected monitor refresh rate is 60 Hz or higher .

3. The ATIWINTURBO model is equivalent to the Gateway A TI GX Mach64 PCI video car d.

4. To support the Boca V oyager 64, select the graphics car d “Trio64 (2 MB)” when configuring the Solaris window system.

5. Used on Compaq QV ision 1280/E Graphics Contr oller and in Compaq Deskpr o 590.

6. The Pr oSignia 300 systems and some models of the Pr oSignia server systems with the Cirr us Logic 5424 graphics chip ar e not supported. However , they may work with the “Cirr us Logic 5424 (512k)” entry listed by the kdmconfig program.

7. For car ds with 70ns VRAM or BIOS r evision 1.01.

8. The Diamond V iper SE is not supported at 76, 80, and 85 Hz in the 1280x1024 r esolution. The r ecommended r efresh rate at this r eolution is 64 Hz. See the Diamond Viper SE manufactur er’s documentation for information on r efresh rates .

9. The ELSA Winner 1000Pr o with the A TT20C498 RAMDAC is supported.

10.Both the ST 1702 and the A TT21C498 RAMDAC ar e supported.

11.Select “Cirr us Logic” when configuring the display adapter during Solaris installation.

12.640x480, 16 colors. Any 256-Kbyte or better VGA adapter supporting standar d IBM mode 0x12 graphics. For VGA with 800x600 virtual scr een, select “16 color , 640x480 VGA panning @800x600 (for experts only , see docs)” when configuring the display adapter during Solaris installation. Warning : This selection enables panning mode on a standar d VGA. This video mode supports a virtual r esolution of 800x600, but is only capable of physically displaying 640x480 pixels at a time. This may be a pr eferred mode to use on small scr eens, but the use of panning may r equir e some training. See x86 Device Configuration Guide for mor e information.

13.To support 1 152x900 or 1280x1024 resolution on the Inter graph TD-1 display adapter , you must select an interlaced monitor type when configuring the Solaris window system. Choose “Multifr equency 56KHz (up to 1280x1024 interlaced)” as the monitor type. See Solaris 2.4 x86 Driver Update Guide for mor e information.

14.To support the Inter graph G90 on a 20-inch monitor , select the graphics car d “Diamond V iper with Inter graph 20-inch monitor” when configuring the Solaris window system.

15.The Inter graph G91 also supports a r esolution of 1600x1280 for 8-bit color .

16.To support the Inter graph G95, select the graphics car d “Matr ox MGA Millenium” when configuring the Solaris window system.

17.To support the Inter graph ISMP , select the graphics car d “Cirr us Logic GD5434” when configuring the Solaris window system.

18.The Number Nine #9GXE video display adapters (ISA and VESA local bus) support 24-bit color in 640x480 mode only.

19.Select “#9GXE 64 (Trio64)” when configuring the display adapter during Solaris installation.

20.Older versions of the Or chid Kelvin64 VLB car d have memory addr essing limitations that may cause pr oblems if your system contains 32 Mbytes or mor e of RAM.

See Solaris 2.4 x86 Driver Update Guide for further information.

PowerGraph ERGO ISA ET4000 PowerGraph PRO PCI PCI S3 Vision 864 Toshiba J3100 — Western Digital 90C31A Trident TVGA 8900C ISA Trident TVGA 9000i 8900C Western Digital Paradise Accelerator ISA WD90C31

Video Display Adapters (Continued)

Vendor Model Bus Chipset^{21}

Resolution and Color Depth 800x600 1024x768 1152x900 1280x1024 1600x1200 8 24 8 24 8 24 8 24 8 24

36 Solaris 2.4 x86 Hardware Compatibility List— March 1996

21.The information in the chipset column does not guarantee that video boar ds made by another manufactur er using the same chipset will work. Only the specific models listed by V endor , Model, Bus, and Chipset have been tested.

“— ” in the Bus column indicates a video contr oller model that is used on video display adapters and motherboar ds..

Supported Devices 37

1. Note that almost any notebook can also be used with a 800x600

virtual scr een.

2. Select “T3400ct,T4700ct,T4800ct,Twinhead 486E, ThinkPad 750:

WD90C24 w/1Mb” when configuring the display adapter during Solaris installation.

Notebook Display V ideo Support (640x480, 256 colors)^1

Ambra SN425C^2

AST PowerExec 4/33SL

Compaq L TE 4/25C Compaq L TE 4/33C

Ergo Power Brick

IBM ThinkPad 750C IBM ThinkPad 750 (with external monitor)

NEC Versa/33 NEC Versa/50 NEC Versa M75C NEC Versa M75HC

Panasonic CF-V21P^2

TI TravelMate 4000E TFT

Toshiba T3400 Toshiba T4400C Toshiba T4600C Toshiba T4700C Toshiba T4800 Toshiba 4900CT

Twinhead Slimnote 486E

Note – For a list of Notebook Computers that have been tested with the Solaris 2.4 operating envir onment, see page 15.

Notebooks W ith External Monitor V ideo Support (1024x768, or 800x600, 16 colors)

AST PowerExec 4/33SL

IBM ThinkPad 750 IBM ThinkPad 750C

NEC Versa/50 (800x600 only) NEC Versa M75C (also supported at 640x480 ) NEC Versa M75HC (also supported at 640x480)

Toshiba 4900CT (also supported at 640x480) Toshiba T4600C Toshiba T4700C

38 Solaris 2.4 x86 Hardware Compatibility List— March 1996

Copyright 1996 Sun Micr osystems Inc., 2550 Gar cia Avenue, Mountain V iew, Californie 94043-1 100, U.S.A.Tous dr oits réservés.

Ce pr oduit ou document est pr otégé par un copyright et distribué avec des licences qui en r estreignent l’utilisation, la copie, la distribution, et la décompilation. Aucune partie de ce pr oduit ou de sa documentation associée ne peut êtr e reproduite sous aucune forme, par quelque moyen que ce soit, sans l’autorisation préalable et écrite de Sun et de ses bailleurs de licence, s’il y en a.

Des parties de ce pr oduit pourr ont êtr e dérivées du système UNIX^® licencié par Novell, Inc. et du système Berkeley 4.3 BSD licencié par l’Université de Californie. UNIX est une mar que enr egistrée aux Etats-Unis et dans d’autr es pays et licenciée exclusivement par X/Open Company Ltd. Le logiciel détenu par des tiers, et qui compr end la technologie r elative aux polices de caractèr es, est pr otégé par un copyright et licencié par des fournisseurs de Sun.

Sun, Sun Micr osystems, le logo Sun, Solaris, et OpenW indows sont des mar ques déposées ou enr egistrées de Sun Micr osystems, Inc. aux Etats-Unis et dans d’autr es pays. T outes les mar ques SPARC, utilisées sous licence, sont des mar ques déposées ou enregistrées de SP ARC International, Inc. aux Etats-Unis et dans d’autr es pays. Les pr oduits portant les mar ques SPARC sont basés sur une ar chitectur e développée par Sun Micr osystems, Inc.PostScript et Display postScript sont des mar ques d’Adobe Systems, Inc. Pentium est une mar que d’Intel Corporation

Les interfaces d ’utilisation graphique OPEN LOOK^® et Sun™ ont été développées par Sun Micr osystems, Inc. pour ses utilisateurs et licenciés. Sun reconnaît les efforts de pionniers de Xer ox pour la r echerche et le développement du concept des interfaces d’utilisation visuelle ou graphique pour l’industrie de l’informatique. Sun détient une licence non exclusive de Xerox sur l’interface d’utilisation graphique, cette licence couvrant aussi les licenciés de Sun qui mettent en place l’interface d’utilisation graphique OPEN LOOK et qui en outr e se conforment aux licences écrites de Sun.

Le système X W indow est un pr oduit du X Consortium, Inc.

CETTE PUBLICATION EST FOURNIE “EN L ’ETAT” SANS GARANTIE D’AUCUNE SOR TE, NI EXPRESSE NI IMPLICITE, Y COMPRIS, ET SANS QUE CETTE LISTE NE SOIT LIMIT ATIVE, DES GARANTIES CONCERNANT LA V ALEUR MARCHANDE, L ’APTITUDE DES PRODUITS A RÉPONDRE A UNE UTILISA TION PARTICULIERE, OU LE FAIT QU’ILS NE SOIENT P AS CONTREFAISANTS DE PRODUITS DE TIERS.