DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10388 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An XBC link was found to be not connected while testing CSR traffic traversability. Data field: (xbcNum 32) | (portNum 48).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An XBC link was found to be not connected while testing CSR traffic traversability. Data field: (xbcNum 32) | (portNum 48).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An XBC link was found to be not connected while testing CSR traffic traversability. Data field: (xbcNum << 32) | (portNum << 48)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10389 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error reading Skyline ALREC_ALB_ID CSR. Data field: (Skyline port) | (Cell number 56).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error reading Skyline ALREC_ALB_ID CSR. Data field: (Skyline port) | (Cell number 56).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error reading Skyline ALREC_ALB_ID CSR Data field: (Skyline port) | (Cell number << 56)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10390 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A circular route was found while testing XBC CSR traffic traversability. Data field: (target XBC 32) | (cellNum 56).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A circular route was found while testing XBC CSR traffic traversability. Data field: (target XBC 32) | (cellNum 56).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A circular route was found while testing XBC CSR traffic traversability. Data field: (target XBC << 32) | (cellNum << 56)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10391 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error reading ALREC_ALB_ID CSR for an XBC port. Data field: (xbcNum 32) | (portNum 48).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error reading ALREC_ALB_ID CSR for an XBC port. Data field: (xbcNum 32) | (portNum 48).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error reading ALREC_ALB_ID CSR for an XBC port. Data field: (xbcNum << 32) | (portNum << 48)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10392 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An XBC-XBC port had an invalid chip type connection. Data field: (expected chip type) | (actual chip type 32).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An XBC-XBC port had an invalid chip type connection. Data field: (expected chip type) | (actual chip type 32).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An XBC-XBC port had an invalid chip type connection. Data field: (expected chip type) | (actual chip type << 32)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10393 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event ArfIsXbcRouteTraversable was called on a back-to-back system which is an improper use of the function. Data field: unused'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event ArfIsXbcRouteTraversable was called on a back-to-back system which is an improper use of the function. Data field: unused: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='ArfIsXbcRouteTraversable was called on a back-to-back system which is an improper use of the function. Data field: unused'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10394 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event In ArfIsXbcRouteTraversable, an XBC-XBC link was found to have fatal errors. Data field: (xbcNum 32) | (portNum 48).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event In ArfIsXbcRouteTraversable, an XBC-XBC link was found to have fatal errors. Data field: (xbcNum 32) | (portNum 48).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='In ArfIsXbcRouteTraversable, an XBC-XBC link was found to have fatal errors. Data field: (xbcNum << 32) | (portNum << 48)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10395 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unable to read the XBC ROUTE_TABLE_ENABLE_MASK CSR. Data field: (xbcNum 32) | (portNum 48).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unable to read the XBC ROUTE_TABLE_ENABLE_MASK CSR. Data field: (xbcNum 32) | (portNum 48).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Unable to read the XBC ROUTE_TABLE_ENABLE_MASK CSR. Data field: (xbcNum << 32) | (portNum << 48)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10396 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error reading an XBC ROUTE_TABLE CSR. Data field: route index | (xbcNum 32) | (portNum 48).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error reading an XBC ROUTE_TABLE CSR. Data field: route index | (xbcNum 32) | (portNum 48).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error reading an XBC ROUTE_TABLE CSR. Data field: route index | (xbcNum << 32) | (portNum << 48)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10397 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error reading ALB ALREC_ALB_ID CSR for an XBC port. Data field: (xbcNum 32) | (portNum 48).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error reading ALB ALREC_ALB_ID CSR for an XBC port. Data field: (xbcNum 32) | (portNum 48).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error reading ALB ALREC_ALB_ID CSR for an XBC port. Data field: (xbcNum << 32) | (portNum << 48)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10398 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An XBC port was found with an unexpected neighbor chip. Data field: expected chip type | (actual chip type 32).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An XBC port was found with an unexpected neighbor chip. Data field: expected chip type | (actual chip type 32).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An XBC port was found with an unexpected neighbor chip. Data field: expected chip type | (actual chip type << 32)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10401 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A cell/port pair was not found in the expected graph data. Data field: (cellNum 32) | CC portNum.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A cell/port pair was not found in the expected graph data. Data field: (cellNum 32) | CC portNum.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A cell/port pair was not found in the expected graph data. Data field: (cellNum << 32) | CC portNum'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10402 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Arches Fabric Traversability code unexpectedly found the local cell link not connected. Data field: linkState (0 = connected, 1 = link pending, 2 = not connected, -1 = error)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Arches Fabric Traversability code unexpectedly found the local cell link not connected. Data field: linkState (0 = connected, 1 = link pending, 2 = not connected, -1 = error): &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Arches Fabric Traversability code unexpectedly found the local cell link not connected. Data field: linkState (0 = connected, 1 = link pending, 2 = not connected, -1 = error)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10403 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error reading the ROUTEx CSR on the XBC. Data field: route index | (xbcNum 32) | (portNum 48).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error reading the ROUTEx CSR on the XBC. Data field: route index | (xbcNum 32) | (portNum 48).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error reading the ROUTEx CSR on the XBC. Data field: route index | (xbcNum << 32) | (portNum << 48)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10404 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unable to read the ALB ALREC_ALB_ID CSR for an XBC port. Data field: (xbcNum 32) | (portNum 48).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unable to read the ALB ALREC_ALB_ID CSR for an XBC port. Data field: (xbcNum 32) | (portNum 48).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Unable to read the ALB ALREC_ALB_ID CSR for an XBC port. Data field: (xbcNum << 32) | (portNum << 48)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10405 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An XBC port has an unexpected neighbor chip type. Data field: expected neighbor chip type | (actual neighbor chip type 32).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An XBC port has an unexpected neighbor chip type. Data field: expected neighbor chip type | (actual neighbor chip type 32).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An XBC port has an unexpected neighbor chip type. Data field: expected neighbor chip type | (actual neighbor chip type << 32)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10406 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A Cell-Cell link has an unexpected neighbor chip type. Data field: expected neighbor chip type | (actual neighbor chip type 32).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A Cell-Cell link has an unexpected neighbor chip type. Data field: expected neighbor chip type | (actual neighbor chip type 32).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A Cell-Cell link has an unexpected neighbor chip type. Data field: expected neighbor chip type | (actual neighbor chip type << 32)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10407 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The cell/port pair does not exist in the Arches Fabric expected graph data. Data field: CC port | (cellNum 32).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The cell/port pair does not exist in the Arches Fabric expected graph data. Data field: CC port | (cellNum 32).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The cell/port pair does not exist in the Arches Fabric expected graph data. Data field: CC port | (cellNum << 32)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10408 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A Cell-Cell link is connected to an unexpected neighbor port. Data field: expected neighbor port | (actual neighbor port 32).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A Cell-Cell link is connected to an unexpected neighbor port. Data field: expected neighbor port | (actual neighbor port 32).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A Cell-Cell link is connected to an unexpected neighbor port. Data field: expected neighbor port | (actual neighbor port << 32)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10409 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A Cell-Cell link is connected to an unexpected cell. Data field: expected neighbor ID | (actual neighbor ID 16) | (target cell 32) | (local cell 48).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A Cell-Cell link is connected to an unexpected cell. Data field: expected neighbor ID | (actual neighbor ID 16) | (target cell 32) | (local cell 48).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A Cell-Cell link is connected to an unexpected cell. Data field: expected neighbor ID | (actual neighbor ID << 16) | (target cell << 32) | (local cell << 48)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10412 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An EFI driver failed to load.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An EFI driver failed to load.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An EFI Driver may be corrupt.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10413 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event VM_FindAllRoutes returned an unexpected error duing Non-Coherent table setup. Data field: (return value) | (source cell 32) | (target cell 48).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event VM_FindAllRoutes returned an unexpected error duing Non-Coherent table setup. Data field: (return value) | (source cell 32) | (target cell 48).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='VM_FindAllRoutes returned an unexpected error duing Non-Coherent table setup. Data field: (return value) | (source cell << 32) | (target cell << 48)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10414 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event In SetupNCTable, a write to the GLOBAL_LINK_SEL_NONCOH CSR failed. Data field: (data written to CSR) | (actual CSR data read 32).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event In SetupNCTable, a write to the GLOBAL_LINK_SEL_NONCOH CSR failed. Data field: (data written to CSR) | (actual CSR data read 32).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='In SetupNCTable, a write to the GLOBAL_LINK_SEL_NONCOH CSR failed. Data field: (data written to CSR) | (actual CSR data read << 32)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10415 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event SetupNCTable failed in ArfPhase3. Data field: cell set passed in to SetupNCTable'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event SetupNCTable failed in ArfPhase3. Data field: cell set passed in to SetupNCTable: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='SetupNCTable failed in ArfPhase3. Data field: cell set passed in to SetupNCTable'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10427 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A failure occurred while prepping a back-to-back system for post-rendezvous Arches Fabric setup. Data field: return value from Phase4BackToBackPrep.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A failure occurred while prepping a back-to-back system for post-rendezvous Arches Fabric setup. Data field: return value from Phase4BackToBackPrep.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A failure occurred while prepping a back-to-back system for post-rendezvous Arches Fabric setup. Data field: return value from Phase4BackToBackPrep'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10429 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event ArfPhase4 was unable to set up the Non-Coherent lnk select to at least one cell in its alive/gsm sharing set. Data field: bitmap of unreachable cells.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event ArfPhase4 was unable to set up the Non-Coherent lnk select to at least one cell in its alive/gsm sharing set. Data field: bitmap of unreachable cells.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='ArfPhase4 was unable to set up the Non-Coherent lnk select to at least one cell in its alive/gsm sharing set. Data field: bitmap of unreachable cells'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10431 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unable to set the Non-Coherent route. Data field: (sourceCell 32) | (cell set passed in to SetupNCTable).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unable to set the Non-Coherent route. Data field: (sourceCell 32) | (cell set passed in to SetupNCTable).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Unable to set the Non-Coherent route. Data field: (sourceCell << 32) | (cell set passed in to SetupNCTable)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10432 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unable to setup the Coherent route table for a cell in our partition. Data field: (sourceCell 32) | (cell set passed in to SetupCohTable).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unable to setup the Coherent route table for a cell in our partition. Data field: (sourceCell 32) | (cell set passed in to SetupCohTable).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Unable to setup the Coherent route table for a cell in our partition. Data field: (sourceCell << 32) | (cell set passed in to SetupCohTable)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10435 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error writing the XBC ROUTE_TABLE_ENABLE_MASK CSR. Data field: (route set to disable) | (xbcNum 32) | (xbc port 48).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error writing the XBC ROUTE_TABLE_ENABLE_MASK CSR. Data field: (route set to disable) | (xbcNum 32) | (xbc port 48).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error writing the XBC ROUTE_TABLE_ENABLE_MASK CSR. Data field: (route set to disable) | (xbcNum << 32) | (xbc port << 48)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10436 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The Arches Fabric vertex module returned an unexpected error duing Non-Coherent table setup. Data field: (return value) | (sourceCell 32) | (dest cell 48).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The Arches Fabric vertex module returned an unexpected error duing Non-Coherent table setup. Data field: (return value) | (sourceCell 32) | (dest cell 48).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Arches Fabric vertex module returned an unexpected error duing Non-Coherent table setup. Data field: (return value) | (sourceCell << 32) | (dest cell << 48)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10439 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A write to a Skyline Global LINK_SEL_COHx CSR failed. Data field: cell number of the Skyline that failed.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A write to a Skyline Global LINK_SEL_COHx CSR failed. Data field: cell number of the Skyline that failed.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A write to a Skyline Global LINK_SEL_COHx CSR failed. Data field: cell number of the Skyline that failed, bits [7:0]. Other bits unused'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10475 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unable to write the XBC port scratch CSR with the routing state. Data field: (routing state) | (xbcNum 32) | (portNum 48).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unable to write the XBC port scratch CSR with the routing state. Data field: (routing state) | (xbcNum 32) | (portNum 48).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Unable to write the XBC port scratch CSR with the routing state. Data field: (routing state) | (xbcNum << 32) | (portNum << 48)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10481 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event System Firmware was unable to access the configured set stored in the complex profile.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event System Firmware was unable to access the configured set stored in the complex profile.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Couldn t get the configured set during Fabric Init'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10482 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event System Firmware detected an error during Fabric Init.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event System Firmware detected an error during Fabric Init.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error while running the Arches Fabric API part of Fabric Init.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10483 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event System Firmware detected a failure during Fabric Init.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event System Firmware detected a failure during Fabric Init.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failure while running the Fabric API part of Fabric Init.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10487 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event System Firmware detected an error during Fabric Optimize.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event System Firmware detected an error during Fabric Optimize.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error was encountered while running the Fabric API to optimize the fabric.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10489 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Input power to the specified UPS has failed.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Input power to the specified UPS has failed.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Input power to the specified UPS has failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10490 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Input power to the specified UPS has been restored.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Input power to the specified UPS has been restored.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Input power to the specified UPS has been restored.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10495 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event UPS power exhausted. The system is being powered down.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event UPS power exhausted. The system is being powered down.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The system is being powered down as UPS power is exhausted.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10509 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event During Machine Check handling, SAL failed to rendezvous all the processors.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event During Machine Check handling, SAL failed to rendezvous all the processors.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='During SAL Machine Check handling, SAL fail to round up all the processor entering SAL Machine check handler.'

