DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11569 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event IO Backplane +12V power fault'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event IO Backplane +12V power fault: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='IO Backplane +12V power fault'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11575 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event IO Backplane 1.5V temperature fault'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event IO Backplane 1.5V temperature fault: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='IO Backplane 1.5V temperature fault'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11576 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event IO Backplane 3.3V temperature fault'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event IO Backplane 3.3V temperature fault: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='IO Backplane 3.3V temperature fault'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11578 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event IO Backplane -12.0V temperature fault'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event IO Backplane -12.0V temperature fault: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='IO Backplane -12.0V temperature fault'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11579 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event IO Backplane +12.0V temperature fault'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event IO Backplane +12.0V temperature fault: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='IO Backplane +12.0V temperature fault'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11580 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The local cell was unable to clear the link_off bit on at least one CC-CC link. Data field: return value of Phase3BackToBackPrep()'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The local cell was unable to clear the link_off bit on at least one CC-CC link. Data field: return value of Phase3BackToBackPrep(): &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The local cell was unable to clear the link_off bit on at least one CC-CC link. Data field: return value of Phase3BackToBackPrep()'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11581 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event ArfOLAPreRendez() was unable to reach the added cell. Data field: bitmap of unreachable cells'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event ArfOLAPreRendez() was unable to reach the added cell. Data field: bitmap of unreachable cells: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='ArfOLAPreRendez() was unable to reach the added cell. Data field: bitmap of unreachable cells'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11582 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An unexpected error occurred in SetupNCTable(). Data field: return value from SetupNCTable().'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An unexpected error occurred in SetupNCTable(). Data field: return value from SetupNCTable().: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An unexpected error occurred in SetupNCTable(). Data field: return value from SetupNCTable()'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11583 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Phase4BackToBackPrep() unexpectedly failed. Data field: return value of Phase4BackToBackPrep()'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Phase4BackToBackPrep() unexpectedly failed. Data field: return value of Phase4BackToBackPrep(): &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Phase4BackToBackPrep() unexpectedly failed. Data field: return value of Phase4BackToBackPrep()'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11584 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unable to synch graphs between all cells in the partition after an OLA. Data field: (master cell number 56) | (bitmap of cells to synch).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unable to synch graphs between all cells in the partition after an OLA. Data field: (master cell number 56) | (bitmap of cells to synch).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Data field: (master cell number << 56) | (bitmap of cells to synch)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11585 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Data field: bitmap of unreachable cells.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Data field: bitmap of unreachable cells.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Data field: bitmap of unreachable cells.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11586 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An unexpected error occurred while setting up the Non-Coherent or Coherent tables after an OLA. Data field: return value from SetupNCTable() or SetupCohTable()'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An unexpected error occurred while setting up the Non-Coherent or Coherent tables after an OLA. Data field: return value from SetupNCTable() or SetupCohTable(): &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Data field: return value from SetupNCTable() or SetupCohTable()'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11597 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event ArfRouteEnable() returned an unexpected error while enabling routes to the local cell. Data field: (local cell number 56) | (bitmap of routes to enable)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event ArfRouteEnable() returned an unexpected error while enabling routes to the local cell. Data field: (local cell number 56) | (bitmap of routes to enable): &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Data field: (local cell number << 56) | (bitmap of routes to enable)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11598 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event ArfRouteDiable() returned an unexpected error while disabling routes during an OLA operation. Data field: (bitmap of cells 32) | (bitmap of routes to disable)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event ArfRouteDiable() returned an unexpected error while disabling routes during an OLA operation. Data field: (bitmap of cells 32) | (bitmap of routes to disable): &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Data field: (bitmap of cells << 32) | (bitmap of routes to disable)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11599 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event ArfRouteDiable() returned an unexpected error while disabling routes in ArfPhase4. Data field: (bitmap of source cells 32) | (bitmap of routes to disable).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event ArfRouteDiable() returned an unexpected error while disabling routes in ArfPhase4. Data field: (bitmap of source cells 32) | (bitmap of routes to disable).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Data field: (bitmap of source cells << 32) | (bitmap of routes to disable)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11603 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Memory allocation failed. The data is the size of the memory block which could not be allocated'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Memory allocation failed. The data is the size of the memory block which could not be allocated: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Memory allocation failed. The data is the size of the memory block which could not be allocated.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11604 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Memory locking failed. The data is the size of the memory block which could not be locked'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Memory locking failed. The data is the size of the memory block which could not be locked: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Memory locking failed. The data is the size of the memory block which could not be locked.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11605 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The minimum number of processors required is more than the number available. The data is the number of available processors'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The minimum number of processors required is more than the number available. The data is the number of available processors: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The minimum number of processors required is more than the number available. The data is the number of available processors.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11606 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A syntax error was found while reading the configuration file. The data is the line number of the line where the error was discovered.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A syntax error was found while reading the configuration file. The data is the line number of the line where the error was discovered.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A syntax error was found while reading the configuration file. The data is the line number of the line where the error was discovered.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11607 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The guest operating system performed an operation which could not be handled by the virtual machine. The virtual machine could not continue running the guest so it stopped.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The guest operating system performed an operation which could not be handled by the virtual machine. The virtual machine could not continue running the guest so it stopped.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The guest operating system performed an operation which could not be handled by the virtual machine. The virtual machine could not continue running the guest so it stopped.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11696 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Kernel driver failed to lock memory'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Kernel driver failed to lock memory: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Kernel driver failed to lock memory'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11700 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The code which initializes the MMIO/IOP map found that the table already contained information.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The code which initializes the MMIO/IOP map found that the table already contained information.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The code which initializes the MMIO/IOP map found that the table already contained information.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11702 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An attempt was made to add a PCI bus whith a number greater than the maximum allowed.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An attempt was made to add a PCI bus whith a number greater than the maximum allowed.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An attempt was made to add a PCI bus whith a number greater than the maximum allowed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11703 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The configured CPU generation is not supported'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The configured CPU generation is not supported: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The configured CPU generation is not supported'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11705 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An ISA UART was created without a data structure. A PCI UART structure exists'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An ISA UART was created without a data structure. A PCI UART structure exists: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An ISA UART was created without a data structure. A PCI UART structure exists'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11706 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A TCGETS or TCSETS IOCTL failed. The errno status will be in a subsequent event.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A TCGETS or TCSETS IOCTL failed. The errno status will be in a subsequent event.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A TCGETS or TCSETS IOCTL failed. The errno status will be in a subsequent event.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11707 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A stat call on the PMAN failed. The next event contains the failure errno.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A stat call on the PMAN failed. The next event contains the failure errno.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A stat call on the PMAN failed. The next event contains the failure errno.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11708 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The virtual machine driver could not be opened'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The virtual machine driver could not be opened: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The virtual machine driver could not be opened'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11709 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The virtual machine driver could not create a virtual machine'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The virtual machine driver could not create a virtual machine: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The virtual machine driver could not create a virtual machine'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11710 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Could not create a file system node for communication between the vmm driver and the virtual machine. The next event contains the error from the Unix system call.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Could not create a file system node for communication between the vmm driver and the virtual machine. The next event contains the error from the Unix system call.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Could not create a file system node for communication between the vmm driver and the virtual machine. The next event contains the error from the Unix system call.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11711 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The vm device was created but cannot be opened'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The vm device was created but cannot be opened: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The vm device was created but cannot be opened'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11712 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The virtual machine driver has not been loaded'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The virtual machine driver has not been loaded: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The virtual machine driver has not been loaded'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11718 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An attempt to create a thread on the PMAN has failed. The next event contains the Unix error number.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An attempt to create a thread on the PMAN has failed. The next event contains the Unix error number.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An attempt to create a thread on the PMAN has failed. The next event contains the Unix error number.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11719 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event VM Driver was unable to communicate with virtual machine'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event VM Driver was unable to communicate with virtual machine: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='VM Driver was unable to communicate with virtual machine'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11720 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The configuration file could not be read'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The configuration file could not be read: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The configuration file could not be read'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11721 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Memory allocation for a firmware table has failed. The data contains the name of the firmware table.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Memory allocation for a firmware table has failed. The data contains the name of the firmware table.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Memory allocation for a firmware table has failed. The data contains the name of the firmware table.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11723 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Driver was unable to build map tables'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Driver was unable to build map tables: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Driver was unable to build map tables'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11724 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Reboot failed. The virtual machine will exit.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Reboot failed. The virtual machine will exit.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Reboot failed. The virtual machine will exit.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11775 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event SetupInitialCohTables() returned an error. Data field: (cell set 32) | (return value from SetupInitialCohTables()).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event SetupInitialCohTables() returned an error. Data field: (cell set 32) | (return value from SetupInitialCohTables()).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Data field: (cell set << 32) | (return value from SetupInitialCohTables())'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11780 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Stable store read or write to flash failed.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Stable store read or write to flash failed.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Stable store read or write to flash failed.'

