DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8806 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Means that the error log space in the Nvram has not been allocated.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Means that the error log space in the Nvram has not been allocated.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This chassis code shows that the error log space in the NVRAM has not been allocated for the current error event. This will be emitted out whenever a error section is attempted to be logged without allocation of log space in NVRAM'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8807 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event This indicates the maximum number of logs for the event.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event This indicates the maximum number of logs for the event.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This indicates that the error logs for a particular event type have reached the maximum allowed to be stored in the NVRAM. The event type is indicated in the data field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8814 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event On Line Delete operation was begun but firmware couldn t find a deletable cell'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event On Line Delete operation was begun but firmware couldn t find a deletable cell: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System firmware has been invoked to perform a cell delete operation but no cell in the system appears to be ready for deletion.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8817 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The bulk power system is above its current capacity.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The bulk power system is above its current capacity.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The bulk power supply is overcurrent'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8818 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The bulk specified is warning of a potential thermal problem.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The bulk specified is warning of a potential thermal problem.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Data: Bulk location.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8819 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Malloc failed while trying to process and ERM'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Malloc failed while trying to process and ERM: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error Response Mode code attempted a malloc of heap space that failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8821 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Dimm at physical location in data field is not supported on this platform.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Dimm at physical location in data field is not supported on this platform.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The dimm in the physical location given by the data field is not supported on this platform. The dimm may not be supported by the hardware, or the dimm may not have been properly qualified for this platform.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8828 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The OPTIONS component received a memory allocation error.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The OPTIONS component received a memory allocation error.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The OPTIONS component was unable to allocate NVRAM memory in order to store a non-volatile variable. The storage area for NVRAM options may be full, or there may be undetected corruption.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8837 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A dimm or CPU has is deconfigured or failed testing'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A dimm or CPU has is deconfigured or failed testing: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A dimm or CPU has failed and is not operational for the system. This event is emmitted prior to determining if the cell should be integrated into the Partition.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8839 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The cell will not join the PD'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The cell will not join the PD: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A cpu or dimm error has been detected, and the Complex Profile, Cell Integration Table, Cell integration policy says to not integrate the cell into the PD. The data field is unused, but the cell that emitted this event is the one that did not'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='get integrated.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8842 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The error context in NVM was corrupt'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The error context in NVM was corrupt: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The IO error context is corrupt. This will impair IO error reporting.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8843 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A rope went fatal from the SBA'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A rope went fatal from the SBA: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A rope went fatal from the SBA to the LBA. If all the ropes go fatal the IO subsystem is dead. Any I/O below the rope will not be accessible. The data field gives the physical location of the rope that went fatal. Some ROPE_FATAL conditions'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='will not cause the system to go down. For Example, a rope that has gone fatal during an OLAR operation will only cause warnings to the user, not bring the partition down.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8844 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A PCI bus on the system went fatal.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A PCI bus on the system went fatal.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A PCI bus on the system is fatal. Any device on this bus is unavailable. Firmware was unable to complete card initialization due to an error. Data field contains physical location of failed bus.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8845 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event One of the rope units in the SBA is dead.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event One of the rope units in the SBA is dead.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='One of the rope units in the SBA failed. If all of the rope units fail, then IO will not be available on this cell.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8851 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The System Flash Write Enable bit is incorrectly set and now clearing by PDC'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The System Flash Write Enable bit is incorrectly set and now clearing by PDC: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The System Flash Write Enable bit is incorrectly set and now clearing by PDC. The Data fileld contains the value of PDH Miscellaneous Signal Register read before System Flash bit is cleared.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8855 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Firmware encountered a problem trying to initialize'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Firmware encountered a problem trying to initialize: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System firmware encountered an error while trying to perform an operation during system initialization. This event ID will always be emmitted before an event ID that describes the status of the operation that failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8857 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event This means that all the cpus in the cell did not show up.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event This means that all the cpus in the cell did not show up.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This means that all the cpus in the cell did not show up.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8858 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event This means that all the cells did not rendezvous during the PD rendezvous.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event This means that all the cells did not rendezvous during the PD rendezvous.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This means that all the cells did not rendezvous during the PD rendezvous. The data part will contain the Expected data and the actual mask of the cells that rendezvoused.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8859 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The FW tree sanity check failed during the MCA error processing.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The FW tree sanity check failed during the MCA error processing.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The FW tree sanity check failed during the MCA error processing.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8860 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event This means that the registry sanity check failed during MCA error handling.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event This means that the registry sanity check failed during MCA error handling.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This means that the registry sanity check failed during MCA error handling.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8861 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event This means that MCA occurred while OS_MCA was parforming error recovery.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event This means that MCA occurred while OS_MCA was parforming error recovery.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This means that MCA occurred while OS_MCA was performing error recovery.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8864 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event One of the BT errors occurred that results in abandoning memory dump.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event One of the BT errors occurred that results in abandoning memory dump.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This means that memory dump will be abandoned due to work-around for CN2272. This happens when one of the Blocking timout in the Processor input block of the Cell Controller occurs.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8865 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The firmware tree is not complete and hence there will be no PD rendezvous.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The firmware tree is not complete and hence there will be no PD rendezvous.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The firmware tree is not complete and hence there will be no PD rendezvous.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8872 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event ACPI configuration mismatch across cells in the partition'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event ACPI configuration mismatch across cells in the partition: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The firmware parameter that defines the ACPI configuration is inconsistent in at least one of the cells in the partition.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8873 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed clearing of the XIN_ERR_ORDER_STATUS CSR'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed clearing of the XIN_ERR_ORDER_STATUS CSR: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Writing the XIN_ERR_ORDER_STATUS register of the CC failed. This is some sort of a hardware failure. Data Field: return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8876 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unexpected fabric firmware error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unexpected fabric firmware error: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An unexpected error occurred while initializing the fabric. The firmware is not able to analyze this error. Clues to the cause of this error may be found in the IPMI forward progress log (FPL) either shortly before or after this log entry'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='occurred. The FPL is available from the management processor using the  sl  command. HP-UX also saves these logs in the /var/stm/logs/os directory, and they can be viewed using the slview utility.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8877 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Invalid data read from a CPU module s Processor Information ROM.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Invalid data read from a CPU module s Processor Information ROM.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A value read by the PDHC from a CPU module s Processor Information ROM was not within acceptable limits.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8882 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Invalid paramater when setting cpu frequency ratios'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Invalid paramater when setting cpu frequency ratios: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An invalid parameter was specified when trying to set the cpu bus config register, cpu frequencies ratio field. Valid range is 0xe - 0x17'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8883 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Option block in nvram has a checksum error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Option block in nvram has a checksum error: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The overhead structure of the OPTIONS block in NVRAM has a checksum error.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8894 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CC to CC link did not initialize on the local cell'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CC to CC link did not initialize on the local cell: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='During a cell OLA, the link on the local cell failed to initialize. Data Field: (my cell << 32) | XIN Link State'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8895 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to write the CC link disable register'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to write the CC link disable register: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An attempt to disable the fabric link failed because writing the CC CSR failed. Data Field: (cell << 56) | return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8896 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An unknown backplane type was found'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An unknown backplane type was found: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Could not determine the system type in order to write the appropriate error mask for the fabric link. Data Field: system type'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8897 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error writing the CC link error mask'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error writing the CC link error mask: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failed writing the XIN error mask for CC s fabric link. Data Field: (cell << 56) | return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8898 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to read the CC s fabric link error mask'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to read the CC s fabric link error mask: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Could not read the XIN Link error mask register. Data Field: (cell << 56) | return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8900 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Could not initialize the CC to CC link upon boot.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Could not initialize the CC to CC link upon boot.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The CC to CC link initialization sequence has failed. Data Field: link init status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8906 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An Error occurred trying to notify the MP of the attempted reset.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An Error occurred trying to notify the MP of the attempted reset.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while trying to notify the MP that a reset is about to occure (QPartitionReleaseBIB command). The status is in the data field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8924 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error Data tied to a previous Error Assert event'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error Data tied to a previous Error Assert event: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A software error has occurred. Data field consists of data pertinent to the error. Lab involvement is indicated.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8926 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed disabling the XIN link for a single cell model'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed disabling the XIN link for a single cell model: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A fabric access error occurred while trying to disable the CC to CC link on a single cell Medel system. This cell will halt. Data field: error status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8930 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error while getting the XBC Semaphore'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error while getting the XBC Semaphore: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='While updating the Port State register, the cell could not get the XBC semaphore. Data field is: (Port Num << 44 | XBC num << 32 | return status). Where return status is: (0 Success; -1 Access Failure; -2 Semaphore Owned By Another, -3'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='Semaphore Already Owned; -4 XBC Key Contention)  '

