--MibName=cpqHostOs
-- ****************************************************************************
--
--                  Host Operating System Information
--         Management Information Base for SNMP Network Management
--
--
--      Copyright 1993,2003 Hewlett-Packard Development Company, L.P.
--
--      Hewlett-Packard Company shall not be liable for technical or
--      editorial errors or omissions contained herein. The information in
--      this document is provided "as is" without warranty of any kind and
--      is subject to change without notice. The warranties for HP products
--      are set forth in the express limited warranty statements
--      accompanying such products. Nothing herein should be construed as
--      constituting an additional warranty.
--
--      Confidential computer software. Valid license from HP required for
--      possession, use or copying. Consistent with FAR 12.211 and 12.212,
--      Commercial Computer Software, Computer Software Documentation, and
--      Technical Data for Commercial Items are licensed to the U.S.
--      Government under vendor's standard commercial license.
--
--      Refer to the READMIB.RDM file for more information about the
--      organization of the information in the Compaq Enterprise.
--
--      The Compaq Enterprise number is 232.
--      The ASN.1 prefix to, and including the Compaq Enterprise is:
--           1.3.6.1.4.1.232
--
-- ****************************************************************************


CPQHOST-MIB DEFINITIONS ::= BEGIN

    IMPORTS
        enterprises             FROM RFC1155-SMI
        IpAddress               FROM RFC1155-SMI
        DisplayString           FROM RFC1213-MIB
        OBJECT-TYPE             FROM RFC-1212
        TRAP-TYPE               FROM RFC-1215
        sysName                 FROM RFC1213-MIB;

    compaq              OBJECT IDENTIFIER ::= { enterprises 232 }
    cpqHostOs           OBJECT IDENTIFIER ::= { compaq 11 }
    cpqHoMibRev         OBJECT IDENTIFIER ::= { cpqHostOs 1 }
    cpqHoComponent      OBJECT IDENTIFIER ::= { cpqHostOs 2 }

    cpqHoInterface      OBJECT IDENTIFIER ::= { cpqHoComponent 1 }
    cpqHoInfo           OBJECT IDENTIFIER ::= { cpqHoComponent 2 }
    cpqHoUtil           OBJECT IDENTIFIER ::= { cpqHoComponent 3 }
    cpqHoFileSys        OBJECT IDENTIFIER ::= { cpqHoComponent 4 }
-- The cpqHoIfPhysMap group has been deprecated.
    cpqHoIfPhysMap      OBJECT IDENTIFIER ::= { cpqHoComponent 5 }
    cpqHoSWRunning      OBJECT IDENTIFIER ::= { cpqHoComponent 6 }
    cpqHoSwVer          OBJECT IDENTIFIER ::= { cpqHoComponent 7 }
    cpqHoGeneric        OBJECT IDENTIFIER ::= { cpqHoComponent 8 }
    cpqHoSwPerf         OBJECT IDENTIFIER ::= { cpqHoComponent 9 }
    cpqHoSystemStatus   OBJECT IDENTIFIER ::= { cpqHoComponent 10 }
    cpqHoTrapInfo       OBJECT IDENTIFIER ::= { cpqHoComponent 11 }
    cpqHoClients        OBJECT IDENTIFIER ::= { cpqHoComponent 12 }
    cpqHoMemory         OBJECT IDENTIFIER ::= { cpqHoComponent 13 }
    cpqHoFwVer          OBJECT IDENTIFIER ::= { cpqHoComponent 14 }
    cpqHoHWInfo         OBJECT IDENTIFIER ::= { cpqHoComponent 15 }

    cpqHoOsCommon       OBJECT IDENTIFIER ::= { cpqHoInterface 4 }

-- ****************************************************************************
--   Host OS Information MIB Revision
--   ================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqHostOs Group                (1.3.6.1.4.1.232.11)
--       cpqHoMibRev Group             (1.3.6.1.4.1.232.11.1)
--
--      Implementation of the cpqHoMibRev group is mandatory for all agents
--      supporting the Host OS MIB.
--
--      A Management Agent conforming to this document will return a
--      cpqHoMibRevMajor of one (1) and a cpqHoMibRevMinor of twenty-four (24).
--
-- ****************************************************************************

    cpqHoMibRevMajor OBJECT-TYPE
        SYNTAX  INTEGER (1..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The Major Revision level of the MIB.

            A change in the major revision level represents a major change
            in the architecture of the MIB.  A change in the major revision
            level may indicate a significant change in the information
            supported and/or the meaning of the supported information.
            Correct interpretation of data may require a MIB document with
            the same major revision level."
        ::= { cpqHoMibRev 1 }

    cpqHoMibRevMinor OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The Minor Revision level of the MIB.

            A change in the minor revision level may represent some minor
            additional support, no changes to any pre-existing information
            has occurred."
        ::= { cpqHoMibRev 2 }

    cpqHoMibCondition OBJECT-TYPE
        SYNTAX  INTEGER {
            unknown(1),
            ok(2),              -- default state
            degraded(3),
            failed(4)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The overall condition.

             This object represents the overall status of the server's host
             system represented by this MIB."
        ::= { cpqHoMibRev 3 }

-- ****************************************************************************
--   Host OS Common
--   ==============
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqHostOs Group                (1.3.6.1.4.1.232.11)
--       cpqHoComponent Group          (1.3.6.1.4.1.232.11.2)
--        cpqHoInterface Group         (1.3.6.1.4.1.232.11.2.1)
--         cpqHoOsCommon Group         (1.3.6.1.4.1.232.11.2.1.4)
--
--
--  Implementation of the cpqHoOsCommon group is mandatory for all
--  agents that support the Host OS MIB.
--
-- ****************************************************************************

    cpqHoOsCommonPollFreq OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "The Insight Agent's polling frequency.

            The frequency, in seconds, at which the Insight Agent requests
            information from the device driver.  A frequency of zero (0)
            indicates that the Insight Agent retrieves the information upon
            request of a management station, it does not poll the device
            driver at a specific interval.

            If the poll frequency is zero (0) all attempts to write to this
            object will fail.  If the poll frequency is non-zero,
            setting this value will change the polling frequency of the
            Insight Agent.  Setting the poll frequency to zero (0) will
            always fail.  An agent may choose to fail any request to change
            the poll frequency to a value that would severely impact system
            performance."
        ::= { cpqHoOsCommon 1 }

-- ****************************************************************************
--   Host OS Common Module Table
--   ===========================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqHostOs Group                (1.3.6.1.4.1.232.11)
--       cpqHoComponent Group          (1.3.6.1.4.1.232.11.2)
--        cpqHoInterface Group         (1.3.6.1.4.1.232.11.2.1)
--         cpqHoOsCommon Group         (1.3.6.1.4.1.232.11.2.1.4)
--          cpqHoOsCommonModuleTable   (1.3.6.1.4.1.232.11.2.1.4.2) deprecated
--
-- ****************************************************************************

    cpqHoOsCommonModuleTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqHoOsCommonModuleEntry
        ACCESS  not-accessible
        STATUS  deprecated
        DESCRIPTION
            "A table of software modules that provide an interface to the
            device this MIB describes."
        ::= { cpqHoOsCommon 2 }

    cpqHoOsCommonModuleEntry OBJECT-TYPE
        SYNTAX  CpqHoOsCommonModuleEntry
        ACCESS  not-accessible
        STATUS  deprecated
        DESCRIPTION
            "A description of a software module that provides an interface
            to the device this MIB describes."
        INDEX   { cpqHoOsCommonModuleIndex }
        ::= { cpqHoOsCommonModuleTable 1 }

        CpqHoOsCommonModuleEntry ::= SEQUENCE {
            cpqHoOsCommonModuleIndex       INTEGER,
            cpqHoOsCommonModuleName        DisplayString,
            cpqHoOsCommonModuleVersion     DisplayString,
            cpqHoOsCommonModuleDate        OCTET STRING,
            cpqHoOsCommonModulePurpose     DisplayString
        }

    cpqHoOsCommonModuleIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "A unique index for this module description."
        ::= { cpqHoOsCommonModuleEntry 1 }

    cpqHoOsCommonModuleName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The module name."
        ::= { cpqHoOsCommonModuleEntry 2 }

    cpqHoOsCommonModuleVersion OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..5))
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The module version in XX.YY format.

            Where XX is the major version number and YY is the minor version
            number.  This field will be null (size 0) string if the agent
            cannot provide the module version."
        ::= { cpqHoOsCommonModuleEntry 3 }

    cpqHoOsCommonModuleDate OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (7))
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The module date.

             field  octets  contents                  range
             =====  ======  =======                  =====
               1      1-2   year                      0..65536
               2       3    month                     1..12
               3       4    day                       1..31
               4       5    hour                      0..23
               5       6    minute                    0..59
               6       7    second                    0..60
                            (use 60 for leap-second)


            This field will be set to year = 0 if the agent cannot provide
            the module date.  The hour, minute, and second field will be set
            to zero (0) if they are not relevant.  The year field is set
            with the most significant octet first."
        ::= { cpqHoOsCommonModuleEntry 4 }

    cpqHoOsCommonModulePurpose OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The purpose of the module described in this entry."
        ::= { cpqHoOsCommonModuleEntry 5 }

-- ****************************************************************************
--   Host OS Information Group
--   =========================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqHostOs Group                (1.3.6.1.4.1.232.11)
--       cpqHoComponent Group          (1.3.6.1.4.1.232.11.2)
--        cpqHoInfo Group              (1.3.6.1.4.1.232.11.2.2)
--
--
--      The cpqHoInfo group describes some general information about the
--      host OS.
--
--      Implementation of the cpqHoInfo group is mandatory for all
--      agents supporting the Host OS MIB.
--
-- ****************************************************************************


    cpqHoName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The name of the host operating system (OS)."
        ::= { cpqHoInfo 1 }

    cpqHoVersion OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The version of the host OS."
        ::= { cpqHoInfo 2 }

    cpqHoDesc OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A further description of the host OS."
        ::= { cpqHoInfo 3 }

    cpqHoOsType OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            netware(2),                -- Novell NetWare
            windowsnt(3),              -- Microsoft Windows NT
            sco-unix(4),               -- SCO UNIX
            unixware(5),               -- Novell UnixWare
            os-2(6),                   -- IBM OS/2
            ms-dos(7),                 -- Microsoft DOS
            dos-windows(8),            -- Microsoft DOS + Microsoft Windows
            windows95(9),              -- Microsoft Windows 95
            windows98(10),             -- Microsoft Windows 98
            open-vms(11),              -- Open VMS
            nsk(12),                   -- Non Stop Kernel
            windowsCE(13),             -- Microsoft Windows CE
            linux(14),                 -- Linux
            windows2000(15),           -- Microsoft Windows 2000
            tru64UNIX(16),             -- Tru64 UNIX
            windowsdotNet(17),         -- Microsoft Windows .NET
            windowsdotNet-64-bit(18),  -- Microsoft Windows .NET 64-bit Edition
            solaris(19)                -- Sun Solaris 
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Host Operating system enumeration."
         ::= { cpqHoInfo 4 }

    cpqHoTelnet OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            available(2),
            notavailable(3)             -- default
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "Telnet on socket 23 is available."
--
-- This variable specifies the availability of telnet.  Only socket 23 is
-- checked for telnet services.
--
         ::= { cpqHoInfo 5 }

    cpqHoSystemRole OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "The system role.

            This is a settable free form text field intended to be assigned
            by a remote console briefly describing the system's function."
        ::= { cpqHoInfo 6 }

    cpqHoSystemRoleDetail OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..512))
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "The system detailed description.

            This is a settable free form text field intended to be assigned
            by a remote console describing the system function in detail."
        ::= { cpqHoInfo 7 }

    cpqHoCrashDumpState OBJECT-TYPE
        SYNTAX INTEGER {
            completememorydump(1),
            kernelmemorydump(2),
            smallmemorydump(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Crash dump state.
             Value of 'Unknown (-1)' is returned when crash dump state could 
             not be determined."
        ::= { cpqHoInfo 8 }

    cpqHoCrashDumpCondition OBJECT-TYPE
        SYNTAX INTEGER {
            other(1),           -- (Crash Dump settings unknown or none)
            ok(2),		-- (Crash dump settings OK) and (paging file size >= minimum) and (free disk space >= minimum)
            degraded(3),	-- (Crash dump settings disabled or unknown) or (paging file size < minimum) or (free disk space < minimum)
            failed(4)		-- N/A
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The condition of the Crash dump configuration."
        ::= { cpqHoInfo 9 }

-- ****************************************************************************
--   Host OS CPU Utilization Table
--   =============================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqHostOs Group                (1.3.6.1.4.1.232.11)
--       cpqHoComponent Group          (1.3.6.1.4.1.232.11.2)
--        cpqHoUtil Group              (1.3.6.1.4.1.232.11.2.3)
--         cpqHoCpuUtilTable           (1.3.6.1.4.1.232.11.2.3.1)
--
--
--  The cpqHoUtil group contains measures of system utilization.
--
--  Implementation of the cpqHoUtil group is mandatory for all agents
--  that support the Host OS MIB.
--
-- ****************************************************************************



    cpqHoCpuUtilTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqHoCpuUtilEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A table of CPU utilization entries."
        ::= { cpqHoUtil 1 }

    cpqHoCpuUtilEntry OBJECT-TYPE
        SYNTAX  CpqHoCpuUtilEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A description of a CPU's utilization."
        INDEX   { cpqHoCpuUtilUnitIndex }
        ::= { cpqHoCpuUtilTable 1 }

        CpqHoCpuUtilEntry ::= SEQUENCE {
            cpqHoCpuUtilUnitIndex   INTEGER,
            cpqHoCpuUtilMin         INTEGER,
            cpqHoCpuUtilFiveMin     INTEGER,
            cpqHoCpuUtilThirtyMin   INTEGER,
            cpqHoCpuUtilHour        INTEGER,
            cpqHoCpuUtilHwLocation  DisplayString
        }

    cpqHoCpuUtilUnitIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This number uniquely specifies a processor unit.

            A processing unit may be a set of processing chips that are
            on the same board or for other reasons work together as a unit.
            The main processor unit (if such a concept is valid for this
            machine) will always have the lowest (first) index."
        ::= { cpqHoCpuUtilEntry 1 }

    cpqHoCpuUtilMin OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The CPU utilization as a percentage of the theoretical
            maximum during the last minute.  A value of -1 indicates
            that no CPU utilization information is available for this
            processor."
        ::= { cpqHoCpuUtilEntry 2 }

    cpqHoCpuUtilFiveMin OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The CPU utilization as a percentage of the theoretical
            maximum during the last five minutes.  A value of -1 indicates
            that no CPU utilization information is available for this
            processor."
        ::= { cpqHoCpuUtilEntry 3 }

    cpqHoCpuUtilThirtyMin OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The CPU utilization as a percentage of the theoretical
            maximum during the last thirty minutes.  A value of -1 indicates
            that no CPU utilization information is available for this
            processor."
        ::= { cpqHoCpuUtilEntry 4 }

    cpqHoCpuUtilHour OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The CPU utilization as a percentage of the theoretical
            maximum during the last hour.  A value of -1 indicates
            that no CPU utilization information is available for this
            processor."
        ::= { cpqHoCpuUtilEntry 5 }

    cpqHoCpuUtilHwLocation  OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "A text description of the hardware location, on complex
             multi SBB hardware only, for the CPU.
             A NULL string indicates that the hardware location could not
             be determined or is irrelevant."
        ::= { cpqHoCpuUtilEntry 6 }


-- ****************************************************************************
--   Host OS File System Table
--   =========================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqHostOs Group                (1.3.6.1.4.1.232.11)
--       cpqHoComponent Group          (1.3.6.1.4.1.232.11.2)
--        cpqHoFileSys Group           (1.3.6.1.4.1.232.11.2.4)
--         cpqHoFileSysTable           (1.3.6.1.4.1.232.11.2.4.1)
--
--  The cpqHoFileSys group contains configuration and status information
--  about the file system.
--
-- ****************************************************************************



    cpqHoFileSysTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqHoFileSysEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A table of file system descriptions."
        ::= { cpqHoFileSys 1 }     

    cpqHoFileSysEntry OBJECT-TYPE
        SYNTAX  CpqHoFileSysEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A file system description."
        INDEX   { cpqHoFileSysIndex }
        ::= { cpqHoFileSysTable 1 }

    CpqHoFileSysEntry ::= SEQUENCE {
        cpqHoFileSysIndex              INTEGER,
        cpqHoFileSysDesc               DisplayString,
        cpqHoFileSysSpaceTotal         INTEGER,
        cpqHoFileSysSpaceUsed          INTEGER,
        cpqHoFileSysPercentSpaceUsed   INTEGER,
        cpqHoFileSysAllocUnitsTotal    INTEGER,
        cpqHoFileSysAllocUnitsUsed     INTEGER
    }

    cpqHoFileSysIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "An index that uniquely specifies this entry."
        ::= { cpqHoFileSysEntry 1 }

    cpqHoFileSysDesc OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A description of the file system."
        ::= { cpqHoFileSysEntry 2 }

    cpqHoFileSysSpaceTotal OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The file system size in megabytes.

             This item will be set to -1 if the agent is unable to determine
             this information."
        ::= { cpqHoFileSysEntry 3 }

    cpqHoFileSysSpaceUsed OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The megabytes of file system space currently in use.

             This item will be set to -1 if the agent is unable to determine
             this information."
        ::= { cpqHoFileSysEntry 4 }


    cpqHoFileSysPercentSpaceUsed OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The percent of file system space currently in use.
             This item will be set to -1 if this information is not
             available."

        ::= { cpqHoFileSysEntry 5 }

    cpqHoFileSysAllocUnitsTotal OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The total number of files (directory entries) that can be
             stored on the file system if a limit exists other than
             total space used.  This item will be set to -1 if no such
             limit exists."
        ::= { cpqHoFileSysEntry 6 }

    cpqHoFileSysAllocUnitsUsed OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The number of files (directory entries) on this file system.
            This item will be set to -1 if the agent does not determine this
            information."
        ::= { cpqHoFileSysEntry 7 }


-- ****************************************************************************
--   Host OS Interface Physical Map Table
--   ====================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqHostOs Group                (1.3.6.1.4.1.232.11)
--       cpqHoComponent Group          (1.3.6.1.4.1.232.11.2)
--        cpqHoIfPhysMap Group         (1.3.6.1.4.1.232.11.2.5)    deprecated
--         cpqHoIfPhysMapTable         (1.3.6.1.4.1.232.11.2.5.1)  deprecated
--
--
--  The cpqHoIfPhysMap group contains information to map interface numbers
--  in the MIB-II interface group to the physical interface cards that
--  implement the interface.
--
--  Implementation of the cpqHoIfPhysMap group is mandatory for all agents
--  that support the Host OS MIB.
--
-- ****************************************************************************

    cpqHoIfPhysMapTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqHoIfPhysMapEntry
        ACCESS  not-accessible
        STATUS  deprecated
        DESCRIPTION
            "A table of interface to physical hardware mappings."
        ::= { cpqHoIfPhysMap 1 }

    cpqHoIfPhysMapEntry OBJECT-TYPE
        SYNTAX  CpqHoIfPhysMapEntry
        ACCESS  not-accessible
        STATUS  deprecated
        DESCRIPTION
            "A mapping of an interface table entry to physical hardware."
        INDEX   { cpqHoIfPhysMapIndex }
        ::= { cpqHoIfPhysMapTable 1 }

    CpqHoIfPhysMapEntry ::= SEQUENCE {
        cpqHoIfPhysMapIndex              INTEGER,
        cpqHoIfPhysMapSlot               INTEGER,
        cpqHoIfPhysMapIoBaseAddr         INTEGER,
        cpqHoIfPhysMapIrq                INTEGER,
        cpqHoIfPhysMapDma                INTEGER,
        cpqHoIfPhysMapMemBaseAddr        INTEGER,
        cpqHoIfPhysMapPort               INTEGER,
        cpqHoIfPhysMapDuplexState        INTEGER,
        cpqHoIfPhysMapCondition          INTEGER
    }

    cpqHoIfPhysMapIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "An index that uniquely specifies this entry.  This value is
            equal to the index of the entry in the MIB-II interface table
            to which this entry corresponds."
        ::= { cpqHoIfPhysMapEntry 1 }

    cpqHoIfPhysMapSlot OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The number of the slot containing the physical hardware that
            implements this interface.  The number zero (0) indicates an
            embedded interface (on the system board) or an interface whose
            slot is unknown.  Values may be unknown if the physical
            hardware has not been configured using the EISA Configuration
            Utility."
        ::= { cpqHoIfPhysMapEntry 2 }

    cpqHoIfPhysMapIoBaseAddr OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The base I/O address of the physical hardware that implements
            this interface."
        ::= { cpqHoIfPhysMapEntry 3 }

    cpqHoIfPhysMapIrq OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The number of the IRQ (interrupt) used for this physical
             hardware interface.  The number zero (0) indicates that this
             device does not use an IRQ or this information is unavailable."
        ::= { cpqHoIfPhysMapEntry 4 }

    cpqHoIfPhysMapDma OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The number of the DMA channel used for this physical hardware
            interface.  The number -1 indicates that this device does not
            use a DMA channel or this information is unavailable."
        ::= { cpqHoIfPhysMapEntry 5 }

    cpqHoIfPhysMapMemBaseAddr OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The base memory address used by this physical hardware
            interface.  The number zero (0) indicates that this device does
            not use system memory or this information is unavailable."
        ::= { cpqHoIfPhysMapEntry 6 }

    cpqHoIfPhysMapPort OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The port number of the interface for multi-port NICs.
            A port number of -1 indicates that the port could not
            be determined."
        ::= { cpqHoIfPhysMapEntry 7 }

    cpqHoIfPhysMapDuplexState OBJECT-TYPE
        SYNTAX  INTEGER {
        other(1), -- default
        half(2),
        full(3)
        }
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "This variable describes the configured duplex state of the NIC."

        ::= { cpqHoIfPhysMapEntry 8 }

    cpqHoIfPhysMapCondition OBJECT-TYPE
        SYNTAX  INTEGER
        {
            other(1),    -- default
            ok(2),
            degraded(3),
            failed(4)
        }
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The condition of this interface."
        ::= { cpqHoIfPhysMapEntry 9 }

    cpqHoIfPhysMapOverallCondition OBJECT-TYPE
        SYNTAX  INTEGER
        {
            other(1),    -- default
            ok(2),
            degraded(3),
            failed(4)
        }
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The overall condition of all interfaces."
        ::= { cpqHoIfPhysMap 2 }

-- ****************************************************************************
--   Host OS Software Running Table
--   ==============================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqHostOs Group                (1.3.6.1.4.1.232.11)
--       cpqHoComponent Group          (1.3.6.1.4.1.232.11.2)
--        cpqHoSWRunning Group         (1.3.6.1.4.1.232.11.2.6)
--         cpqHoSWRunningTable         (1.3.6.1.4.1.232.11.2.6.1)
--         cpqHoSwRunningTrapDesc      (1.3.6.1.4.1.232.11.2.6.2)
--
--
--  The cpqHoSWRunning group contains configuration and status information
--  about the software running on the host OS.
--
--  Implementation of the cpqHoSWRunning group is optional for agents
--  that support the Host OS MIB.
--
-- ****************************************************************************

    cpqHoSWRunningTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqHoSWRunningEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A table of descriptions of software running on the system."
        ::= { cpqHoSWRunning 1 }

    cpqHoSWRunningEntry OBJECT-TYPE
        SYNTAX  CpqHoSWRunningEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A description of a software program running on the system."
        INDEX   { cpqHoSWRunningIndex }
        ::= { cpqHoSWRunningTable 1 }

    CpqHoSWRunningEntry ::= SEQUENCE {
        cpqHoSWRunningIndex              INTEGER,
        cpqHoSWRunningName               DisplayString,
        cpqHoSWRunningDesc               DisplayString,
        cpqHoSWRunningVersion            DisplayString,
        cpqHoSWRunningDate               OCTET STRING,
        cpqHoSWRunningMonitor            INTEGER,
        cpqHoSWRunningState              INTEGER,
        cpqHoSWRunningCount              INTEGER,
        cpqHoSWRunningCountMin           INTEGER,
        cpqHoSWRunningCountMax           INTEGER,
        cpqHoSWRunningEventTime          OCTET STRING
    }

    cpqHoSWRunningIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "An index that uniquely specifies this entry."
        ::= { cpqHoSWRunningEntry 1 }

    cpqHoSWRunningName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The name of the software."
        ::= { cpqHoSWRunningEntry 2 }

    cpqHoSWRunningDesc OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A description of the software."
        ::= { cpqHoSWRunningEntry 3 }

    cpqHoSWRunningVersion OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The version of the software.

            This field will be a null (size 0) string if the agent cannot
            provide the software version."
        ::= { cpqHoSWRunningEntry 4 }

    cpqHoSWRunningDate OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (7))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The software date.

             field  octets  contents                  range
             =====  ======  =======                  =====
               1      1-2   year                      0..65536
               2       3    month                     1..12
               3       4    day                       1..31
               4       5    hour                      0..23
               5       6    minute                    0..59
               6       7    second                    0..60
                            (use 60 for leap-second)


            This field will be set to year = 0 if the agent cannot provide
            the software date.  The hour, minute, and second field will be
            set to zero (0) if they are not relevant."
        ::= { cpqHoSWRunningEntry 5 }

    cpqHoSWRunningMonitor OBJECT-TYPE
        SYNTAX  INTEGER
        {
            other(1),    -- default
            start(2),
            stop(3),
            startAndStop(4),
            count(5),
            startAndCount(6),
            countAndStop(7),
            startCountAndStop(8)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The user specified monitor option for a process."
        ::= { cpqHoSWRunningEntry 6 }

    cpqHoSWRunningState OBJECT-TYPE
        SYNTAX  INTEGER
        {
            other(1),    -- default
            started(2),
            stopped(3)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The current state of monitored process."
        ::= { cpqHoSWRunningEntry 7 }

    cpqHoSWRunningCount OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "For each process name, the number of instances of the process running on the system is
            kept count of, in this variable."
        ::= { cpqHoSWRunningEntry 8 }

    cpqHoSWRunningCountMin OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-write
        STATUS  optional
        DESCRIPTION
            "This is the lower threshold on cpqHoSWRunningCount to be set by the user."
        ::= { cpqHoSWRunningEntry 9 }

    cpqHoSWRunningCountMax OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-write
        STATUS  optional
        DESCRIPTION
            "This is the upper threshold on cpqHoSWRunningCount to be set by the user."
        ::= { cpqHoSWRunningEntry 10 }

    cpqHoSWRunningEventTime OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (7))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "The system time at which the monitored event, as per cpqHoSWRunningMonitor, last occurred.

             field  octets  contents                  range
             =====  ======  ========                  =====
               1      1-2   year                      0..65536
               2       3    month                     1..12
               3       4    day                       1..31
               4       5    hour                      0..23
               5       6    minute                    0..59
               6       7    second                    0..60
                            (use 60 for leap-second)

            The hour, minute, and second field will be set to zero (0) if they are not relevant."
        ::= { cpqHoSWRunningEntry 11 }

    cpqHoSwRunningTrapDesc OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The error message for a process monitor event."
        ::= { cpqHoSWRunning 2 }


-- ****************************************************************************
--   Config Software Version Instrumentation Group
--  ===============================================
--
-- The compaq enterprise              (1.3.6.1.4.1.232)
--      cpqHostOs Group               (1.3.6.1.4.1.232.11)
--       cpqHoComponent Group         (1.3.6.1.4.1.232.11.2)
--        cpqHoSwVer Group            (1.3.6.1.4.1.232.11.2.7)
--        cpqHoSwVerTable             (1.3.6.1.4.1.232.11.2.7.2)
--        cpqHoSwVerAgentsVer         (1.3.6.1.4.1.232.11.2.7.3)
--
--  The cpqSwVer group describes the software version table.
--
--  Implementation of the cpqSwVer group is mandatory for all
--  agents that support the Host MIB.
--
--  The read-write elements of this table should be saved from instance to
--  instance of the agent.
--
--  This table can be added to by writing to the cpqHoSwVerName (using the
--  cpqHoSwVerNextIndex index) field with a new driver name.  Writing to
--  this field causes the creation of a new table row (and any data that can
--  be obtained will be filled in, the remainder will be set to the defaults.)
--
--  A row may be deleted by writing to the cpqHoSwVerName field with a null
--  entry.
-- ****************************************************************************

    cpqHoSwVerNextIndex OBJECT-TYPE
           SYNTAX INTEGER
           ACCESS read-only
           STATUS mandatory
           DESCRIPTION
               "The index of the next available entry in the cpqHoSwVer
                table.  If the maximum number of entries to the cpqHoSwVer
                table has been reached, this index will contain -1."
--
-- Writing to the cpqHoSwVerName variable using this index will cause a new
-- entry in the table to be created.
--
           ::= { cpqHoSwVer 1 }

    cpqHoSwVerTable OBJECT-TYPE
           SYNTAX SEQUENCE OF CpqHoSwVerEntry
           ACCESS not-accessible
           STATUS mandatory
           DESCRIPTION
               "A list of software item entries."
           ::= { cpqHoSwVer 2 }

    cpqHoSwVerEntry OBJECT-TYPE
        SYNTAX CpqHoSwVerEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION
               "A list of software items that are on the machine."
        INDEX { cpqHoSwVerIndex }
        ::= { cpqHoSwVerTable 1 }

    CpqHoSwVerEntry ::= SEQUENCE {
              cpqHoSwVerIndex                      INTEGER,
              cpqHoSwVerStatus                     INTEGER,
              cpqHoSwVerType                       INTEGER,
              cpqHoSwVerName                       DisplayString,
              cpqHoSwVerDescription                DisplayString,
              cpqHoSwVerDate                       OCTET STRING,
              cpqHoSwVerLocation                   DisplayString,
              cpqHoSwVerVersion                    DisplayString,
              cpqHoSwVerVersionBinary              DisplayString
       }

    cpqHoSwVerIndex OBJECT-TYPE
        SYNTAX INTEGER (0..65535)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION
              "An index that uniquely identifies an entry in the
              cpqHoSwVer table."
        ::= { cpqHoSwVerEntry 1 }

    cpqHoSwVerStatus OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),           -- undefined (default)
            loaded(2),          -- and running
            notloaded(3)        -- found but not loaded
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
                "Status for the software item."
--
--      Items of type 'other' are those items which the agent could
--      not locate.
--
        ::= { cpqHoSwVerEntry 2 }

    cpqHoSwVerType OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            driver(2),          -- (default)
            agent(3),
            sysutil(4),
            application(5),
            keyfile(6)
            }
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
                "Type of software item."
        ::= { cpqHoSwVerEntry 3 }

    cpqHoSwVerName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..127))
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
                "The name of this software item."
--
--      Writing to this entry with an index equal to cpqHoSwVerNextIndex
--      causes a table row to be created, and all entries to be filled in.
--
--      Writing to this entry with a NULL name deletes the current row.
--
        ::= { cpqHoSwVerEntry 4 }

    cpqHoSwVerDescription OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..127))
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
                "The description of this software item."
--
--      A length of 0 indicates that the description of this item is
--      not available.
--
--      Writing to this entry can cause the entire row to be updated.
--
        ::= { cpqHoSwVerEntry 5 }

    cpqHoSwVerDate OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (7))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The date of the software item, if any.

             field  octets  contents                  range
             =====  ======  =======                  =====
               1      1-2   year                      0..65535
               2       3    month                     1..12
               3       4    day                       1..31
               4       5    hour                      0..23
               5       6    minute                    0..59
               6       7    second                    0..60
                            (use 60 for leap-second)

            The year field is set with the most significant octet first.

            An entry of zero (0) means that there is no date associated with
            this software item.  Zero is the default."
        ::= { cpqHoSwVerEntry 6 }

    cpqHoSwVerLocation OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
                "The location of this software item on the server."
        ::= { cpqHoSwVerEntry 7 }

    cpqHoSwVerVersion OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..50))
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION
              "An string that specifies the version of this item."
         ::= { cpqHoSwVerEntry 8 }

    cpqHoSwVerVersionBinary OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..50))
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION
              "An string that specifies the version of this item based on
              the binary version resource."
         ::= { cpqHoSwVerEntry 9 }

--
-- New for release 7.10: cpqHoSwVerAgentsVer
--
    cpqHoSwVerAgentsVer OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..50))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A string that specifies the version of the Insight
             Management Agents running on the system."
        ::= { cpqHoSwVer 3 }


-- ****************************************************************************
-- The cpqHoGeneric group holds only the generic trap
--
-- The compaq enterprise              (1.3.6.1.4.1.232)
--      cpqHostOS Group               (1.3.6.1.4.1.232.11)
--       cpqHoComponent Group         (1.3.6.1.4.1.232.11.2)
--        cpqHoGeneric Group          (1.3.6.1.4.1.232.11.2.8)
--
-- Implementation of this group is optional.
--
-- ****************************************************************************
    cpqHoGenericData OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..254))
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
        "Data for the generic trap."
--
-- This is the data variable that is sent with the generic trap below.
--
-- Writing to this variable will cause the generic trap to be sent with
-- the newly written data.
--
         ::= { cpqHoGeneric 1 }

    cpqHoCriticalSoftwareUpdateData OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..512))
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
        "Data for the Critical Software Update trap."
--
-- This is the data variable that is sent with the Critical Software
-- update Notification Trap below.
-- Writing to this variable will cause the Critical Software update Notification Trap
-- to be sent with the newly written data.
--
         ::= { cpqHoGeneric 2 }

-- ****************************************************************************
--   Software Performance Group
--  ===========================
--
-- The compaq enterprise              (1.3.6.1.4.1.232)
--      cpqHostOS Group               (1.3.6.1.4.1.232.11)
--       cpqHoComponent Group         (1.3.6.1.4.1.232.11.2)
--        cpqHoSwPerf Group           (1.3.6.1.4.1.232.11.2.9)
--
-- Implementation of this group is optional.
--
-- ****************************************************************************
    cpqHoSwPerfAppErrorDesc OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..254))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
         " This string holds error information about the last application
           error that occurred in the system. "

         ::= { cpqHoSwPerf 1 }

-- ****************************************************************************
--   System Status Group
--   ===================
--
-- The compaq enterprise              (1.3.6.1.4.1.232)
--      cpqHostOS Group               (1.3.6.1.4.1.232.11)
--       cpqHoComponent Group         (1.3.6.1.4.1.232.11.2)
--        cpqHoSystemStatus Group     (1.3.6.1.4.1.232.11.2.10)
--
-- Implementation of this group is mandatory.
--
-- ****************************************************************************

    cpqHoMibStatusArray OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (4..256))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The MIB Status Array is an array of MIB status structures. Each
            structure is made up of 4 octets.  The first octet is the MIB
            presence.  The second octet is MIB condition.  The third octet is
            MIB major revision.  The fourth octet is MIB minor revision. These
            blocks of 4 octets each are index by the mib identifier just after
            the compaq enterprise (eg in 1.3.6.1.232.11 mib, the index is 11).
            The 4 octets in the first block (block 0) are reserved for systems
            management and serve as an aggregate of the other mibs.

            Array element 0 is the status for all MIBs in the Compaq
            Enterprise.  Array element n, where n > 0, is the status for the
            nth MIB in the Compaq Enterprise (.1.3.6.1.4.1.232.n).

             Octet   Element   Field
            ======== ======= =========
               0        0    Status of any Compaq MIBs
               1             Condition of all Compaq MIBs
               2             System Flags (see below)
               3             Detailed type (see below)
               4        1    Status of Compaq MIB 1
               5             Condition of Compaq MIB 1
               6             Major Revision of Compaq MIB 1
               7             Minor Revision of Compaq MIB 1
               8        2    Status of Compaq MIB 2
               9             Condition of Compaq MIB 2
              10             Major Revision of Compaq MIB 2
              11             Minor Revision of Compaq MIB 2
               .        .
               .
               .
             n*4        n    Status of Compaq MIB n
            (n*4)+1          Condition of Compaq MIB n
            (n*4)+2          Major Revision of Compaq MIB n
            (n*4)+3          Minor Revision of Compaq MIB n

             System Flags (octet 2)
             Bit        Meaning
            =====       =========
              0         Equals 1 if the device is not a server, see detailed type below
                        Equals 0 if the device is a server
              1         This system contains enabled remote console
                        functionality.
              2         This system is configured to be an Integration Server.
              3         Web Based Management is enabled.
             4-7        Reserved (reserved Bits should be zero)

            Detailed Type (octet 3)
            Bits 0-4    Detailed Type, only used if bit 0 in octet 2 is 1.
            Bits 5-7    Reserved for expansion. note, use these last in case we
                        need more then 32 types someday.

            Type Values for Bits 0-4 (maps to CIM7 types)
            Unknown                    =  0
            Server                     =  1  (yes a duplicate of the server flag)
            Desktop                    =  2
            Workstation                =  3
            Portable                   =  4
            Router                     =  5
            Cluster                    =  6
            Printer                    =  7
            Switch                     =  8  (network switch)
            Repeater                   =  9
            Remote Access Device       = 10
            Other                      = 11
            Management Processor       = 12  (rib, RILOE, iLo)
            Rack                       = 13
            Enclosure                  = 14
            KVM Switch                 = 15  (IP enabled keyboard video mouse switch).
            UPS                        = 16
            Power Distribution Unit    = 17
            Environmental Monitor      = 18  (eg CMC)


            For all other blocks, they are defined as:
            Status         This is a collection of flags.  Each bit has the
                           following meaning when it is on (1):

                           Bit 2-7:   RESERVED: Always 0
                           Bit 1:     MIB is from offline data (only applies
                                      to global system status)
                           Bit 0:     MIB is available

                           NOTE:   bit 7 is the most significant bit, bit 0
                                   is the least significant.

            Condition      0 - Not available
                           1 - Other
                           2 - OK
                           3 - Degraded
                           4 - Failed

            Major Revision 0..255, where 0 is not available
            Minor Revision 0..255, where 0 is not available"



        ::= { cpqHoSystemStatus 1 }

    cpqHoConfigChangedDate OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (7))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The date/time when the agents were last loaded.

             field  octets  contents                  range
             =====  ======  =======                  =====
               1      1-2   year                      0..65536
               2       3    month                     1..12
               3       4    day                       1..31
               4       5    hour                      0..23
               5       6    minute                    0..59
               6       7    second                    0..60
                            (use 60 for leap-second)


            This field will be set to year = 0 if the agent cannot provide
            the date/time.  The year field is set with the most significant
            octet first."
        ::= { cpqHoSystemStatus 2 }

    cpqHoGUID OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (16..17))
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "The globally unique identifier of this server.
             If the OS cannot determine a unique ID, it will default the
             variable to contain all 0's.  The management station can then
             perform a SET to this variable to provide the unique ID.
             When the system is cellular, it will have its partition number
             appended at the end."
       ::= { cpqHoSystemStatus 3 }

    cpqHoCodeServer OBJECT-TYPE
        SYNTAX    INTEGER
        ACCESS    read-only
        STATUS    mandatory
        DESCRIPTION
            "This item indicates how many code server shares are currently
            configured on the system.  If the value of this attribute is
            0, this server has not been configured with code server shares."
        ::= { cpqHoSystemStatus 4 }

    cpqHoWebMgmtPort OBJECT-TYPE
        SYNTAX    INTEGER
        ACCESS    read-only
        STATUS    mandatory
        DESCRIPTION
            "This item indicates the port used by the Insight Web Agent.
            If the port cannot be determined or the Web Management agent
            is not enabled, this value will be -1."
        ::= { cpqHoSystemStatus 5 }

-- ****************************************************************************
--   Trap Info Group
--   ================
--
-- The compaq enterprise              (1.3.6.1.4.1.232)
--      cpqHostOS Group               (1.3.6.1.4.1.232.11)
--       cpqHoComponent Group         (1.3.6.1.4.1.232.11.2)
--        cpqHoTrapInfo Group         (1.3.6.1.4.1.232.11.2.11)
--
-- Implementation of this group is mandatory.
--
-- ****************************************************************************

    cpqHoTrapFlags OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The Trap Flags.


            This is a collection of flags used during trap delivery.
            Each bit has the following meaning:

                Bit 5-31: RESERVED: Always 0.
                Bit 2-4: Trap Condition
                             0 = Not used (for backward compatibility)
                             1 = Condition unknown or N/A
                             2 = Condition ok
                             3 = Condition degraded
                             4 = Condition failed
                             5-7 = reserved
                Bit 1:    Client IP address type
                             0 = static entry
                             1 = DHCP entry
                Bit 0:    Agent Type
                             0 = Server
                             1 = Client

            NOTE:   bit 31 is the most significant bit, bit 0 is the least
                    significant."

        ::= { cpqHoTrapInfo 1 }


-- ****************************************************************************
--   OS Client Table
--   ====================
--
-- The compaq enterprise              (1.3.6.1.4.1.232)
--      cpqHostOS Group               (1.3.6.1.4.1.232.11)
--       cpqHoComponent Group         (1.3.6.1.4.1.232.11.2)
---       cpqHoClient Group           (1.3.6.1.4.1.232.11.2.12)
--
--      The cpqHoClient table contains entries describing identification,
--      address, and status information about each unit that is using
--      services provided by this unit.
--
-- ****************************************************************************



    cpqHoClientLastModified OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (7))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The date/time of the last modification to the client table.

             field  octets  contents                  range
             =====  ======  =======                  =====
               1      1-2   year                      0..65536
               2       3    month                     1..12
               3       4    day                       1..31
               4       5    hour                      0..23
               5       6    minute                    0..59
               6       7    second                    0..60
                            (use 60 for leap-second)


            This field will be set to all 0's if there are no entries to the
            client table.

            The year field will be set to 0xFFFF if the agent does not support
            the client table.

            The year field is set with the most significant octet first."
        ::= { cpqHoClients 1 }

    cpqHoClientDelete OBJECT-TYPE
        SYNTAX DisplayString (SIZE (0..15))
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION
        "Setting this variable to the name of a client in the client table
         will cause that row in the table to be deleted.  Any other set
         will fail.

         Note that the indices of the table will (most likely) be renumbered
         following a deletion."
        ::= { cpqHoClients 2 }


    cpqHoClientTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqHoClientEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A table of client descriptions."
        ::= { cpqHoClients 3 }

    cpqHoClientEntry OBJECT-TYPE
        SYNTAX  CpqHoClientEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A client description."
        INDEX   { cpqHoClientIndex }
        ::= { cpqHoClientTable 1 }

    CpqHoClientEntry ::= SEQUENCE {
        cpqHoClientIndex              INTEGER,
        cpqHoClientName               DisplayString,
        cpqHoClientIpxAddress         OCTET STRING,
        cpqHoClientIpAddress          IpAddress,
        cpqHoClientCommunity          DisplayString,
        cpqHoClientID                 OCTET STRING
    }

    cpqHoClientIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "An index that uniquely specifies this entry."
        ::= { cpqHoClientEntry 1 }

    cpqHoClientName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..15))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The Win95 machine name of this client."

-- Note that Win95 limits the machine name to a maximum of 15 characters.

        ::= { cpqHoClientEntry 2 }

    cpqHoClientIpxAddress OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (20))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The IPX address for this client, all octets should be set to
             0xff if this machine does not support IPX.

             The format is NetAddr:NodeNumber and sent in MSB order:

                                  1111111111
                       01234567:890123456789"

-- Note, this item is still in definition and probably will change.

        ::= { cpqHoClientEntry 3 }

    cpqHoClientIpAddress OBJECT-TYPE
        SYNTAX  IpAddress
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The IP address for this client, all octets should be set to
             0xff if this machine does not support IP.  The order will be
             in network byte order (ie MSB first.)"

        ::= { cpqHoClientEntry 4 }

    cpqHoClientCommunity OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..48))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A community name that can be used to query the client with SNMP.
             This community name should have, but is not required to have,
             the greatest possible access to client information."
        ::= { cpqHoClientEntry 5 }

    cpqHoClientID OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (16))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The unique identifier of this client."
        ::= { cpqHoClientEntry 6 }

-- ****************************************************************************
--   OS Memory Group
--   ===============
--
-- The compaq enterprise              (1.3.6.1.4.1.232)
--      cpqHostOS Group               (1.3.6.1.4.1.232.11)
--       cpqHoComponent Group         (1.3.6.1.4.1.232.11.2)
---       cpqHoMemory Group           (1.3.6.1.4.1.232.11.2.13)
--
--      The cpqHoMemory group contains entries describing memory
--      as seen by the OS.
--
-- ****************************************************************************

    cpqHoPhysicalMemorySize OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Total amount of physical memory as seen by the OS (in megabytes).

            A -1 will be returned if this value could not be determined."
        ::= { cpqHoMemory 1 }

    cpqHoPhysicalMemoryFree OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The amount of free physical memory (in megabytes).

            A -1 will be returned if this value could not be determined."
        ::= { cpqHoMemory 2 }

    cpqHoPagingMemorySize OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Total virtual memory available from the OS (in megabytes).

            A -1 will be returned if this value could not be determined."
        ::= { cpqHoMemory 3 }

    cpqHoPagingMemoryFree OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Available paging memory (in megabytes).

            A -1 will be returned if this value could not be determined."
        ::= { cpqHoMemory 4 }

    cpqHoBootPagingFileSize OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..10))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The paging file size of the boot volume in the format xxxMB or 
            xxxGB, where xxx is the paging file size in that unit shown right 
            after it.

            NULL value will be returned if this value could not be determined."
        ::= { cpqHoMemory 5 }

    cpqHoBootPagingFileMinimumSize OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..10))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
	    "Minimum paging file size of the boot volume required to save the 
            memory dump in the event of a system crash. The format is xxxMB or 
            xxxGB, where xxx is the minimum paging file size in that unit shown 
            right after it."
        ::= { cpqHoMemory 6 }


-- ****************************************************************************
--  Firmware Version Instrumentation Group
--  ======================================
--
-- The compaq enterprise              (1.3.6.1.4.1.232)
--      cpqHostOs Group               (1.3.6.1.4.1.232.11)
--       cpqHoComponent Group         (1.3.6.1.4.1.232.11.2)
--        cpqHoFwVer Group            (1.3.6.1.4.1.232.11.2.14)
--        cpqHoFwVerTable             (1.3.6.1.4.1.232.11.2.14.1)
--
--  The cpqHoFwVer group describes the firmware version table.
--
--  Implementation of the cpqHoFwVer group is mandatory for all
--  agents that support the Host MIB.
--
-- ****************************************************************************

    cpqHoFwVerTable OBJECT-TYPE
           SYNTAX SEQUENCE OF CpqHoFwVerEntry
           ACCESS not-accessible
           STATUS mandatory
           DESCRIPTION
               "A list of firmware item entries."
           ::= { cpqHoFwVer 1 }

    cpqHoFwVerEntry OBJECT-TYPE
        SYNTAX CpqHoFwVerEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION
               "A list of firmware items that are on the machine."
        INDEX { cpqHoFwVerIndex }
        ::= { cpqHoFwVerTable 1 }

    CpqHoFwVerEntry ::= SEQUENCE {
              cpqHoFwVerIndex                      INTEGER,
              cpqHoFwVerCategory                   INTEGER,
              cpqHoFwVerDeviceType                 INTEGER,
              cpqHoFwVerDisplayName                DisplayString,
              cpqHoFwVerVersion                    DisplayString,
              cpqHoFwVerLocation                   DisplayString,
              cpqHoFwVerXmlString                  DisplayString,
              cpqHoFwVerKeyString                  DisplayString,
              cpqHoFwVerUpdateMethod               INTEGER
       }

    cpqHoFwVerIndex OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION
            "Firmware Version Index.

            The firmware version index uniquely identifies an entry in the
            cpqHoFwVer table."
        ::= { cpqHoFwVerEntry 1 }

    cpqHoFwVerCategory OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            storage(2),
            nic(3),
            rib(4),
            system(5)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Firmware Version Category."
        ::= { cpqHoFwVerEntry 2 }

    cpqHoFwVerDeviceType OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            internalArrayController(2),
            fibreArrayController(3),
            scsiController(4),
            fibreChannelTapeController(5),
            modularDataRouter(6),
            ideCdRomDrive(7),
            ideDiskDrive(8),
            scsiCdRom-ScsiAttached(9),
            scsiDiskDrive-ScsiAttached(10),
            scsiTapeDrive-ScsiAttached(11),
            scsiTapeLibrary-ScsiAttached(12),
            scsiDiskDrive-ArrayAttached(13),
            scsiTapeDrive-ArrayAttached(14),
            scsiTapeLibrary-ArrayAttached(15),
            scsiDiskDrive-FibreAttached(16),
            scsiTapeDrive-FibreAttached(17),
            scsiTapeLibrary-FibreAttached(18),
            scsiEnclosureBackplaneRom-ScsiAttached(19),
            scsiEnclosureBackplaneRom-ArrayAttached(20),
            scsiEnclosureBackplaneRom-FibreAttached(21),
            scsiEnclosureBackplaneRom-ra4x00(22),
            systemRom(23),
            networkInterfaceController(24),
            remoteInsightBoard(25)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Firmware Version Device Type."
        ::= { cpqHoFwVerEntry 3 }

    cpqHoFwVerDisplayName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Firmware Version Device Display Name.

            This is the display name of the device containing the firmware."
        ::= { cpqHoFwVerEntry 4 }

    cpqHoFwVerVersion OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..31))
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION
            "Firmware Version.

            This is the version of the device firmware."
        ::= { cpqHoFwVerEntry 5 }

    cpqHoFwVerLocation OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Firmware Version Device Location.

            This is a printable string that specifies the location of the
            device that contains the firmware."
        ::= { cpqHoFwVerEntry 6 }

    cpqHoFwVerXmlString OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION
            "Firmware Version Xml String.

            This is an XML string that specifies the location of the device
            that contains the firmware."
        ::= { cpqHoFwVerEntry 7 }

    cpqHoFwVerKeyString OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Firmware Version Key String.

            This field is differentiate devices of the same type."
        ::= { cpqHoFwVerEntry 8 }


    cpqHoFwVerUpdateMethod OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            noUpdate(2),
            softwareflash(3),
            replacePhysicalRom(4)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Firmware Version update method."
        ::= { cpqHoFwVerEntry 9 }


-- ****************************************************************************
--  Hardware Information Group
--  ======================================
--
-- The compaq enterprise              (1.3.6.1.4.1.232)
--      cpqHostOs Group               (1.3.6.1.4.1.232.11)
--       cpqHoComponent Group         (1.3.6.1.4.1.232.11.2)
--        cpqHoHWInfo Group           (1.3.6.1.4.1.232.11.2.15)
--        cpqHoHWInfoPlatform         (1.3.6.1.4.1.232.11.2.15.1)
--
--  The cpqHoHWInfo group describes some hw information necessary to other agents.
--
--  Implementation of the cpqHoHWInfo group is optional for
--  agents that support the Host MIB.
--
-- ****************************************************************************
    cpqHoHWInfoPlatform OBJECT-TYPE
        SYNTAX  INTEGER {
            unknown(1),
            cellular(2),
            foundation(3),
            virtualMachine(4)
            }
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "Hardware platform type.

             This object represents the platform type of the server's host
             system represented by this MIB."
        ::= { cpqHoHWInfo 1 }


-- ****************************************************************************
--  Host MIB Trap Definitions
--  =========================
--
--  The SNMP trap messages must not be bigger than 484 octets (bytes).
--
--  Trap support in an SNMP agent implementation is optional.  An SNMP
--  agent implementation may support all, some, or none of the traps.
--  If traps are supported, The user should be provided with the option of
--  disabling traps.
--
--  Implementation of cpqHoGenericTrap is a mandatory part of the Generic
--  group.
--
-- **************************************************************************

    cpqHoGenericTrap TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES { cpqHoGenericData }
        DESCRIPTION
        --  This trap is a generic trap, and left undefined.
            "Generic trap."

              --#TYPE "Generic trap (11001)"
              --#SUMMARY "%s"
              --#ARGUMENTS {0}
              --#SEVERITY MAJOR
              --#TIMEINDEX 99

        ::= 11001

    cpqHoAppErrorTrap TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES { cpqHoSwPerfAppErrorDesc }
        DESCRIPTION
            "An application has generated an exception.  Specific
             error information is contained in the variable
             cpqHoSwPerfAppErrorDesc."

              --#TYPE "Application Error Trap (11002)"
              --#SUMMARY "%s"
              --#ARGUMENTS {0}
              --#SEVERITY MAJOR
              --#TIMEINDEX 99

        ::= 11002


    cpqHo2GenericTrap TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES { sysName, cpqHoTrapFlags, cpqHoGenericData }
        DESCRIPTION
        --  This trap is a generic trap, and left undefined.
            "Generic trap."

              --#TYPE "Generic trap (11003)"
              --#SUMMARY "%s"
              --#ARGUMENTS {2}
              --#SEVERITY MAJOR
              --#TIMEINDEX 99

        ::= 11003

    cpqHo2AppErrorTrap TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES { sysName, cpqHoTrapFlags, cpqHoSwPerfAppErrorDesc }
        DESCRIPTION
            "An application has generated an exception.  Specific
             error information is contained in the variable
             cpqHoSwPerfAppErrorDesc."

              --#TYPE "Application Error Trap (11004)"
              --#SUMMARY "%s"
              --#ARGUMENTS {2}
              --#SEVERITY MAJOR
              --#TIMEINDEX 99

        ::= 11004

    cpqHo2NicStatusOk TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES { sysName, cpqHoTrapFlags, cpqHoIfPhysMapSlot }
        DESCRIPTION
            "This trap will be sent any time the status of a NIC changes to
            the OK condition."

             --#TYPE "Status Trap (11005)"
             --#SUMMARY "NIC Status is OK for slot %s."
             --#ARGUMENTS {2}
             --#SEVERITY MAJOR
             --#TIMEINDEX 99
        ::= 11005

    cpqHo2NicStatusFailed TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES { sysName, cpqHoTrapFlags, cpqHoIfPhysMapSlot }
        DESCRIPTION
            "This trap will be sent any time the status of a NIC changes to
            the Failed condition."

             --#TYPE "Status Trap (11006)"
             --#SUMMARY "NIC Status is Failed for slot %s."
             --#ARGUMENTS {2}
             --#SEVERITY MAJOR
             --#TIMEINDEX 99
        ::= 11006

    cpqHo2NicSwitchoverOccurred TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES { sysName, cpqHoTrapFlags, cpqHoIfPhysMapSlot, cpqHoIfPhysMapSlot }
        DESCRIPTION
            "This trap will be sent any time the configured redundant NIC
            becomes the active NIC."

             --#TYPE "Status Trap (11007)"
             --#SUMMARY "NIC switchover to slot %s from slot %s."
             --#ARGUMENTS {2, 3}
             --#SEVERITY MAJOR
             --#TIMEINDEX 99
        ::= 11007


    cpqHo2NicStatusOk2 TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES { sysName, cpqHoTrapFlags, cpqHoIfPhysMapSlot,
                    cpqHoIfPhysMapPort }
        DESCRIPTION
            "This trap will be sent any time the status of a NIC changes to
            the OK condition."

             --#TYPE "Status Trap (11008)"
             --#SUMMARY "NIC Status is OK for slot %s, port %s."
             --#ARGUMENTS {2, 3}
             --#SEVERITY MAJOR
             --#TIMEINDEX 99
        ::= 11008

    cpqHo2NicStatusFailed2 TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES { sysName, cpqHoTrapFlags, cpqHoIfPhysMapSlot,
                    cpqHoIfPhysMapPort }
        DESCRIPTION
            "This trap will be sent any time the status of a NIC changes to
            the Failed condition."

             --#TYPE "Status Trap (11009)"
             --#SUMMARY "NIC Status is Failed for slot %s, port %s."
             --#ARGUMENTS {2, 3}
             --#SEVERITY MAJOR
             --#TIMEINDEX 99
        ::= 11009

    cpqHo2NicSwitchoverOccurred2 TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES { sysName, cpqHoTrapFlags, cpqHoIfPhysMapSlot,
                    cpqHoIfPhysMapPort, cpqHoIfPhysMapSlot,
                    cpqHoIfPhysMapPort }
        DESCRIPTION
            "This trap will be sent any time the configured redundant NIC
            becomes the active NIC."

             --#TYPE "Status Trap (11010)"
             --#SUMMARY "NIC switchover to slot %s, port %s from slot %s, port %s."
             --#ARGUMENTS {2, 3, 4, 5}
             --#SEVERITY MAJOR
             --#TIMEINDEX 99
        ::= 11010

    cpqHoProcessEventTrap TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES { sysName, cpqHoTrapFlags, cpqHoSwRunningTrapDesc }
        DESCRIPTION
            "A monitored process has either started or stopped running."

              --#TYPE "Process Monitor Event Trap (11011)"
              --#SUMMARY "%s"
              --#ARGUMENTS {2}
              --#SEVERITY MAJOR
              --#TIMEINDEX 99

        ::= 11011

    cpqHoProcessCountWarning TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES { sysName, cpqHoTrapFlags, cpqHoSWRunningName, cpqHoSWRunningCount,
                    cpqHoSWRunningCountMin, cpqHoSWRunningCountMax,
                    cpqHoSWRunningEventTime }
        DESCRIPTION
            "A monitored process count has violated the thresholds set on cpqHoSWRunningCount"

              --#TYPE "Process Count Event Trap (11012)"
              --#SUMMARY "Process %s has count %s which violates the thresholds %s to %s."
              --#ARGUMENTS {2, 3, 4, 5}
              --#SEVERITY MAJOR
              --#TIMEINDEX 99
              --#STATE DEGRADED

        ::= 11012

    cpqHoProcessCountNormal TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES { sysName, cpqHoTrapFlags, cpqHoSWRunningName, cpqHoSWRunningCount,
                    cpqHoSWRunningCountMin, cpqHoSWRunningCountMax,
                    cpqHoSWRunningEventTime }
        DESCRIPTION
            "A monitored process count has returned back to normal."

              --#TYPE "Process Monitor Event Trap (11013)"
              --#SUMMARY "Process %s has count %s which respects the thresholds %s to %s."
              --#ARGUMENTS {2, 3, 4, 5}
              --#SEVERITY INFORMATIONAL
              --#TIMEINDEX 99
              --#STATE OPERATIONAL

        ::= 11013

   cpqHoCriticalSoftwareUpdateTrap TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES { sysName, cpqHoTrapFlags, cpqHoCriticalSoftwareUpdateData }
        DESCRIPTION
            "This trap is a send to the user to notify him of a Critical Software Update."

              --#TYPE "Critical Software update Notification Trap (11014)"
              --#SUMMARY "%s"
              --#ARGUMENTS {2}
              --#SEVERITY CRITICAL
              --#TIMEINDEX 99

        ::= 11014

   cpqHoCrashDumpNotEnabledTrap TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES { sysName, cpqHoTrapFlags, cpqHoCrashDumpState }
        DESCRIPTION
            "This trap is sent to the user to notify him that the Crash Dump is not enabled."

              --#TYPE "Crash Dump not enabled Notification Trap (11015)"
              --#SUMMARY "Crash Dump is not enabled."
              --#ARGUMENTS {}
              --#SEVERITY WARNING
              --#TIMEINDEX 99

        ::= 11015

   cpqHoBootPagingFileTooSmallTrap TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES { sysName, cpqHoTrapFlags, cpqHoCrashDumpState, cpqHoBootPagingFileSize, cpqHoBootPagingFileMinimumSize }
        DESCRIPTION
            "This trap is sent when the paging file size of the boot volume or the target volume of the memory dump file is too small to hold a crash dump."

              --#TYPE "Boot Paging File Or Memory Dump Target Volume Too Small Notification Trap (11016)"
              --#SUMMARY "The paging file size of the boot volume (%s) or the target volume of the memory dump file is not large enough to hold a crash dump in the event of a system crash (%s)."
              --#ARGUMENTS {3, 4}
              --#SEVERITY WARNING
              --#TIMEINDEX 99

        ::= 11016
  
  END
