DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11033 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unable to generate an ALB address in Arches Fabric ArfSetDefaultCSRs() function. Data field:(cell number 56) | (port number 48) | (xbc ID 32) | (return value).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unable to generate an ALB address in Arches Fabric ArfSetDefaultCSRs() function. Data field:(cell number 56) | (port number 48) | (xbc ID 32) | (return value).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Unable to generate an ALB address in Arches Fabric ArfSetDefaultCSRs() function. Data field:(cell number << 56) | (port number << 48) | (xbc ID < 32) | (return value)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11034 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event SetDefaultCSRs function failed unexpectedly. Arches Fabric was unable to set XBC CSRs to default values. Data field: return value from SetDefaultCSRs.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event SetDefaultCSRs function failed unexpectedly. Arches Fabric was unable to set XBC CSRs to default values. Data field: return value from SetDefaultCSRs.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='SetDefaultCSRs function failed unexpectedly. Arches Fabric was unable to set XBC CSRs to default values. Data field: return value from SetDefaultCSRs'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11038 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A problem was encountered while routing which prevented an appropriate route from being chosen. Data Field: Destination Cell 56 | XBC Port 44 | XBC # 32 | return status.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A problem was encountered while routing which prevented an appropriate route from being chosen. Data Field: Destination Cell 56 | XBC Port 44 | XBC # 32 | return status.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A problem was encountered while routing which prevented an appropriate route from being chosen. Data Field: Destination Cell << 56 | XBC Port << 44 | XBC # << 32 | return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11039 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An error was encountered while routing the fabric. This error prevents an appropriate route from being selected. Data Field: Destination Cell 56 | XBC Port 44 | XBC # 32 | return status.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An error was encountered while routing the fabric. This error prevents an appropriate route from being selected. Data Field: Destination Cell 56 | XBC Port 44 | XBC # 32 | return status.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error was encountered while routing the fabric. This error prevents an appropriate route from being selected. Data Field: Destination Cell << 56 | XBC Port << 44 | XBC # << 32 | return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11040 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An error was encountered while routing the fabric. This error prevents an appropriate route from being selected. Data Field: Destination Cell 56 | XBC Port 44 | XBC # 32 | return status.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An error was encountered while routing the fabric. This error prevents an appropriate route from being selected. Data Field: Destination Cell 56 | XBC Port 44 | XBC # 32 | return status.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error was encountered while routing the fabric. This error prevents an appropriate route from being selected. Data Field: Destination Cell << 56 | XBC Port << 44 | XBC # << 32 | return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11042 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An error was encountered while routing the fabric. This error prevents an appropriate route from being selected. Data Field: Destination Cell 56 | XBC Port 44 | XBC # 32 | switch fabric'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An error was encountered while routing the fabric. This error prevents an appropriate route from being selected. Data Field: Destination Cell 56 | XBC Port 44 | XBC # 32 | switch fabric: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error was encountered while routing the fabric. This error prevents an appropriate route from being selected. Data Field: Destination Cell << 56 | XBC Port << 44 | XBC # << 32 | switch fabric'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11452 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event System backplane power has reported a 1.2v LDO fault. The data field contains the physical location of the fault.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event System backplane power has reported a 1.2v LDO fault. The data field contains the physical location of the fault.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System backplane power has reported a 1.2v LDO fault. The data field contains the physical location of the fault.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11454 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event System backplane power has reported a 2.5v LDO fault. The data field contains the physical location of the fault.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event System backplane power has reported a 2.5v LDO fault. The data field contains the physical location of the fault.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System backplane power has reported a 2.5v LDO fault. The data field contains the physical location of the fault.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11456 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event System backplane power has reported a 3.3v house keeping power fault. The data field contains the physical location of the fault.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event System backplane power has reported a 3.3v house keeping power fault. The data field contains the physical location of the fault.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System backplane power has reported a 3.3v house keeping power fault. The data field contains the physical location of the fault.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11459 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event System backplane power has reported a 12v power fault. The data field contains the physical location of the fault.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event System backplane power has reported a 12v power fault. The data field contains the physical location of the fault.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System backplane power has reported a 12v power fault. The data field contains the physical location of the fault.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11461 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event System backplane power has reported a 3.3v power fault. The data field contains the physical location of the fault.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event System backplane power has reported a 3.3v power fault. The data field contains the physical location of the fault.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System backplane power has reported a 3.3v power fault. The data field contains the physical location of the fault.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11463 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event System backplane power has reported a 1.5v power fault. The data field contains the physical location of the fault.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event System backplane power has reported a 1.5v power fault. The data field contains the physical location of the fault.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System backplane power has reported a 1.5v power fault. The data field contains the physical location of the fault.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11465 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event System backplane power has reported a 2.5v power fault. The data field contains the physical location of the fault.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event System backplane power has reported a 2.5v power fault. The data field contains the physical location of the fault.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System backplane power has reported a 2.5v power fault. The data field contains the physical location of the fault.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11467 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event One or more power rails is providing insufficient power to the backplane.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event One or more power rails is providing insufficient power to the backplane.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='One or more power rails is providing insufficient power to the backplane.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11468 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Clock fault for clocks supplied from the Redundant Clock Source (RCS) board to the system backplane. RCS board is no longer providing clocks to the backplane. The data field contains the physical location of the RCS.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Clock fault for clocks supplied from the Redundant Clock Source (RCS) board to the system backplane. RCS board is no longer providing clocks to the backplane. The data field contains the physical location of the RCS.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Clock fault for clocks supplied from the Redundant Clock Source (RCS) board to the system backplane. RCS board is no longer providing clocks to the backplane. The data field contains the physical location of the RCS.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11471 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Clock fault for clocks supplied from the Hot Swap Oscillator (HSO) board to the system backplane. HSO has reported a fault or has been removed. The data field contains the physical location of the HSO.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Clock fault for clocks supplied from the Hot Swap Oscillator (HSO) board to the system backplane. HSO has reported a fault or has been removed. The data field contains the physical location of the HSO.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Clock fault for clocks supplied from the Hot Swap Oscillator (HSO) board to the system backplane. HSO has reported a fault or has been removed. The data field contains the physical location of the HSO.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11478 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The operational clock frequencies do not match between the Redundant Clock Source (RCS) and the Hot Swap Oscillator (HSO). The data field contains the physical location of the HSO.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The operational clock frequencies do not match between the Redundant Clock Source (RCS) and the Hot Swap Oscillator (HSO). The data field contains the physical location of the HSO.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The operational clock frequencies do not match between the Redundant Clock Source (RCS) and the Hot Swap Oscillator (HSO). The data field contains the physical location of the HSO.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11479 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The clock margin of the system backplane failed.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The clock margin of the system backplane failed.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The clock margin of the system backplane failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11481 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event System backplane Hot Swap Oscillator (HSO) boards are NOT redundant.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event System backplane Hot Swap Oscillator (HSO) boards are NOT redundant.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System backplane Hot Swap Oscillator (HSO) boards are NOT redundant.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11482 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event System backplane Hot Swap Oscillator (HSO) boards are insufficient.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event System backplane Hot Swap Oscillator (HSO) boards are insufficient.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System backplane Hot Swap Oscillator (HSO) boards are insufficient.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11483 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failure reading Redundant Clock Source (RCS) or Hot Swap Oscillator HSO boards EEPROM.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failure reading Redundant Clock Source (RCS) or Hot Swap Oscillator HSO boards EEPROM.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failure reading Redundant Clock Source (RCS) or Hot Swap Oscillator HSO boards EEPROM. Data field contains the physical location of the device.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11484 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failure writing Redundant Clock Source (RCS) or Hot Swap Oscillator HSO boards EEPROM.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failure writing Redundant Clock Source (RCS) or Hot Swap Oscillator HSO boards EEPROM.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failure writing Redundant Clock Source (RCS) or Hot Swap Oscillator HSO boards EEPROM. Data field contains the physical location of the device'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11485 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failure reading the Reset and Power Monitors (RPM) EEPROM.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failure reading the Reset and Power Monitors (RPM) EEPROM.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failure reading the Reset and Power Monitors (RPM) EEPROM. Data field contains the physical location of the device.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11486 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failure writing the Reset and Power Monitors (RPM) EEPROM.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failure writing the Reset and Power Monitors (RPM) EEPROM.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failure writing the Reset and Power Monitors (RPM) EEPROM. Datafield contains the physical location of the device'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11487 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failure reading the Onboard System Programmers (OSP) EEPROM.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failure reading the Onboard System Programmers (OSP) EEPROM.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failure reading the Onboard System Programmers (OSP) EEPROM. Datafield contains the physical location of the device'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11488 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failure writing the Onboard System Programmers (OSP) EEPROM.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failure writing the Onboard System Programmers (OSP) EEPROM.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failure writing the Onboard System Programmers (OSP) EEPROM. Datafield contains physical location of the device'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11489 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event SBS fault on startup.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event SBS fault on startup.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Serial Bit Stream (SBS) fault on startup. An SBS fault results in the MOAB s not being configured correctly.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11495 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failure reading IO backplane LPM.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failure reading IO backplane LPM.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failure reading IO backplane LPM. Datafield contains the physical location of the device.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11496 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failure writing IO backplane LPM.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failure writing IO backplane LPM.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failure writing IO backplane LPM. Datafield contains physical location of device.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11515 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The system software violated one of the  well-behavedness  rules of soft partitions and tried to call a firmware procedure within the firmware instance of a sibling. This is an access violation and firmware rejects the call.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The system software violated one of the  well-behavedness  rules of soft partitions and tried to call a firmware procedure within the firmware instance of a sibling. This is an access violation and firmware rejects the call.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The system software violated one of the  well-behavedness  rules of soft partitions and tried to call a firmware procedure within the firmware instance of a sibling. This is an access violation and firmware rejects the call'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11521 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event AlbInitPrep was unable to read the ALREC_CONFIG CSR to determine whether the link is up or not. Data field: unused'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event AlbInitPrep was unable to read the ALREC_CONFIG CSR to determine whether the link is up or not. Data field: unused: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='AlbInitPrep was unable to read the ALREC_CONFIG CSR to determine whether the link is up or not. Data field: unused'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11529 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The fPar whose ID is identified in the event detail is disabled from booting because it has no bootable, healthy CPU. It may not own any CPU or the CPUs it owns are Unhealthy (or deconfigured)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The fPar whose ID is identified in the event detail is disabled from booting because it has no bootable, healthy CPU. It may not own any CPU or the CPUs it owns are Unhealthy (or deconfigured): &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The fPar whose ID is identified in the event detail is disabled from booting because it has no bootable, healthy CPU. It may not own any CPU or the CPUs it owns are Unhealthy (or deconfigured)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11530 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Non-critical event announces that an fPar is enabled to boot but has inadequate memory resources to instantiate the firmware for the fPar. The configuration is modified to disable but not delete this fPar.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Non-critical event announces that an fPar is enabled to boot but has inadequate memory resources to instantiate the firmware for the fPar. The configuration is modified to disable but not delete this fPar.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Non-critical event announces that an fPar is enabled to boot but has inadequate memory resources to instantiate the firmware for the fPar. The configuration is modified to disable but not delete this fPar.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11531 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The fPar has been enabled to boot, and contains at least one CPU and adequate memory but has not been given any IO resources. It must be reconfigured and reset before it may boot an operating system.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The fPar has been enabled to boot, and contains at least one CPU and adequate memory but has not been given any IO resources. It must be reconfigured and reset before it may boot an operating system.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The fPar has been enabled to boot, and contains at least one CPU and adequate memory but has not been given any IO resources. The soft partition (fPar) may therefore only boot as far as the EFI shell. It must be reconfigured and reset before'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='it may boot an operating system.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11537 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event All processors are scheduled for deconfiguration.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event All processors are scheduled for deconfiguration.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='All CPUs were scheduled to be deconfigured'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11538 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Processors have been reconfigured due to installation of a new processor type, or SFW revision change.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Processors have been reconfigured due to installation of a new processor type, or SFW revision change.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='All CPUs have been auto reconfigured'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11566 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event IO Backplane 3.3V power fault'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event IO Backplane 3.3V power fault: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='IO Backplane 3.3V power fault'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11567 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event IO Backplane 5.0V power fault'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event IO Backplane 5.0V power fault: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='IO Backplane 5.0V power fault'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11568 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event IO Backplane -12V power fault'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event IO Backplane -12V power fault: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='IO Backplane -12V power fault'

