DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5567 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event This indicates the failure in collecting the Complex profile info.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event This indicates the failure in collecting the Complex profile info.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This chassis code reports the failure in collecting the ICM parameters needed for the cell interleaving.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5568 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event This chassis code indicates the failure in collecting the cell info.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event This chassis code indicates the failure in collecting the cell info.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This chassis code indicates that the cell intearleaving routine could not get the information on the cell memory.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5569 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event This indicates the failure in updating the GNI info of the cell with CLM.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event This indicates the failure in updating the GNI info of the cell with CLM.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This chassis code is used to represent the failure in updating the GNI information of the cell with the CLM ( cell local memory) information obtained from the Complex Profile.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5570 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event This indicates the failure in adjusting the mem info with Minimum ZI req.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event This indicates the failure in adjusting the mem info with Minimum ZI req.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This represents the failure in adjusting the memory information with the minimum ZI requirements.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5572 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Complex Profile A has a checksum error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Complex Profile A has a checksum error: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Complex Profile A (Stable Profile) stored checksum does not match the calculated checksum. The expected data and actual data are displayed in the 2 reporting event Ids.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5573 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A Checksum error was encountered in the dynamic profile'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A Checksum error was encountered in the dynamic profile: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Dynamic Complex Profile (Group B) stored checksum did not equal the calculated checksum. The Expected Data and Actual date are displayed in successive chassis codes.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5574 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A checksum error occurred on the Partitioin Profile.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A checksum error occurred on the Partitioin Profile.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The stored value of the complex profile Group C does not match the calcuated value. Expected data and actual data are stored in successive chassis codes.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5575 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The Stable Complex Profile Sequence Id is invalid'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The Stable Complex Profile Sequence Id is invalid: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Complex Profile Group A sequence ID is invalid. Booting cannot continue. The actual data is in the chassis code data field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5577 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The Dynamic Complex Profile Sequence ID is invalid'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The Dynamic Complex Profile Sequence ID is invalid: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Dynamic Complex Profile (Group B) sequence ID is invalid. The invalid Sequence ID is displayed in the data field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5578 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The Partition Profile Sequence ID is invalid'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The Partition Profile Sequence ID is invalid: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Group C Partition Complex Profile Sequence ID is invalid. The value read is displayed in the data field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5579 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Internal Firmware Programming Error from the EFI portion of the firmware'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Internal Firmware Programming Error from the EFI portion of the firmware: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An internal EFI firmware error was encountered. This is usually caused by a bad parameter passed to a function, corrupt memory, corrupt malloc, corrupt firmware tree or something similar. The data field contains the IP address of the function'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='that encountered the error.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5580 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The PD numbers in Group A and Group C of the complex profile are inconsistant.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The PD numbers in Group A and Group C of the complex profile are inconsistant.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Complex Profile Group A PD assignment for this cell does not match the PD or Partition number in Group C of the complex profile. This is a fatal condition for the cell. The PD number from group A will be emmitted first, followed by a'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='subsequent code for the PD assigned in group C.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5581 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The PD number specified in the complex profile is out of range.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The PD number specified in the complex profile is out of range.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Partition (PD) assigned to this cell in the complex profile group A and C is larger than the maximum allowed number of PDs as specified by Group A.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5583 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Could not obtain the crossbar port semaphore'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Could not obtain the crossbar port semaphore: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Tried to obtain the port semaphore but GetPortSemaphore returned an ERROR. Could be a failed write to the port semaphore crossbar CSR or another cell owned the semaphore. Data field bits 32:63 contain the crossbar ID and bits 0:31 contain the'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='port number for which the semaphore was being obtained.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5584 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Could not release the crossbar port semaphore.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Could not release the crossbar port semaphore.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Currently owned the port semaphore but could not release the semaphore. Data field bits 32:63 contain the crossbar ID and bits 0:32 contain the port number.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5594 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event BMC token upload failure'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event BMC token upload failure: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='There was an error reading from the BMC token when attempting to write to SAL NVM. This is a stop boot condition. Data: Lower 32 bits, BMC Token Number. Upper 32 bits, bmc return status.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5595 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event NVM token access failure'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event NVM token access failure: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The read from SAL NVM has failed. This is a stop boot condition. Data: The token number on which the read failed'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5596 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event BMC token download failure'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event BMC token download failure: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='There was an error when trying to write to a BMC Token. This is a boot warning condition. Data: lower 32 bits are BMC token number, upper 32 bits is the status return from the BMC.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5597 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error Writing BMC first boot token'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error Writing BMC first boot token: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='There has been an error writing the BMC_FIRST_BOOT token. This is a stop boot condition.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5598 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Fru Id read error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Fru Id read error: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The read of a FRU has failed. Data: Device ID of device that failed the FRU read.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5599 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Fru Id checksum error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Fru Id checksum error: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The read of a FRU has failed the checksum test. Data: Device ID of device that failed the FRU read.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5600 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Fru Id version error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Fru Id version error: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The read of a FRU has failed due to a version problem. Data: Device ID of device that failed the FRU read.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5601 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Rom revision not equal to FIT revision'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Rom revision not equal to FIT revision: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A ROM Rev and FIT Rev do not match. Data: Code for what didn t match: 0x1 = PAL_A, 0x2 = PAL_B, 0x4 = SAL_A, 0x8 = ACPI, 0xA = EFI'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5602 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event ROM revision not equal to Rev block'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event ROM revision not equal to Rev block: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A ROM Rev and Rev Block do not match. Data: Code for what didn t match: 0x3 = PAL, 0x5 = SAL_A, 0x7 = SAL_B, 0x9 = ACPI, 0xB = EFI, 0xC = BMC'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5603 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Primary Fit bad'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Primary Fit bad: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The FIT is bad.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5604 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Secondary Fit bad'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Secondary Fit bad: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The FIT is bad.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5605 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PAL A execution rom warning'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PAL A execution rom warning: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='PAL_A_ROM has generated a warning.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5606 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PAL B execution rom warning'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PAL B execution rom warning: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='PAL_B_ROM has generated a warning.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5607 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An error was encountered when firmware tried to update the Group B Profile'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An error was encountered when firmware tried to update the Group B Profile: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware tried to default the Dynamic (Group B) complex profile and encountered an error.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5617 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PCI parity error detected.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PCI parity error detected.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An I/O device (or host bridge) detected a bus parity error. An I/O device (or host bridge) mastered a bus transaction and received a parity error response from the target. Data Field: Physical location of the I/O device (or host bridge).'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5618 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PCI system error detected'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PCI system error detected: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An I/O device (or host bridge) detected an internal error. An I/O device (or host bridge) detected a bus error. Data Field: Physical location of the I/O device (or host bridge).'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5619 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event I/O host bridge is deconfigured'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event I/O host bridge is deconfigured: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware has deconfigured an I/O host bridge due to an error (see earlier error event). Firmware will display the following EFI warning message,  Failed I/O slot(s) deconfigured.  Data Field: Physical location of the deconfigured I/O host'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='bridge.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5621 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Firmware was unable to publish the Partition Profile'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Firmware was unable to publish the Partition Profile: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware tried to default the Partition (Group C) complex profile and encountered an error.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5622 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The reporting cell is not configured to be in a PD.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The reporting cell is not configured to be in a PD.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Reporting Cell is not configured to be in a PD, according to Complex Profile Group A.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5623 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event DIMM thermal loading order warning'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event DIMM thermal loading order warning: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='DIMMs are not loaded on the extender in a thermally optimal way. Boot is still possible, but the DIMM arrangement should be changed to the loading order recommended in the users manual. The data field indicates the number of the extender with'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='incorrectly loaded DIMMs.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5626 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The PD cannot boot, a majority of cells did not arrive at Rendezvous'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The PD cannot boot, a majority of cells did not arrive at Rendezvous: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Not enough cells made the Rendezvous for boot to continue. The rules are listed in the cause action section.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5638 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event INIT: Monarch failed in slave rendezvous'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event INIT: Monarch failed in slave rendezvous: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='SFW s INIT handler failed to rendezvous the processors.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5646 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event MC: I/O error log/clear error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event MC: I/O error log/clear error: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='SFW s Machine Check Handler was unable to log or clear I/O error registers.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5655 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event MC: MCA to BERR escalation not supported by PAL'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event MC: MCA to BERR escalation not supported by PAL: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Cannot escalate an MCA to BERR'

