DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9496 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The SBA type is unknown to the system firmware'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The SBA type is unknown to the system firmware: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The SBA type is unknown to the system firmware. The I/O on the reporting cell is not available.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9497 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An embedded I/O device is missing.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An embedded I/O device is missing.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An expected I/O device cannot be detected by the system firmware.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9498 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Fabric link route around failed because the route around port was bad'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Fabric link route around failed because the route around port was bad: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT=' Too many broken links! The XBC port route around failed because the route-around port was bad too. Data field: (XBC port << 44) | (XBC num << 32) | port state'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9652 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Predictive Failure in Memory'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Predictive Failure in Memory: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='ECC (Error Checking and Correcting) memory is designed to detect and correct single-bit errors that occasionally occur in computer systems. This memory module is currently correcting many single bit errors.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9653 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Windows: Server Agents Management data not accessible, locked property'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Windows: Server Agents Management data not accessible, locked property: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Server Agents SNMP branch is not responding due to a portion of the IPMI Management Subsystem being locked by another entity.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9658 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PCI slot exceeds power limit'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PCI slot exceeds power limit: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A non-hot plug I/O slot s power consumption increases the total I/O power consumption beyond the supported limit. Firmware will display the following EFI error message,  I/O configuration exceeds power limit  and disallow O/S boot. Data Field:'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='Physical location of the I/O slot.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9659 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event (warning) Outputted in MFG, when Memory SBE Seeding is enabled'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event (warning) Outputted in MFG, when Memory SBE Seeding is enabled: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This is a warning that the system is running in a degregated mode. It will only be emitted in MFG mode when Memory SBE Seeding is enabled. This is only for testing of SBE seeding for LAB and possibly MFG use ONLY. It should NEVER be seen in'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='the field.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9661 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to read the fabric topology information from the XBC'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to read the fabric topology information from the XBC: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Read failure while writing the number of failed links to the XBC. Data Field: Return Status (SUCCESS = 0, FAILURE = -1)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9663 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PDC failed to initalize PA specific fields of group C after finding IA bit set.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PDC failed to initalize PA specific fields of group C after finding IA bit set.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='PDC could not access a complex profile. The partition will be reset because the available complex profile is not valid. Data field contains the return status from the function that encountered the error.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9666 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unexpected fabric firmware error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unexpected fabric firmware error: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An unexpected error occurred while initializing the fabric. The firmware is not able to analyze this error. Clues to the cause of this error may be found in the IPMI forward progress log (FPL) either shortly before or after this log entry'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='occurred. The FPL is available from the management processor using the  sl  command. HP-UX also saves these logs in the /var/stm/logs/os directory, and they can be viewed using the slview utility.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9668 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PDC could not read the copy of profile C stored in ICM'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PDC could not read the copy of profile C stored in ICM: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='PDC could not access a complex profile. The partition will be reset. Data field contains the return status from the function that encountered the error.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9670 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Could not disable the XIN link before a fabricless boot'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Could not disable the XIN link before a fabricless boot: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Before attempting a fabricless boot, the cell s link to the fabric should be disabled to provide isolation and stability. The link could not be disabled, so the cell will halt.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9674 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Fail to GetSiblingCpuCoreNum() in BootGetSpiromData()'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Fail to GetSiblingCpuCoreNum() in BootGetSpiromData(): &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Configuration information on the processor was invalid. The cell will be halted. Data field contains the return value from the function that encountered the error.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9678 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The clock ratio reported by manageability does not match the actual clock ratio'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The clock ratio reported by manageability does not match the actual clock ratio: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The clock ratio that the processor is running at does not match the clock ratio that manageability is reporting.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9681 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Manual override of fatal stop boot condition'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Manual override of fatal stop boot condition: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The user has manually bypassed a stop boot condition (caused by an error during boot) and continued to boot an O/S. The system might experience unpredictable failures.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9682 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Firmware unable to relocate VGA BIOS'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Firmware unable to relocate VGA BIOS: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware was unable to relocate the VGA BIOS to the hardcoded VGA BIOS region in main memory (physical address range 0xc0000 - 0xdffff). VGA routing has been disabled by firmware. No VGA device will be accessible on this boot.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9685 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The Compatability Matrix stored in NVRAM has a checksum error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The Compatability Matrix stored in NVRAM has a checksum error: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The componenet compatability matrix stored in NVRAM and used by system firmware has a checksum error. The stored value does not equal the calculated value. The data field will contain first the expected value, and the subsequent code will'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='contain the actual data.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9695 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PDC failed its attempt to get default RDR values'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PDC failed its attempt to get default RDR values: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='PDC could not read an internal CPU register. The partition will be reset. Data field is the return status from the function that encountered the error.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9696 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PDC could not read current RDR values of the executing CPU'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PDC could not read current RDR values of the executing CPU: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='PDC could not read an internal CPU register. The partition will be reset. Data field is the return status from the function that encountered the error.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9697 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PDC failed reading a specific value from its own copy of the RDRs'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PDC failed reading a specific value from its own copy of the RDRs: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='PDC failed reading a value out of its own copy of the internal CPU register settings. Data field is a status return indicating the type of failure.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9698 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PDC failed reading a specific value from its own copy of the RDRs'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PDC failed reading a specific value from its own copy of the RDRs: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='PDC failed reading a value out of its own copy of the internal CPU register settings. Data field is a status return indicating the type of failure.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9700 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PDC failed attempting to update ZLCO and PREFETCH RDR settings'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PDC failed attempting to update ZLCO and PREFETCH RDR settings: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='PDC attempted to update CPU registers to match their respective settings in the complex profile, but a failure was returned from the call to accomplish the update. Data field contains the failure.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9701 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PDC failed to read the HV Flag in the Partition Configuration Data'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PDC failed to read the HV Flag in the Partition Configuration Data: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='PDC could not access a complex profile. The partition will be reset.. Data field contains the return status from the function that encountered the error.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9706 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to get the configured set from the Complex Profiles A and C'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to get the configured set from the Complex Profiles A and C: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='PDC could not access a complex profile. The cell will be reset. Data field contains the return status from the function that encountered the error.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9707 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event No possible core cells were found in the configured set'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event No possible core cells were found in the configured set: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Could not find a potential core cell for the partition in the configured set. This cell will reset for reconfiguration. Data Field: return status from failing function'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9708 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Could not find a viable core cell in the partition'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Could not find a viable core cell in the partition: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The potential core cell was not viable (ie. no core I/O, etc). This cell will reset for reconfiguration. Data Field: bit mask of cells that made the rendezvous set'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9709 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Could not find a viable core cell in the partition'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Could not find a viable core cell in the partition: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The potential core cell was not viable (ie. no core I/O, etc). This cell will reset for reconfiguration. Data Field: bit mask of cells that made the rendezvous set'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9710 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The core cell selected is not in the rendezvoused partition'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The core cell selected is not in the rendezvoused partition: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The potential core cell did not rendezvous with the rest of the partition. This cell cannot talk to the selected core cell. This cell will reset for reconfiguration. Data Field: bit mask of cells that made the rendezvous set'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9711 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The local cell is not viable'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The local cell is not viable: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The local cell is disconnected from the rest of the system due to the main backplane configuration. While the partition is only configured to contain a single cell, the local cell is not a viable core cell. The cell will reset for'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='reconfiguration. Data Field: bit mask of cells that made the rendezvous set  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9712 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event cell cannot reach the fabric, partition contains 3 or more cells'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event cell cannot reach the fabric, partition contains 3 or more cells: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This cell has booted without the main backplane, probably due to prior main backplane errors. The partition it is in is configured with 3 or more cells. The combination of these two configurations is not allowed. The cell will reset for'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='reconfiguration. Data Field: configured set  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9719 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The RTC is providing inconsistent data.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The RTC is providing inconsistent data.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='While validating the internal RTC data the data is read twice and compared. If the comparison fails to match the read is performed again up a maximum of 50 times. If we cannot get a match in 50 retries we issue this event.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9727 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PDC failed to read the processor architecture for another cell in the partition'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PDC failed to read the processor architecture for another cell in the partition: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='PDC attempts to make sure that all of the cells in a partition are installed in the same processor architecture. PDC failed to read the architecture for another cell. PDC will reset all of the cells in the partition when this error is'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='detected. The data field contains the physical location of the cell reporting the event.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9740 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The buffer size is too small for the XBC error log'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The buffer size is too small for the XBC error log: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The buffer size passed in to the XBC error logging routine through SAL_GET_STATE_INFO, SAL_CLEAR_STATE_INFO, or MCA logging is too small for the XBC error log Data field consists of: XBC number (32:43)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9741 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event System firmware was unable to clear an XBC error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event System firmware was unable to clear an XBC error: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System firmware was unable to clear an XBC error. The data field contains: XBC number (32:43) port number (44:55) error type (0:31)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9742 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Firmware detected a possible Cabinet Power Timeout'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Firmware detected a possible Cabinet Power Timeout: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System Firmware detected a possible timeout waiting for the other cabinet to power on. System firmware queried the utilities system to see what cells are installed. This indicated that cells are installed in the other cabinet but none are'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='powered on. Firmware delayed fabric routing, waiting for the other cabinet cells to power on, but eventually timed out and went on.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9744 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error encountered while collecting PCI error logs'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error encountered while collecting PCI error logs: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='error code'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9745 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error encountered while collecting SBA error logs'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error encountered while collecting SBA error logs: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='error code'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9746 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Fabric is unable to route the crossbar after multiple retry attempts'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Fabric is unable to route the crossbar after multiple retry attempts: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='During fabric initialization, if a crossbar is found to be in an unexpected state, the number of retries is incremented. If the number of retries exceeds the maximum, then something is wrong and there is no way to initialize the fabric. Data'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='field: number of retries (0:31), crossbar number (32:63)  '

