DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7786 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event AC power to the PDCA was removed. Data Byte 3 specifies PDCA number.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event AC power to the PDCA was removed. Data Byte 3 specifies PDCA number.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The AC power connected to the PDCA (Power Distribution Control Assembly) was removed. The data field contains the physical location of the PDCA. The PDCA source that was deleted can be identified by the implementation dependent field (data'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='byte 3) of the physical location: data byte[3]: 0 for PDCA 0, 1 for PDCA 1.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7791 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cabinet Main Blower Failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cabinet Main Blower Failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A cabinet main blower has failed. Depending on the number of blowers still operating, the cabinet may or may not shut down. View the Error Log entries to determine if the cabinet is operating. If many log entries call out entities powering off'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='during the same time frame as this BLOWR_FAIL, the cabinet has probably shutdown. Carefully review the log for the first few events within the same time frame for the root cause of the problem. The GSP command, PS, will show a detailed power  '
DEFine MSGACTion Name=(*,40)
ACTION=ANNOTATE TEXT='status for a cabinet. If the +48V LED on the Front Panel Board is not lit, power is not enabled to the cabinet. This is an indication the cabinet blowers have probably gone from N to N - 1 status requiring an immediate cabinet shutdown." '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7793 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event 48 Volt Converter Failed. Data Byte 3 specifies PDCA number.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event 48 Volt Converter Failed. Data Byte 3 specifies PDCA number.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A 48 Volt DC Converter powered by the specified PDCA failed on the designated Bulk Power Supply. The PDCA powering the converter on the BPS that failed can be identified by the implementation dependent field (data byte 3) of the BPS  physical'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='location: data byte[3]: 0 for PDCA 0, 1 for PDCA 1.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7795 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Fan failed in designated Bulk Power Supply'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Fan failed in designated Bulk Power Supply: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The designated Bulk Power Supply is reporting its fan has failed. '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7796 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event 1 Side Converter Over Temp'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event 1 Side Converter Over Temp: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The 48 Volt DC Converter powered by the specified PDCA in the designated Bulk Power Supply, is in over temp condition. The PDCA powering the converter on the BPS that failed can be identified by the activity status (last byte of chassis code):'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='e = PDCA 1 f = PDCA 0  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7798 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Bulk Power Supplies are not Redundant.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Bulk Power Supplies are not Redundant.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The number of functioning Bulk Power Supplies has decreased to where the Cabinet Power supplied (number of available Bulk Power Supplies times power output per each) minus the estimated Cabinet Power consumed is greater than 0, but less than'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='the output of one Bulk Power Supply.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7799 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event +48V DC has exceeded its upper limit'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event +48V DC has exceeded its upper limit: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The PM has detected the value of +48V power, as measured on the UGUY board, has exceeded an upper threshold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7803 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event +48V DC has fallen below its lower limit'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event +48V DC has fallen below its lower limit: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The PM has detected the value of +48V power, as measured on the UGUY board, has fallen below a lower threshold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7806 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cabinet Fan Failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cabinet Fan Failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A cabinet fan has failed. Depending on the number of cabinet fans still operating, the cabinet may or may not shut down. View the Error Log entries to determine if the cabinet is operating.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7822 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Housekeeping power has exceeded expected levels.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Housekeeping power has exceeded expected levels.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Housekeeping power has exceeded expected levels.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7823 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Housekeeping power has fallen below expected levels.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Housekeeping power has fallen below expected levels.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Housekeeping power has fallen below expected levels.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7824 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The BPSs for the cabinet are illegally configured. Data Byte 3 = PDCA number.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The BPSs for the cabinet are illegally configured. Data Byte 3 = PDCA number.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Through failures or reconfiguration, the BPS for the cabinet named are illegally configured. There must be a BPS connected to each phase of the power. Phase 1 feeds BPS slots 0 & 1, phase 2 feeds slots 2 & 3, and phase 3 feeds 4 & 5. There'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='must be a BPS connected to each phase. If 4 BPS are installed in a cabinet in slots 0 - 3 and 4 & 5 were empty, this would be an illegal configuration. They should be installed in 0,1,2,and 4 or 0,1,3,and 5 or some combination thereof. The PDCA  '
DEFine MSGACTion Name=(*,40)
ACTION=ANNOTATE TEXT='physical location determines which phase is configured incorrectly. Data Byte 3 (implementation dependent field) indicates the PDCA number used when the configuration error occurred:" '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7825 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event BPS ID received from installed Bulk Power Supply was unknown'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event BPS ID received from installed Bulk Power Supply was unknown: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A Bulk Power Supply is reporting an unknown BPS ID. The Bulk Power Supply will not be powered up and added to the Power Available tally. If cabinet is not powered up, it will refuse to power up until this fault is corrected.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7827 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Ambient Air Sensor Overtemp Warning'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Ambient Air Sensor Overtemp Warning: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The cabinet s Ambient Air Sensor detected a change in air temperature entering the over-temp-high range. The Cabinet will be shutting itself down to prevent component damage.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7828 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Ambient Air Sensor Overtemp Warning'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Ambient Air Sensor Overtemp Warning: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The cabinet s Ambient Air Sensor detected a change in air temperature crossing to the low range. The air temperature may be rising or falling. This is just a reporting of entering the over-temp-low range.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7829 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Ambient Air Sensor Overtemp Warning'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Ambient Air Sensor Overtemp Warning: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The cabinet s Ambient Air Sensor detected a change in air temperature crossing to the mid range. The air temperature may be rising or falling. This is just a reporting of entering the over-temp-mid range..'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7836 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event IO Fan Failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event IO Fan Failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An IO Chassis cooling fan has failed. Depending on the number of fans still operating, the cabinet may or may not shut down. View Error Log entries to determine if the cabinet is operating. If many log entries call out entities powering off'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='during the same time frame as this IOFAN_FAIL, the cabinet has probably shutdown. Carefully review the log for the first few events within the same time frame for the root cause of the problem. The Guardian Service Processor command, PS, will  '
DEFine MSGACTion Name=(*,40)
ACTION=ANNOTATE TEXT='show a detailed power status for a cabinet. The +48V LED on the Front Panel Board not lit, power is not enabled to the cabinet, indicating the cabinet IO Chassis fans have probably gone from N to N - 1 status requiring an immediate cabinet  '
DEFine MSGACTion Name=(*,50)
ACTION=ANNOTATE TEXT='shutdown." '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7842 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cabinet Power System is in overload.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cabinet Power System is in overload.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This code is issued when the Cabinet Power supplied (number of Bulk Power Supplies times power output per each) minus the estimated Cabinet Power consumed drops below 0. Utilities firmware will not allow a cabinet in this state to power up'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='(see ABORT_PWRUP_BPS). Utilities firmware will not shut down a cabinet in this state. However, there is a possibility of a cabinet brownout, making the cabinet unreliable.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7845 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cabinet Shutdown - Insufficient Blowers'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cabinet Shutdown - Insufficient Blowers: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='After a BLOWR_FAIL, there were N-1 blowers functioning. This is an illegal condition causing immediate cabinet shutdown to prevent component damage.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7846 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cabinet Shutdown - Insufficient IO Fans'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cabinet Shutdown - Insufficient IO Fans: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='After a IOFAN_FAIL, there were N-1 fans functioning. This is an illegal condition causing immediate cabinet shutdown to prevent component damage.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7849 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event IO Expansion Utility Cabinet Fan Failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event IO Expansion Utility Cabinet Fan Failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='One of two fans in the Utility chassis of the IO Expansion Cabinet has failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7855 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Watchdog Timer Expired'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Watchdog Timer Expired: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Watchdog Timer checks for inactivity, or hung state, of the Cabinet Level Utilities (CLU) portion of the UGUY. During activity, the timer is continually reset. If the timer expires, it will automatically reset the CLU microprocessor. This'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='will not affect running partitions.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7856 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Invalid checksum from EEPROM'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Invalid checksum from EEPROM: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An invalid checksum was received when reading the FRUID EEPROM for the device named in the chassis code. If this is a single error, the fault lies with the named FRU. If there are many INVALID_CKSM entries in the Event Log, there is probably a'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='problem with the I2C bus.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7858 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event System Backplane Power Board Fault'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event System Backplane Power Board Fault: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT=' One or more of the System Backplane Power Boards is reporting a DC Fault through the System Backplane Local Power Monitor. The physical location of the failing power board is in the Data Field of the event.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7863 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Read of EEPROM failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Read of EEPROM failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An attempt to read the EEPROM (FRUID) on the IO Backplane Board failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7864 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Read of EEPROM failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Read of EEPROM failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An attempt to read the EEPROM (FRUID) on the IO Backplane Power Board failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7865 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Read of LPM Fault failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Read of LPM Fault failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An attempt to read the Local Power Monitor Fault register on the IO Backplane Power Board failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7866 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event IO Power Board Overtemperature'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event IO Power Board Overtemperature: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Local Power Monitor of the named IO Chassis is reporting a Power Brick overtemperature condition.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7867 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event IO Power Board Fault'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event IO Power Board Fault: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Local Power Monitor on the named IO Chassis has reported a power fault condition.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7871 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Voltage Margin on IO Power Board failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Voltage Margin on IO Power Board failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Local Power Monitor on the named IO Power Board failed to properly margin the power as commanded.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7872 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failure to read data from a FRUID EEPROM'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failure to read data from a FRUID EEPROM: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='During command execution or as part of initialization, the data from a FRUID EEPROM failed to be read. This does not necessarily mean the FRU has failed, just that the FRUID can t be read. The data field is defined as follows: data field:'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='0xXXXXFFFFFFFFFFFF Where XXXX is the specific FRU Handle of the failing FRUID. The bits are defined as follows: FRU handle Reserved fields should be set to zero to be forward compatible with future FRU handle modifications Bits 15 - 12: Cabinet  '
DEFine MSGACTion Name=(*,40)
ACTION=ANNOTATE TEXT='number field Bits 11 - 9: FRU family field 0 - Utility 1 - Misc 2 - Power 3 - Memory 4 - Reserved 5 - Reserved 6 - Reserved 7 - Reserved Bits 8 - 0: Free format field based on FRU family field Utility family field Bits 8 - 6: Utility type field  '
DEFine MSGACTion Name=(*,50)
ACTION=ANNOTATE TEXT='0 - MP Bits 5 - 0: Reserved 1 - SBCH Bits 5 - 0: Reserved 2 - UGUY Bits 5 - 0: Reserved 3 - CIO Bits 5 - 4: Reserved Bits 3 - 2: Master IO backplane number Bits 1 - 0: IO bay number 4 - PDH daughtercard Bits 5 - 3: Reserved Bits 2 - 0: Slot  '
DEFine MSGACTion Name=(*,60)
ACTION=ANNOTATE TEXT='number 5 - Reserved Bits 5 - 0: Reserved 6 - Reserved Bits 5 - 0: Reserved 7 - Reserved Bits 5 - 0: Reserved Misc family field Bits 8 - 6: Misc type field 0 - Main backplane Bits 5 - 0: Reserved 1 - IO bay Bits 5 - 4: Reserved Bits 3 - 2:  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7873 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failure to read data from a SBCH FRUID EEPROM'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failure to read data from a SBCH FRUID EEPROM: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Either by command or as part of initialization, the data from a FRUID EEPROM failed a read command. This does not necessarily mean the FRU has failed, just that the FRUID data cannot be read.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7874 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failure to read data from a UGUY FRUID EEPROM'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failure to read data from a UGUY FRUID EEPROM: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Either by command or as part of initialization, the data from a FRUID EEPROM failed a read command. This does not necessarily mean the FRU has failed, just that the FRUID can t be read.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7875 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Read EEPROM failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Read EEPROM failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An attempt to read the EEPROM (FRUID) on the System Backplane failed'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7877 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Read command on System Backplane I2C bus failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Read command on System Backplane I2C bus failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A read command on the system backplane I2C bus failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7878 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Write command on System Backplane I2C bus failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Write command on System Backplane I2C bus failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A write command on the system backplane I2C bus failed. The type of command that failed can be identified by the activity status field (last byte) of the encoded field. B = RC Cable Configuration Register write C = Backplane Voltage Margin'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='Register write 9 = Flex circuit configuration register write  '

