DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9896 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Not enough error free memory to run late sefltests'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Not enough error free memory to run late sefltests: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='There was not enough error free memory in the system to run the late selftests.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10060 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The left cell latch is open.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The left cell latch is open.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The left cell ejector on the specified cell is open.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10061 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Right ejector latch is open'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Right ejector latch is open: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The right ejector latch on the specified cell board is open.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10062 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The optical emitters on the cell latch sensors are not functioning'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The optical emitters on the cell latch sensors are not functioning: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The optical emitters on the cell latch sensors are not functioning.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10063 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The vrm on the specified cell is reporting a voltage fault.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The vrm on the specified cell is reporting a voltage fault.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The specified vrm is reporting a fault.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10064 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The vrm on the specified cell is reporting a temperature fault.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The vrm on the specified cell is reporting a temperature fault.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The specified vrm is reporting a fault.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10065 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The rail on a cell is reporting a fault.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The rail on a cell is reporting a fault.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The specified rail is reporting a fault.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10068 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A I/O backplane vrm is reporting a voltage fault.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A I/O backplane vrm is reporting a voltage fault.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The specified pci vrm is reporting a voltage fault.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10069 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A I/O backplane power brick is reporting a voltage fault.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A I/O backplane power brick is reporting a voltage fault.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The specified pci power brick is reporting a voltage fault.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10070 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A I/O backplane vrm is reporting a temperature fault.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A I/O backplane vrm is reporting a temperature fault.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The specified vrm is reporting a temperature fault.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10071 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A I/O backplane power brick is reporting a temperature fault.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A I/O backplane power brick is reporting a temperature fault.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The specified pci power brick is reporting a temperature fault.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10072 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A I/O backplane vrm rail is reporting a fault.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A I/O backplane vrm rail is reporting a fault.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The specified vrm rail is reporting a fault.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10073 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A I/O backplane power brick is reporting a rail fault.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A I/O backplane power brick is reporting a rail fault.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The specified pci brick is reporting a fault.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10103 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The specified system backplane vrm is reporting a module voltage fault.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The specified system backplane vrm is reporting a module voltage fault.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The specified system backplane vrm is reporting a module voltage fault.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10104 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The specified system backplane vrm is reporting a temperature fault.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The specified system backplane vrm is reporting a temperature fault.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The specified system backplane vrm is reporting a temperature fault.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10105 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The specifed system backplane rail is reporting a fault'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The specifed system backplane rail is reporting a fault: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The specifed system backplane rail is reporting a fault'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10115 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Master MP failure. Slave MP has taken control'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Master MP failure. Slave MP has taken control: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The master mp has failed. The slave has taken over management of the cabinet.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10116 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The NVRAM service was unable to satisfy an NVRAM allocation request'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The NVRAM service was unable to satisfy an NVRAM allocation request: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The NVRAM service was unable to satisfy an NVRAM allocation request.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10132 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The RTC not updating its internal time registers'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The RTC not updating its internal time registers: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The RTC seems to not be updating its internal time registers. The cell cannot boot without the RTC.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10159 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Uncorrectable PAA fault on MX2'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Uncorrectable PAA fault on MX2: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An uncorrectable Power Aware Architecture (PAA) fault has occurred on the MX2 module and PAA firmware has halted. The system will continue to run without PAA firmware.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10209 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event fabric API is about to open the a link going out of the local cell'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event fabric API is about to open the a link going out of the local cell: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='fabric API is about to open the a link going out of the local cell'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10272 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An Arches fabric CSR read was unsuccessful because of a timeout.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An Arches fabric CSR read was unsuccessful because of a timeout.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An Arches fabric CSR read was unsuccessful because of a timeout.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10273 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An Arches fabric CSR write was unsuccessful.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An Arches fabric CSR write was unsuccessful.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An Arches fabric CSR write was unsuccessful'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10343 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The event data details the error that was encountered'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The event data details the error that was encountered: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The event data details the error return status from Phase3BackToBackPrep. Internal debug only, this refers to an unexpected firmware error or data corruption.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10351 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The maximum memory supported by this system has been exceeded.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The maximum memory supported by this system has been exceeded.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The maximum memory supported by this system has been exceeded. The data field contains the amount of memory supported by the system.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10357 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to delete a bad port while routing the fabric. Data field indicates return status.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to delete a bad port while routing the fabric. Data field indicates return status.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failed to delete a bad port while routing the fabric. Data field indicates return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10358 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to delete an edge that was found to be bad during routing.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to delete an edge that was found to be bad during routing.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='failed to delete an edge that was found to be bad during routing'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10361 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A command to the memory buffer chip failed to complete.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A command to the memory buffer chip failed to complete.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A command to the memory buffer chip failed to complete.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10375 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The Arches Fabric function ArfIsCsrRouteTraversable was called for a back-to-back system. This is unsupported, ArfIsCsrRouteTraversable should only be called for systems with crossbars. No data.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The Arches Fabric function ArfIsCsrRouteTraversable was called for a back-to-back system. This is unsupported, ArfIsCsrRouteTraversable should only be called for systems with crossbars. No data.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Arches Fabric function ArfIsCsrRouteTraversable was called for a back-to-back system. This is unsupported, ArfIsCsrRouteTraversable should only be called for systems with crossbars. No data.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10376 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An invalid port number was given as an input to an Arches Fabric Traversability function. The port is expected to be an internal XBC num (8-15), but the actual port was not. Data field: (XBC number 32) | (port number 48).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An invalid port number was given as an input to an Arches Fabric Traversability function. The port is expected to be an internal XBC num (8-15), but the actual port was not. Data field: (XBC number 32) | (port number 48).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An invalid port number was given as an input to an Arches Fabric Traversability function. The port is expected to be an internal XBC num (8-15), but the actual port was not. Data field: (XBC number << 32) | (port number << 48)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10377 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unable to read XBC port neighbor information. Data field: (xbcNum 32) | (portNum 48).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unable to read XBC port neighbor information. Data field: (xbcNum 32) | (portNum 48).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Unable to read XBC port neighbor information. Data field: (xbcNum << 32) | (portNum << 48)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10378 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event XBC port with an unexpected neighbor chip type. Data field: (expected chip type) | (actual chip type 16) | (xbcNum 32) |(portNum 48).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event XBC port with an unexpected neighbor chip type. Data field: (expected chip type) | (actual chip type 16) | (xbcNum 32) |(portNum 48).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='XBC port with an unexpected neighbor chip type. Data field: (expected chip type) | (actual chip type << 16) | (xbcNum << 32) | (portNum << 48)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10379 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An XBC port was found to have an unexpected neighbor ID. Data field: (expected NID) | (actual NID 16) | (xbcNum 32) | (portNum 48)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An XBC port was found to have an unexpected neighbor ID. Data field: (expected NID) | (actual NID 16) | (xbcNum 32) | (portNum 48): &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An XBC port was found to have an unexpected neighbor ID. Data field: (expected NID) | (actual NID << 16) | (xbcNum << 32) | (portNum << 48)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10380 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An XBC was found to have an unexpected neighbor port connection. Data field: (expected port) | (actual port 16) | (xbcNum 32) | (portNum 48)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An XBC was found to have an unexpected neighbor port connection. Data field: (expected port) | (actual port 16) | (xbcNum 32) | (portNum 48): &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An XBC was found to have an unexpected neighbor port connection. Data field: (expected port) | (actual port << 16) | (xbcNum << 32) | (portNum << 48)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10381 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The expected data was not found in the Arches Fabric expected edge list. Data field is unused.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The expected data was not found in the Arches Fabric expected edge list. Data field is unused.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The expected data was not found in the Arches Fabric expected edge list. Data field is unused'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10382 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An XBC port has an unexpected neighbor chip type. Data field: neighbor type found.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An XBC port has an unexpected neighbor chip type. Data field: neighbor type found.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An XBC port has an unexpected neighbor chip type. Data field: neighbor type found, bits [7:0], other bits unused'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10384 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A previously good XBC-XBC link was found to be down. Data field: (xbcNum 32) | (portNum 48).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A previously good XBC-XBC link was found to be down. Data field: (xbcNum 32) | (portNum 48).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A previously good XBC-XBC link was found to be down. Data field: (xbcNum << 32) | (portNum << 48)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10385 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An XBC port was found to have a Fatal Error during traversability test. Data field: (xbcNum 32) | (portNum 48).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An XBC port was found to have a Fatal Error during traversability test. Data field: (xbcNum 32) | (portNum 48).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An XBC port was found to have a Fatal Error during traversability test. Data field: (xbcNum << 32) | (portNum << 48)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10386 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unable to read the local cell s LINK_SEL_FABRIC CSR. Data field: unused'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unable to read the local cell s LINK_SEL_FABRIC CSR. Data field: unused: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Unable to read the local cell s LINK_SEL_FABRIC CSR Data field: unused'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10387 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unable to read the XBC route table. Data field: (route index) | (xbcNum 32) | (portNum 48).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unable to read the XBC route table. Data field: (route index) | (xbcNum 32) | (portNum 48).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Unable to read the XBC route table. Data field: (route index) | (xbcNum << 32) | (portNum << 48)'

