DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 752 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Temperature sensor crossed lower non-critical threshold'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Temperature sensor crossed lower non-critical threshold: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='One of the temperature sensors crossed its lower non-critical threshold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 753 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A temperature inside the server went far outside the factory specified range'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A temperature inside the server went far outside the factory specified range: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='One of the temperature sensors crossed its upper critical threshold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 754 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Temperature sensor crossed upper non-recoverable threshold.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Temperature sensor crossed upper non-recoverable threshold.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='One of the temperature sensors crossed its upper non-recoverable threshold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 4 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A temperature inside the server has gone outside the factory specified range.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A temperature inside the server has gone outside the factory specified range.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='One of the temperature sensors crossed its upper non-critical threshold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A temperature inside the server has gone far outside the factory specified range.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A temperature inside the server has gone far outside the factory specified range.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='One of the temperature sensors crossed its upper critical threshold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 6 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Temperature sensor crossed upper non-recoverable threshold'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Temperature sensor crossed upper non-recoverable threshold: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='One of the temperature sensors crossed its upper non-recoverable threshold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 755 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event One of the temperature sensors crossed its upper non-critical threshold.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event One of the temperature sensors crossed its upper non-critical threshold.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A temperature inside the server has gone outside the factory specified range.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 756 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A temperature inside the server went far outside the factory specified range.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A temperature inside the server went far outside the factory specified range.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='One of the temperature sensors crossed its upper critical threshold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A measured voltage in the server has gone far outside the factory specified lower voltage range.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A measured voltage in the server has gone far outside the factory specified lower voltage range.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='One of the voltage sensors crossed its lower critical threshold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Voltage sensor crossed lower non-recoverable threshold'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Voltage sensor crossed lower non-recoverable threshold: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='One of the voltage sensors crossed its lower non-recoverable threshold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A measured voltage in the server has gone outside the factory specified upper voltage range.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A measured voltage in the server has gone outside the factory specified upper voltage range.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='One of the voltage sensors crossed its upper non-critical threshold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Voltage sensor crossed upper non-recoverable threshold'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Voltage sensor crossed upper non-recoverable threshold: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='One of the voltage sensors crossed its upper non-recoverable threshold - Check all boards with this voltage'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 704 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Voltage insufficient'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Voltage insufficient: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Voltage fault - Check all boards with this voltage'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 728 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Voltage reached critical level'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Voltage reached critical level: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Voltage degraded to critical level from less severe - Check all boards with this voltage'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 705 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Voltage reached critical level'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Voltage reached critical level: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Voltage degraded to non-recoverable level from less severe - Check all boards with this voltage'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 706 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Power Pod Voltage Fault'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Power Pod Voltage Fault: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Voltage becomes non-recoverable from either critical level or less severe level - Check all boards with this voltage'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 707 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Voltage absent'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Voltage absent: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Voltage absent'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 710 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Fan speed lags'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Fan speed lags: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Fan speed lags'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 26 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The server s built-in sensors have detected an open chassis door.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The server s built-in sensors have detected an open chassis door.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The chassis has been opened.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 730 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The BMC firmware did not detect the system firmware boot'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The BMC firmware did not detect the system firmware boot: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The BMC firmware did not detect the system firmware boot.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 727 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Power supply failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Power supply failed: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Power supply failure detected.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 720 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Power supply failure'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Power supply failure: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Power supply failed or disconnected'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 732 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The power supply sensors detect a possible problem'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The power supply sensors detect a possible problem: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Power supply s sensors detect possible problems'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 722 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Power supply AC lost'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Power supply AC lost: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Power supply AC lost'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 757 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The AC voltage to the power supply was lost or is out of range.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The AC voltage to the power supply was lost or is out of range.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Power Supply AC voltage was lost or is out of range.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 758 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The power supply AC voltage is out of range.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The power supply AC voltage is out of range.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The AC voltage connected to the power supply is out of range.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 62 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Power supply subsystem redundancy lost.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Power supply subsystem redundancy lost.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Power supply subsystem redundancy lost.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 731 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A/C Power failed, disconnected, or out of range'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A/C Power failed, disconnected, or out of range: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A/C Failed, disconnected, or out of range'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 726 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Power failure in power supply'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Power failure in power supply: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A/C Failed, disconnected, or out of range'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 733 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cooling unit warning'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cooling unit warning: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Cooling unit warning'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 734 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cooling unit failure'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cooling unit failure: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Cooling unit failure'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 518 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Uncorrectable multi-bit ECC error has occurred'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Uncorrectable multi-bit ECC error has occurred: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Uncorrectable multi-bit ECC error has occurred in memory module'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 76 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Hot swap Cage: Drive removed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Hot swap Cage: Drive removed: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A drive has been removed'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 700 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Generic trap for Critical or Fatal type E0 event from system firmware'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Generic trap for Critical or Fatal type E0 event from system firmware: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System firmware error'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 744 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event System event log almost full'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event System event log almost full: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System event log almost full'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 735 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event BMC entering special mode'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event BMC entering special mode: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='BMC entering special mode'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 729 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event System shut-down or reset caused by sensor reading'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event System shut-down or reset caused by sensor reading: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System shut-down or reset caused by sensor reading. '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 745 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event TOC interrupt (crash dump)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event TOC interrupt (crash dump): &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='TOC interrupt (crash dump)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 746 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event INIT Initiated'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event INIT Initiated: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='INIT Initiated'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 751 * * * 1.3.6.1.4.1.11.2.23.45.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PCI parity error detected'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PCI parity error detected: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='PCI parity error detected'

