DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5140 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PCI bus unmap unknown error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PCI bus unmap unknown error: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware encountered an unexpected error while attempting to clear resource allocations on an I/O host bridge s I/O devices. Data Field: Physical location of the I/O host bridge.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5141 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PCIXCAP sampling error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PCIXCAP sampling error: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An I/O host bridge failed to determine the appropriate PCI[X] mode and frequency (PCI, PCI-X 66 MHz, PCI-X 133 MHz, etc.) for its bus. Firmware will deconfigure the I/O host bridge and display the following EFI warning message,  Failed I/O'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='slot(s) deconfigured.  Data Field: Physical location of the failed I/O host bridge.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5142 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Power monitor failed to respond'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Power monitor failed to respond: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware is unable to access the power monitor. Firmware will assume that there is sufficient power and proceed to power on an I/O slot. Data Field: Physical location of the I/O slot.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5143 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event I/O rope reset failed to complete'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event I/O rope reset failed to complete: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An I/O controller rope reset did not complete within the expected time limit. Firmware will deconfigure the I/O host bridge attached to the rope. Data Field: Physical location of the deconfigured I/O host bridge.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5144 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event I/O SBA clear error failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event I/O SBA clear error failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='During I/O chipset configuration, firmware found a persistent error condition. Firmware will attempt to continue the boot. Data Field: Physical location of the I/O chipset.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5145 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PCI slot has incorrect default power state'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PCI slot has incorrect default power state: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='During boot, firmware has found a hot-plug I/O slot with an incorrect default power state. The slot power should be off by default. Data Field: Physical location of the I/O slot.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5146 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PCI slot power on error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PCI slot power on error: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware encountered an error while attempting to power on an I/O slot. Firmware will deconfigure the I/O slot and display the following EFI warning message,  Failed I/O slot(s) deconfigured.  Data Field: Physical location of the I/O slot.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5147 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PCI slot s standby power failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PCI slot s standby power failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An I/O slot s standby (Vaux) power has failed. Firmware will deconfigure the I/O slot and display the following EFI warning message,  Failed I/O slot(s) deconfigured.  Data Field: Physical location of the failed I/O slot.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5148 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Found invalid PCIXCAP value'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Found invalid PCIXCAP value: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An I/O host bridge or hot-plug controller reported an illegal PCI[X] bus mode for its bus or slot, respectively. Firmware will deconfigure the I/O host bridge or I/O slot and display the following EFI warning,  Failed I/O slot(s)'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='deconfigured.  Data Field: Physical location of the failed I/O host bridge or the failed I/O slot.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5149 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unsupported rope frequency'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unsupported rope frequency: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware attempted to configure an I/O controller rope to an unsupported frequency. Firmware will deconfigure any I/O host bridge connected to the rope and display the following EFI warning message,  Failed I/O slot(s) deconfigured.  Data'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='Field: Physical location of the failed rope.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5150 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unsupported host bridge type'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unsupported host bridge type: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware has found an unsupported I/O host bridge type. Firmware will deconfigure the I/O host bridge and display the following EFI warning message,  Failed I/O slot(s) deconfigured.  Data Field: Physical location of the I/O host bridge.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5152 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Machine Check initiated'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Machine Check initiated: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A Machine Check has been initiated'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5155 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error in temporary mdt area'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error in temporary mdt area: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='There has been a problem building the Memory Data Table (MDT).'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5156 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to find lmmio entry in mdt'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to find lmmio entry in mdt: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='There has been a problem building the Memory Data Table (MDT).'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5157 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Memory page zero bad'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Memory page zero bad: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Memory page 0 was slated for deallocation in the PDT. EFI cannot launch with page 0 bad, so the system will halt.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5158 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to find space in mdt'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to find space in mdt: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='There has been a problem building the Memory Data Table (MDT).'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5159 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Media failure: info was not retrieved/logged'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Media failure: info was not retrieved/logged: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='There has been a media failure.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5160 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Bus interface register test failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Bus interface register test failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Indicates that the chipset register test has failed. The data field contains the physical address of the failing register.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5161 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Memory ECC normal write/read test failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Memory ECC normal write/read test failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='After FW s first access to main memory, FW detected that the CEC logged an error after reading back what was just written.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5171 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event DIMM loading order error: DIMM deallocated'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event DIMM loading order error: DIMM deallocated: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A DIMM that is required to be loaded in order for this DIMM to function properly is not loaded, so FW will deallocate this DIMM. Currently, none of the platforms require any DIMMs to be loaded in order for this DIMM to work properly.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5172 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event DIMM SPD checksum failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event DIMM SPD checksum failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The DIMM specified by the physical location has an SPD EEPROM that has a bad checksum. The Data field is the physical location of the DIMM.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5173 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event DIMM SPD fatal error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event DIMM SPD fatal error: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Detected a error in DIMM SPD'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5174 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unsupported memory DIMM type'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unsupported memory DIMM type: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A DIMM was installed whose DIMM type is not compatible with the current set of supported DIMMs for this platform.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5175 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The DIMM type of this DIMM doesn t match with others in the DIMM group'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The DIMM type of this DIMM doesn t match with others in the DIMM group: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The DIMM type of this DIMM is not the same as the other DIMMs in the same group. The group of DIMMs is deallocated. If this is the last active group of DIMMs in the system, the system is halted.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5176 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The DIMM type table is full. New DIMM type cannot be added.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The DIMM type table is full. New DIMM type cannot be added.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The DIMM type table is full'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5179 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event DIMM number not found in DMT Table'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event DIMM number not found in DMT Table: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An entry for the DIMM was not found in the DMT table. The data field contains the DMT entry that the caller wanted to find (in Dimm number format, which is 2 bytes, upper byte is the extender number, lower byte is the chipselect of the rank'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='caller is looking for.)  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5180 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Memory ECC multiple-bit data error detection failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Memory ECC multiple-bit data error detection failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The FW selftest of CEC multi-bit error (MBE) detection has failed. The upper 32 bits of the data field contain the Dword offset within the cacheline of the failed MBE detection. The lower 32 bits are split in two, and they contain the bit'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='numbers within the Dword that were flipped in order to cause an MBE.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5181 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Memory ECC multiple-bit ECC error signalling failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Memory ECC multiple-bit ECC error signalling failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The FW selftest of CEC multi-bit error (MBE) signaling has failed. The upper 32 bits of the data field contain the Dword offset within the cacheline of the failed MBE detection. The lower 32 bits are split in two, and they contain the bit'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='numbers within the Dword that were flipped in order to cause an MBE.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5182 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Memory ECC single-bit data error detection failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Memory ECC single-bit data error detection failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The FW selftest of CEC single-bit error (SBE) detection has failed. The data field contains the bit within the Dword that was flipped that caused the CEC to not see an SBE.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5183 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Memory ECC single-bit ECC error detection failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Memory ECC single-bit ECC error detection failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The FW selftest of CEC single-bit error (SBE) detection has failed. The data field contains the bit within the Dword that was flipped that caused the CEC to not see an SBE.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5185 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Insufficient memory for operation'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Insufficient memory for operation: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Memory FW detected errors below 1MB. FW will not allow boot in this case, so memory FW will reinterleave and retest.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5186 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Memory address not found in MBAT'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Memory address not found in MBAT: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Memory FW could not figure out which rank maps to the physical address specified in the data field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5187 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Memory Error Information not cleared'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Memory Error Information not cleared: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Memory FW was unable to clear the platform error logs on the CEC. The Datafield contains the error status of the CEC.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5189 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Couldn t clear memory error logs'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Couldn t clear memory error logs: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Memory FW was unable to clear the platform error logs on the CEC. The Datafield contains the error status of the CEC.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5190 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Memory error clear failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Memory error clear failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Error registers in the CEC have failed to clear. The data field contains the error status of the CEC after the attempted clear.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5191 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event DIMM loading order error: DIMM deallocated'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event DIMM loading order error: DIMM deallocated: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A DIMM that is required to be loaded in order for this DIMM to function properly is not loaded, so FW will deallocate this DIMM. Currently, none of the platforms require any DIMMs to be loaded in order for this DIMM to work properly.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5193 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Generic memory firmware error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Generic memory firmware error: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred that memory FW does not know how to handle.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5199 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Memory interleaving algorithm failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Memory interleaving algorithm failed: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The memory interleaving code failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5202 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Memory interleave generation failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Memory interleave generation failed: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='FW was unable to create a memory configuration with no errors in low memory to hand off to EFI.'

