--MibName=cpqSsStorageSys
-- ****************************************************************************
--
--                            Storage Systems
--         Management Information Base for SNMP Network Management
--
--
--      Copyright 1992,2005 Hewlett-Packard Development Company, L.P.
--      Hewlett-Packard Company shall not be liable for technical or
--      editorial errors or omissions contained herein. The information in
--      this document is provided "as is" without warranty of any kind and
--      is subject to change without notice. The warranties for HP products
--      are set forth in the express limited warranty statements
--      accompanying such products. Nothing herein should be construed as
--      constituting an additional warranty.
--
--      Confidential computer software. Valid license from HP required for
--      possession, use or copying. Consistent with FAR 12.211 and 12.212,
--      Commercial Computer Software, Computer Software Documentation, and
--      Technical Data for Commercial Items are licensed to the U.S.
--      Government under vendor's standard commercial license.
--
--      Refer to the READMIB.RDM file for more information about the
--      organization of the information in the Compaq Enterprise.
--
--      The Compaq Enterprise number is 232.
--      The ASN.1 prefix to, and including the Compaq Enterprise is:
--           1.3.6.1.4.1.232
--
-- ****************************************************************************

CPQSTSYS-MIB DEFINITIONS ::= BEGIN

    IMPORTS
        compaq                  FROM CPQHOST-MIB
        enterprises             FROM RFC1155-SMI
        Counter                 FROM RFC1155-SMI
        DisplayString           FROM RFC1213-MIB
        OBJECT-TYPE             FROM RFC-1212
        TRAP-TYPE               FROM RFC-1215
        sysName                 FROM RFC1213-MIB
        cpqHoTrapFlags          FROM CPQHOST-MIB;

  compaq            OBJECT IDENTIFIER ::= { enterprises 232 }

    cpqSsStorageSys   OBJECT IDENTIFIER ::= { compaq 8 }
    cpqSsMibRev       OBJECT IDENTIFIER ::= { cpqSsStorageSys 1 }
    cpqSsDrvBox       OBJECT IDENTIFIER ::= { cpqSsStorageSys 2 }
    cpqSsTrap         OBJECT IDENTIFIER ::= { cpqSsStorageSys 3 }
    cpqSsRaidSystem   OBJECT IDENTIFIER ::= { cpqSsStorageSys 4 }
    cpqSsBoxExtended  OBJECT IDENTIFIER ::= { cpqSsDrvBox 2 }

-- ****************************************************************************
--   Storage System MIB Revision
--   ===========================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSsStorageSys Group          (1.3.6.1.4.1.232.8)
--       cpqSsMibRev Group             (1.3.6.1.4.1.232.8.1)
--
--
--      An agent conforming to this document will return a cpqSsMibRevMajor
--      of one (1) and a cpqSsMibRevMinor of twenty six (26).
--
--    Implementation of the MibRev group is mandatory.
--
-- ****************************************************************************

    cpqSsMibRevMajor OBJECT-TYPE
        SYNTAX  INTEGER (1..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "The Major Revision level.
         A change in the major revision level represents a major change in
         the architecture of the MIB.  A change in the major revision level
         may indicate a significant change in the information supported
         and/or the meaning of the supported information, correct
         interpretation of data may require a MIB document with the same
         major revision level."
    ::= { cpqSsMibRev 1 }

    cpqSsMibRevMinor OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "The Minor Revision level.
         A change in the minor revision level may represent some minor
         additional support; no changes to any pre-existing information
         has occurred."
    ::= { cpqSsMibRev 2 }

    cpqSsMibCondition OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            ok(2),
            degraded(3),
            failed(4)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The overall condition (status) of the system represented by
            this MIB."
        ::= { cpqSsMibRev 3 }

-- ****************************************************************************
--   Storage System Drive Box Group
--   ==============================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSsStorageSys Group          (1.3.6.1.4.1.232.8)
--       cpqSsDrvBox Group             (1.3.6.1.4.1.232.8.2)
--        cpqSsDrvBoxTable             (1.3.6.1.4.1.232.8.2.1)
--
--  Implementation of the Drive Box group is mandatory.
--
-- ****************************************************************************

    cpqSsDrvBoxTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSsDrvBoxEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
        "Drive Box Table."
    ::= { cpqSsDrvBox 1 }

    cpqSsDrvBoxEntry OBJECT-TYPE
        SYNTAX  CpqSsDrvBoxEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
        "Drive Box Entry."
    INDEX   { cpqSsBoxCntlrIndex, cpqSsBoxBusIndex }
    ::= { cpqSsDrvBoxTable 1 }

        CpqSsDrvBoxEntry ::= SEQUENCE
        {
              cpqSsBoxCntlrIndex            INTEGER,
              cpqSsBoxBusIndex              INTEGER,
              cpqSsBoxType                  INTEGER,
              cpqSsBoxModel                 DisplayString,
              cpqSsBoxFWRev                 DisplayString,
              cpqSsBoxVendor                DisplayString,
              cpqSsBoxFanStatus             INTEGER,
              cpqSsBoxCondition             INTEGER,
              cpqSsBoxTempStatus            INTEGER,
              cpqSsBoxSidePanelStatus       INTEGER,
              cpqSsBoxFltTolPwrSupplyStatus INTEGER,
              cpqSsBoxBackPlaneVersion      INTEGER,
              cpqSsBoxTotalBays             INTEGER,
              cpqSsBoxPlacement             INTEGER,
              cpqSsBoxDuplexOption          INTEGER,
              cpqSsBoxBoardRevision         INTEGER,
              cpqSsBoxSerialNumber          DisplayString,
              cpqSsBoxCntlrHwLocation       DisplayString,
              cpqSsBoxBackplaneSpeed        INTEGER,
              cpqSsBoxConnectionType        INTEGER,
              cpqSsBoxHostConnector         DisplayString,
              cpqSsBoxBoxOnConnector        INTEGER,
              cpqSsBoxLocationString        DisplayString
        }

    cpqSsBoxCntlrIndex OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Drive Box Controller Index.

        The controller index indicates to which adapter card instance
        this table entry belongs."
    ::= { cpqSsDrvBoxEntry 1 }

    cpqSsBoxBusIndex OBJECT-TYPE
        SYNTAX  INTEGER (1..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Drive Box Bus Index.

        The bus index indicates to which bus instance on an adapter card
        this table entry belongs.  The instances start at one and
        increment for each bus on a card."
    ::= { cpqSsDrvBoxEntry 2 }

    cpqSsBoxType OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          proLiant(2),
          proLiant2(3),
          proLiant2Internal(4),
          proLiant2DuplexTop(5),
          proLiant2DuplexBottom(6),
          proLiant2InternalDuplexTop(7),
          proLiant2InternalDuplexBottom(8)
        }
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
        "Drive Box Type.

        This is the type of drive box.  The following types are defined:

            other(1)
              The agent does not recognize this drive storage system.

            proLiant(2)
              This is a ProLiant Storage System.

            proLiant2(3)
              This is a ProLiant-2 Storage System.

            proLiant2Internal(4)
              This is an internal ProLiant-2 Storage System that is found
              in some servers.

            proLiant2DuplexTop(5)
              This is the top portion of a ProLiant-2 Storage System that
              has dual SCSI busses which are duplexed.

            proLiant2DuplexBottom(6)
              This is the bottom portion of a ProLiant-2 Storage System that
              has dual SCSI busses which are duplexed.

            proLiant2InternalDuplexTop(7)
              This is the top portion of a ProLiant Server into which the
              internal SCSI busses are duplexed.

            proLiant2InternalDuplexBottom(8)
              This is the bottom portion of a ProLiant Server into which the
              internal SCSI busses are duplexed."
    ::= { cpqSsDrvBoxEntry 3 }

    cpqSsBoxModel OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..17))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Drive Box Model.

        This is a description of the drive box's model.
        This can be used for identification purposes."
    ::= { cpqSsDrvBoxEntry 4 }

    cpqSsBoxFWRev OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..8))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Drive Box Firmware Revision.

        This is the revision level of the drive box.
        This can be used for identification purposes."
    ::= { cpqSsDrvBoxEntry 5 }

    cpqSsBoxVendor OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..9))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Drive Box Vendor

        This is the drive box's vendor name.
        This can be used for identification purposes."
    ::= { cpqSsDrvBoxEntry 6 }

    cpqSsBoxFanStatus OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          ok(2),
          failed(3),
          noFan(4),
          degraded(5)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Drive Box Fan Status.

         This is the current status of the fans in the drive box.
         This value will be one of the following:
            other(1)
              Fan monitoring is not supported by this system
              or it is not supported by the driver.

            ok(2)
              All fans are working normally.

            failed(3)
              One or more storage system fans have failed.  The fan(s) should
              be replaced immediately to avoid hardware damage.

            noFan(4)
              This unit does not support fan monitoring.

            degraded(5)
              At least one storage system fan has failed, but there is still
              sufficient cooling capacity to allow the system to continue.
              The fan should be replaced."

    ::= { cpqSsDrvBoxEntry 7 }

    cpqSsBoxCondition OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          ok(2),
          degraded(3),
          failed(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "SCSI Drive Box Condition.

        This is the overall condition of the drive box.
        The following values are defined:

            other(1)
              The agent does not recognize the status.  You may need to
              upgrade your software.

            ok(2)
              The storage system is operating normally.  No user
              action is required.

            degraded(3)
              The storage system is degraded. You need to check the
              temperature status or power supply status of this
              storage system.  Additionally, if the side panel for
              the storage system is removed, the air flow changes
              could result in improper cooling of the drives and affect
              the temperature status.

            failed(4)
              The storage system has failed."
    ::= { cpqSsDrvBoxEntry 8 }

    cpqSsBoxTempStatus OBJECT-TYPE
        SYNTAX  INTEGER
        {
            other(1),
            ok(2),
            degraded(3),
            failed(4),
            noTemp(5)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The temperature of the drive system.

            This value will be one of the following:
            other(1)
              Temperature monitoring is not supported by this system
              or it is not supported by the driver.

            ok(2)
              The temperature is within normal operating range.

            degraded(3)
              The temperature is outside of normal operating range.

            failed(4)
              The temperature could permanently damage the system.
              The storage system will automatically shutdown if this
              condition is detected.

            noTemp(5)
              This unit does not support temperature monitoring."

    ::= { cpqSsDrvBoxEntry 9 }

    cpqSsBoxSidePanelStatus OBJECT-TYPE
            SYNTAX  INTEGER
            {
                other(1),
                sidePanelInPlace(2),
                sidePanelRemoved(3),
                noSidePanelStatus(4)
            }
            ACCESS  read-only
            STATUS  mandatory
            DESCRIPTION
            "Drive Box Side Panel Status.

            This value will be one of the following:
            other(1)
              The agent does not recognize the status.  You may need to
              upgrade your software.

            sidePanelInPlace(2)
              The side panel is properly installed on the storage system.

            sidePanelRemoved(3)
              The side panel is not properly installed on the storage system.

            noSidePanelStatus(4)
              This unit does not support side panel status monitoring."

    ::= { cpqSsDrvBoxEntry 10 }

    cpqSsBoxFltTolPwrSupplyStatus OBJECT-TYPE
            SYNTAX  INTEGER
            {
              other(1),
              ok(2),
              degraded(3),
              failed(4),
              noFltTolPower(5)
            }
            ACCESS  read-only
            STATUS  mandatory
            DESCRIPTION
            "This value specifies the overall status of the fault tolerant
             power supply sub-system in a drive box.

            This value will be one of the following:
            other(1)
              The power supply status cannot be determined.

            ok(2)
              There are no detected power supply failures.

            degraded(3)
              One of the power supply units in a fault tolerant power
              supply has failed.

            failed(4)
              No failure conditions can currently be determined.

            noFltTolPower(5)
              This unit does not support fault tolerant power supply
              monitoring."

    ::= { cpqSsDrvBoxEntry 11 }

    cpqSsBoxBackPlaneVersion OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          proLiant(2),
          proLiant2(3),
          proLiant3(4),
          proLiant4(5),
          proLiant5(6)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Drive Box Back Plane Version.

        This is the version of the drive box back plane.  The following
        types are defined:

            other(1)
               The agent does not recognize this drive storage system back
               plane.

            proLiant(2)
              This is a ProLiant Storage System.

            proLiant2(3)
              This is a ProLiant-2 Storage System.

            proLiant3(4)
              This is a ProLiant-3 Storage System.

            proLiant4(5)
              This is a 4th generation Proliant Storage System.

            proLiant5(6)
              This is a 5th generation ProLiant Storage System."
    ::= { cpqSsDrvBoxEntry 12 }


    cpqSsBoxTotalBays OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
           "Drive Box Total Bays.

            This is the total number of bays in this storage system."
    ::= { cpqSsDrvBoxEntry 13 }


    cpqSsBoxPlacement OBJECT-TYPE
        SYNTAX  INTEGER
        {
           other(1),
           internal(2),
           external(3)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
           "Drive Box Placement.

            The following values are defined:

            other(1)
              The agent is unable to determine if this storage system is
              located internal or external to the system chassis.

            internal(2)
              The storage system is located in the system chassis.

            external(3)
              The storage system is located outside the system chassis
              in an expansion box."
    ::= { cpqSsDrvBoxEntry 14 }


    cpqSsBoxDuplexOption OBJECT-TYPE
        SYNTAX  INTEGER
        {
           other(1),
           notDuplexed(2),
           duplexTop(3),
           duplexBottom(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
           "Drive Box Duplex Option.

            The following values are defined:

            other(1)
              The agent is unable to determine if this storage system is
              duplexed.

            notDuplexed(2)
              This storage system is not duplexed.

            duplexTop(3)
              This is the top portion of a duplexed storage system.

            duplexBottom(4)
              This is the bottom portion of a duplexed storage system."
    ::= { cpqSsDrvBoxEntry 15 }

    cpqSsBoxBoardRevision OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
           "Drive Box Board Revision.

            This is the board revision of this storage system backplane."
    ::= { cpqSsDrvBoxEntry 16 }

    cpqSsBoxSerialNumber OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..24))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
           "Drive Box Serial Number.

            This is the drive box's serial number which is normally display
            on the front panel.  This can be used for identification
            purposes."
    ::= { cpqSsDrvBoxEntry 17 }

    cpqSsBoxCntlrHwLocation OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
           "A text description of the hardware location of the controller
            to which this box is attached.  A NULL string indicates that
            the hardware location could not be determined or is irrelevant."
    ::= { cpqSsDrvBoxEntry 18 }

    cpqSsBoxBackplaneSpeed OBJECT-TYPE
        SYNTAX  INTEGER
        {
           other(1),
           ultra3(2),
           ultra320(3)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
           "Drive Box Backplane Speed.

            The following values are defined:

            other(1)
              The agent is unable to determine the backplane speed for this
              storage system.

            ultra3(2)
              This storage system is capable of Ultra3 speeds.

            ultra320(3)
              This storage system is capable of Ultra320 speeds."
    ::= { cpqSsDrvBoxEntry 19 }

    cpqSsBoxConnectionType OBJECT-TYPE
        SYNTAX  INTEGER
        {
           other(1),
           scsiAttached(2),
           sasAttached(3)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
           "Drive Box Backplane Speed.

            The following values are defined:

            other(1)
              The agent is unable to determine the type of connection to
              this storage system.

            scsiAttached(2)
              This storage system is attached to the host via SCSI.

            sasAttached(3)
              This storage system is attached to the host via SAS."
    ::= { cpqSsDrvBoxEntry 20 }

    cpqSsBoxHostConnector OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..4))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
           "Drive Box Host Connector.

            This is the host connector to which the drive box is attached.
            If the host connector cannot be determined, the agent will
            return a NULL string."
    ::= { cpqSsDrvBoxEntry 21 }

    cpqSsBoxBoxOnConnector OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
           "Drive Box, Box on Connector.

            The box on connector indicates which box instance this table
            entry belongs.  The instances start at one and increment for
            each box attached to a connector."
    ::= { cpqSsDrvBoxEntry 22 }

    cpqSsBoxLocationString OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
           "Drive Box Location String.

            This string describes the location of the drive box in relation
            to the controller to which it is attached.  If the location
            string cannot be determined, the agent will return a NULL string."
    ::= { cpqSsDrvBoxEntry 23 }


-- ****************************************************************************
--   Storage System Chassis Group
--   ============================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSsStorageSys Group          (1.3.6.1.4.1.232.8)
--       cpqSsDrvBox Group             (1.3.6.1.4.1.232.8.2)
--        cpqSsBoxExtended Group       (1.3.6.1.4.1.232.8.2.2)
--         cpqSsChassisTable           (1.3.6.1.4.1.232.8.2.2.1)
--
-- ****************************************************************************

    cpqSsChassisTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSsChassisEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
        "Storage System Chassis Table."
    ::= { cpqSsBoxExtended 1 }

    cpqSsChassisEntry OBJECT-TYPE
        SYNTAX  CpqSsChassisEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
        "Storage System Chassis Entry."
    INDEX   { cpqSsChassisIndex }
    ::= { cpqSsChassisTable 1 }

        CpqSsChassisEntry ::= SEQUENCE
        {
              cpqSsChassisIndex                    INTEGER,
              cpqSsChassisConnectionType           INTEGER,
              cpqSsChassisSerialNumber             DisplayString,
              cpqSsChassisName                     DisplayString,
              cpqSsChassisSystemBoardSerNum        DisplayString,
              cpqSsChassisSystemBoardRev           DisplayString,
              cpqSsChassisPowerBoardSerNum         DisplayString,
              cpqSsChassisPowerBoardRev            DisplayString,
              cpqSsChassisScsiBoardSerNum          DisplayString,
              cpqSsChassisScsiBoardRev             DisplayString,
              cpqSsChassisOverallCondition         INTEGER,
              cpqSsChassisPowerSupplyCondition     INTEGER,
              cpqSsChassisFanCondition             INTEGER,
              cpqSsChassisTemperatureCondition     INTEGER,
              cpqSsChassisFcaCntlrCondition        INTEGER,
              cpqSsChassisFcaLogicalDriveCondition INTEGER,
              cpqSsChassisFcaPhysDrvCondition      INTEGER,
              cpqSsChassisTime                     INTEGER,
              cpqSsChassisModel                    INTEGER,
              cpqSsChassisBackplaneCondition       INTEGER,
              cpqSsChassisFcaTapeDrvCondition      INTEGER,
              cpqSsChassisRsoStatus                INTEGER,
              cpqSsChassisRsoCondition             INTEGER,
              cpqSsChassisScsiIoModuleType         INTEGER,
              cpqSsChassisPreferredPathMode        INTEGER,
              cpqSsChassisProductId                DisplayString
        }

    cpqSsChassisIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Chassis Index.

        The chassis index uniquely identifies a storage system chassis."
    ::= { cpqSsChassisEntry 1 }

    cpqSsChassisConnectionType OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          fibreAttached(2),
          scsiAttached(3),
          iScsiAttached(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Chassis Connection Type.

        The following values are defined:

            other(1)
              The agent is unable to determine the type of connection to
              this chassis.

            fibreAttached(2)
              This chassis is attached to the server via Fibre Channel.

            scsiAttached(3)
              This chassis is attached to the server via SCSI.

            iScsiAttached(4)
              This chassis is attached to the server via iSCSI."
    ::= { cpqSsChassisEntry 2 }

    cpqSsChassisSerialNumber OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..32))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Chassis Serial Number.

        This is the storage system chassis's serial number which is normally
        displayed on the front panel.  This can be used for identification
        purposes."
    ::= { cpqSsChassisEntry 3 }

    cpqSsChassisName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..32))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Chassis Name.

        This is a user defined name for this storage system chassis."
    ::= { cpqSsChassisEntry 4 }

    cpqSsChassisSystemBoardSerNum OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..24))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Chassis System Controller Board Serial Number.

        This is the system controller board's serial number.  This can be
        used for identification purposes."
    ::= { cpqSsChassisEntry 5 }

    cpqSsChassisSystemBoardRev OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..8))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Chassis System Controller Board Revision.

        This is the system controller board revision."
    ::= { cpqSsChassisEntry 6 }

    cpqSsChassisPowerBoardSerNum OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..24))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Chassis Power Backplane Board Serial Number.

        This is the power backplane board's serial number.  This can be used
        for identification purposes."
    ::= { cpqSsChassisEntry 7 }

    cpqSsChassisPowerBoardRev OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..8))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Chassis Power Backplane Board Revision.

        This is the power backplane board revision."
    ::= { cpqSsChassisEntry 8 }

    cpqSsChassisScsiBoardSerNum OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..24))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Chassis SCSI Drive Backplane Board Serial
         Number.

        This is the SCSI drive backplane board's serial number.  This can be
        used for identification purposes."
    ::= { cpqSsChassisEntry 9 }

    cpqSsChassisScsiBoardRev OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..8))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Chassis SCSI Drive Backplane Board Revision.

        This is the SCSI drive backplane board revision."
    ::= { cpqSsChassisEntry 10 }

    cpqSsChassisOverallCondition OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          ok(2),
          degraded(3),
          failed(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Chassis Overall Condition.

        This is the condition of the storage system chassis and all of its
        components.  The following values are defined:

            other(1)
              The agent does not recognize the status.  You may need to
              upgrade your software.

            ok(2)
              The storage system is operating normally.  No user
              action is required.

            degraded(3)
              The storage system chassis is degraded.

            failed(4)
              The storage system chassis is failed."
    ::= { cpqSsChassisEntry 11 }

    cpqSsChassisPowerSupplyCondition OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          ok(2),
          degraded(3),
          failed(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Power Supply Condition.

        This is the aggregate condition of all power supplies in
        the storage system chassis.  The following values are defined:

            other(1)
              The agent does not recognize the status.  You may need to
              upgrade your software.

            ok(2)
              All power supplies are operating normally.

            degraded(3)
              At least one power supply is degraded or failed.

            failed(4)
              All power supplies are failed."
    ::= { cpqSsChassisEntry 12 }

    cpqSsChassisFanCondition OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          ok(2),
          degraded(3),
          failed(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Fan Condition.

        This is the aggregate condition of all fan modules in the
        storage system chassis.  The following values are defined:

            other(1)
              The agent does not recognize the status.  You may need to
              upgrade your software.

            ok(2)
              All fan modules are operating normally.

            degraded(3)
              At least one fan module is degraded.

            failed(4)
              At least one fan module is failed."
    ::= { cpqSsChassisEntry 13 }

    cpqSsChassisTemperatureCondition OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          ok(2),
          degraded(3),
          failed(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Temperature Condition.

        This is the aggregate condition of all the temperatur sensors
        in the storage system chassis.  The following values are defined:

            other(1)
              The agent does not recognize the status.  You may need to
              upgrade your software.

            ok(2)
              All temperature sensors are reading within normal limits.

            degraded(3)
              At least one temperature sensor is reading degraded.

            failed(4)
              At least one temperature sensor is reading failed."
    ::= { cpqSsChassisEntry 14 }

    cpqSsChassisFcaCntlrCondition OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          ok(2),
          degraded(3),
          failed(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Fibre Channel Array Controller Condition.

        This is the aggregate condition of all Fibre Channel Array controllers
        in the storage system chassis.  The following values are defined:

            other(1)
              The condition cannot be determined or is not supported on
              this storage system.

            ok(2)
              All Fibre Channel Array Controllers are operating normally.

            degraded(3)
              At least one Fibre Channel Array Controller is degraded or
              failed.

            failed(4)
              All Fibre Channel Array Controllers are failed."
    ::= { cpqSsChassisEntry 15 }

    cpqSsChassisFcaLogicalDriveCondition OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          ok(2),
          degraded(3),
          failed(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Fibre Channel Array Logical Drive Condition.

        This is the aggregate condition of all Fibre Channel Array Logical
        Drives in this storage system chassis.
        The following values are defined:

            other(1)
              The condition cannot be determined or is not supported on
              this storage system.

            ok(2)
              All Fibre Channel Array Controllers Logical Drives are
              operating normally.

            degraded(3)
              At least one Fibre Channel Array Controller Logical Drive
              is degraded.

            failed(4)
              At least one Fibre Channel Array Controller Logical Drive
              is failed."
    ::= { cpqSsChassisEntry 16 }

    cpqSsChassisFcaPhysDrvCondition OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          ok(2),
          degraded(3),
          failed(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Fibre Channel Array Physical Drive Condition.

        This is the aggregate condition of all Fibre Channel Array Physical
        Drives in this storage system chassis.
        The following values are defined:

            other(1)
              The condition cannot be determined or is not supported on
              this storage system.

            ok(2)
              All Fibre Channel Array Controllers Physical Drives are
              operating normally.

            degraded(3)
              At least one Fibre Channel Array Controller Physical Drive
              is degraded.

            failed(4)
              At least one Fibre Channel Array Controller Physical Drive
              is failed."
    ::= { cpqSsChassisEntry 17 }

    cpqSsChassisTime OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Chassis Time.

        This is the storage system chassis's time in tenths of seconds.
        If the chassis time is not supported, the agent will return 0."
    ::= { cpqSsChassisEntry 18 }

    cpqSsChassisModel OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          ra4x00(2),
          msa1000(3),
          smartArrayClusterStorage(4),
          enterpriseModularArray(5),
          enterpriseVirtualArray(6),
          msa500G2(7),
          msa20(8),
          msa1500cs(9),
          msa1510i(10)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Chassis Model.

        The following values are defined:

            other(1)
              The agent is unable to determine the model of this chassis.

            ra4x00(2)
              Compaq StorageWorks RAID Array 4000/4100.

            msa1000(3)
              Compaq StorageWorks Modular Smart Array 1000.

            smartArrayClusterStorage(4)
              HP StorageWorks Modular Smart Array 500
              (Formerly Smart Array Cluster Storage).

            enterpriseModularArray(5)
              Compaq StorageWorks Enterprise/Modular RAID Array.

            enterpriseVirtualArray(6)
              Compaq StorageWorks Enterprise Virtual Array.

            msa500G2(7)
              HP StorageWorks Modular Smart Array 500 G2.

            msa20(8)
              HP StorageWorks Modular Smart Array 20.

            msa1500cs(9)
              HP StorageWorks Modular Smart Array 1500 CS.

            msa1510i(10)
              HP StorageWorks Modular Smart Array 1510i."
    ::= { cpqSsChassisEntry 19 }

    cpqSsChassisBackplaneCondition OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          ok(2),
          degraded(3),
          failed(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Backplane Condition.

        This is the aggregate condition of all the backplanes for the
        storage system chassis.  The following values are defined:

            other(1)
              The agent does not recognize the status.  You may need to
              upgrade your software.

            ok(2)
              All backplanes are operating normally.

            degraded(3)
              At least one storage system is degraded.

            failed(4)
              At least one storage system is failed."
    ::= { cpqSsChassisEntry 20 }

    cpqSsChassisFcaTapeDrvCondition OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          ok(2),
          degraded(3),
          failed(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Array Tape Drive Condition.

        This is the aggregate condition of all tape drives in this storage
        system chassis.
        The following values are defined:

            other(1)
              The condition cannot be determined or is not supported on
              this storage system.

            ok(2)
              All tape drives are operating normally.

            degraded(3)
              At least one tape drive is degraded.

            failed(4)
              At least one tape drive is failed."
    ::= { cpqSsChassisEntry 21 }

    cpqSsChassisRsoStatus OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          notSupported(2),
          notConfigured(3),
          disabled(4),
          daemonDownDisabled(5),
          ok(6),
          daemonDownActive(7),
          noSecondary(8),
          daemonDownNoSecondary(9),
          linkDown(10),
          daemonDownLinkDown(11),
          secondaryRunningAuto(12),
          secondaryRunningUser(13),
          evTimeoutError(14)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Chassis Recovery Server Option Status.

        The following values are defined:

            other(1)
              The recovery server option status cannot be determined for
              this storage system.

            notSupported(2)
              The recovery server option is not supported for this storage
              system.

            notConfigured(3)
              The recovery server option is supported, but is not
              configured on this storage system.

            disabled(4)
              The recovery server option is configured as primary, but
              has been disabled by software.

            daemonDownDisabled(5)
              The recovery server option operating system daemon is no
              longer running.  The last status of RSO was disabled(4).

            ok(6)
              The recovery server option is configured as primary and
              everything is working correctly.

            daemonDownActive(7)
              The recovery server option operating system daemon is no
              longer running.  The last status of RSO was ok(6).

            noSecondary(8)
              The recovery server option is configured as primary, but
              communication with the standby server has not been established.

            daemonDownNoSecondary(9)
              The recovery server option operating system daemon is no
              longer running.  The last status of RSO was noSecondary(8).

            linkDown(10)
              The recovery server option is configured as primary, but
              communication with the standby server has failed.

            daemonDownLinkDown(11)
              The recovery server option operating system daemon is no
              longer running.  The last status of RSO was linkDown(10).

            secondaryRunningAuto(12)
              The recovery server option is configured and the standby
              server is running.  The secondary server assumed control
              after communication with the primary server failed.

            secondaryRunningUser(13)
              The recovery server option is configured and the standby
              server is running.  A user forced the secondary server to
              assume control.

            evTimeoutError(14)
              The recovery server option environment variable cannot be
              accessed."
    ::= { cpqSsChassisEntry 22 }

    cpqSsChassisRsoCondition OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          ok(2),
          degraded(3),
          failed(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Chassis Recovery Server Option Condition.

        This is the condition of the recovery server option.  The
        following values are defined:

            other(1)
              The agent does not recognize the status.  You may need to
              upgrade your software.

            ok(2)
              The recovery server option is operating normally.  No user
              action is required.

            degraded(3)
              The recovery server option is degraded.

            failed(4)
              The recovery server option is failed."
    ::= { cpqSsChassisEntry 23 }

    cpqSsChassisScsiIoModuleType OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          io2port(2),
          io4portUpgradeFirmware(3),
          io4port(4),
          io2port320(5),
          io4port320(6),
          io1port320(7)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Chassis SCSI I/O Module Type.

        The following values are defined:

            other(1)
              The agent does not recognize SCSI I/O module type.  You may
              need to upgrade your software.

            io2port(2)
              A 2-Port Ultra3 SCSI I/O Module is installed.

            io4portUpgradeFirmware(3)
              A 4-Port Shared Storage Module for Smart Array Cluster Storage
              is installed, but the current controller firmware does not
              support it.  Upgrade your controller firmware.

            io4port(4)
              A 4-Port Shared Storage Module for Smart Array Cluster Storage
              is installed.

            io2port320(5)
              A 2-Port Ultra320 SCSI I/O Module is installed.

            io4port320(6)
              A 4-Port Ultra320 SCSI I/O Module is installed.

            io1port320(7)
              A 1-Port Ultra320 SCSI I/O Module is installed."
    ::= { cpqSsChassisEntry 24 }

     cpqSsChassisPreferredPathMode OBJECT-TYPE
        SYNTAX  INTEGER
        {
            other(1),
            notActiveActive(2),
            automatic(3),
            manual(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Array Controller Preferred Path Mode.

            This is the storage system active/active preferred path mode.
            The following values are valid:

            other (1)
              Indicates that the agent does not recognize the preferred path
              mode of the storage system.  You may need to upgrade the agent.

            notActiveActive (2)
              The storage system is not configured as active/active.

            automatic (3)
              The storage system automatically selects the preferred path
              for each logical drive based on host I/O patterns.

            manual (4)
              The preferred path for each logical drive is manually
              configured by the storage system administrator."
        ::= { cpqSsChassisEntry 25 }

    cpqSsChassisProductId OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..32))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Chassis Product Identifier.

        This is the storage system chassis's product identifier.  This can
        be used for identification purposes.  If the product identifier can
        not be determined, the agent will return a NULL string."
    ::= { cpqSsChassisEntry 26 }


-- ****************************************************************************
--   Storage System I/O Slot Table
--   =============================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSsStorageSys Group          (1.3.6.1.4.1.232.8)
--       cpqSsDrvBox Group             (1.3.6.1.4.1.232.8.2)
--        cpqSsBoxExtended Group       (1.3.6.1.4.1.232.8.2.2)
--         cpqSsIoSlotTable            (1.3.6.1.4.1.232.8.2.2.2)
--
-- ****************************************************************************

    cpqSsIoSlotTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSsIoSlotEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
        "Storage System I/O Slot Table."
    ::= { cpqSsBoxExtended 2 }

    cpqSsIoSlotEntry OBJECT-TYPE
        SYNTAX  CpqSsIoSlotEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
        "Storage System I/O Slot Entry."
    INDEX   { cpqSsIoSlotChassisIndex, cpqSsIoSlotIndex }
    ::= { cpqSsIoSlotTable 1 }

        CpqSsIoSlotEntry ::= SEQUENCE
        {
              cpqSsIoSlotChassisIndex       INTEGER,
              cpqSsIoSlotIndex              INTEGER,
              cpqSsIoSlotControllerType     INTEGER
        }

    cpqSsIoSlotChassisIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System I/O Slot Chassis Index.

        The chassis index uniquely identifies a storage system chassis."
    ::= { cpqSsIoSlotEntry 1 }

    cpqSsIoSlotIndex OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System I/O Slot Index.

        This index uniquely identifies a storage system I/O Slot."
    ::= { cpqSsIoSlotEntry 2 }

    cpqSsIoSlotControllerType OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          notInstalled(2),
          unknownBoard(3),
          fibreArray(4),
          scsiArray(5),
          noSlot(6),
          iScsiArray(7)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System I/O Slot Controller Type.

         The following values are defined:

            other(1)
              The agent is unable to determine if anything is installed in
              this storage system I/O slot.

            notInstalled(2)
              Nothing is installed in this storage system I/O slot.

            unknownBoardInstalled(3)
              An unknown controller is installed in this storage system
              I/O slot.

            fibreArray(4)
              A Fibre Channel Array controller is installed in this storage
              system I/O slot.

            scsiArray(5)
              A SCSI Array controller is installed in this storage system
              I/O slot.

            noSlot(6)
              The slot does not exist on this chassis.

            iScsiArray(7)
              An  iSCSI Array controller is installed in this storage system
              I/O slot."
    ::= { cpqSsIoSlotEntry 3 }


-- ****************************************************************************
--   Storage System Power Supply Table
--   =================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSsStorageSys Group          (1.3.6.1.4.1.232.8)
--       cpqSsDrvBox Group             (1.3.6.1.4.1.232.8.2)
--        cpqSsBoxExtended Group       (1.3.6.1.4.1.232.8.2.2)
--         cpqSsPowerSupplyTable       (1.3.6.1.4.1.232.8.2.2.3)
--
-- ****************************************************************************

    cpqSsPowerSupplyTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSsPowerSupplyEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
        "Storage System Power Supply Table."
    ::= { cpqSsBoxExtended 3 }

    cpqSsPowerSupplyEntry OBJECT-TYPE
        SYNTAX  CpqSsPowerSupplyEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
        "Storage System Power Supply Entry."
    INDEX   { cpqSsPowerSupplyChassisIndex, cpqSsPowerSupplyIndex }
    ::= { cpqSsPowerSupplyTable 1 }

        CpqSsPowerSupplyEntry ::= SEQUENCE
        {
              cpqSsPowerSupplyChassisIndex       INTEGER,
              cpqSsPowerSupplyIndex              INTEGER,
              cpqSsPowerSupplyBay                INTEGER,
              cpqSsPowerSupplyStatus             INTEGER,
              cpqSsPowerSupplyUpsStatus          INTEGER,
              cpqSsPowerSupplyCondition          INTEGER,
              cpqSsPowerSupplySerialNumber       DisplayString,
              cpqSsPowerSupplyBoardRevision      DisplayString,
              cpqSsPowerSupplyFirmwareRevision   DisplayString
        }

    cpqSsPowerSupplyChassisIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Power Supply Chassis Index.

        The chassis index uniquely identifies a storage system chassis."
    ::= { cpqSsPowerSupplyEntry 1 }

    cpqSsPowerSupplyIndex OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Power Supply Bay.

        This index uniquely identifies a power supply bay."
    ::= { cpqSsPowerSupplyEntry 2 }

    cpqSsPowerSupplyBay OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          powerBay1(2),
          powerBay2(3),
          composite(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Power Supply Bay.

        The following values are defined:

            other(1)
              The agent does not recognize the bay.  You may need to upgrade
              your software.

            powerBay1(2)
              The power supply is installed in the first power supply bay.

            powerBay2(3)
              The power supply is installed in the second power supply bay.

            composite(4)
              The power supply information is a composite of all power
              supplies in the storage system."
    ::= { cpqSsPowerSupplyEntry 3 }

    cpqSsPowerSupplyStatus OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          notInstalled(2),
          ok(3),
          failed(4),
          degraded(5)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Power Supply Status.

         The following values are defined:

            other(1)
              The agent is unable to determine if this storage system power
              supply bay is occupied.

            notInstalled(2)
              Nothing is installed in this power supply bay.

            ok(3)
              A power supply is installed and operating normally.

            failed(4)
              A power supply is installed and is no longer operating.
              Replace the power supply.

            degraded(5)
              For composite power supplies, this indicates that at least one
              power supply has failed or lost power."
    ::= { cpqSsPowerSupplyEntry 4 }

    cpqSsPowerSupplyUpsStatus OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          noUps(2),
          ok(3),
          powerFailed(4),
          batteryLow(5)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Power Supply Uninterruptible Power Supply (UPS)
        Status.

         The following values are defined:

            other(1)
              The agent is unable to determine if this power supply is
              attached to an Uninterruptible Power Supply (UPS).

            noUps(2)
              No UPS is attached to the power supply.

            ok(3)
              A UPS is attached to the power supply and is operating
              normally.

            powerFailed(4)
              A UPS is attached to the power supply and the AC power has
              failed.

            batteryLow(5)
              A UPS is attached to the power supply, the AC power has
              failed and the UPS battery is low."
    ::= { cpqSsPowerSupplyEntry 5 }

    cpqSsPowerSupplyCondition OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          ok(2),
          degraded(3),
          failed(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Power Supply Condition.

        This is the condition of the storage system chassis and all of
        its components.  The following values are defined:

            other(1)
              The agent does not recognize the status.  You may need to
              upgrade your software.

            ok(2)
              The power supply is operating normally.  No user action is
              required.

            degraded(3)
              The power supply is degraded. You need to check the power
              supply or its attached UPS for problems.

            failed(4)
              The power supply has failed."
    ::= { cpqSsPowerSupplyEntry 6 }

    cpqSsPowerSupplySerialNumber OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..24))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Power Supply Serial Number.

        This is the power supply's serial number.  This can be used
        for identification purposes.  If the serial number is not supported,
        the agent will return a NULL string."
    ::= { cpqSsPowerSupplyEntry 7 }

    cpqSsPowerSupplyBoardRevision OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..8))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Power Supply Board Revision.

        This is the power supply board revision.  If the board revision is
        not supported, the agent will return a NULL string."
    ::= { cpqSsPowerSupplyEntry 8 }

    cpqSsPowerSupplyFirmwareRevision OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..8))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Power Supply Firmware Revision.

        This is the power supply firmware revision.  If the firmware revision
        is not supported, the agent will return a NULL string."
    ::= { cpqSsPowerSupplyEntry 9 }


-- ****************************************************************************
--   Storage System Fan Module Table
--   ===============================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSsStorageSys Group          (1.3.6.1.4.1.232.8)
--       cpqSsDrvBox Group             (1.3.6.1.4.1.232.8.2)
--        cpqSsBoxExtended Group       (1.3.6.1.4.1.232.8.2.2)
--         cpqSsFanModuleTable         (1.3.6.1.4.1.232.8.2.2.4)
--
-- ****************************************************************************

    cpqSsFanModuleTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSsFanModuleEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
        "Storage System Fan Module Table."
    ::= { cpqSsBoxExtended 4 }

    cpqSsFanModuleEntry OBJECT-TYPE
        SYNTAX  CpqSsFanModuleEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
        "Storage System Fan Module Entry."
    INDEX   { cpqSsFanModuleChassisIndex, cpqSsFanModuleIndex }
    ::= { cpqSsFanModuleTable 1 }

        CpqSsFanModuleEntry ::= SEQUENCE
        {
              cpqSsFanModuleChassisIndex       INTEGER,
              cpqSsFanModuleIndex              INTEGER,
              cpqSsFanModuleStatus             INTEGER,
              cpqSsFanModuleCondition          INTEGER,
              cpqSsFanModuleLocation           INTEGER,
              cpqSsFanModuleSerialNumber       DisplayString,
              cpqSsFanModuleBoardRevision      DisplayString
        }

    cpqSsFanModuleChassisIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Fan Module Chassis Index.

        The chassis index uniquely identifies a storage system chassis."
    ::= { cpqSsFanModuleEntry 1 }

    cpqSsFanModuleIndex OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Fan Module Index.

        This index uniquely identifies a storage system fan module."
    ::= { cpqSsFanModuleEntry 2 }

    cpqSsFanModuleStatus OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          notInstalled(2),
          ok(3),
          degraded(4),
          failed(5)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Fan Module Status.

         The following values are defined:

            other(1)
              The agent is unable to determine if this storage system fan
              module is installed.

            notInstalled(3)
              The fan module is not installed.

            ok(2)
              The fan module is installed and operating normally.

            degraded(4)
              The fan module degraded.

            failed(5)
              The fan module is failed.  Replace the fan module."
    ::= { cpqSsFanModuleEntry 3 }

    cpqSsFanModuleCondition OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          ok(2),
          degraded(3),
          failed(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Fan Module Condition.

        This is the condition of the storage system fan module.
        The following values are defined:

            other(1)
              The agent does not recognize the status.  You may need to
              upgrade your software.

            ok(2)
              The fan module is operating normally.  No user action is
              required.

            degraded(3)
              The fan module is degraded. You need to check the fan module
              for problems.

            failed(4)
              The fan module has failed.  Replace the fan module."
    ::= { cpqSsFanModuleEntry 4 }

    cpqSsFanModuleLocation OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          fanBay(2),
          composite(3)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Fan Module Location.

         The following values are defined:

            other(1)
              The agent is unable to determine the location of this storage
              system fan module.

            fanBay(2)
              This fan module is installed in the fan bay.

            composite(3)
              The fan information is a composite of all fans in the storage
              system."
    ::= { cpqSsFanModuleEntry 5 }

    cpqSsFanModuleSerialNumber OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..24))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Fan Module Serial Number.

        This is the fan module's serial number.  This can be used
        for identification purposes."
    ::= { cpqSsFanModuleEntry 6 }

    cpqSsFanModuleBoardRevision OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..8))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Fan Module Board Revision.

        This is the fan module board revision."
    ::= { cpqSsFanModuleEntry 7 }


-- ****************************************************************************
--   Storage System Temperature Sensor Table
--   =======================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSsStorageSys Group          (1.3.6.1.4.1.232.8)
--       cpqSsDrvBox Group             (1.3.6.1.4.1.232.8.2)
--        cpqSsBoxExtended Group       (1.3.6.1.4.1.232.8.2.2)
--         cpqSsTempSensorTable        (1.3.6.1.4.1.232.8.2.2.5)
--
-- ****************************************************************************

    cpqSsTempSensorTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSsTempSensorEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
        "Storage System Temperature Sensor Table."
    ::= { cpqSsBoxExtended 5 }

    cpqSsTempSensorEntry OBJECT-TYPE
        SYNTAX  CpqSsTempSensorEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
        "Storage System Temperature Sensor Entry."
    INDEX   { cpqSsTempSensorChassisIndex, cpqSsTempSensorIndex }
    ::= { cpqSsTempSensorTable 1 }

        CpqSsTempSensorEntry ::= SEQUENCE
        {
              cpqSsTempSensorChassisIndex       INTEGER,
              cpqSsTempSensorIndex              INTEGER,
              cpqSsTempSensorStatus             INTEGER,
              cpqSsTempSensorCondition          INTEGER,
              cpqSsTempSensorLocation           INTEGER,
              cpqSsTempSensorCurrentValue       INTEGER,
              cpqSsTempSensorLimitValue         INTEGER,
              cpqSsTempSensorHysteresisValue    INTEGER
        }

    cpqSsTempSensorChassisIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Temperature Sensor Chassis Index.

        The chassis index uniquely identifies a storage system chassis."
    ::= { cpqSsTempSensorEntry 1 }

    cpqSsTempSensorIndex OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Temperature Sensor Index.

        This index uniquely identifies a temperature sensor."
    ::= { cpqSsTempSensorEntry 2 }

    cpqSsTempSensorStatus OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          ok(2),
          degraded(3),
          failed(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Temperature Sensor Status.

         The following values are defined:

            other(1)
              The agent is unable to determine if the storage system
              temperature sensor status.

            ok(2)
              The temperature is OK.

            degraded(3)
              The temperature is degraded.

            failed(4)
              The temperature is failed."
    ::= { cpqSsTempSensorEntry 3 }

    cpqSsTempSensorCondition OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          ok(2),
          degraded(3),
          failed(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Fan Module Condition.

        This is the condition of the storage system temperature sensor.
        The following values are defined:

            other(1)
              The agent does not recognize the status.  You may need to
              upgrade your software.

            ok(2)
              The temperature is within normal operating range.  No user
              action is required.

            degraded(3)
              The temperature is outside of normal operating range.

            failed(4)
              The temperature could permanently damage the system.
              The storage system will automatically shutdown if this
              condition is detected."
    ::= { cpqSsTempSensorEntry 4 }

    cpqSsTempSensorLocation OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          fanBay(2),
          backplane(3)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Fan Module Location.

         The following values are defined:

            other(1)
              The agent is unable to determine the location of this storage
              system temperature sensor.

            fanBay(2)
              This temperature sensor is located on the fan module in the
              fan bay.

            backplane(3)
              This temperature is located on the SCSI drive backplane."
    ::= { cpqSsTempSensorEntry 5 }

    cpqSsTempSensorCurrentValue OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Temperature Sensor Current Value.

        The current value of the temperature sensor in degrees Celsius."
    ::= { cpqSsTempSensorEntry 6 }

    cpqSsTempSensorLimitValue OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Temperature Sensor Limit Value.

        The limit value of the temperature sensor in degrees Celsius."
    ::= { cpqSsTempSensorEntry 7 }

    cpqSsTempSensorHysteresisValue OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Temperature Sensor Hysteresis Value.

        The hysteresis value of the temperature sensor in degrees Celsius."
    ::= { cpqSsTempSensorEntry 8 }


-- ****************************************************************************
--   Storage System SCSI Backplane Table
--   ===================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSsStorageSys Group          (1.3.6.1.4.1.232.8)
--       cpqSsDrvBox Group             (1.3.6.1.4.1.232.8.2)
--        cpqSsBoxExtended Group       (1.3.6.1.4.1.232.8.2.2)
--         cpqSsBackplaneTable         (1.3.6.1.4.1.232.8.2.2.6)
--
-- ****************************************************************************

    cpqSsBackplaneTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSsBackplaneEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
        "Storage System SCSI Backplane Table."
    ::= { cpqSsBoxExtended 6 }

    cpqSsBackplaneEntry OBJECT-TYPE
        SYNTAX  CpqSsBackplaneEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
        "Storage System SCSI Backplane Entry."
    INDEX   { cpqSsBackplaneChassisIndex, cpqSsBackplaneIndex }
    ::= { cpqSsBackplaneTable 1 }

        CpqSsBackplaneEntry ::= SEQUENCE
        {
              cpqSsBackplaneChassisIndex       INTEGER,
              cpqSsBackplaneIndex              INTEGER,
              cpqSsBackplaneFWRev              DisplayString,
              cpqSsBackplaneDriveBays          INTEGER,
              cpqSsBackplaneDuplexOption       INTEGER,
              cpqSsBackplaneCondition          INTEGER,
              cpqSsBackplaneVersion            INTEGER,
              cpqSsBackplaneVendor             DisplayString,
              cpqSsBackplaneModel              DisplayString,
              cpqSsBackplaneFanStatus          INTEGER,
              cpqSsBackplaneTempStatus         INTEGER,
              cpqSsBackplaneFtpsStatus         INTEGER,
              cpqSsBackplaneSerialNumber       DisplayString,
              cpqSsBackplanePlacement          INTEGER,
              cpqSsBackplaneBoardRevision      INTEGER,
              cpqSsBackplaneSpeed              INTEGER

        }

    cpqSsBackplaneChassisIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Backplane Chassis Index.

        The chassis index uniquely identifies a storage system chassis."
    ::= { cpqSsBackplaneEntry 1 }

    cpqSsBackplaneIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Backplane Index.

        This index uniquely identifies a storage system backplane."
    ::= { cpqSsBackplaneEntry 2 }

    cpqSsBackplaneFWRev OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..8))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Backplane Firmware Revision.

        This is the revision level of storage system backplane."
    ::= { cpqSsBackplaneEntry 3 }

    cpqSsBackplaneDriveBays OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Backplane Drive Bays.

        This is the number of bays on this storage system backplane."
    ::= { cpqSsBackplaneEntry 4 }

    cpqSsBackplaneDuplexOption OBJECT-TYPE
        SYNTAX  INTEGER
        {
           other(1),
           notDuplexed(2),
           duplexTop(3),
           duplexBottom(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Backplane Duplex Option.

        The following values are defined:

            other (1)
              The agent is unable to determine if this storage
              system is duplexed.

            notDuplexed(2)
              This storage system is not duplexed.

            duplexTop(3)
              This is the top portion of a duplexed storage system.

            duplexBottom(4)
              This is the bottom portion of a duplexed storage system."
    ::= { cpqSsBackplaneEntry 5 }

    cpqSsBackplaneCondition OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          ok(2),
          degraded(3),
          failed(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Backplane Condition.

        This is the overall condition of the backplane.
        The following values are defined:

            other(1)
              The agent does not recognize the status.  You may need to
              upgrade your software.

            ok(2)
              The storage system is operating normally.  No user
              action is required.

            degraded(3)
              The storage system is degraded. You need to check the
              temperature status or power supply status of this
              storage system.

            failed(4)
              The storage system has failed."
    ::= { cpqSsBackplaneEntry 6 }

    cpqSsBackplaneVersion OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Backplane Version.

        This is the version of the drive box back plane."
    ::= { cpqSsBackplaneEntry 7 }

    cpqSsBackplaneVendor OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..9))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Backplane Vendor

        This is the storage box's vendor name.
        This can be used for identification purposes."
    ::= { cpqSsBackplaneEntry 8 }

    cpqSsBackplaneModel OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..17))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Backplane Model.

        This is a description of the storage system's model.
        This can be used for identification purposes."
    ::= { cpqSsBackplaneEntry 9 }

    cpqSsBackplaneFanStatus OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          notInstalled(2),
          ok(3),
          degraded(4),
          failed(5),
          notSupported(6)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Backplane Fan Status.

         This is the current status of the fans in the storage system.
         This value will be one of the following:

            other(1)
              The agent is unable to determine if this storage system has
              fan monitoring.

            notInstalled(2)
              This unit does not support fan monitoring.

            ok(3)
              All fans are working normally.

            degraded(4)
              At least one storage system fan has failed, but there is still
              sufficient cooling capacity to allow the system to continue.
              The fan should be replaced.

            failed(5)
              One or more storage system fans have failed.  The fan(s) should
              be replaced immediately to avoid hardware damage.

            notSupported(6)
              The storage system does not support reporting fan status
              through this backplane.  The fan status is reported through the
              first backplane on this storage system."
    ::= { cpqSsBackplaneEntry 10 }

    cpqSsBackplaneTempStatus OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          noTemp(2),
          ok(3),
          degraded(4),
          failed(5),
          notSupported(6)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Backplane Fan Status.

         This value will be one of the following:

            other(1)
              The agent is unable to determine if this storage system has
              temperature monitoring.

            noTemp(2)
              This unit does not support temperature monitoring.

            ok(3)
              The temperature is within normal operating range.

            degraded(4)
              The temperature is outside of normal operating range.

            failed(5)
              The temperature could permanently damage the system.

            notSupported(6)
              The storage system does not support reporting temperature
              status through this backplane.  The temperature status is
              reported through the first backplane on this storage system."
    ::= { cpqSsBackplaneEntry 11 }

    cpqSsBackplaneFtpsStatus OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          noFltTolPower(2),
          ok(3),
          degraded(4),
          failed(5),
          notSupported(6)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Backplane Fault Tolerant Power Supply Status.

            This value specifies the overall status of the redundant power
            supply in a drive box.  This value will be one of the following:

            other(1)
              The agent is unable to determine if this storage system has
              redundant power supplies.

            noFltTolPower(2)
              This unit does not have a redundant supply.

            ok(3)
              There are no detected power supply failures.

            degraded(4)
              One of the power supply units has failed.

            failed(5)
              All of the power supplies have failed.  A status of failed can
              not currently be determined.

            notSupported(6)
              The storage system does not support reporting fault tolerant
              power supply status through this backplane.  The fault tolerant
              power supply status is reported through the first backplane on
              this storage system."
    ::= { cpqSsBackplaneEntry 12 }

    cpqSsBackplaneSerialNumber OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..24))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Backplane Serial Number.

        This is the storage system backplane serial number which is normally
        displayed on the front bezel.  This can be used for identification
        purposes."
    ::= { cpqSsBackplaneEntry 13 }

    cpqSsBackplanePlacement OBJECT-TYPE
        SYNTAX  INTEGER
        {
           other(1),
           internal(2),
           external(3)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
           "Storage System Backplane Placement.

            The following values are defined:

            other(1)
              The agent is unable to determine if this storage system is
              located internal or external to the system chassis.

            internal(2)
              The storage system is located in the system chassis.

            external(3)
              The storage system is located outside the system chassis
              in an expansion box."
    ::= { cpqSsBackplaneEntry 14 }

    cpqSsBackplaneBoardRevision OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
           "Storage System Backplane Board Revision.

            This is the board revision of this storage system backplane."
    ::= { cpqSsBackplaneEntry 15 }

    cpqSsBackplaneSpeed OBJECT-TYPE
        SYNTAX  INTEGER
        {
           other(1),
           ultra3(2),
           ultra320(3),
           sata(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
           "Storage System Backplane Speed.

            The following values are defined:

            other(1)
              The agent is unable to determine the backplane speed for this
              storage system.

            ultra3(2)
              This storage system is capable of Ultra3 speeds.

            ultra320(3)
              This storage system is capable of Ultra320 speeds.

            sata(4)
              This storage system is capable of SATA speeds."
    ::= { cpqSsBackplaneEntry 16 }


-- ****************************************************************************
--   Storage System Fibre Attachment Table
--   =====================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSsStorageSys Group          (1.3.6.1.4.1.232.8)
--       cpqSsDrvBox Group             (1.3.6.1.4.1.232.8.2)
--        cpqSsBoxExtended Group       (1.3.6.1.4.1.232.8.2.2)
--         cpqSsFibreAttachmentTable   (1.3.6.1.4.1.232.8.2.2.7)
--
-- The Storage System Fibre Attachment Group contains associations between
-- Fibre channel host controllers and the Fibre devices that are attached to
-- them.  Since there can be multiple paths to some Fibre devices, there may
-- be multiple entries for a given device.
--
-- ****************************************************************************

    cpqSsFibreAttachmentTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSsFibreAttachmentEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
        "Storage System Fibre Attachment Table."
    ::= { cpqSsBoxExtended 7 }

    cpqSsFibreAttachmentEntry OBJECT-TYPE
        SYNTAX  CpqSsFibreAttachmentEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
        "Storage System Fibre Attachment Entry."
    INDEX   { cpqSsFibreAttachmentIndex }
    ::= { cpqSsFibreAttachmentTable 1 }

        CpqSsFibreAttachmentEntry ::= SEQUENCE
        {
              cpqSsFibreAttachmentIndex               INTEGER,
              cpqSsFibreAttachmentHostControllerIndex INTEGER,
              cpqSsFibreAttachmentHostControllerPort  INTEGER,
              cpqSsFibreAttachmentDeviceType          INTEGER,
              cpqSsFibreAttachmentDeviceIndex         INTEGER,
              cpqSsFibreAttachmentDevicePort          INTEGER
        }

    cpqSsFibreAttachmentIndex OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Fibre Attachment Index.

        The index uniquely identifies a Fibre Attachment association entry."
    ::= { cpqSsFibreAttachmentEntry 1 }

    cpqSsFibreAttachmentHostControllerIndex OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Fibre Attachment Host Controller Index.

        The host controller index indicates which host controller is
        associated with this entry.  This is equal to cpqFcaHostCntlrIndex,
        from the Fibre Channel Host Controller Table."
    ::= { cpqSsFibreAttachmentEntry 2 }

    cpqSsFibreAttachmentHostControllerPort OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Fibre Attachment Host Controller Port.

        This is the Fibre port number of the host controller.  For each host
        controller, the port number starts at 1 and increments for each port.
        This is currently set to 1."
    ::= { cpqSsFibreAttachmentEntry 3 }

    cpqSsFibreAttachmentDeviceType OBJECT-TYPE
        SYNTAX  INTEGER
        {
           other(1),
           storageBox(2),
           tapeController(3),
           fibreChannelSwitch(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Fibre Attachment Device Type.

        This is the type of device associated with this entry.
        The following values are defined:

        other(1)
         The agent is unable to determine if the type of this device.

        storageBox(2)
         The device is a Fibre attached storage system.

        tapeController(3)
         The device is a Fibre attached tape controller.

        fibreChannelSwitch(4)
         The device is a Fibre channel switch."
    ::= { cpqSsFibreAttachmentEntry 4 }

    cpqSsFibreAttachmentDeviceIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Fibre Attachment Device Index.

        The is the index for the Fibre attached device.  For a Fibre
        attached storage system, this is equal to cpqSsChassisIndex from the
        Storage System Chassis Table.  For a Fibre attached tape controller,
        this is equal to cpqFcTapeCntlrIndex from the Fibre Channel Tape
        Controller Table.  For a Fibre channel switch, this is equal to
        cpqFcSwitchIndex from the Fibre Channel Switch Table."
    ::= { cpqSsFibreAttachmentEntry 5 }

    cpqSsFibreAttachmentDevicePort OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System Fibre Attachment Device Port.

        This is the Fibre port on a device.  For a Fibre attached storage
        system, this is equal to cpqFcaCntlrBoxIoSlot from the Fibre Channel
        Array Controller Table.  For a Fibre attached tape controller,
        this is currently set to 1.  For a Fibre channel switch, this is
        currently set to 1."
    ::= { cpqSsFibreAttachmentEntry 6 }


-- ****************************************************************************
--   Storage System Scsi Attachment Table
--   ====================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSsStorageSys Group          (1.3.6.1.4.1.232.8)
--       cpqSsDrvBox Group             (1.3.6.1.4.1.232.8.2)
--        cpqSsBoxExtended Group       (1.3.6.1.4.1.232.8.2.2)
--         cpqSsScsiAttachmentTable    (1.3.6.1.4.1.232.8.2.2.8)
--
-- The Storage System Scsi Attachment Group contains associations between
-- internal array controllers and the external arrays that are attached to
-- them.  Since there can be multiple paths to some external arrays, there
-- may be multiple entries for a given device.
--
-- ****************************************************************************

    cpqSsScsiAttachmentTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSsScsiAttachmentEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
        "Storage System SCSI Attachment Table."
    ::= { cpqSsBoxExtended 8 }

    cpqSsScsiAttachmentEntry OBJECT-TYPE
        SYNTAX  CpqSsScsiAttachmentEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
        "Storage System SCSI Attachment Entry."
    INDEX   { cpqSsScsiAttachmentIndex }
    ::= { cpqSsScsiAttachmentTable 1 }

        CpqSsScsiAttachmentEntry ::= SEQUENCE
        {
              cpqSsScsiAttachmentIndex             INTEGER,
              cpqSsScsiAttachmentControllerIndex   INTEGER,
              cpqSsScsiAttachmentControllerPort    INTEGER,
              cpqSsScsiAttachmentControllerTarget  INTEGER,
              cpqSsScsiAttachmentControllerLun     INTEGER,
              cpqSsScsiAttachmentChassisIndex      INTEGER,
              cpqSsScsiAttachmentChassisIoSlot     INTEGER,
              cpqSsScsiAttachmentPathStatus        INTEGER,
              cpqSsScsiAttachmentPathCondition     INTEGER
        }

    cpqSsScsiAttachmentIndex OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System SCSI Attachment Index.

        The index uniquely identifies a SCSI Attachment association entry."
    ::= { cpqSsScsiAttachmentEntry 1 }

    cpqSsScsiAttachmentControllerIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System SCSI Attachment Controller Index.

        The controller index indicates which internal array controller is
        associated with this entry.  This is equal to cpqDaCntlrIndex,
        from the Array Controller Table."
    ::= { cpqSsScsiAttachmentEntry 2 }

    cpqSsScsiAttachmentControllerPort OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System SCSI Attachment Controller Port.

        The controller port indicates which SCSI port of an internal
        controller is associated with this entry."
    ::= { cpqSsScsiAttachmentEntry 3 }

    cpqSsScsiAttachmentControllerTarget OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System SCSI Attachment Controller Target.

        The controller target indicates which SCSI target is associated with
        this entry."
    ::= { cpqSsScsiAttachmentEntry 4 }

    cpqSsScsiAttachmentControllerLun OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System SCSI Attachment Controller Lun.

        The controller Lun indicates which SCSI Lun is associated with this
        entry."
    ::= { cpqSsScsiAttachmentEntry 5 }

    cpqSsScsiAttachmentChassisIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System SCSI Attachment Chassis Index.

        The is the index for the SCSI attached storage system.  This is equal
        to cpqSsChassisIndex from the Storage System Chassis Table."
    ::= { cpqSsScsiAttachmentEntry 6 }

    cpqSsScsiAttachmentChassisIoSlot OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System SCSI Attachment Chassis I/O Slot.

        This is the I/O slot in the SCSI attached storage system.  This is
        equal to cpqFcaCntlrBoxIoSlot from the Fibre Channel Array Controller
        Table."
    ::= { cpqSsScsiAttachmentEntry 7 }

    cpqSsScsiAttachmentPathStatus OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          ok(2),
          offline(3)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System SCSI Attachment Path Status.

        This is the status of this path to the chassis.  The following
        values are defined:

            other(1)
              The agent does not recognize the status.  You may need to
              upgrade your software.

            ok(2)
              The path is operating normally.

            offline(3)
              The path is offline."
    ::= { cpqSsScsiAttachmentEntry 8 }

    cpqSsScsiAttachmentPathCondition OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          ok(2),
          degraded(3),
          failed(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Storage System SCSI Attachment Path Condition.

        This is the condition of this path to the chassis."
    ::= { cpqSsScsiAttachmentEntry 9 }


-- ****************************************************************************
--   Storage System Trap Group
--   =========================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSsStorageSys Group          (1.3.6.1.4.1.232.8)
--       cpqSsTrap Group               (1.3.6.1.4.1.232.8.3)   (deprecated)
--
--
--  The trap group maintains information about the number of traps issued
--  from the storageSys enterprise.  The trap group also maintains a table of
--  the last several traps issued.  This table is intended to give a
--  management application some recent status information immediately upon
--  accessing the agent.
--
--  Implementation of the Trap group is optional for agents.
--  The trap group has been deprecated for Insight v2.00 Agents.
--
-- ****************************************************************************

    cpqSsTrapPkts OBJECT-TYPE
        SYNTAX  Counter
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
          "The total number of trap packets issued by the enterprise since
           the instrument agent was loaded."
        ::= { cpqSsTrap 1 }

    cpqSsTrapLogMaxSize OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
           "The maximum number of entries that will currently be kept in
            the trap log.  If the maximum size has been reached and a new
            trap occurs the oldest trap will be removed."
       ::= { cpqSsTrap 2 }

-- ****************************************************************************
--   Storage System Trap Log Table
--   =============================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSsStorageSys Group          (1.3.6.1.4.1.232.8)
--       cpqSsTrap Group               (1.3.6.1.4.1.232.8.3)     (deprecated)
--        cpqSsTrapLogTable            (1.3.6.1.4.1.232.8.3.3)   (deprecated)
--
-- ****************************************************************************

    cpqSsTrapLogTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSsTrapLogEntry
        ACCESS  not-accessible
        STATUS  deprecated
        DESCRIPTION
           "An ordered list of trap log entries (conceptually a queue).
            The trap log entries will be kept in the order in which they
            were generated with the most recent trap at index 1 and the
            oldest trap entry at index trapLogMaxSize.  If the maximum
            number size has been reached and a new trap occurs the oldest
            trap will be removed when the new trap is added so the
            trapMaxLogSize is not exceeded."
       ::= { cpqSsTrap 3 }

    cpqSsTrapLogEntry OBJECT-TYPE
        SYNTAX  CpqSsTrapLogEntry
        ACCESS  not-accessible
        STATUS  deprecated
        DESCRIPTION
           "A description of a trap event."
        INDEX   { cpqSsTrapLogIndex }
        ::= { cpqSsTrapLogTable 1 }

        CpqSsTrapLogEntry ::= SEQUENCE
        {
              cpqSsTrapLogIndex        INTEGER,
              cpqSsTrapType            INTEGER,
              cpqSsTrapTime            OCTET STRING
        }

    cpqSsTrapLogIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
           "The value of this object uniquely identifies this trapLogEntry
            at this time.  The most recent trap will have an index of 1 and
            the oldest trap will have an index of trapLogMaxSize.  Because of
            the queue-like nature of the trapLog this particular trap event's
            index will change as new traps are issued."
        ::= { cpqSsTrapLogEntry 1 }

    cpqSsTrapType OBJECT-TYPE
        SYNTAX  INTEGER
        {
              cpqSsFanStatusChange(1),
              cpqSs2FanStatusChange(8001),
              cpqSsTempFailed(8002),
              cpqSsTempDegraded(8003),
              cpqSsTempOk(8004),
              cpqSsSidePanelInPlace(8005),
              cpqSsSidePanelRemoved(8006)
        }
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
           "The type of the trap event that this entry describes.  This
            number refers to an entry in a list of traps enumerating the
            possible traps the agent may issue."
    ::= { cpqSsTrapLogEntry 2 }

    cpqSsTrapTime OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (6))
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
           "The time of the trap event that this entry describes.  The time
            is given in year (first octet), month, day of month, hour,
            minute, second (last octet) order.  Each octet gives the value in
            BCD."
        ::= { cpqSsTrapLogEntry 3 }


-- ****************************************************************************
--   RAID Storage System Group
--   ==============================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSsStorageSys Group          (1.3.6.1.4.1.232.8)
--       cpqSsRaidSystem Group         (1.3.6.1.4.1.232.8.4)
--        cpqSsRaidSystemTable         (1.3.6.1.4.1.232.8.4.1)
--
--  Implementation of the RAID Storage System group is mandatory.
--
-- ****************************************************************************

    cpqSsRaidSystemTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSsRaidSystemEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
        "RAID Storage System Table."
    ::= { cpqSsRaidSystem 1 }

    cpqSsRaidSystemEntry OBJECT-TYPE
        SYNTAX  CpqSsRaidSystemEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
        "RAID Storage System Entry."
    INDEX   { cpqSsRaidSystemIndex }
    ::= { cpqSsRaidSystemTable 1 }

        CpqSsRaidSystemEntry ::= SEQUENCE
        {
              cpqSsRaidSystemIndex                    INTEGER,
              cpqSsRaidSystemName                     DisplayString,
              cpqSsRaidSystemStatus                   INTEGER,
              cpqSsRaidSystemCondition                INTEGER,
              cpqSsRaidSystemCntlr1SerialNumber       DisplayString,
              cpqSsRaidSystemCntlr2SerialNumber       DisplayString
        }

    cpqSsRaidSystemIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "RAID Storage System Index.

        The RAID Storage System index indicates to which storage system instance
        this table entry belongs."

    ::= { cpqSsRaidSystemEntry 1 }

    cpqSsRaidSystemName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "RAID Storage System Name.

        This is a description of the RAID Storage System's name.
        This can be used for identification purposes."

    ::= { cpqSsRaidSystemEntry 2 }

    cpqSsRaidSystemStatus OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          agentNotRunning(2),
          good(3),
          warning(4),
          communicationLoss(5)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "RAID Storage System Status.

         This is the current status of the RAID Storage System.
         This value will be one of the following:

            other(1)
              Indicates that the agent does not recognize the state of the
              RAID Storage System.  You may need to upgrade the agent.

            agentNotRunning(2)
              Indicates that the Storage Work agent is not running.  You need
              to restart the Storage Work agent.

            good(3)
              Indicates that the system is operating properly.

            warning(4)
              At least one component of the system failed.

            communicationLoss(5)
              The RAID Storage System has a cable or communication problem.
              Please check all cable connects to the host server."


    ::= { cpqSsRaidSystemEntry 3 }

    cpqSsRaidSystemCondition OBJECT-TYPE
        SYNTAX  INTEGER
        {
          other(1),
          ok(2),
          degraded(3),
          failed(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "RAID Storage System Condition.

        This is the overall condition of the storage system.
        The following values are defined:

            other(1)
              The agent does not recognize the status.  You may need to
              upgrade your software.

            ok(2)
              The storage system is operating normally.  No user
              action is required.

            degraded(3)
              The storage system is degraded. At least one component
              of the storage system failed.

            failed(4)
              The storage system has failed."

    ::= { cpqSsRaidSystemEntry 4 }

    cpqSsRaidSystemCntlr1SerialNumber OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..24))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "RAID Storage System Controller 1 Serial Number.

        This is the controller number 1's serial number which is normally
        display on the front panel.  This can be used for
        identification purposes."

    ::= { cpqSsRaidSystemEntry 5 }

    cpqSsRaidSystemCntlr2SerialNumber OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..24))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "RAID Storage System Controller 2 Serial Number.

        This is the controller number 2's serial number which is normally
        display on the front panel.  This can be used for
        identification purposes."

    ::= { cpqSsRaidSystemEntry 6 }


-- ****************************************************************************
--   Storage System Trap Definitions
--   ===============================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--
--  The SNMP trap messages must not be bigger than 484 octets (bytes).
--
--  Trap support in an SNMP agent implementation is optional.  An SNMP
--  agent implementation may support all, some, or none of the traps.
--  If traps are supported, The user should be provided with the option of
--  disabling traps.
--
-- **************************************************************************

    cpqSsFanStatusChange TRAP-TYPE
        ENTERPRISE cpqSsStorageSys
        VARIABLES  { cpqSsBoxFanStatus }
        DESCRIPTION
           "Storage System fan status change.

            The agent has detected a change in the Fan Status of a storage
            system.  The variable cpqSsBoxFanStatus indicates the current
            fan status."

              --#TYPE "Fan Status Change (1)"
              --#SUMMARY "Storage System fan status changed to %d."
              --#ARGUMENTS {0}
              --#SEVERITY CRITICAL
              --#TIMEINDEX 99

        ::= 1

    cpqSs2FanStatusChange TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { cpqSsBoxFanStatus }
        DESCRIPTION
           "Storage System fan status change.

            The agent has detected a change in the Fan Status of a storage
            system.  The variable cpqSsBoxFanStatus indicates the current
            fan status."

              --#TYPE "Fan Status Change (8001)"
              --#SUMMARY "Storage System fan status changed to %d."
              --#ARGUMENTS {0}
              --#SEVERITY CRITICAL
              --#TIMEINDEX 99

        ::= 8001

    cpqSsTempFailed TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { cpqSsBoxTempStatus }
        DESCRIPTION
           "Storage System temperature failure.

            The agent has detected that a temperature status has been set
            to failed.  The storage system will be shutdown."

              --#TYPE "Storage System Temperature Failure (8002)"
              --#SUMMARY "Storage System will be shutdown."
              --#ARGUMENTS {}
              --#SEVERITY CRITICAL
              --#TIMEINDEX 99
              --#STATE   NONOPERATIONAL

        ::= 8002

    cpqSsTempDegraded TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { cpqSsBoxTempStatus }
        DESCRIPTION
           "Storage System temperature degraded.

            The agent has detected a temperature status that has been set to
            degraded.  The storage system's temperature is outside of the
            normal operating range."

              --#TYPE "Storage System Temp Degraded (8003)"
              --#SUMMARY "Temp is outside of normal range."
              --#ARGUMENTS {}
              --#SEVERITY MAJOR
              --#TIMEINDEX 99
              --#STATE   DEGRADED

        ::= 8003

    cpqSsTempOk TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { cpqSsBoxTempStatus }
        DESCRIPTION
           "Storage System temperature ok.

            The temperature status has been set to OK.  The storage
            system's temperature has returned to normal operating range.
            It may be reactivated by the administrator."

              --#TYPE "Storage System Temp OK (8004)"
              --#SUMMARY "Storage System temperature ok."
              --#ARGUMENTS {}
              --#SEVERITY INFORMATIONAL
              --#TIMEINDEX 99
              --#STATE OPERATIONAL

        ::= 8004

    cpqSsSidePanelInPlace TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { cpqSsBoxSidePanelStatus }
        DESCRIPTION
           "Storage System side panel is in place.

            The side panel status has been set to in place.  The storage
            system's side panel has returned to a properly installed state."

              --#TYPE "Storage System side panel is in place (8005)"
              --#SUMMARY "Side panel is re-installed on unit."
              --#ARGUMENTS {}
              --#SEVERITY INFORMATIONAL
              --#TIMEINDEX 99
              --#STATE OPERATIONAL

        ::= 8005


    cpqSsSidePanelRemoved TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { cpqSsBoxSidePanelStatus }
        DESCRIPTION
           "Storage System side panel is removed.

            The side panel status has been set to removed.  The storage
            system's side panel is not in a properly installed state. This
            situation may result in improper cooling of the drives in the
            storage system due to air flow changes caused by the missing
            side panel."

              --#TYPE "Storage System side panel is removed (8006)"
              --#SUMMARY "Side panel is removed from unit."
              --#ARGUMENTS {}
              --#SEVERITY MAJOR
              --#TIMEINDEX 99
              --#STATE DEGRADED

        ::= 8006

    cpqSsPwrSupplyDegraded TRAP-TYPE
        ENTERPRISE compaq
        DESCRIPTION
            "A storage system power supply status has been set to degraded."

        --#TYPE "Power Supply Degraded (8007)"
        --#SUMMARY "A storage system power supply unit has become degraded"
        --#ARGUMENTS {}
        --#SEVERITY CRITICAL
        --#TIMEINDEX 99
        --#STATE   DEGRADED

        ::= 8007


    cpqSs3FanStatusChange TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSsBoxFanStatus }
        DESCRIPTION
           "Storage System fan status change.

            The agent has detected a change in the Fan Status of a storage
            system.  The variable cpqSsBoxFanStatus indicates the current
            fan status.

            User Action: If the fan status is degraded or failed, replace
            any failed fans."

              --#TYPE "Fan Status Change (8008)"
              --#SUMMARY "Storage System fan status changed to %d."
              --#ARGUMENTS {2}
              --#SEVERITY CRITICAL
              --#TIMEINDEX 99

        ::= 8008

    cpqSs3TempFailed TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSsBoxTempStatus }
        DESCRIPTION
           "Storage System temperature failure.

            The agent has detected that a temperature status has been set to
            failed.  The storage system will be shutdown.

            User Action: Shutdown the storage system as soon as possible.
            Insure that the storage system environment is being cooled
            properly and that no components are overheated."

              --#TYPE "Storage System Temperature Failure (8009)"
              --#SUMMARY "Storage System will be shutdown."
              --#ARGUMENTS {}
              --#SEVERITY CRITICAL
              --#TIMEINDEX 99
              --#STATE   NONOPERATIONAL

        ::= 8009

    cpqSs3TempDegraded TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSsBoxTempStatus }
        DESCRIPTION
           "Storage System temperature degraded.

            The agent has detected a temperature status that has been set to
            degraded.  The storage system's temperature is outside of the
            normal operating range.

            User Action: Shutdown the storage system as soon as possible.
            Insure that the storage system environment is being cooled
            properly and that no components are overheated."

              --#TYPE "Storage System Temp Degraded (8010)"
              --#SUMMARY "Temp is outside of normal range."
              --#ARGUMENTS {}
              --#SEVERITY MAJOR
              --#TIMEINDEX 99
              --#STATE   DEGRADED

        ::= 8010

    cpqSs3TempOk TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSsBoxTempStatus }
        DESCRIPTION
           "Storage System temperature ok.

            The temperature status has been set to OK.  The storage
            system's temperature has returned to normal operating range.
            It may be reactivated by the administrator.

            User Action: None."

              --#TYPE "Storage System Temp OK (8011)"
              --#SUMMARY "Storage System temperature ok."
              --#ARGUMENTS {}
              --#SEVERITY INFORMATIONAL
              --#TIMEINDEX 99
              --#STATE OPERATIONAL

        ::= 8011

    cpqSs3SidePanelInPlace TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSsBoxSidePanelStatus }
        DESCRIPTION
           "Storage System side panel is in place.

            The side panel status has been set to in place.  The storage
            system's side panel has returned to a properly installed state.

            User Action: None."

              --#TYPE "Storage System side panel is in place (8012)"
              --#SUMMARY "Side panel is re-installed on unit."
              --#ARGUMENTS {}
              --#SEVERITY INFORMATIONAL
              --#TIMEINDEX 99
              --#STATE OPERATIONAL

        ::= 8012


    cpqSs3SidePanelRemoved TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSsBoxSidePanelStatus }
        DESCRIPTION
           "Storage System side panel is removed.

            The side panel status has been set to removed.  The storage
            system's side panel is not in a properly installed state. This
            situation may result in improper cooling of the drives in the
            storage system due to air flow changes caused by the missing
            side panel.

            User Action: Replace the storage system side panel."

              --#TYPE "Storage System side panel is removed (8013)"
              --#SUMMARY "Side panel is removed from unit."
              --#ARGUMENTS {}
              --#SEVERITY MAJOR
              --#TIMEINDEX 99
              --#STATE DEGRADED

        ::= 8013

    cpqSs3PwrSupplyDegraded TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags }
        DESCRIPTION
            "A storage system power supply status has been set to degraded."

        --#TYPE "Power Supply Degraded (8014)"
        --#SUMMARY "A storage system power supply unit has become degraded"
        --#ARGUMENTS {}
        --#SEVERITY CRITICAL
        --#TIMEINDEX 99
        --#STATE   DEGRADED
        ::= 8014

    cpqSs4PwrSupplyDegraded TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSsBoxFltTolPwrSupplyStatus }
        DESCRIPTION
            "A storage system power supply status has been set to degraded.

            User Action: Take action to restore power or replace any failed
            storage system power supply."

        --#TYPE "Power Supply Degraded (8015)"
        --#SUMMARY "A storage system power supply unit has become degraded"
        --#ARGUMENTS {}
        --#SEVERITY CRITICAL
        --#TIMEINDEX 99
        --#STATE   DEGRADED

        ::= 8015


    cpqSsExFanStatusChange TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSsChassisName,
                     cpqSsChassisTime, cpqSsFanModuleLocation,
                     cpqSsFanModuleStatus }
        DESCRIPTION
           "Storage system fan status change.

            The agent has detected a change in the Fan Module Status of a
            storage system.  The variable cpqSsFanModuleStatus indicates the
            current fan status.

            User Action: If the fan status is degraded or failed, replace
            any failed fans."

              --#TYPE "Fan Status Change (8016)"
              --#SUMMARY "Storage system fan status changed to %d."
              --#ARGUMENTS {5}
              --#SEVERITY CRITICAL
              --#TIMEINDEX 99

        ::= 8016

    cpqSsExPowerSupplyStatusChange TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSsChassisName,
                     cpqSsChassisTime, cpqSsPowerSupplyBay,
                     cpqSsPowerSupplyStatus }
        DESCRIPTION
           "Storage system power supply status change.

            The agent has detected a change in the power supply status of a
            storage system.  The variable cpqSsPowerSupplyStatus indicates
            the current status.

            User Action: If the power supply status is failed, take action to
            restore power or replace the failed power supply."

              --#TYPE "Power Supply Status Change (8017)"
              --#SUMMARY "Storage system power supply status changed to %d."
              --#ARGUMENTS {5}
              --#SEVERITY CRITICAL
              --#TIMEINDEX 99

        ::= 8017

    cpqSsExPowerSupplyUpsStatusChange TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSsChassisName,
                     cpqSsChassisTime, cpqSsPowerSupplyBay,
                     cpqSsPowerSupplyUpsStatus }
        DESCRIPTION
           "Storage system power supply UPS status change.

            The agent has detected a change status of a UPS attached to a
            storage system power supply.  The variable
            cpqSsPowerSupplyUpsStatus indicates the current status.

            User Action: If the UPS status is powerFailed(4) or batteryLow(5),
            take action to restore power to the UPS."

              --#TYPE "Power Supply UPS Status Change (8018)"
              --#SUMMARY "Storage system power supply UPS status changed to %d."
              --#ARGUMENTS {5}
              --#SEVERITY CRITICAL
              --#TIMEINDEX 99

        ::= 8018

    cpqSsExTempSensorStatusChange TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSsChassisName,
                     cpqSsChassisTime, cpqSsTempSensorLocation,
                     cpqSsTempSensorStatus, cpqSsTempSensorCurrentValue }
        DESCRIPTION
           "Storage system temperature sensor status change.

            The agent has detected a change in the status of a storage
            system temperature sensor.  The variable cpqSsTempSensorStatus
            indicates the current status.

            User Action: If the temperature status is degraded or failed,
            shutdown the storage system as soon as possible.  Insure that
            the storage system environment is being cooled properly and that
            no components are overheated."

              --#TYPE "Temperature Sensor Status Change (8019)"
              --#SUMMARY "Storage system temperature sensor status changed to %d."
              --#ARGUMENTS {5}
              --#SEVERITY CRITICAL
              --#TIMEINDEX 99
              --#VARBINDSEVERITY 2

        ::= 8019

    cpqSsEx2FanStatusChange TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSsChassisName,
                     cpqSsChassisTime, cpqSsFanModuleLocation,
                     cpqSsFanModuleStatus, cpqSsFanModuleSerialNumber,
                     cpqSsFanModuleBoardRevision }
        DESCRIPTION
           "Storage system fan status change.

            The agent has detected a change in the fan module status of a
            storage system.  The variable cpqSsFanModuleStatus indicates the
            current fan status.

            User Action: If the fan status is degraded or failed, replace
            any failed fans."

              --#TYPE "Fan Status Change (8020)"
              --#SUMMARY "Storage system fan status changed to %d."
              --#ARGUMENTS {5}
              --#SEVERITY CRITICAL
              --#TIMEINDEX 99
              --#VARBINDSEVERITY 2

        ::= 8020

    cpqSsEx2PowerSupplyStatusChange TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSsChassisName,
                     cpqSsChassisTime, cpqSsPowerSupplyBay,
                     cpqSsPowerSupplyStatus, cpqSsPowerSupplySerialNumber,
                     cpqSsPowerSupplyBoardRevision,
                     cpqSsPowerSupplyFirmwareRevision }
        DESCRIPTION
           "Storage system power supply status change.

            The agent has detected a change in the power supply status of a
            storage system.  The variable cpqSsPowerSupplyStatus indicates
            the current status.

            User Action: If the power supply status is failed, take action to
            restore power or replace the failed power supply."

              --#TYPE "Power Supply Status Change (8021)"
              --#SUMMARY "Storage system power supply status changed to %d."
              --#ARGUMENTS {5}
              --#SEVERITY CRITICAL
              --#TIMEINDEX 99
              --#VARBINDSEVERITY 2

        ::= 8021

    cpqSsExBackplaneFanStatusChange TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSsChassisName,
                     cpqSsChassisTime, cpqSsBackplaneIndex,
                     cpqSsBackplaneVendor, cpqSsBackplaneModel,
                     cpqSsBackplaneSerialNumber, cpqSsBackplaneFanStatus }
        DESCRIPTION
           "Storage system fan status change.

            The agent has detected a change in the fan status of a storage
            system.  The variable cpqSsBackplaneFanStatus indicates the
            current fan status.

            User Action: If the fan status is degraded or failed, replace
            any failed fans."

              --#TYPE "Storage System Fan Status Change (8022)"
              --#SUMMARY "Storage system fan status changed to %d."
              --#ARGUMENTS {8}
              --#SEVERITY CRITICAL
              --#TIMEINDEX 99
              --#VARBINDSEVERITY 2

        ::= 8022

    cpqSsExBackplaneTempStatusChange TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSsChassisName,
                     cpqSsChassisTime, cpqSsBackplaneIndex,
                     cpqSsBackplaneVendor, cpqSsBackplaneModel,
                     cpqSsBackplaneSerialNumber, cpqSsBackplaneTempStatus }
        DESCRIPTION
           "Storage system temperature status change.

            The agent has detected a change in the status of the temperature
            in a storage system.  The variable cpqSsBackplaneTempStatus
            indicates the current status.

            User Action: If the temperature status is degraded or failed,
            shutdown the storage system as soon as possible.  Insure that
            the storage system environment is being cooled properly and that
            no components are overheated."

              --#TYPE "Storage System Temperature Status Change (8023)"
              --#SUMMARY "Storage system temperature status changed to %d."
              --#ARGUMENTS {8}
              --#SEVERITY CRITICAL
              --#TIMEINDEX 99
              --#VARBINDSEVERITY 2

        ::= 8023

    cpqSsExBackplanePowerSupplyStatusChange TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSsChassisName,
                     cpqSsChassisTime, cpqSsBackplaneIndex,
                     cpqSsBackplaneVendor, cpqSsBackplaneModel,
                     cpqSsBackplaneSerialNumber, cpqSsBackplaneFtpsStatus }
        DESCRIPTION
           "Storage system power supply status change.

            The agent has detected a change in the power supply status of a
            storage system.  The variable cpqSsBackplaneFtpsStatus indicates
            the current status.

            User Action: If the power supply status is degraded, take action to
            restore power or replace the failed power supply."

              --#TYPE "Power Supply Status Change (8024)"
              --#SUMMARY "Storage system power supply status changed to %d."
              --#ARGUMENTS {8}
              --#SEVERITY CRITICAL
              --#TIMEINDEX 99
              --#VARBINDSEVERITY 2

        ::= 8024

    cpqSsExRecoveryServerStatusChange TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSsChassisName,
                     cpqSsChassisTime,  cpqSsChassisRsoStatus,
                     cpqSsChassisIndex }
        DESCRIPTION
           "Storage system recovery server option status change.

            The agent has detected a change in the recovery server option
            status of a storage system.  The variable cpqSsChassisRsoStatus
            indicates the current status.

            User Action: If the RSO status is noSecondary(6) or linkDown(7),
            insure the secondary server is operational and all cables are
            connected properly.  If the RSO status is secondaryRunningAuto(8)
            or secondaryRunningUser(9), examine the the primary server for
            failed components."

              --#TYPE "Recovery Server Option Status Change (8025)"
              --#SUMMARY "Storage system recovery server option status changed to %d."
              --#ARGUMENTS {4}
              --#SEVERITY MAJOR
              --#TIMEINDEX 99
              --#VARBINDSEVERITY 2

        ::= 8025

    cpqSs5FanStatusChange TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSsBoxCntlrHwLocation,
                     cpqSsBoxCntlrIndex, cpqSsBoxBusIndex, cpqSsBoxVendor,
                     cpqSsBoxModel, cpqSsBoxSerialNumber, cpqSsBoxFanStatus }
        DESCRIPTION
           "Storage System fan status change.

            The agent has detected a change in the Fan Status of a storage
            system.  The variable cpqSsBoxFanStatus indicates the current
            fan status.

            User Action: If the fan status is degraded or failed, replace
            any failed fans."

              --#TYPE "Fan Status Change (8026)"
              --#SUMMARY "Storage System fan status changed to %d."
              --#ARGUMENTS {8}
              --#SEVERITY CRITICAL
              --#TIMEINDEX 99

        ::= 8026

    cpqSs5TempStatusChange TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSsBoxCntlrHwLocation,
                     cpqSsBoxCntlrIndex, cpqSsBoxBusIndex, cpqSsBoxVendor,
                     cpqSsBoxModel, cpqSsBoxSerialNumber, cpqSsBoxTempStatus }
        DESCRIPTION
           "Storage System temperature status change.

            The agent has detected a change in the temperature status of a
            storage system.  The variable cpqSsBoxTempStatus indicates the
            current temperature status.

            User Action: If the temperature status is degraded or failed,
            shutdown the storage system as soon as possible.  Insure that
            the storage system environment is being cooled properly and that
            no components are overheated."

              --#TYPE "Temperature Status Change (8027)"
              --#SUMMARY "Storage System temperature status changed to %d."
              --#ARGUMENTS {8}
              --#SEVERITY CRITICAL
              --#TIMEINDEX 99

        ::= 8027

    cpqSs5PwrSupplyStatusChange TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSsBoxCntlrHwLocation,
                     cpqSsBoxCntlrIndex, cpqSsBoxBusIndex, cpqSsBoxVendor,
                     cpqSsBoxModel, cpqSsBoxSerialNumber,
                     cpqSsBoxFltTolPwrSupplyStatus }
        DESCRIPTION
            "Storage system power supply status change.

            The agent has detected a change in the power supply status of a
            storage system.  The variable cpqSsBoxFltTolPwrSupplyStatus
            indicates the current power supply status.

            User Action: If the power supply status is degraded, take action
            to restore power or replace the failed power supply."

              --#TYPE "Power Supply Status Change (8028)"
              --#SUMMARY "Storage system power supply status changed to %d."
              --#ARGUMENTS {8}
              --#SEVERITY CRITICAL
              --#TIMEINDEX 99

        ::= 8028

    cpqSs6FanStatusChange TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSsBoxCntlrHwLocation,
                     cpqSsBoxCntlrIndex, cpqSsBoxBusIndex, cpqSsBoxVendor,
                     cpqSsBoxModel, cpqSsBoxSerialNumber,
                     cpqSsBoxFanStatus, cpqSsBoxLocationString }
        DESCRIPTION
           "Storage System fan status change.

            The agent has detected a change in the Fan Status of a storage
            system.  The variable cpqSsBoxFanStatus indicates the current
            fan status.

            User Action: If the fan status is degraded or failed, replace
            any failed fans."

              --#TYPE "Fan Status Change (8029)"
              --#SUMMARY "Storage System fan status changed to %d."
              --#ARGUMENTS {8}
              --#SEVERITY CRITICAL
              --#TIMEINDEX 99
              --#VARBINDSEVERITY 2

        ::= 8029

    cpqSs6TempStatusChange TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSsBoxCntlrHwLocation,
                     cpqSsBoxCntlrIndex, cpqSsBoxBusIndex, cpqSsBoxVendor,
                     cpqSsBoxModel, cpqSsBoxSerialNumber,
                     cpqSsBoxTempStatus, cpqSsBoxLocationString }
        DESCRIPTION
           "Storage System temperature status change.

            The agent has detected a change in the temperature status of a
            storage system.  The variable cpqSsBoxTempStatus indicates the
            current temperature status.

            User Action: If the temperature status is degraded or failed,
            shutdown the storage system as soon as possible.  Insure that
            the storage system environment is being cooled properly and that
            no components are overheated."

              --#TYPE "Temperature Status Change (8030)"
              --#SUMMARY "Storage System temperature status changed to %d."
              --#ARGUMENTS {8}
              --#SEVERITY CRITICAL
              --#TIMEINDEX 99
              --#VARBINDSEVERITY 2

        ::= 8030

    cpqSs6PwrSupplyStatusChange TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSsBoxCntlrHwLocation,
                     cpqSsBoxCntlrIndex, cpqSsBoxBusIndex, cpqSsBoxVendor,
                     cpqSsBoxModel, cpqSsBoxSerialNumber,
                     cpqSsBoxFltTolPwrSupplyStatus, cpqSsBoxLocationString }
        DESCRIPTION
            "Storage system power supply status change.

            The agent has detected a change in the power supply status of a
            storage system.  The variable cpqSsBoxFltTolPwrSupplyStatus
            indicates the current power supply status.

            User Action: If the power supply status is degraded, take action
            to restore power or replace the failed power supply."

              --#TYPE "Power Supply Status Change (8031)"
              --#SUMMARY "Storage system power supply status changed to %d."
              --#ARGUMENTS {8}
              --#SEVERITY CRITICAL
              --#TIMEINDEX 99
              --#VARBINDSEVERITY 2

        ::= 8031

END
