DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10702 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Firmware is out of NVRAM and cannot built the ILM memory slice device map'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Firmware is out of NVRAM and cannot built the ILM memory slice device map: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware is out of NVRAM and cannot built the ILM memory slice device map'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10703 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The NVRAM for the CPU map is corrupt and cannot be trusted. It appears that there are more CPUs in the map than the size of the map can hold.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The NVRAM for the CPU map is corrupt and cannot be trusted. It appears that there are more CPUs in the map than the size of the map can hold.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The NVRAM for the CPU map is corrupt and cannot be trusted. It appears that there are more CPUs in the map than the size of the map can hold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10704 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The NVRAM for the IO device ownership map is corrupt and cannot be trusted. It appears that there are more IO devices in the map than the size of the map can hold.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The NVRAM for the IO device ownership map is corrupt and cannot be trusted. It appears that there are more IO devices in the map than the size of the map can hold.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The NVRAM for the IO device ownership map is corrupt and cannot be trusted. It appears that there are more IO devices in the map than the size of the map can hold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10705 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The NVRAM for the cell local memory map is corrupt and cannot be trusted. It appears that there are more memory slices in the map than the size of the map can hold.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The NVRAM for the cell local memory map is corrupt and cannot be trusted. It appears that there are more memory slices in the map than the size of the map can hold.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The NVRAM for the cell local memory map is corrupt and cannot be trusted. It appears that there are more memory slices in the map than the size of the map can hold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10706 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An internal firmware inconsistency exists or the server exhausted its internal resources and is unable to create an fPars EFI ownership variable for a CPU device in the partition.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An internal firmware inconsistency exists or the server exhausted its internal resources and is unable to create an fPars EFI ownership variable for a CPU device in the partition: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An internal firmware inconsistency exists or the server exhausted its internal resources and is unable to create an fPars EFI ownership variable for a CPU device in the partition. Either of these conditions is fatal.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10707 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An internal firmware inconsistency exists or the server exhausted its internal resources and is unable to create an fPars EFI ownership variable for an IO device in the partition.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An internal firmware inconsistency exists or the server exhausted its internal resources and is unable to create an fPars EFI ownership variable for an IO device in the partition: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An internal firmware inconsistency exists or the server exhausted its internal resources and is unable to create an fPars EFI ownership variable for an IO device in the partition. Either of these conditions is fatal.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10708 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An internal firmware inconsistency exists or the server exhausted its internal resources and is unable to create an fPars EFI ownership variable for a CLM device in the partition. Either of these conditions is fatal.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An internal firmware inconsistency exists or the server exhausted its internal resources and is unable to create an fPars EFI ownership variable for a CLM device in the partition: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An internal firmware inconsistency exists or the server exhausted its internal resources and is unable to create an fPars EFI ownership variable for a CLM device in the partition. Either of these conditions is fatal.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10771 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Firmware has run out of NVRAM and cannot create the needed variable(s)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Firmware has run out of NVRAM and cannot create the needed variable(s): &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware has run out of NVRAM and cannot create the needed variable(s)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10772 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The call to the IOC firmware component method  LbaReconfig  failed, probably a low-level hardware error.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The call to the IOC firmware component method  LbaReconfig  failed, probably a low-level hardware error: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The call to the IOC firmware component method  LbaReconfig  failed, probably a low-level hardware error. The fPar BSP is identified in bits 63..32 of the event detail,'
DEFine MSGACTion Name=(*,30)
        ACTION=ANNOTATE TEXT='the fPar owning this CPU and LBA is identified in bits 31..16 and the number of the Rope is identified in bits 15..0.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10779 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The CPU modules have been installed in an illegal configuration on the cell board'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The CPU modules have been installed in an illegal configuration on the cell board: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The CPU modules have been installed in an illegal configuration on the cell board.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10780 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Invalid CPU terminator installed on the cell board.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Invalid CPU terminator installed on the cell board.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An invalid CPU terminator card is installed on the cell board. The data field indicates the physical location of the offending socket.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10793 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Invocation of the soft reset code code from an interrupt or similar vector,'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Invocation of the soft reset code code from an interrupt or similar vector,: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Invocation of the soft reset code code from an interrupt or similar vector, or improper locking/releasing of semaphores.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10794 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Data field is count of cpus held by the sm4 which issues the event (and is trying to reset itself). Indicates invocation of the SoftResetCpu code from an interrupt or similar vector.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Data field is count of cpus held by the sm4 which issues the event (and is trying to reset itself). Indicates invocation of the SoftResetCpu code from an interrupt or similar vector.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Data field is count of cpus held by the sm4 which issues the event (and is trying to reset itself). Indicates invocation of the SoftResetCpu code from an interrupt or similar vector where the processor was modifying critical resources, or'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='improper locking/releasing of semaphores.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10795 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A reset of an fPar discovered that an fPar failed to release critical resources within a reasonable time.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A reset of an fPar discovered that an fPar failed to release critical resources within a reasonable time.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A reset of an fPar discovered that an fPar failed to release critical resources within a reasonable time.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10814 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Significant numbers of corrected memory errors have been detected on the memory subsystem'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Significant numbers of corrected memory errors have been detected on the memory subsystem: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Significant numbers of corrected memory errors have been detected on the memory subsystem'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10822 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Over-temperature condition detected on a processor'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Over-temperature condition detected on a processor: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Over-temperature condition detected on a processor'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10823 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cache errors detected on a processor'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cache errors detected on a processor: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Cache errors detected on a processor'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10824 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Corrected errors detected in the cache portion of the memory for a processor module'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Corrected errors detected in the cache portion of the memory for a processor module: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Corrected errors detected in the cache portion of the memory for a processor module'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10825 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Corrected errors detected on the system bus for a processor module'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Corrected errors detected on the system bus for a processor module: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Corrected errors detected on the system bus for a processor module'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10826 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Corrected errors detected on the processor bus for a processor module'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Corrected errors detected on the processor bus for a processor module: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Corrected errors detected on the processor bus for a processor module'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10827 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Corrected errors detected in the tag portion of the memory for a processor module'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Corrected errors detected in the tag portion of the memory for a processor module: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Corrected errors detected in the tag portion of the memory for a processor module'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10830 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event fPars-mode EFI variable is set to enable fPars operation but no fPars are actually enabled to boot. So the server boots in hard partition mode.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event fPars-mode EFI variable is set to enable fPars operation but no fPars are actually enabled to boot. So the server boots in hard partition mode.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='fPars-mode EFI variable is set to enable fPars operation but no fPars are actually enabled to boot. So the server boots in hard partition mode.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10832 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An fPar was directed to reset using the ESIT DirectedfParResetAndMigrate() service but the target (recipient) fPar of the resources is in a state that cannot receive ownership of these resources.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An fPar was directed to reset using the ESIT DirectedfParResetAndMigrate() service but the target (recipient) fPar of the resources is in a state that cannot receive ownership of these resources.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An fPar was directed to reset using the ESIT DirectedfParResetAndMigrate() service but the target (recipient) fPar of the resources is in a state that cannot receive ownership of these resources.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10833 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Firmware error setting the NVRAM value of preferred-bsp for the vPars monitor. The partition will boot using the PD monarch, but the value of preferred-bsp may not match this CPU.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Firmware error setting the NVRAM value of preferred-bsp for the vPars monitor. The partition will boot using the PD monarch, but the value of preferred-bsp may not match this CPU.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware error setting the NVRAM value of preferred-bsp for the vPars monitor. The partition will boot using the PD monarch, but the value of preferred-bsp may not match this CPU.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10842 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unable to write to an XBC port ROUTE_TABLE_ENABLE_MASK CSR in Arches Fabric Phase3. Data field: (XBC port 48) | (XBC ID 32) | (route).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unable to write to an XBC port ROUTE_TABLE_ENABLE_MASK CSR in Arches Fabric Phase3. Data field: (XBC port 48) | (XBC ID 32) | (route).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Unable to write to an XBC port ROUTE_TABLE_ENABLE_MASK CSR in Arches Fabric Phase3. Data field: (XBC port << 48) | (XBC ID < 32) | (route)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10853 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An unrecoverable processor interrupt occured. IPF firmware owned the processor interrupt vector table (IVT) at the time of the interrupt.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An unrecoverable processor interrupt occured. IPF firmware owned the processor interrupt vector table (IVT) at the time of the interrupt.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An unrecoverable processor interrupt occured. IPF firmware owned the processor interrupt vector table (IVT) at the time of the interrupt.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10871 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event SBA call to LBA SetDeviceMask method fails.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event SBA call to LBA SetDeviceMask method fails.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='SBA call to LBA SetDeviceMask method fails.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10927 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event LBA slot device scan error.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event LBA slot device scan error.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='LBA slot device scan error'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10936 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event There is none (or inadequate) memory slice resoruce assigned to the fPar so it cannot boot its instance. The fPar will be disabled (enter a spinloop) because it cannot boot, or if in vPars mode will return control to the monitor.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event There is none (or inadequate) memory slice resoruce assigned to the fPar so it cannot boot its instance: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='There is none (or inadequate) memory slice resoruce assigned to the fPar so it cannot boot its instance. The fPar will be disabled (enter a spinloop) because it cannot boot, or if in vPars mode will return control to the monitor.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10937 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Couldn t collect vertex information during Fabric Info call. Data Field: return status.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Couldn t collect vertex information during Fabric Info call. Data Field: return status.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Couldn t collect vertex information during Fabric Info call. Data Field: return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10938 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Couldn t collect the vertices during the Fabric Info call. Data Field: number of vertices returned.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Couldn t collect the vertices during the Fabric Info call. Data Field: number of vertices returned.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Couldn t collect the vertices during the Fabric Info call. Data Field: number of vertices returned'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10939 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Couldn t find all the edges during a procedure call. Data Field: return status.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Couldn t find all the edges during a procedure call. Data Field: return status.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Couldn t find all the edges during a procedure call. Data Field: return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10940 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Couldn t find an appropriate number of edges during a procedure call. Data Field: the number of edges found.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Couldn t find an appropriate number of edges during a procedure call. Data Field: the number of edges found.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Couldn t find an appropriate number of edges during a procedure call. Data Field: the number of edges found'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10941 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Too many edges were encountered during a procedure call. Data Field: link count.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Too many edges were encountered during a procedure call. Data Field: link count.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Too many edges were encountered during a procedure call. Data Field: link count'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10943 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to get an address during a procedure call. Data Field: return status.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to get an address during a procedure call. Data Field: return status.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failed to get an address during a procedure call. Data Field: return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10944 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An unexpected state was encountered during a procedure call. Data Field: state returned.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An unexpected state was encountered during a procedure call. Data Field: state returned.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An unexpected state was encountered during a procedure call. Data Field: state returned'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10945 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unable to get the link health state during a procedure call. Data Field: return status.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unable to get the link health state during a procedure call. Data Field: return status.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Unable to get the link health state during a procedure call. Data Field: (cell num << 56) | (port << 44) | (xbc << 32)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10946 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The fabric data failed a CRC check. Data Field: (xbc port 44 ) | (xbc 32) | return status).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The fabric data failed a CRC check. Data Field: (xbc port 44 ) | (xbc 32) | return status).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The fabric data failed a CRC check. Data Field: (xbc port << 44 ) | (xbc << 32) | return status)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11032 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event VM_CollectVertices failed unexpectedly. Could possibly be a data corruption problem. Data field: (cell number 56) | (return value from VM_CollectVertices).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event VM_CollectVertices failed unexpectedly. Could possibly be a data corruption problem. Data field: (cell number 56) | (return value from VM_CollectVertices): &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='VM_CollectVertices failed unexpectedly. Could possibly be a data corruption problem. Data field: (cell number << 56) | (return value from VM_CollectVertices)'

