DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5204 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Uncorrectable (multiple-bit) ECC error in DIMM'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Uncorrectable (multiple-bit) ECC error in DIMM: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A series of MEM_MBE_IN_RANK chassis code will be sent when an error is detected by firmware. The data fields will contain information on the error based on the data type as follows: Physical Location - location of dimm(s) in error; Physical'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='Address - address affect by error; Syndrome - Firmware generated ECC syndrome that can be used to further isolate the error.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5205 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Memory register test failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Memory register test failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The chipset s memory controller failed the register test. The data field contains the address of the register that failed selftest.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5208 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event SPD found no memory DIMMs'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event SPD found no memory DIMMs: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Memory Discovery could not detect any DIMMs installed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5209 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event No memory found'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event No memory found: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='FW could not continue because there are no valid memory ranks loaded.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5211 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cannot log memory error because PDT is disabled'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cannot log memory error because PDT is disabled: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The PDT has been disabled, and FW found memory errors during selftest. This is a stopboot condition. Also, the PDT will never be disabled in customer systems, so this event should never be seen in the field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5212 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PDT is disabled'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PDT is disabled: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An event indicating that the user has the PDT disabled on this boot. The PDT will never be disabled in customer systems, so this event should never be seen in the field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5214 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error adding entry to PDT'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error adding entry to PDT: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error writing entry into the PDT.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5216 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cannot add PDT entry-PDT full'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cannot add PDT entry-PDT full: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An attempt was made to add an entry to a full PDT. The entry is not added, and this event is sent.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5218 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Memory platform data update failure'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Memory platform data update failure: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Memory FW was unable to save or restore the original error configuration (including CEC error log and signal enable and CPU ECC detection). This event should never be seen in the field unless there is a FW problem'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5219 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Can t find memory rank entry'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Can t find memory rank entry: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The rank structure that corresponds to the rankID in the data field could not be found in the Rank table. The Data field is the rankID of the structure it is looking for. This error event should never be seen.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5237 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Memory error overflow:'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Memory error overflow:: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='More than one error type was detected when only one error type was expected.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5238 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Memory forward progress code invalid'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Memory forward progress code invalid: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The forward progress bits that memory FW uses to track state are invalid. The data field is the fwd progress field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5244 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Memory error status invalid'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Memory error status invalid: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The memory error status has bits set in it that indicate another non-memory error occurred. The data field contains the CEC s error status.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5245 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Memory error summary bits invalid'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Memory error summary bits invalid: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The memory test summary bits are invalid. The data field is the test summary bits.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5248 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unexpected machine check during memory code'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unexpected machine check during memory code: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Memory rank shadowing has been selected but is not supported by the revision of the memory controller.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5250 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The DIMM distribution check was bypassed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The DIMM distribution check was bypassed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The control bit to skip the DIMM distribution check is set and the DIMM distribution check was skipped. This bit should only be done in the factory and not in the field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5252 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The DIMM Loading Order check was bypassed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The DIMM Loading Order check was bypassed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The control bit to skip the DIMM loading order check is set and the DIMM loading order check was skipped. This bit should only be done in the factory and not in the field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5253 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Looping on destructive memory tests'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Looping on destructive memory tests: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The control bit to loop on destructive memory test is set and the destructive memory tests are run continously. This bit should only be done in the factory and not in the field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5255 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event DIMM Set Check has been skipped'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event DIMM Set Check has been skipped: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The control bit to skip the DIMM set check is set and the DIMM set check was skipped. This bit should only be done in the factory and not in the field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5256 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Serial Presence Detect (SPD) has been skipped'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Serial Presence Detect (SPD) has been skipped: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The control bit to skip the DIMM SPD check is set and the checking of the DIMM SPD was skipped. This bit should only be done in the factory and not in the field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5257 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An Alternate Memory Config has been loaded into the system'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An Alternate Memory Config has been loaded into the system: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The control bit to load an alternate memory configuration is set and an alternate memory configuration has been loaded. This bit should only be set in the factory and not in the field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5260 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event OS INIT address not registered'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event OS INIT address not registered: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The OS_INIT vector has not been registered'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5263 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event OS MCA address not registered'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event OS MCA address not registered: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The OS_MCA vector has not been registered'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5264 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event OS MCA did not correct the Machine Check'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event OS MCA did not correct the Machine Check: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An Uncorrected Machine Check has occurred'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5266 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Found bad miscellaneous register'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Found bad miscellaneous register: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A PDH register has failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5268 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event SAL_CHECK failed for an unknown reason'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event SAL_CHECK failed for an unknown reason: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The handler for SAL_CHECK has failed for an unknown reason.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5270 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event SAL_INIT failed for an unknown reason'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event SAL_INIT failed for an unknown reason: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The handler for SAL_INIT has failed for an unknown reason.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5278 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unspecified memory interleave error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unspecified memory interleave error: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Indicates that FW encountered a Fatal interleaving error. The data field contains the return status from the interleaving procedure call.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5279 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unexpected return to SAL_CHECK'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unexpected return to SAL_CHECK: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Unexpected return to SAL_CHECK.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5280 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unexpected return to SAL_INIT'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unexpected return to SAL_INIT: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The SFW TOC vector (SAL_INIT) has been unexpectedly returned to.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5335 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Firmware is adding a DEGRADED cpu node to the device tree.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Firmware is adding a DEGRADED cpu node to the device tree.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware is adding a device tree node for a CPU that is degraded in functionality. The cpu should not be trusted and will not be active in the system.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5354 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PD rendezvous will fail do to a Firmware Tree error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PD rendezvous will fail do to a Firmware Tree error: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware was unable to locate a required element in the device tree and cannot create a partition. The resource that cannot be located is listed as an ansii string in the data field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5359 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The current cell is not configured as part of the expected set'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The current cell is not configured as part of the expected set: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The currently executing cell is not configured to be part of the cell set it is attempting to rendezvous with.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5360 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A remote CSR could not be read'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A remote CSR could not be read: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The current cell could not read a remote cells CSR. The remote cell number is displayed in the data field. These cells will not be able to rendezvous.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5361 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The current cell is too late to rendezvous with other cells'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The current cell is too late to rendezvous with other cells: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The currently executing cell arrived too late to rendezvous with the other cells described in the complex profile as cells it should rendezvous with.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5365 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The current cell detected incompatible CPUs on another cell'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The current cell detected incompatible CPUs on another cell: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The currently executing cell detected CPUs that are incompatible with it to be installed on a cell that the current cell is trying to rendezvous with.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5366 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Current cell was too slow creating the local rendezvous set'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Current cell was too slow creating the local rendezvous set: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The current cell was too slow creating the local rendezvous set and the other cells have left it behind. It will not be able to participate in the remainder of the rendezvous. The data field is unused, but the cell emitting this event is the'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='one too late to rendevous.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5376 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Reporting cell was not included in the global cell set'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Reporting cell was not included in the global cell set: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The reporting cell was not included in the final global set that was agreed upon. This means that another cell either could not reach the reporting cell or the reporting cell was too late ariving to a required state.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5380 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event No Core Cell can be selected in the PD.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event No Core Cell can be selected in the PD.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='No cells in the PD can be a core cell. This is fatal.'

