DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12208 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event fPars PMI handler was unable to Notify a CPU s new owner after a migrate.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event fPars PMI handler was unable to Notify a CPU s new owner after a migrate.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='FSHWA was unable to notify the new owner of a CPU migrate. This event is emitted 2 times: 1. Data field: IOSAPIC Address 2. Data field: Virtual IOSAPIC SCI redir'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12210 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The operating system set the watchdog timer to time out if it was not reset within a specified time. It was not reset and has timed out. The management processor will now take the action specified when the timer was set.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The operating system set the watchdog timer to time out if it was not reset within a specified time. It was not reset and has timed out. The management processor will now take the action specified when the timer was set.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The operating system set the watchdog timer to time out if it was not reset within a specified time. It was not reset and has timed out. The management processor will now take the action specified when the timer was set.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12217 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An OS is shutting down due to an MCA (Machine Check Abort) or INIT.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An OS is shutting down due to an MCA (Machine Check Abort) or INIT.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An OS is shutting down due to an MCA (Machine Check Abort) or INIT.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12218 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An OS is shutting down due to a panic.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An OS is shutting down due to a panic.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An OS is shutting down due to a panic.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 1222 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An instance of CLU FW has an installed firmware revision that is incompatible with the system type. Many system operations will fail until this condition is resolved.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An instance of CLU FW has an installed firmware revision that is incompatible with the system type. Many system operations will fail until this condition is resolved.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12227 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The online diagnostics have identified a hardware problem.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The online diagnostics have identified a hardware problem.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Diagnostics running under the OS have detected a problem with the identified hardware.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12228 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Over-Temperature or power condition detected for processor'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Over-Temperature or power condition detected for processor: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The processor temperature has exceeded normal limits. HP s Enhanced Thermal Management (ETM) feature has been employed to cool the processor. If the temperature problem persists, this will have an adverse impact on the performance of this'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='processor.   '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12229 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An error occurred while checking the fabricless boot state'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An error occurred while checking the fabricless boot state: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while checking the fabricless boot state'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12230 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event System firmware was unable to clear the link error masks'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event System firmware was unable to clear the link error masks: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System firmware was unable to clear the link error masks'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12231 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event System firmware could not determine a link s address'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event System firmware could not determine a link s address: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System firmware could not determine a link s address'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12232 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event System firmware was unable to turn a bad link off'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event System firmware was unable to turn a bad link off: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System firmware was unable to turn a bad link off'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12244 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The windows watchdog timer has expired. The partition associated with the cell with the expired timer will be reset.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The windows watchdog timer has expired. The partition associated with the cell with the expired timer will be reset.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Wiindows watchdog timer has expired. The nPartition will either be reset or powered off. The data field contains the following information: byte 2 - cell slot number of the cell that generated the timeout event byte 3 - nPartition number'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='(SX2000 superdome only) byte 4 - timeout action (0 = Reset, 1 = Power off) byte 7 - cabinet number   '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12251 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An entity s MP Bus communications controller is reporting a hardware revision that is known to cause MP Bus communications failures.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An entity s MP Bus communications controller is reporting a hardware revision that is known to cause MP Bus communications failures.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An MP Bus communications device is reporting a hardware revision that is known to cause MP Bus communications failures. The value in the data field indicates the physical location of the PM, CLU, or PDHC device that is failing.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12255 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event 12v power to a PCI slot located on the IO Chassis has power faulted.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event 12v power to a PCI slot located on the IO Chassis has power faulted.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Main power at the PCI slot located on the IO Chassis has faulted.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12289 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event SFW detected a failure while optimizing the fabric.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event SFW detected a failure while optimizing the fabric.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A failure was encountered while running the Fabric API to optimize the fabric.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12291 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A critical failure occured during a cell online add or delete.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A critical failure occured during a cell online add or delete.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A critical failure occured during a cell online add or delete call.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12296 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The cell being added has incompatible hardware or firmware revision with the partition.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The cell being added has incompatible hardware or firmware revision with the partition.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A cell being added is not compatible with the partition.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12297 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The System Firmware revision on the cell being added does not match the partition firmware revision.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The System Firmware revision on the cell being added does not match the partition firmware revision.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Firmware revision of the cell being added is different from the nPar.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12324 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Bad cell board (on cellular system), or bad processor board (on non-cellular system).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Bad cell board (on cellular system), or bad processor board (on non-cellular system).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Bad cell board (on cellular system), or bad processor board (on non-cellular system).'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12343 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU performance degraded due to excessive errors in third level cache'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU performance degraded due to excessive errors in third level cache: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='CPU performance degraded due to excessive errors in third level cache.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12352 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The alternate ROM failed to authenticate. The current (primary) ROM will continue to be used'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The alternate ROM failed to authenticate. The current (primary) ROM will continue to be used: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The alternate ROM failed to authenticate. The current (primary) ROM will continue to be used'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12354 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The alternate ROM was successfully authenticated but the primary and alternate ROM could not be swapped. The current primary will still be used.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The alternate ROM was successfully authenticated but the primary and alternate ROM could not be swapped. The current primary will still be used.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The alternate ROM was successfully authenticated but the primary and alternate ROM could not be swapped. The current primary will still be used'

