#* **************************************************************************
#*
#*                  Insight Integration for CA Unicenter
#*
#*      Copyright 1996,2006 Hewlett-Packard Development Company, L.P.
#*
#*      Hewlett-Packard Company shall not be liable for technical or
#*      editorial errors or omissions contained herein. The information in
#*      this document is provided "as is" without warranty of any kind and
#*      is subject to change without notice. The warranties for HP products
#*      are set forth in the express limited warranty statements
#*      accompanying such products. Nothing herein should be construed as
#*      constituting an additional warranty.
#*
#*      Confidential computer software. Valid license from HP required for
#*      possession, use or copying. Consistent with FAR 12.211 and 12.212,
#*      Commercial Computer Software, Computer Software Documentation, and
#*      Technical Data for Commercial Items are licensed to the U.S.
#*      Government under vendor's standard commercial license.
#*
#* **************************************************************************
#*                                                                        
#* PROPRIETARY NOTE:                                                      
#*     This document contains information confidential and proprietary to 
#*     Hewlett-Packard and shall not be reproduced or transferred to other
#*     documents or disclosed to others or used for any purpose other than 
#*     that for which it was obtained without the expressed written consent
#*     of Hewlett-Packard Company.
#*                                                                        
#* **************************************************************************

# Standard Equipment traps from version 7.40 to 7.60 of the management agents


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 1005*'
       MSGNODE=*
       DEScription='HP - CPU error threshold passed '
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - CPU error threshold passed '
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap is sent when an internal CPU error threshold has been passed on a particular CPU causing it to go degraded. This trap will be sent when cpqSeCpuThreshPassed transitions from false to true.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 1006*'
       MSGNODE=*
       DEScription='HP - Processor Status Change'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Processor Status Change'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 1006 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Processor Status Change: Unknown'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Processor Status Change: Unknown (Index: &26, Slot: &31, Name: &36, Speed: &41, Location: &66)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 1006 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Processor Status Change: OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Processor Status Change: OK (Index: &26, Slot: &31, Name: &36, Speed: &41, Location: &66)'
       SEVERITY=S
       ATTRIB=default
       COLOR=Green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 1006 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Processor Status Change: Degraded'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Processor Status Change: Degraded (Index: &26, Slot: &31, Name: &36, Speed: &41, Location: &66)'
       SEVERITY=W
       ATTRIB=default
       COLOR=Orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 1006 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Processor Status Change: Failed'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Processor Status Change: Failed (Index: &26, Slot: &31, Name: &36, Speed: &41, Location: &66)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 1006 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - Processor Status Change: Disabled'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Processor Status Change: Disabled (Index: &26, Slot: &31, Name: &36, Speed: &41, Location: &66)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red





DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 1007*'
       MSGNODE=*
       DEScription='HP - Processor Power Pod Status Change'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Processor Power Pod Status Change'
       SEVERITY=E
       ATTRIB=default
       COLOR=REd

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 1007 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Processor Power Pod Status Change: Not Failed'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Processor Power Pod Status Change: Not Failed (Index: &26, Slot: &31, Name: &36, Speed: &41, Location: &66)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 1007 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Processor Power Pod Status Change: Failed'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Processor Power Pod Status Change: Failed (Index: &26, Slot: &31, Name: &36, Speed: &41, Location: &66)'
       SEVERITY=E
       ATTRIB=default
       COLOR=RED

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 1008*'
       MSGNODE=*
       DEScription='HP - USB storage device attached (1008)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - USB storage device attached (1008)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='A USB storage device has been attached to the system.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 1009*'
       MSGNODE=*
       DEScription='HP - USB storage device removed (1009)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - USB storage device removed (1009)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='A USB storage device has been removed from the system.'
