DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5734 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event some processors not compatible'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event some processors not compatible: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Installed processors are not of compatible models or families'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5735 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event caches sizes are inconsistent'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event caches sizes are inconsistent: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Processors with different cache sizes are installed'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5737 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event selecting new monarch'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event selecting new monarch: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='SFW is selecting a new monarch processor due to compatibility problems.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5738 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event monarch not lowest stepping'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event monarch not lowest stepping: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The monarch stepping is not equal to the lowest installed CPU stepping.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5740 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event processors are over clocked'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event processors are over clocked: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CPU s FSB frequency is overclocked. Data: Local CPU Number.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5741 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event cpu access error on processor info area'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event cpu access error on processor info area: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='There was an error reading the info ROM area of the CPU. Data: Local CPU Number'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5742 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PAL A was not executed - HALT'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PAL A was not executed - HALT: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='PAL_A has not been executed and control has been transferred back to SAL_B.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5743 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PAL B was not executed - HALT'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PAL B was not executed - HALT: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='PAL_B has not been executed and control has been transferred back to SAL_B.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5744 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Prototype CPU installed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Prototype CPU installed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Data: Lower 32 bits have Local CPU Number'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5745 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event final boot rendezvous monarch watchdog timeout'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event final boot rendezvous monarch watchdog timeout: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Data: Monarch s Local CPU Number'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5746 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Supplemental cpu tests generated an unexpected result'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Supplemental cpu tests generated an unexpected result: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Supplemental tests have been run on the cpus in the node and an error was encountered. If this event id is only emmitted once, then the cpu detected that it failed on its own and the offending CPU id is in the data field. If the event is'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='emmitted three times, then the monarch CPU on the cell detected the error and the offending CPU id, expected data and actual data are reported in the data field of the three events.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5747 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A multi-bit error was found while reading a XBC CSR'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A multi-bit error was found while reading a XBC CSR: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='While reading a XBC CSR, a multi-bit error was found.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5749 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The return value from a function was an unknown value.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The return value from a function was an unknown value.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The return value from a function was an unknown value. Data field is the unknown status that was returned.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5750 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cannot get system ID status from BMC'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cannot get system ID status from BMC: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='EFI queries the BMC on the system board for the status of a system ID. The BMC could not complete the request successfully or on time. Data Field: Internal EFI function status.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5751 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cannot read a system ID'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cannot read a system ID: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='BMC reported a system ID status as inaccessible, reported invalid status or cannot return the current value of a system ID. Data Field: uuid status or internal EFI function status. System ID status: a 1 byte value 0 extended to 64bits: 0x00 ->'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='primary and secondary values are valid 0x01 -> primary and secondary values are magic 0x02 -> primary and secondary values are inaccessible 0x04 -> primary and secondary values are invalid 0x08 -> primary and secondary values are null (UUID  '
DEFine MSGACTion Name=(*,40)
ACTION=ANNOTATE TEXT='only) 0x10 -> primary and secondary values are different, value (primary or secondary) is valid 0x11 -> primary and secondary values are different, value (primary or secondary) is magic 0x12 -> primary and secondary values are different, value  '
DEFine MSGACTion Name=(*,50)
ACTION=ANNOTATE TEXT='(primary or secondary) is inaccessible 0x14 -> primary and secondary values are different, value (primary or secondary) is invalid 0x18 -> primary and secondary values are different, value (primary or secondary) is null (UUID only)" '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5752 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to write new system ID. BMC reported an error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to write new system ID. BMC reported an error: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware tried to write a primary or secondary system ID as requested by the user during the boot sequence. The write failed. Data Field: Internal EFI function status.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5753 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The system ID(s) currently in the system is invalid'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The system ID(s) currently in the system is invalid: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The system ID(s) currently in the system is either invalid or, if the EFI_SYSID_BMC_WARNING, EFI_SYSID_BMC_READ_ERROR or EFI_SYSID_BMC_WRITE_ERROR events are also present, inaccessible to the system firmware. A stop boot condition will be'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='generated and software license will probably be invalid. Data Field: 64-bit value. If preceded by 0xbad00000000000 the following valid values are possible: 0000 -> valid UUID (should never see this one) 0001 -> magic UUID 0002 -> inaccessible  '
DEFine MSGACTion Name=(*,40)
ACTION=ANNOTATE TEXT='UUID 0004 -> invalid (bad CRC) UUID If zero, then one of the following conditions occurred: Invalid combination of primary and secondary system ID values User declined copying/entering system ID values when prompted by firmware All other values  '
DEFine MSGACTion Name=(*,50)
ACTION=ANNOTATE TEXT='indicate failure during attempt to update system IDs." '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5755 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event EFI unable to find the SAL services for installing interrupt handlers'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event EFI unable to find the SAL services for installing interrupt handlers: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='EFI is unable to find the SAL services for installing interrupt handlers. EFI was trying to install the run-time handlers that are required for normal EFI booting. EFI will be halting. Data Field: internal EFI function status.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5756 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event EFI unable to find the SAL service to install run-time interrupt handlers'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event EFI unable to find the SAL service to install run-time interrupt handlers: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='EFI is unable to find the SAL service to install run-time interrupt handlers. These handlers are required for normal EFI booting. EFI will be halting. Data Field: internal EFI function status.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5757 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event EFI unable to find the SAL services for installing interrupt handlers'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event EFI unable to find the SAL services for installing interrupt handlers: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT=' EFI is unable to find the SAL services for installing interrupt handlers. EFI was trying to install the boot-time handlers that are required for normal EFI booting. EFI will be halting. Data Field: internal EFI function status.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5758 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event EFI unable to find the SAL service to install boot-time interrupt handlers'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event EFI unable to find the SAL service to install boot-time interrupt handlers: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='EFI is unable to find the SAL service to install boot-time interrupt handlers. These handlers are required for normal EFI booting. EFI will be halting. Data Field: internal EFI function status.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5760 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Too many parameters were passed to the utilities system'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Too many parameters were passed to the utilities system: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Too many parameters were passed in a request for the utilities system to perform an operation. No more data is provided.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5762 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A crossbar port is unexpectedly not present.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A crossbar port is unexpectedly not present.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A crossbar port is expected to be present, but its presence detect bit is not set. Data field bits 32:43 contain the crossbar ID, bits 44:55 contain the port number for which the error occurred, and bits 0:31 contain the port status'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='information.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5763 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A crossbar port unexpectedly has its HW_LINK_OK bit not set.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A crossbar port unexpectedly has its HW_LINK_OK bit not set.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A crossbar port is expected to have its HW_LINK_OK bit set, but it is not. Data field bits 32:43 contain the crossbar ID, bits 44:55 contain the port number for which the error occurred, and bits 0:31 contain the port status information.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5764 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A connected port was found to be in FE'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A connected port was found to be in FE: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A connected crossbar port was found to have its FE bit set. Data field bits 32:43 contain the crossbar ID, bits 44:55 contain the port number for which the error occurred, and bits 0:31 contain the port status information.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5766 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event There was an error while initializing the Concorde-Xbc interface.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event There was an error while initializing the Concorde-Xbc interface.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='There was an error while initializing the Cell Controller-Xbc interface. The data field contains the address of the Cell Controller CSR for which the error occurred.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5767 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The CC - XBC link failed to initialize.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The CC - XBC link failed to initialize.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The CC - XBC link failed to initialize.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5768 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unable to determine system mode because EFI/SAL interface not initialized'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unable to determine system mode because EFI/SAL interface not initialized: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='EFI is unable to determine current system mode. The EFI/SAL interface is not initialized. This interface should have been initialized before now. This event indicates an internal EFI error. EFI will continue executing.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5769 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event BMC returned an invalid system mode'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event BMC returned an invalid system mode: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The BMC has returned an invalid system mode. Data Field: the invalid mode. Expected values are 0 or 1.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5770 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event EFI unable to specify system mode because EFI/SAL interface not initialized'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event EFI unable to specify system mode because EFI/SAL interface not initialized: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='EFI is unable to specify a new system mode. The EFI/SAL interface point is not initialized. This interface should have been initialized before now. This event indicates an internal EFI error. EFI will continue executing in the current mode.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5771 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unable to enter normal system mode because EFI/SAL interface not initialized'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unable to enter normal system mode because EFI/SAL interface not initialized: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='EFI is unable to enter normal system mode. The EFI/SAL interface is not initialized. This interface should have been initialized before now. This event indicates an internal EFI error. EFI will continue executing in the current mode.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5772 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unable to initialize part of the SAL/EFI interface'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unable to initialize part of the SAL/EFI interface: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='EFI is unable to initialize part of the SAL/EFI interface. This crucial service provides access to certain BMC functionality such as the security system. EFI will halt. Data Field: Return status from internal EFI function.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5774 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An expected tree node was not found'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An expected tree node was not found: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A needed tree node was not found. The data field contains the ascii name of the tree node that was not found.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5776 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event EFI unable to modify system state to  running '
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event EFI unable to modify system state to  running : &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='EFI is unable to modify the system state from  booting  to  running . This is done as part of Exit Boot Services. The system will not be able to enter a sleep mode. Data Field: For errors, this data is zero. For warnings, this data indicates'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='the current system state as: 0 Error 1 booting 2 running 3 attention 4 fault 5 booting + attention  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5777 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event /options settings for CPUBusConfigValue aren t compatible with PAL'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event /options settings for CPUBusConfigValue aren t compatible with PAL: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='CPUBusConfigValue setting in options as been compared with what is reported by PAL as settable and CPUBusConfigValue is specifying at least one bit that is not supported by this version of PAL using the Get Processor Bus Dependent'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='Configuration Features. This chassis code is emmitted in pairs, the first data field contains the PAL expected values; the second data field contains the requested setting from options.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5778 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The Get Processor Bus Dependent Configuration Features PAL call failed.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The Get Processor Bus Dependent Configuration Features PAL call failed.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware was unable to correctly issue the Get Processor Bus Dependent Configuration Features command.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5779 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event memory DIMM pair mismatch'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event memory DIMM pair mismatch: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A pair of DIMMs installed in the system are mismatched, and that pair of DIMMs will not be used. The data field indicates which pair of DIMMs are mismatched in the format 0x000000000000XBXA where X is the number of the rank that is'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='mismatched.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5784 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event EFI unable to initialize internal library'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event EFI unable to initialize internal library: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='EFI is unable to initialize internal library. This collection of internal services is required for much of EFI s functionality. EFI is halting.'

