DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11783 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error reading or writing the stable store NVM area'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error reading or writing the stable store NVM area: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error reading or writing the stable store NVM area'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11784 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event FW has detected an illegal memory config using 4GB DIMMs. The system will be halted.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event FW has detected an illegal memory config using 4GB DIMMs. The system will be halted.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='SFW has detected an illegal memory config using 4GB DIMMs. The system will be halted'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11788 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event SFW failed to allocate enough NVM to store all required data.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event SFW failed to allocate enough NVM to store all required data.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='SFW component NVM space is not big enough to store all it data. Check the ASCII data field to determine which component caused the error.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11789 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event SFW failed to allocate enough SCR RAM to store all required data.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event SFW failed to allocate enough SCR RAM to store all required data.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='SFW component does not allocate enough SCR ram space to store it data.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11797 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event SetupIntialCohTables() returned an error in ArfPhase3. Data field: cell set [63:32], return value [31:0]'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event SetupIntialCohTables() returned an error in ArfPhase3. Data field: cell set [63:32], return value [31:0]: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Data field: cell set [63:32], return value [31:0]'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11807 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error writing the error masks for ALREC and ALTRAN. Data field: cell ID [63:56], port num [55:44], XBC ID [43:32]'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error writing the error masks for ALREC and ALTRAN. Data field: cell ID [63:56], port num [55:44], XBC ID [43:32]: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Data field: cell ID [63:56], port num [55:44], XBC ID [43:32]'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11840 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Firmware had an unexpected internal error from the vertex module.. Data field: vType1 [63:56] | vPort1 [55:48] | vId1 [47:32] | vType2 [31:24] | vPort2 [23:16] | vId2 [15:0]'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Firmware had an unexpected internal error from the vertex module.. Data field: vType1 [63:56] | vPort1 [55:48] | vId1 [47:32] | vType2 [31:24] | vPort2 [23:16] | vId2 [15:0]: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Data field: vType1 [63:56] | vPort1 [55:48] | vId1 [47:32] | vType2 [31:24] | vPort2 [23:16] | vId2 [15:0]'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11850 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The OS being booted is not supported in a partition containing a mix of processor stepping revisions.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The OS being booted is not supported in a partition containing a mix of processor stepping revisions.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The OS being booted is not supported in a partition containing a mix of processor stepping revisions.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11851 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Firmware had an unexpected error while setting up links. Data field: vType1 [63:56] | vPort1 [55:48] | vId1 [47:32] | vType2 [31:24] | vPort2 [23:16] | vId2 [15:0]'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Firmware had an unexpected error while setting up links. Data field: vType1 [63:56] | vPort1 [55:48] | vId1 [47:32] | vType2 [31:24] | vPort2 [23:16] | vId2 [15:0]: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Data field: vType1 [63:56] | vPort1 [55:48] | vId1 [47:32] | vType2 [31:24] | vPort2 [23:16] | vId2 [15:0]'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11863 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Firmware was unable to write the Skyline global LINK_SEL_COHx CSR. Data field: cell num [63:56] | link sel coh CSR (0 or 1) [0:0]'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Firmware was unable to write the Skyline global LINK_SEL_COHx CSR. Data field: cell num [63:56] | link sel coh CSR (0 or 1) [0:0]: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Data field: cell num [63:56] | link sel coh CSR (0 or 1) [0:0]'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11870 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The requested OS does not support booting with mixed CPU revisions'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The requested OS does not support booting with mixed CPU revisions: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The OS suitable for booting in this mode does not support booting in the current configuration due to the existence of cpus of differing revisions.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11885 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event System firmware experienced an error while updating the link sel value. Data field indicates return status.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event System firmware experienced an error while updating the link sel value. Data field indicates return status.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System firmware experienced an error while updating the link sel value. Data field indicates return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11904 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Fabric was unable to generate a Skyline CSR address. Data field: cell number [63:56] and return value from address function [31:0].'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Fabric was unable to generate a Skyline CSR address. Data field: cell number [63:56] and return value from address function [31:0].: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Fabric was unable to generate a Skyline CSR address Data field: cell number [63:56] and return value from address function [31:0]'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11905 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Firmware was unable to generate a Skyline CSR address. Data field: cell number [63:56] | return value [31:0].'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Firmware was unable to generate a Skyline CSR address. Data field: cell number [63:56] | return value [31:0].: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware was unable to generate a Skyline CSR address. Data field: cell number [63:56] | return value [31:0]'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11932 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Invalid or no OS boot rendezvous entry point for target CPU'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Invalid or no OS boot rendezvous entry point for target CPU: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Target CPU receives wakeup interrupt to join the OS but the OS_BOOT_RENDEZ entry point is invalid or none-existent'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11933 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Checksum verification failed for OS_BOOT_RENDEZ entry point'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Checksum verification failed for OS_BOOT_RENDEZ entry point: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The entry point for OS_BOOT_RENDEZ exists, but fails the checksum test performed by firmware'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11960 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The System Firmware call to PAL_COPY_INFO failed.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The System Firmware call to PAL_COPY_INFO failed.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The System Firmware call to PAL_COPY_INFO failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11961 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The System Firmware call to PAL_COPY_PAL failed.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The System Firmware call to PAL_COPY_PAL failed.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The System Firmware call to PAL_COPY_PAL failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11962 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The System Firmware call to PAL_CACHE_FLUSH failed.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The System Firmware call to PAL_CACHE_FLUSH failed.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The System Firmware call to PAL_CACHE_FLUSH failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11964 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cell on line add/delete is not initialized'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cell on line add/delete is not initialized: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Cell on line add/delete is not initialized and cannot be used.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11966 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An FPARs component on which cell on-line add/delete depends is broken or missing.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An FPARs component on which cell on-line add/delete depends is broken or missing.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='In FPARs mode, cell on line add/delete depends on functionality in the FPARs component. This is either broken or missing.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11967 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cell on-line add/delete in FPARs mode failed to get the FPARs semaphore.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cell on-line add/delete in FPARs mode failed to get the FPARs semaphore.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Cell on line add/delete in FPARs mode failed to get the FPARs semaphore.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11968 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event More than one processor from an FPAR called into cell on-line add/delete'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event More than one processor from an FPAR called into cell on-line add/delete: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='More than one processor from an FPAR called into cell on line add/delete'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11969 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event All FPARs processors failed to rendezvous during a cell on line add/delete operation'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event All FPARs processors failed to rendezvous during a cell on line add/delete operation: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='All FPARs processors failed to rendezvous during a cell on line add/delete op'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11970 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Encountered unexpected error during cell OLA activity.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Encountered unexpected error during cell OLA activity.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Unable to setup Skyline LINK_SEL_COHx CSRs on the running partition to the newly added cell. Data field: cell set [63:32] | return val [31:0]'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11971 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event MCA occurred prior to completion of previous MCA.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event MCA occurred prior to completion of previous MCA.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This indicates an MCA happening before a previous MCA was not completely handled.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11972 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event MCA during init event processing'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event MCA during init event processing: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This indicates an MCA event happening before a previous INIT event was not completely processed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11974 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event unable to find a bad edge in an untraversable route'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event unable to find a bad edge in an untraversable route: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware was unable to find a bad edge in an untraversable route. Data Field: (destCell << 56 | port num < 44 | xbc num << 32 | return status)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 11989 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unknown entity drawing power from bus bars.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unknown entity drawing power from bus bars.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Some entity that is not known to the firmware, is drawing power from the bus bars.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12001 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Soft partition could not be booted, reverting to nPars.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Soft partition could not be booted, reverting to nPars.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Rebooting the partition to nPars because a soft partition could not be booted.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12008 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unable to route around broken link.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unable to route around broken link.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware was unable to find a replacement route for the broken link. Data field contains: port << 44, chip id << 32, and number of attempts to find an alternate route'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12013 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unable to set the APER  fabric lockdown  bit'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unable to set the APER  fabric lockdown  bit: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Data field details the cell that failed to set its bit'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12017 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An uncorrectable memory ECC error has occurred. The data field gives the physical location of the DIMM that had the error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An uncorrectable memory ECC error has occurred. The data field gives the physical location of the DIMM that had the error: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Indicates that an uncorrectable ECC error has been encountered, and gives the physical location of the DIMM that had the error.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12025 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An error encountered while retrieving the expected neighbor fabric chip for distributing traffic over crossbar links.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An error encountered while retrieving the expected neighbor fabric chip for distributing traffic over crossbar links.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System firmware experienced an error while retrieving the expected neighbor fabric chip for distributing traffic over crossbarl inks. Data Field: (xbc port # << 44) | (xbc # << 32) | return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12028 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Could not read crossbar neighbor information during routing.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Could not read crossbar neighbor information during routing.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Could not read crossbar neighbor information during routing. Data Field: (xbc port << 44) | (xbc << 32) | error status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12029 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Could not establish route for local crossbar during route around routing.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Could not establish route for local crossbar during route around routing.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Could not establish route for local crossbar during route around routing. Data Field: (xbc port << 44) | (xbc << 32) | error status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12047 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Could not establish route for local crossbar during route around routin'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Could not establish route for local crossbar during route around routin: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An invalid TPM has been detected in the system and is being use. Security might be compromised. Data field unused.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12048 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Invalid or unsupported TPM detected in the system. TPM is disabled.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Invalid or unsupported TPM detected in the system. TPM is disabled.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Invalid or unsupported TPM detected in the system. TPM is disabled. Data filed unused'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12049 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event TPM failed initialization. Security features disabled.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event TPM failed initialization. Security features disabled.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware cannot initialize the TPM. TPM related security feature are disabled Data field unused'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12050 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A CPU module s temperature has exceed the high temperature threshold or a CPU power module fault has occured. As a result of this event, the CPU has been inhibited.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A CPU module s temperature has exceed the high temperature threshold or a CPU power module fault has occured. As a result of this event, the CPU has been inhibited: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CPU module s temperature has exceed the high temperature threshold or a CPU power module fault has occured. As a result of this event, the CPU has been inhibited. The Cell must be powered off then on using the MP s PE command before the CPU'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='module will be powered again.  '

