--MibName=cpqStdEquipment
-- ****************************************************************************
--
--                 Standard PC equipment configuration
--         Management Information Base for SNMP Network Management
--
--
--      Copyright 1992,2003 Hewlett-Packard Development Company, L.P.
--
--      Hewlett-Packard Company shall not be liable for technical or
--      editorial errors or omissions contained herein. The information in
--      this document is provided "as is" without warranty of any kind and
--      is subject to change without notice. The warranties for HP products
--      are set forth in the express limited warranty statements
--      accompanying such products. Nothing herein should be construed as
--      constituting an additional warranty.
--
--      Confidential computer software. Valid license from HP required for
--      possession, use or copying. Consistent with FAR 12.211 and 12.212,
--      Commercial Computer Software, Computer Software Documentation, and
--      Technical Data for Commercial Items are licensed to the U.S.
--      Government under vendor's standard commercial license.
--
--      Refer to the READMIB.RDM file for more information about the
--      organization of the information in the Compaq Enterprise.
--
--      The Compaq Enterprise number is 232.
--      The ASN.1 prefix to, and including the Compaq Enterprise is:
--           1.3.6.1.4.1.232
--
-- ****************************************************************************

CPQSTDEQ-MIB DEFINITIONS ::= BEGIN

    IMPORTS
        compaq                  FROM CPQHOST-MIB
        enterprises             FROM RFC1155-SMI
        DisplayString           FROM RFC1213-MIB
        OBJECT-TYPE             FROM RFC-1212
        TRAP-TYPE               FROM RFC-1215
        sysName                 FROM RFC1213-MIB
        cpqHoTrapFlags          FROM CPQHOST-MIB;


  compaq                   OBJECT IDENTIFIER ::= { enterprises 232 }
    cpqStdEquipment          OBJECT IDENTIFIER ::= { compaq 1 }
    cpqSeMibRev              OBJECT IDENTIFIER ::= { cpqStdEquipment 1 }
    cpqSeComponent           OBJECT IDENTIFIER ::= { cpqStdEquipment 2 }

    cpqSeInterface           OBJECT IDENTIFIER ::= { cpqSeComponent 1 }
    cpqSeProcessor           OBJECT IDENTIFIER ::= { cpqSeComponent 2 }
    cpqSeMemory              OBJECT IDENTIFIER ::= { cpqSeComponent 3 }
    cpqSeIsaCmos             OBJECT IDENTIFIER ::= { cpqSeComponent 4 }
    cpqSeEisaNvram           OBJECT IDENTIFIER ::= { cpqSeComponent 5 }
    cpqSeRom                 OBJECT IDENTIFIER ::= { cpqSeComponent 6 }
    cpqSeKeyboard            OBJECT IDENTIFIER ::= { cpqSeComponent 7 }
    cpqSeVideo               OBJECT IDENTIFIER ::= { cpqSeComponent 8 }
    cpqSeSerialPort          OBJECT IDENTIFIER ::= { cpqSeComponent 9 }
    cpqSeParallelPort        OBJECT IDENTIFIER ::= { cpqSeComponent 10 }
    cpqSeFloppyDisk          OBJECT IDENTIFIER ::= { cpqSeComponent 11 }
    cpqSeFixedDisk           OBJECT IDENTIFIER ::= { cpqSeComponent 12 }
    cpqSePci                 OBJECT IDENTIFIER ::= { cpqSeComponent 13 }
    cpqSePCCard              OBJECT IDENTIFIER ::= { cpqSeComponent 14 }
    cpqSeUSBPort             OBJECT IDENTIFIER ::= { cpqSeComponent 15 }
    cpqSeCell                OBJECT IDENTIFIER ::= { cpqSeComponent 16 }
    cpqSeIOC                 OBJECT IDENTIFIER ::= { cpqSeComponent 17 }
    cpqSePartition           OBJECT IDENTIFIER ::= { cpqSeComponent 18 }
    cpqSeCabinet             OBJECT IDENTIFIER ::= { cpqSeComponent 19 }
    cpqSeComplex             OBJECT IDENTIFIER ::= { cpqSeComponent 20 }
    cpqSeLED                 OBJECT IDENTIFIER ::= { cpqSeComponent 21 }
    cpqSeUSBDevice           OBJECT IDENTIFIER ::= { cpqSeComponent 22 }

    cpqSeOsCommon            OBJECT IDENTIFIER ::= { cpqSeInterface 4 }

    TruthValue ::= INTEGER {
       false(1),
       true(2)
    }

-- ****************************************************************************
--   Standard Equipment MIB Revision
--   ===============================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeMibRev Group             (1.3.6.1.4.1.232.1.1)
--
--      Implementation of the cpqSeMibRev group is mandatory for all agents
--      supporting the Standard Equipment MIB.
--
--      An Insight Agent conforming to this document will return a
--      cpqSeMibRevMajor of one (1) and a cpqSeMibRevMinor of twenty (20).
--
-- ****************************************************************************

    cpqSeMibRevMajor OBJECT-TYPE
        SYNTAX  INTEGER (1..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The Major Revision level of the MIB.

            A change in the major revision level represents a major change
            in the architecture of the MIB.  A change in the major revision
            level may indicate a significant change in the information
            supported and/or the meaning of the supported information,
            correct interpretation of data may require a MIB document with
            the same major revision level."
        ::= { cpqSeMibRev 1 }

    cpqSeMibRevMinor OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The Minor Revision level of the MIB.

            A change in the minor revision level may represent some minor
            additional support, no changes to any pre-existing information
            has occurred."
        ::= { cpqSeMibRev 2 }

    cpqSeMibCondition OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            ok(2),
            degraded(3),
            failed(4)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The overall condition.

            This object represents the overall status of the server
            represented by this MIB."
        ::= { cpqSeMibRev 3 }

-- ****************************************************************************
--   Standard Equipment OS Common Group
--   ==================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--        cpqSeInterface Group         (1.3.6.1.4.1.232.1.2.1)
--         cpqSeOsCommon Group         (1.3.6.1.4.1.232.1.2.1.4)
--
--  Implementation of the cpqSeOsCommon group is mandatory for all
--  agents that support the Standard Equipment MIB.
--
-- ****************************************************************************

    cpqSeOsCommonPollFreq OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "The Insight Agent's polling frequency.

            The frequency, in seconds, at which the Insight Agent requests
            information from the device driver.  A frequency of zero (0)
            indicates that the Insight Agent retrieves the information upon
            request of a management station, it does not poll the device
            driver at a specific interval.

            If the poll frequency is zero (0) all attempts to write to this
            object will fail.  If the poll frequency is non-zero,
            setting this value will change the polling frequency of the
            Insight Agent.  Setting the poll frequency to zero (0) will
            always fail, an agent may also choose to fail any request to
            change the poll frequency to a value that would severely impact
            system performance."
        ::= { cpqSeOsCommon 1 }

-- ****************************************************************************
--   Standard Equipment OS Common Module Table
--   =========================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--        cpqSeInterface Group         (1.3.6.1.4.1.232.1.2.1)
--         cpqSeOsCommon Group         (1.3.6.1.4.1.232.1.2.1.4)
--          cpqSeOsCommonModuleTable   (1.3.6.1.4.1.232.1.2.1.4.2) deprecated
--
-- ***************************************************************************

    cpqSeOsCommonModuleTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSeOsCommonModuleEntry
        ACCESS  not-accessible
        STATUS  deprecated
        DESCRIPTION
            "A table of software modules that provide an interface to the
            device this MIB describes."
        ::= { cpqSeOsCommon 2 } 

    cpqSeOsCommonModuleEntry OBJECT-TYPE
        SYNTAX  CpqSeOsCommonModuleEntry
        ACCESS  not-accessible
        STATUS  deprecated
        DESCRIPTION
            "A description of a software module that provides an interface
            to the device this MIB describes."
        INDEX   { cpqSeOsCommonModuleIndex }
        ::= { cpqSeOsCommonModuleTable 1 }

        CpqSeOsCommonModuleEntry ::= SEQUENCE {
            cpqSeOsCommonModuleIndex       INTEGER,
            cpqSeOsCommonModuleName        DisplayString,
            cpqSeOsCommonModuleVersion     DisplayString,
            cpqSeOsCommonModuleDate        OCTET STRING,
            cpqSeOsCommonModulePurpose     DisplayString
        }

    cpqSeOsCommonModuleIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "A unique index for this module description."
        ::= { cpqSeOsCommonModuleEntry 1 }

    cpqSeOsCommonModuleName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The module name."
        ::= { cpqSeOsCommonModuleEntry 2 }

    cpqSeOsCommonModuleVersion OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..5))
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The module version in XX.YY format.

            Where XX is the major version number and YY is the minor version
            number.  This field will be a null (size 0) string if the agent
            cannot provide the module version."
        ::= { cpqSeOsCommonModuleEntry 3 }

    cpqSeOsCommonModuleDate OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (7))
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The module date.

             field  octets  contents                  range
             =====  ======  =======                  =====
               1      1-2   year                      0..65536
               2       3    month                     1..12
               3       4    day                       1..31
               4       5    hour                      0..23
               5       6    minute                    0..59
               6       7    second                    0..60
                            (use 60 for leap-second)


            This field will be set to year = 0 if the agent cannot provide
            the module date.  The hour, minute, and second field will be set
            to zero (0) if they are not relevant.  The year field is set
        with the most significant octet first."
        ::= { cpqSeOsCommonModuleEntry 4 }

    cpqSeOsCommonModulePurpose OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The purpose of the module described in this entry."
        ::= { cpqSeOsCommonModuleEntry 5 }

-- ****************************************************************************
--   Standard Equipment Processor Group
--   ==================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--        cpqSeProcessor Group         (1.3.6.1.4.1.232.1.2.2)
--         cpqSeCpuTable               (1.3.6.1.4.1.232.1.2.2.1)
--         cpqSeFpuTable               (1.3.6.1.4.1.232.1.2.2.2)
--
--      The cpqSeProcessor group describes the CPUs (central processor
--      units) and FPUs (floating point coprocessor units) in the system.
--
--      A CPU is a chip that performs general purpose processing.  A CPU may
--      be used with or without an FPU.
--
--      A FPU is a chip that performs special purpose processing, an FPU is
--      used by a CPU to handle special computations.  A FPU is always used
--      with a CPU.
--
--      The cpqSeProcessor group contains two tables, the cpqSeCpu table
--      and the cpqSeFpu table.  The cpqSeCpu table has an entry for
--      each CPU in the system.  The cpqSeFpu table has an entry for each
--      FPU in the system.  The two tables are indexed in a way that enables
--      an application to determine the relationship between CPUs and FPUs.
--      Each CPU and FPU entry provides identification, description, and
--      speed information.
--
--
-- ****************************************************************************



    cpqSeCpuTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSeCpuEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A list of the CPUs (processors) in the system.
            
            The main processor (if such a concept is valid for this machine)
            should be the first entry in the table."
        ::= { cpqSeProcessor 1 }

    cpqSeCpuEntry OBJECT-TYPE
        SYNTAX  CpqSeCpuEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A description of a CPU (processor) in the system."
        INDEX   { cpqSeCpuUnitIndex }
        ::= { cpqSeCpuTable 1 }

    CpqSeCpuEntry ::= SEQUENCE {
        cpqSeCpuUnitIndex              INTEGER,
        cpqSeCpuSlot                   INTEGER,
        cpqSeCpuName                   DisplayString,
        cpqSeCpuSpeed                  INTEGER,
        cpqSeCpuStep                   INTEGER,
        cpqSeCpuStatus                 INTEGER,
        cpqSeCpuExtSpeed               INTEGER,
        cpqSeCpuDesigner               INTEGER,
        cpqSeCpuSocketNumber           INTEGER,
        cpqSeCpuThreshPassed           INTEGER,
        cpqSeCpuHwLocation             DisplayString,
        cpqSeCpuCellTablePtr           INTEGER,
        cpqSeCpuPowerpodStatus         INTEGER,
        cpqSeCpuArchitectureRevision   DisplayString,
        cpqSeCpuCore                   INTEGER,
        cpqSeCPUSerialNumber           DisplayString,
        cpqSeCPUPartNumber             DisplayString,
        cpqSeCPUSerialNumberMfgr       DisplayString,
        cpqSeCPUPartNumberMfgr         DisplayString,
        cpqSeCPUCoreIndex              INTEGER,
        cpqSeCPUMaxSpeed               INTEGER,
        cpqSeCPUCoreThreadIndex        INTEGER,
        cpqSeCPUChipGenerationName     DisplayString,
        cpqSeCPUMultiThreadStatus      INTEGER,
        cpqSeCPUCoreMaxThreads         INTEGER,
        cpqSeCpuLowPowerStatus         INTEGER,
        cpqSeCpuPrimary                INTEGER
    }

    cpqSeCpuUnitIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This is a number that uniquely specifies a logical processor 
            unit. A logical processing unit may be a set of processing chips 
            that are on the same board or for other reasons work together as 
            a unit. For multithreaded processors each thread is considered as 
            a logical processing unit.
            The main processor unit (if such a concept is valid for this
            machine) will always have the lowest (first) index."
        ::= { cpqSeCpuEntry 1 }

    cpqSeCpuSlot OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This value represents this processor's slot.
            If the slot cannot be determined the value of zero (0) will be
            returned."
        ::= { cpqSeCpuEntry 2 }

    cpqSeCpuName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The name of this processor.
            For example:
                80386"
        ::= { cpqSeCpuEntry 3 }

    cpqSeCpuSpeed OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This is the internal speed in megahertz of this processor.
            Zero will be returned if this value is not available."
        ::= { cpqSeCpuEntry 4 }

    cpqSeCpuStep OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This step of the processor.
            This will be zero (0) if the step cannot be determined."
        ::= { cpqSeCpuEntry 5 }

    cpqSeCpuStatus OBJECT-TYPE
        SYNTAX  INTEGER {
            unknown(1),
            ok(2),
            degraded(3),
            failed(4),
            disabled(5)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The status of the processor.

            The following values are valid for CPU status:
 
            Unknown (1)
              The status of the CPU could not be determined.

            OK (2)
              The CPU is functioning normally.

            Degraded (3)
              The CPU is in a pre-failure warrantee state.

            Failed (4)
              The CPU is in a failed state.

            Disabled (5)
              The CPU has been disabled during power-on-self-test."

        ::= { cpqSeCpuEntry 6 }

    cpqSeCpuExtSpeed OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This is the external frequency in megahertz of the processor bus.
             Zero will be returned if this value is not available."
        ::= { cpqSeCpuEntry 7 }

    cpqSeCpuDesigner OBJECT-TYPE
        SYNTAX  INTEGER {
            unknown(1),
            intel(2),
            amd(3),
            cyrix(4),
            ti(5),
            nexgen(6),
            compaq(7),
            samsung(8),
            mitsubishi(9),
            mips(10)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This attribute specifies the manufacturer which designs
             this CPU."
        ::= { cpqSeCpuEntry 8 }

    cpqSeCpuSocketNumber OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The physical socket number of the CPU chip.  This number
             helps to identify CPUs on processor boards that contain
             multiple CPU chips. In most cases the CPU Socket number
             should be specified on the board silkscreen or in product
             documentation."
        ::= { cpqSeCpuEntry 9 }

    cpqSeCpuThreshPassed OBJECT-TYPE
        SYNTAX  INTEGER
        {
            unsupported(1),
            false(2),
            true(3)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "CPU threshold passed (Exceeded). When this attribute is set
             to true, it identifies a pre-failure error condition. Processors
             like the Intel Pentium Pro have the capability built into them
             to correct internal error conditions.  Excessive corrected internal
             errors can predict future hard processor failures.  Agent
             instrumentation will set this attribute to true if an internal
             processor error threshold is passed.  It is recommended that the
             user replace the CPU in this case. If the processor does not
             support monitoring internal corrected errors, this value will
             be set to unsupported. "
        ::= { cpqSeCpuEntry 10 }

    cpqSeCpuHwLocation  OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "A text description of the hardware location, on complex
             multi SBB hardware only, for the CPU.
             A NULL string indicates that the hardware location could not
             be determined or is irrelevant."
        ::= { cpqSeCpuEntry 11 }

    cpqSeCpuCellTablePtr OBJECT-TYPE
        SYNTAX  INTEGER (0..15)
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This is the index for the cell in cpqSeCellTable where this CPU is physically located."
        ::= { cpqSeCpuEntry 12 }

    cpqSeCpuPowerpodStatus OBJECT-TYPE
        SYNTAX  INTEGER
        {
            notfailed(1),
            failed(2)
        }
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This is the status of CPU power pod. Potential values in the future could be present/not present."
        ::= { cpqSeCpuEntry 13 }

    cpqSeCpuArchitectureRevision OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This is the CPU architecture revision."
        ::= { cpqSeCpuEntry 14 }

    cpqSeCpuCore OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "The number of cores in this CPU module. Zero will be returned if can not be determined."
        ::= { cpqSeCpuEntry 15 }

    cpqSeCPUSerialNumber OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "The OEM serial number of the CPU."
        ::= { cpqSeCpuEntry 16 }

    cpqSeCPUPartNumber OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "The OEM part number of the CPU."
        ::= { cpqSeCpuEntry 17 }

    cpqSeCPUSerialNumberMfgr OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "The manufacturer serial number of the CPU."
        ::= { cpqSeCpuEntry 18 }

    cpqSeCPUPartNumberMfgr OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "The manufacturer part number of the CPU."
        ::= { cpqSeCpuEntry 19 }

    cpqSeCPUCoreIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This is a number that uniquely identifies a core in a CPU unit."
        ::= { cpqSeCpuEntry 20 }

    cpqSeCPUMaxSpeed OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This is the maximum internal speed in megahertz this processor can support.
            Zero will be returned if this value is not available."
        ::= { cpqSeCpuEntry 21 }

    cpqSeCPUCoreThreadIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This is an unique number to identify the running threads in a CPU core."
        ::= { cpqSeCpuEntry 22 }

    cpqSeCPUChipGenerationName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "CPU chip generation name e.g. Hondo, Montecito, Madison, Opteron."       
        ::= { cpqSeCpuEntry 23 }

    cpqSeCPUMultiThreadStatus OBJECT-TYPE
        SYNTAX  INTEGER {
            unknown(1),
            enabled(2),
            disabled(3)
            }
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This OID identifies whether the CPU threading is enabled or not."
        ::= { cpqSeCpuEntry 24 }

    cpqSeCPUCoreMaxThreads OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This OID indicates the maximum number of threads that a cpu core is capable of."
        ::= { cpqSeCpuEntry 25 }

    cpqSeCpuLowPowerStatus OBJECT-TYPE
        SYNTAX  INTEGER {
            unknown (1),
            lowpowered (2),
            normalpowered (3)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Servers like Itanium has capability to lower power supply
             to CPU if it is idle for specified period of time.

            The following values are valid for CPU Low Powered state:

            Unknown (1)
                The Low Powered status could not be determined.

            Low Powered (2)
                The CPU is Low Power state.

            Normal Powered (3)
                The CPU is normal Power state."

        ::= { cpqSeCpuEntry 26 }

    cpqSeCpuPrimary OBJECT-TYPE
        SYNTAX  INTEGER {
            unknown(1),
            false(2),
            true (3)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "On SMP systems one of the CPU is set to Primary and the  
             other CPU’s as secondary. A value of true is set if the
             CPU is primary.

            The following values are valid for CPU availability status:

            Unknown (1)
              The CPU Primary/Secondary could not be determined.

            false (2)
              The CPU is not primary CPU.

            True (3)
              The CUR is primary CPU."

        ::= { cpqSeCpuEntry 27 }

-- ****************************************************************************
--   The FPU Table
-- ****************************************************************************

    cpqSeFpuTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSeFpuEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A list of the FPUs (floating point coprocessors) in the system."
        ::= { cpqSeProcessor 2 }

    cpqSeFpuEntry OBJECT-TYPE
        SYNTAX  CpqSeFpuEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A description of a FPU in the system.

            The fpuUnitIndex of any entry in this table will equal the
            cpuUnitIndex of the corresponding CPU in the cpqSeCpu table."
        INDEX   { cpqSeFpuUnitIndex , cpqSeFpuChipIndex }
        ::= { cpqSeFpuTable 1 }

    CpqSeFpuEntry ::= SEQUENCE {
        cpqSeFpuUnitIndex    INTEGER,
        cpqSeFpuChipIndex    INTEGER,
        cpqSeFpuSlot         INTEGER,
        cpqSeFpuName         DisplayString,
        cpqSeFpuSpeed        INTEGER,
        cpqSeFpuType         INTEGER,
        cpqSeFpuHwLocation   DisplayString
    }

    cpqSeFpuUnitIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This is a number that uniquely specifies a processor unit.

            A processing unit may be a set of processing chips that are
            on the same board or for other reasons work together as a unit.
            The main processor unit (if there is one) will always have the
            lowest (first) index.  This field can be used to associate
            CPUs with their corresponding FPUs."
        ::= { cpqSeFpuEntry 1 }

    cpqSeFpuChipIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This is a number that uniquely specifies the FPU chip.

            This field is used to distinguish between multiple FPUs that are
            part of the same processor unit.  For example, If a processor
            board contained a Intel 80386 processor with both a Intel 80387
            and a Weitek 3167, both the 80387 and the 3167 would have the
            same fpuUnitIndex (which would match the 80386's cpuUnitIndex)
            but the 80387 and the 3167 would have different fpuChipIndex
            field values."
        ::= { cpqSeFpuEntry 2 }

    cpqSeFpuSlot OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This is the FPU's slot.

            If the slot cannot be determined the value of zero (0) will
            be returned."
        ::= { cpqSeFpuEntry 3 }

    cpqSeFpuName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This is the name of the FPU.

            For example:
                80387
                Weitek 3167"
        ::= { cpqSeFpuEntry 4 }

    cpqSeFpuSpeed OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This is speed in megahertz of the FPU.

            Zero will be returned if this value is not available."
        ::= { cpqSeFpuEntry 5 }

    cpqSeFpuType OBJECT-TYPE
       SYNTAX  INTEGER {
            other(1),
            embedded(2),
            external(3)
            }
       ACCESS  read-only
       STATUS  mandatory
       DESCRIPTION
            "This value indicates if the FPU this entry is describing
            is embedded in the CPU or external to the CPU chip."
        ::= { cpqSeFpuEntry 6 }

    cpqSeFpuHwLocation  OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "A text description of the hardware location, on complex
             multi SBB hardware only, for the FPU.
             A NULL string indicates that the hardware location could not
             be determined or is irrelevant."
        ::= { cpqSeFpuEntry 7 }

-- ****************************************************************************
--   Standard Equipment CPU Cache Table
--   ==================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--        cpqSeProcessor Group         (1.3.6.1.4.1.232.1.2.2)
--         cpqSeCpuCacheTable          (1.3.6.1.4.1.232.1.2.2.3)
--
-- ****************************************************************************

    cpqSeCpuCacheTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSeCpuCacheEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A list of the CPU caches in the system."
        ::= { cpqSeProcessor 3 }

    cpqSeCpuCacheEntry OBJECT-TYPE
        SYNTAX  CpqSeCpuCacheEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A description of a CPU Caches in the system."
        INDEX   { cpqSeCpuCacheUnitIndex, cpqSeCpuCacheLevelIndex }
        ::= { cpqSeCpuCacheTable 1 }

    CpqSeCpuCacheEntry ::= SEQUENCE {
        cpqSeCpuCacheUnitIndex    INTEGER,
        cpqSeCpuCacheLevelIndex   INTEGER,
        cpqSeCpuCacheSize         INTEGER,
        cpqSeCpuCacheSpeed        INTEGER,
        cpqSeCpuCacheStatus       INTEGER,
        cpqSeCpuCacheWritePolicy  INTEGER,
        cpqSeCpuCacheHwLocation   DisplayString,
        cpqSeCpuCacheCpuSlot      INTEGER,
        cpqSeCpuCacheCpuCoreIndex INTEGER
    }

    cpqSeCpuCacheUnitIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This is a number that uniquely specifies a processor unit.

            A processing unit may be a set of processing chips that are
            on the same board or for other reasons work together as a unit.
            The main processor unit (if such a concept is valid for this
            machine) will always have the lowest (first) index."
        ::= { cpqSeCpuCacheEntry 1 }

    cpqSeCpuCacheLevelIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This is the processor cache level.

            The lower the processor cache level, the closer the cache is to
            the processor."
        ::= { cpqSeCpuCacheEntry 2 }

    cpqSeCpuCacheSize OBJECT-TYPE
        SYNTAX  INTEGER  (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The size of the cache in kilobytes."
        ::= { cpqSeCpuCacheEntry 3 }

    cpqSeCpuCacheSpeed OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This is speed in cache memory in nanoseconds (ns).  A value of
             zero (0) means that the cache speed is unknown or unobtainable."
        ::= { cpqSeCpuCacheEntry 4 }

    cpqSeCpuCacheStatus OBJECT-TYPE
        SYNTAX  INTEGER {
            unknown(1),
            ok(2),
            degraded(3),
            failed(4)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The status of the cache unit.  If the cache is optional and not
            installed, unknown(1) will be returned."
        ::= { cpqSeCpuCacheEntry 5 }

    cpqSeCpuCacheWritePolicy OBJECT-TYPE
        SYNTAX  INTEGER {
            unknown(1),
            write-through(2),
            write-back(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Specifies write policy of this cache entry."
        ::= { cpqSeCpuCacheEntry 6 }

    cpqSeCpuCacheHwLocation  OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "A text description of the hardware location, on complex
             multi SBB hardware only, for the CPU cache.
             A NULL string indicates that the hardware location could not
             be determined or is irrelevant."
        ::= { cpqSeCpuCacheEntry 7 }

    cpqSeCpuCacheCpuSlot OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This is the CPU Slot associated with this CPU cache."
        ::= { cpqSeCpuCacheEntry 8 }

    cpqSeCpuCacheCpuCoreIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This is a unique number that identifies the core in the CPU
             slot to which this cache is associated."
        ::= { cpqSeCpuCacheEntry 9 }

-- ****************************************************************************
--   Standard Equipment Memory Group
--   ===============================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--        cpqSeMemory Group            (1.3.6.1.4.1.232.1.2.3)
--
--      The cpqSeMemory group provides the base memory in the system and the
--      total memory in the system.
--
--      Implementation of the cpqSeMemory group is mandatory for all agents
--      supporting the Standard Equipment MIB.
--
-- ****************************************************************************

    cpqSeBaseMem OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The amount of base memory in kilobytes.

            A kilobyte is 1024 bytes."
        ::= { cpqSeMemory 1 }
 
    cpqSeTotalMem OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The total amount of memory in kilobytes.

            A kilobyte is 1024 bytes."
        ::= { cpqSeMemory 2 }

    cpqSeTotalMemMB OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The total amount of memory in megabytes.

            A megabyte is 1024 kilobytes."
        ::= { cpqSeMemory 3 }

-- ****************************************************************************
--   Standard Equipment ISA CMOS Group
--   =================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--        cpqSeIsaCmos Group           (1.3.6.1.4.1.232.1.2.4)
--
--
--     The ISA CMOS group provides an image of the ISA CMOS real time clock,
--     security, and configuration in a raw form.  This group is provided for
--     completeness, most of the important information stored in ISA CMOS can
--     also be found elsewhere in the MIB.
--
--     Implementation of the ISA CMOS group is mandatory for all agents
--     supporting the Standard Equipment MIB.
--
-- ****************************************************************************


    cpqSeIsaCmosRaw OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The contents of the ISA CMOS."
        ::= { cpqSeIsaCmos 1 }

-- ****************************************************************************
--   Standard Equipment EISA NVRAM Slot Table
--   ========================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--        cpqSeEisaNvram Group         (1.3.6.1.4.1.232.1.2.5)
--         cpqSeEisaSlotTable          (1.3.6.1.4.1.232.1.2.5.1)
--
--
--      The EISA NVRAM group provides a set of tables that detail the
--      configuration information stored in an EISA bus architecture system.
--      The EISA slot table contains entries providing information about each
--      slot that currently contains a configured card.
--      The EISA function table contains entries providing information about
--      each function performed by a configured card.  Each card may have
--      one or more defined functions.
--      The rest of the tables: the EISA memory table, the EISA Interrupt
--      table, the EISA DMA table, and the EISA port table, detail the
--      resources used by each function of each configured card.
--
--      Implementation of the eisaNvram group is optional.
--      The eisaNvram group should be included on any system with an EISA bus
--      architecture.
--
-- ****************************************************************************

    cpqSeEisaSlotTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSeEisaSlotEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A list of EISA slot information entries."
        ::= { cpqSeEisaNvram 1 }

    cpqSeEisaSlotEntry OBJECT-TYPE
        SYNTAX  CpqSeEisaSlotEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A description of an EISA slot."
        INDEX   { cpqSeEisaSlotIndex }
        ::= { cpqSeEisaSlotTable 1 }

    CpqSeEisaSlotEntry ::= SEQUENCE {
        cpqSeEisaSlotIndex           INTEGER,
        cpqSeEisaSlotRaw             OCTET STRING,
        cpqSeEisaSlotBoardId         DisplayString,
        cpqSeEisaSlotBoardName       DisplayString,
        cpqSeEisaSlotCfRev           DisplayString,
        cpqSeEisaSlotType            INTEGER
    }

    cpqSeEisaSlotIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255) 
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The EISA slot number for this entry describes."
        ::= { cpqSeEisaSlotEntry 1 }

    cpqSeEisaSlotRaw OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (12))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The EISA slot data for the board in this slot.

            This octet string contains the following EISA slot information:

            The first octet will be zero (0) if this slot contains a
            properly configured board.  Any other value indicates that the
            EISA configuration information for this board is invalid or an
            error occurred when trying to retrieve the information.

            The second octet contains several bit flags about the product ID
            and slot type.

                Bit 7:      0 = No duplicate ID
                            1 = Duplicate IDs

                Bit 6:      0 = Product ID readable
                            1 = Product ID not readable

                Bit 5,4:    00 = Expansion slot
                            01 = Embedded device
                            10 = Virtual device
                            11 = Reserved

                Bit 3..0:   This nibble indicates which CFG file is loaded
                            when duplicate file names are present.
                            0000 = No duplicate ID
                            0001 = First duplicate ID
                            0010 = Second duplicate ID
                            0011 = Third duplicate ID
                              .
                              .
                              .
                            1111 = Fifteenth duplicate ID

            NOTE:   Bit 7 is the most significant bit, bit 0 is the least
                    significant.

            The third octet contains the major revision level of the
            configuration utility.

            The fourth octet contains the minor revision level of the
            configuration utility.

            The fifth octet contains the most significant byte of the
            configuration file checksum.

            The sixth octet contains the least significant byte of the
            configuration file checksum.

            The seventh octet contains the number of device functions defined
            for the board in this slot.

            The eighth octet contains the combined function information.
            This is a set of flags.  Each bit has the following meaning when
            set (1):
                Bit 7:  reserved (0)
                Bit 6:  slot has one or more free form data entries
                Bit 5:  slot has one or more port initialization entries.
                Bit 4:  slot has one or more port range entries.
                Bit 3:  slot has one or more DMA entries.
                Bit 2:  slot has one or more interrupt (IRQ) entries.
                Bit 1:  slot has one or more memory entries.
                Bit 0:  slot has one or more function type definitions.

            NOTE:   bit 7 is the most significant bit, bit 0 is the least
                    significant.

            The ninth, tenth, eleventh, and twelfth octets contain the four
            byte compressed EISA ID.

            For more information about the meaning of this information
            consult the EISA Technical Reference Guide."
        ::= { cpqSeEisaSlotEntry 2 }

    cpqSeEisaSlotBoardId OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (7))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A seven character board ID.

            The first three characters are the manufacturers ID followed by 
            three character product ID followed by a one character revision
            level."
        ::= { cpqSeEisaSlotEntry 3 }

    cpqSeEisaSlotBoardName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The product name (or other suitable description) of this board.

            This field may be empty if no descriptive information is known
            about the board."
        ::= { cpqSeEisaSlotEntry 4 }

    cpqSeEisaSlotCfRev OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..5))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The revision level of the EISA configuration utility that was
            used to configure the system.

            This should be the same version information displayed by the EISA
            configuration utility."
        ::= { cpqSeEisaSlotEntry 5 }

    cpqSeEisaSlotType OBJECT-TYPE
        SYNTAX  INTEGER {
        unknown(1),
        isa8Bit(2),
        isa16Bit(3),
        eisa32Bit(4),
        eisaBusMaster32Bit(5),
        other(6),
        reserved(7),
        reserved2(8)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The type of slot described by this entry."
        ::= { cpqSeEisaSlotEntry 6 }


-- ****************************************************************************
--   Standard Equipment EISA NVRAM Function Table
--   ============================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--        cpqSeEisaNvram Group         (1.3.6.1.4.1.232.1.2.5)
--         cpqSeEisaSlotTable          (1.3.6.1.4.1.232.1.2.5.1)
--         cpqSeEisaFunctTable         (1.3.6.1.4.1.232.1.2.5.2)
--
-- ****************************************************************************

    cpqSeEisaFunctTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSeEisaFunctEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A list EISA function information entries."
        ::= { cpqSeEisaNvram 2 }

    cpqSeEisaFunctEntry OBJECT-TYPE
        SYNTAX  CpqSeEisaFunctEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A description of an EISA function."
        INDEX   { cpqSeEisaFunctSlotIndex , cpqSeEisaFunctIndex }
        ::= { cpqSeEisaFunctTable 1 }

    CpqSeEisaFunctEntry ::= SEQUENCE {
        cpqSeEisaFunctSlotIndex   INTEGER,
        cpqSeEisaFunctIndex       INTEGER,
        cpqSeEisaFunctStatus      INTEGER,
        cpqSeEisaFunctType        DisplayString,
        cpqSeEisaFunctCfgRev      DisplayString,
        cpqSeEisaFunctSels        OCTET STRING,
        cpqSeEisaFunctInfo        INTEGER
    }

    cpqSeEisaFunctSlotIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The EISA slot of the board that registered this function"
        ::= { cpqSeEisaFunctEntry 1 }

    cpqSeEisaFunctIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The number of the function this entry describes."
        ::= { cpqSeEisaFunctEntry 2 }

    cpqSeEisaFunctStatus OBJECT-TYPE
        SYNTAX  INTEGER {
            disabled(2),
            enabled(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The status of the function described by this entry."
        ::= { cpqSeEisaFunctEntry 3 }

    cpqSeEisaFunctType OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..80))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The type of the function.

            The type may be followed by one or more subtype description
            fields. Some currently defined types are:

            Type            Meaning
            ==============  ==================================================
            COM             Communication device
            COM,ASY         ISA compatible 8250 based serial port
            COM,ASY,FIFO    ISA compatible 16550 based serial port (with fifo)
            COM,SYN         ISA compatible SDLC port
            CPU             Microprocessor
            CPU,8086        8086 compatible microprocessor
            CPU,80286       80286 compatible microprocessor
            CPU,80386SX     80386SX compatible microprocessor
            CPU,80386       80386 compatible microprocessor
            CPU,80486       80486 compatible microprocessor
            JOY             ISA compatible joystick adapter
            KEY             Keyboard
            KEY,nnn,KBD=xx  Standard keyboard with nnn keys for country xx
            MEM             Memory board
            MFC             Multifunction board
            MSD             Mass storage device
            MSD,DSKCTL      ISA compatible fixed disk controller
            MSD,FPYCTL      ISA compatible floppy disk controller
            MSD,TAPCTL      Primary tape controller
            NET             Network board
            NPX             Numeric coprocessor
            NPX,287         Intel 287 numeric coprocessor
            NPX,387         Intel 387 numeric coprocessor
            NPX,387SX       Intel 387SX numeric coprocessor
            NPX,W1167       Weitek 1167 numeric coprocessor
            NPX,W3167       Weitek 3167 numeric coprocessor
            OSE             Operating system/environment
            OTH             Other
            PAR             ISA compatible parallel port
            PAR,BID         Bidirectional parallel port
            PTR             Pointing device
            PTR,8042        8042 pointing device (mouse) interface
            SYS             System board
            VID             Video board
            VID,MDA         ISA compatible monochrome adapter
            VID,MDA,MGA     Hercules monochrome adapter
            VID,CGA         CGA, no write sync during retrace required
            VID,CGA,RTR     CGA, write sync during retrace required
            VID,EGA         ISA compatible EGA adapter
            VID,VGA         ISA compatible VGA adapter

            This list is not intended to be complete.  Other types may be
            found in this field.  This list describes some of the more
            common types found, other types should be similarly recognizable
            to someone sufficiently knowledgeable about computer hardware."
      ::= { cpqSeEisaFunctEntry 4 }

    cpqSeEisaFunctCfgRev OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..5))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The revision of the EISA configuration .OVL file used to
            configure this board."
        ::= { cpqSeEisaFunctEntry 5 }

    cpqSeEisaFunctSels OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (0..26))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The selections that were chosen with the EISA CONFIGURATION
            UTILITY to create this function."
        ::= { cpqSeEisaFunctEntry 6 }

    cpqSeEisaFunctInfo OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The EISA function information block.

            This is a set of flags indicating the resources that are
            configured in this EISA function.  Each bit has the following
            meaning when it is set (1):

                Bit 7:  Function is disabled
                Bit 6:  This function contains free-form information.
                Bit 5:  This function contains port initialization entries.
                Bit 4:  This function contains port range entries.
                Bit 3:  This function contains DMA entries.
                Bit 2:  This function contains interrupt (IRQ) entries.
                Bit 1:  This function contains memory entries.
                Bit 0:  This function contains function type definitions.

            NOTE:   bit 7 is the most significant bit, bit 0 is the least
                    significant."
        ::= { cpqSeEisaFunctEntry 7 }

-- ****************************************************************************
--   Standard Equipment EISA Memory Table
--   ====================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--        cpqSeEisaNvram Group         (1.3.6.1.4.1.232.1.2.5)
--         cpqSeEisaSlotTable          (1.3.6.1.4.1.232.1.2.5.1)
--         cpqSeEisaFunctTable         (1.3.6.1.4.1.232.1.2.5.2)
--         cpqSeEisaMemTable           (1.3.6.1.4.1.232.1.2.5.3)
--
-- ****************************************************************************

    cpqSeEisaMemTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSeEisaMemEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A list of EISA function memory configuration entries."
        ::= { cpqSeEisaNvram 3 }

    cpqSeEisaMemEntry OBJECT-TYPE
        SYNTAX  CpqSeEisaMemEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A description of an EISA function memory configuration."
        INDEX   { cpqSeEisaMemSlotIndex , cpqSeEisaMemFunctIndex ,
                  cpqSeEisaMemAllocIndex }
        ::= { cpqSeEisaMemTable 1 }

    CpqSeEisaMemEntry ::= SEQUENCE {
        cpqSeEisaMemSlotIndex         INTEGER,
        cpqSeEisaMemFunctIndex        INTEGER,
        cpqSeEisaMemAllocIndex        INTEGER,
        cpqSeEisaMemStartAddr         INTEGER,
        cpqSeEisaMemSize              INTEGER,
        cpqSeEisaMemShare             INTEGER,
        cpqSeEisaMemType              INTEGER,
        cpqSeEisaMemCache             INTEGER,
        cpqSeEisaMemAccess            INTEGER,
        cpqSeEisaMemDecode            INTEGER,
        cpqSeEisaMemDataSize          INTEGER
    }

    cpqSeEisaMemSlotIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The EISA slot number of the board that registered the memory
            configuration this entry describes."
        ::= { cpqSeEisaMemEntry 1 }

    cpqSeEisaMemFunctIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The function in which this memory configuration was registered."
        ::= { cpqSeEisaMemEntry 2 }

    cpqSeEisaMemAllocIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The index for this memory allocation entry in the EISA function
            block."
        ::= { cpqSeEisaMemEntry 3 }

    cpqSeEisaMemStartAddr OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The starting address of the memory configuration."
        ::= { cpqSeEisaMemEntry 4 }

    cpqSeEisaMemSize OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The size in bytes of the memory configuration."
        ::= { cpqSeEisaMemEntry 5 }

    cpqSeEisaMemShare OBJECT-TYPE
        SYNTAX  INTEGER {
            nonshareable(1),
            shareable(2)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This value indicates if the memory is shareable."
        ::= { cpqSeEisaMemEntry 6 }

    cpqSeEisaMemType OBJECT-TYPE
        SYNTAX  INTEGER {
            systemBaseOrExtended(1),
            expanded(2),
            virtual(3),
            other(4)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The type of memory."
        ::= { cpqSeEisaMemEntry 7 }

    cpqSeEisaMemCache OBJECT-TYPE
        SYNTAX  INTEGER {
            notCached(1),
            writeThroughCached(2),
        writeBackCached(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This value indicates if the memory is cached."
        ::= { cpqSeEisaMemEntry 8 }

    cpqSeEisaMemAccess OBJECT-TYPE
        SYNTAX  INTEGER {
            readOnly(1),
            readWrite(2)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The type of access permitted for this memory."
        ::= { cpqSeEisaMemEntry 9 }

    cpqSeEisaMemDecode OBJECT-TYPE
        SYNTAX  INTEGER (0..65536)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The memory decode size (the number of address lines supported)."
        ::= { cpqSeEisaMemEntry 10 }

    cpqSeEisaMemDataSize OBJECT-TYPE
        SYNTAX  INTEGER (0..65536)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The data access size for the memory in bits."
        ::= { cpqSeEisaMemEntry 11 }

-- ****************************************************************************
--   Standard Equipment EISA Interrupt Table
--   =======================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--        cpqSeEisaNvram Group         (1.3.6.1.4.1.232.1.2.5)
--         cpqSeEisaSlotTable          (1.3.6.1.4.1.232.1.2.5.1)
--         cpqSeEisaFunctTable         (1.3.6.1.4.1.232.1.2.5.2)
--         cpqSeEisaMemTable           (1.3.6.1.4.1.232.1.2.5.3)
--         cpqSeEisaIntTable           (1.3.6.1.4.1.232.1.2.5.4)
--
-- ****************************************************************************

    cpqSeEisaIntTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSeEisaIntEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A list of EISA function interrupt configuration entries."
        ::= { cpqSeEisaNvram 4 }

    cpqSeEisaIntEntry OBJECT-TYPE
        SYNTAX  CpqSeEisaIntEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION 
            "A description of an EISA function interrupt configuration."
        INDEX   { cpqSeEisaIntSlotIndex , cpqSeEisaIntFunctIndex ,
                  cpqSeEisaIntAllocIndex }
        ::= { cpqSeEisaIntTable 1 }

    CpqSeEisaIntEntry ::= SEQUENCE {
        cpqSeEisaIntSlotIndex          INTEGER,
        cpqSeEisaIntFunctIndex         INTEGER,
        cpqSeEisaIntAllocIndex         INTEGER,
        cpqSeEisaIntNum                INTEGER,
        cpqSeEisaIntShare              INTEGER,
        cpqSeEisaIntTrigger            INTEGER
    }

    cpqSeEisaIntSlotIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The EISA slot number of the board that registered the interrupt
            configuration this entry describes."
        ::= { cpqSeEisaIntEntry 1 }

    cpqSeEisaIntFunctIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The function in which this interrupt configuration was
            registered."
        ::= { cpqSeEisaIntEntry 2 }

    cpqSeEisaIntAllocIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The index for this interrupt allocation entry in the EISA
            function block."
        ::= { cpqSeEisaIntEntry 3 }

    cpqSeEisaIntNum OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The interrupt described in this entry."
        ::= { cpqSeEisaIntEntry 4 }

    cpqSeEisaIntShare OBJECT-TYPE
        SYNTAX  INTEGER {
            nonshareable(1),
            shareable(2)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This value indicates if the interrupt is shareable."
        ::= { cpqSeEisaIntEntry 5 }

    cpqSeEisaIntTrigger OBJECT-TYPE
        SYNTAX  INTEGER {
            edge(1),
            level(2)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This value indicates if the interrupt is edge or level
            triggered."
        ::= { cpqSeEisaIntEntry 6 }

-- ****************************************************************************
--   Standard Equipment EISA DMA Table
--   =================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--        cpqSeEisaNvram Group         (1.3.6.1.4.1.232.1.2.5)
--         cpqSeEisaSlotTable          (1.3.6.1.4.1.232.1.2.5.1)
--         cpqSeEisaFunctTable         (1.3.6.1.4.1.232.1.2.5.2)
--         cpqSeEisaMemTable           (1.3.6.1.4.1.232.1.2.5.3)
--         cpqSeEisaIntTable           (1.3.6.1.4.1.232.1.2.5.4)
--         cpqSeEisaDmaTable           (1.3.6.1.4.1.232.1.2.5.5)
--
-- ****************************************************************************

    cpqSeEisaDmaTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSeEisaDmaEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A list of EISA function DMA configuration entries."
        ::= { cpqSeEisaNvram 5 }

    cpqSeEisaDmaEntry OBJECT-TYPE
        SYNTAX  CpqSeEisaDmaEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A description of an EISA function DMA configuration."
        INDEX   { cpqSeEisaDmaSlotIndex , cpqSeEisaDmaFunctIndex ,
                  cpqSeEisaDmaAllocIndex }
        ::= { cpqSeEisaDmaTable 1 }

    CpqSeEisaDmaEntry ::= SEQUENCE {
        cpqSeEisaDmaSlotIndex        INTEGER,
        cpqSeEisaDmaFunctIndex       INTEGER,
        cpqSeEisaDmaAllocIndex       INTEGER,
        cpqSeEisaDmaChannel          INTEGER,
        cpqSeEisaDmaShare            INTEGER,
        cpqSeEisaDmaTiming           INTEGER,
        cpqSeEisaDmaXfer             INTEGER,
        cpqSeEisaDmaXferCount        INTEGER
    }

    cpqSeEisaDmaSlotIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The EISA slot number of the board that registered the DMA
            configuration this entry describes."
        ::= { cpqSeEisaDmaEntry 1 }

    cpqSeEisaDmaFunctIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The function in which this DMA configuration was registered."
        ::= { cpqSeEisaDmaEntry 2 }

    cpqSeEisaDmaAllocIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The index for this DMA channel allocation entry in the EISA
            function block."
        ::= { cpqSeEisaDmaEntry 3 }

    cpqSeEisaDmaChannel OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The DMA channel described in this entry."
        ::= { cpqSeEisaDmaEntry 4 }

    cpqSeEisaDmaShare OBJECT-TYPE
        SYNTAX  INTEGER {
            nonshareable(1),
            shareable(2)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This value indicates if the DMA channel is shareable."
        ::= { cpqSeEisaDmaEntry 5 }

    cpqSeEisaDmaTiming OBJECT-TYPE
        SYNTAX  INTEGER {
            isaTiming(1),
            typeA(2),
            typeB(3),
            burstTypeC(4)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This value indicates the timing (transfer rate) associated with
            this configuration of the DMA channel."
        ::= { cpqSeEisaDmaEntry 6 }

    cpqSeEisaDmaXfer OBJECT-TYPE
        SYNTAX  INTEGER  (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This value indicates the transfer size in bits used over this
            DMA channel."
        ::= { cpqSeEisaDmaEntry 7 }

    cpqSeEisaDmaXferCount OBJECT-TYPE
        SYNTAX  INTEGER {
            byte(1),
            word(2)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This value indicates the addressing scheme for the DMA channel."
        ::= { cpqSeEisaDmaEntry 8 }


-- ****************************************************************************
--   Standard Equipment EISA Port Table
--   ==================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--        cpqSeEisaNvram Group         (1.3.6.1.4.1.232.1.2.5)
--         cpqSeEisaSlotTable          (1.3.6.1.4.1.232.1.2.5.1)
--         cpqSeEisaFunctTable         (1.3.6.1.4.1.232.1.2.5.2)
--         cpqSeEisaMemTable           (1.3.6.1.4.1.232.1.2.5.3)
--         cpqSeEisaIntTable           (1.3.6.1.4.1.232.1.2.5.4)
--         cpqSeEisaDmaTable           (1.3.6.1.4.1.232.1.2.5.5)
--         cpqSeEisaPortTable          (1.3.6.1.4.1.232.1.2.5.6)
--
-- ****************************************************************************

    cpqSeEisaPortTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSeEisaPortEntry
        ACCESS  not-accessible 
        STATUS  mandatory
        DESCRIPTION
            "A list of EISA function port I/O configuration entries."
        ::= { cpqSeEisaNvram 6 }

    cpqSeEisaPortEntry OBJECT-TYPE
        SYNTAX  CpqSeEisaPortEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A description of an EISA function port I/O configuration."
        INDEX   { cpqSeEisaPortSlotIndex , cpqSeEisaPortFunctIndex ,
                cpqSeEisaPortAllocIndex }
        ::= { cpqSeEisaPortTable 1 }

    CpqSeEisaPortEntry ::= SEQUENCE {
        cpqSeEisaPortSlotIndex       INTEGER,
        cpqSeEisaPortFunctIndex      INTEGER,
        cpqSeEisaPortAllocIndex      INTEGER,
        cpqSeEisaPortAddr            INTEGER,
        cpqSeEisaPortShare           INTEGER,
        cpqSeEisaPortSize            INTEGER
    }

    cpqSeEisaPortSlotIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The EISA slot number of the board that registered the I/O port
            configuration this entry describes."
        ::= { cpqSeEisaPortEntry 1 }

    cpqSeEisaPortFunctIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only 
        STATUS  mandatory
        DESCRIPTION
            "The function in which this port I/O configuration was
            registered."
        ::= { cpqSeEisaPortEntry 2 }

    cpqSeEisaPortAllocIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The index for this I/O port range allocation entry in the EISA
            function block."
        ::= { cpqSeEisaPortEntry 3 }

    cpqSeEisaPortAddr OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The I/O port address being described in this entry."
        ::= { cpqSeEisaPortEntry 4 }

    cpqSeEisaPortShare OBJECT-TYPE
        SYNTAX  INTEGER {
            nonshareable(1),
            shareable(2)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This value indicates if the port is shareable."
        ::= { cpqSeEisaPortEntry 5 }

    cpqSeEisaPortSize OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The number of sequential ports starting at the
            eisaPortAddrIndex that are be configured."
        ::= { cpqSeEisaPortEntry 6 }

-- ****************************************************************************
--   Standard Equipment EISA Free Form Table
--   =======================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--        cpqSeEisaNvram Group         (1.3.6.1.4.1.232.1.2.5)
--         cpqSeEisaSlotTable          (1.3.6.1.4.1.232.1.2.5.1)
--         cpqSeEisaFunctTable         (1.3.6.1.4.1.232.1.2.5.2)
--         cpqSeEisaMemTable           (1.3.6.1.4.1.232.1.2.5.3)
--         cpqSeEisaIntTable           (1.3.6.1.4.1.232.1.2.5.4)
--         cpqSeEisaDmaTable           (1.3.6.1.4.1.232.1.2.5.5)
--         cpqSeEisaPortTable          (1.3.6.1.4.1.232.1.2.5.6)
--         cpqSeEisaFreeFormTable      (1.3.6.1.4.1.232.1.2.5.7)
--
-- ****************************************************************************

    cpqSeEisaFreeFormTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSeEisaFreeFormEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A list of EISA function free form entries."
        ::= { cpqSeEisaNvram 7 }

    cpqSeEisaFreeFormEntry OBJECT-TYPE
        SYNTAX  CpqSeEisaFreeFormEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A description of an EISA function free form."
        INDEX   { cpqSeEisaFreeFormSlotIndex ,
                cpqSeEisaFreeFormFunctIndex }
        ::= { cpqSeEisaFreeFormTable 1 }

    CpqSeEisaFreeFormEntry ::= SEQUENCE {
        cpqSeEisaFreeFormSlotIndex           INTEGER,
        cpqSeEisaFreeFormFunctIndex          INTEGER,
        cpqSeEisaFreeFormValue               OCTET STRING
    }

    cpqSeEisaFreeFormSlotIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The EISA slot number of the board that registered the free form
            information this entry describes."
        ::= { cpqSeEisaFreeFormEntry 1 }

    cpqSeEisaFreeFormFunctIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The function in which this free form was registered."
        ::= { cpqSeEisaFreeFormEntry 2 }

    cpqSeEisaFreeFormValue OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (0..205))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The free form value."
        ::= { cpqSeEisaFreeFormEntry 3 }

-- ****************************************************************************
--   Standard Equipment EISA Function Port Initialization Table
--   ==========================================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--        cpqSeEisaNvram Group         (1.3.6.1.4.1.232.1.2.5)
--         cpqSeEisaSlotTable          (1.3.6.1.4.1.232.1.2.5.1)
--         cpqSeEisaFunctTable         (1.3.6.1.4.1.232.1.2.5.2)
--         cpqSeEisaMemTable           (1.3.6.1.4.1.232.1.2.5.3)
--         cpqSeEisaIntTable           (1.3.6.1.4.1.232.1.2.5.4)
--         cpqSeEisaDmaTable           (1.3.6.1.4.1.232.1.2.5.5)
--         cpqSeEisaPortTable          (1.3.6.1.4.1.232.1.2.5.6)
--         cpqSeEisaFreeFormTable      (1.3.6.1.4.1.232.1.2.5.7)
--         cpqSeEisaInitTable          (1.3.6.1.4.1.232.1.2.5.8)
--
-- ****************************************************************************

    cpqSeEisaInitTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSeEisaInitEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A list of EISA function port initialization entries."
        ::= { cpqSeEisaNvram 8 }

    cpqSeEisaInitEntry OBJECT-TYPE
        SYNTAX  CpqSeEisaInitEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A description of an EISA function port initialization."
        INDEX   { cpqSeEisaInitSlotIndex , cpqSeEisaInitFunctIndex ,
                  cpqSeEisaInitAllocIndex }
        ::= { cpqSeEisaInitTable 1 }

    CpqSeEisaInitEntry ::= SEQUENCE {
        cpqSeEisaInitSlotIndex         INTEGER,
        cpqSeEisaInitFunctIndex        INTEGER,
        cpqSeEisaInitAllocIndex        INTEGER,
        cpqSeEisaInitUseMask           INTEGER,
        cpqSeEisaInitAccess            INTEGER,
        cpqSeEisaInitAddr              INTEGER,
        cpqSeEisaInitValue             INTEGER,
        cpqSeEisaInitMask              INTEGER
    }

    cpqSeEisaInitSlotIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The EISA slot number of the board that registered the port
            initialization this entry describes."
        ::= { cpqSeEisaInitEntry 1 }

    cpqSeEisaInitFunctIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The function in which this port initialization was registered."
        ::= { cpqSeEisaInitEntry 2 }

    cpqSeEisaInitAllocIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The index for this port initialization entry in the EISA
            function block."
        ::= { cpqSeEisaInitEntry 3 }

    cpqSeEisaInitUseMask OBJECT-TYPE
        SYNTAX  INTEGER {
            useValueOnly(1),
            useValueAndMask(2)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This indicates if a mask will be used when performing
            initialization."
        ::= { cpqSeEisaInitEntry 4 }

    cpqSeEisaInitAccess OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            eightBitAddress(2),
            sixteenBitAddress(3),
            thirtyTwoBitAddress(4)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This value indicates the number of bits this entry initializes."
        ::= { cpqSeEisaInitEntry 5 }

    cpqSeEisaInitAddr OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This value indicates the port address this entry initializes."
        ::= { cpqSeEisaInitEntry 6 }

    cpqSeEisaInitValue OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This indicates the value to which this port is initialized."
        ::= { cpqSeEisaInitEntry 7 }

    cpqSeEisaInitMask OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This value indicates the mask to use when performing
            initialization."
        ::= { cpqSeEisaInitEntry 8 }


-- ****************************************************************************
--   Standard Equipment ROM Description Table
--   ========================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--        cpqSeRom Group               (1.3.6.1.4.1.232.1.2.6)
--        cpqSeSysRomVer               (1.3.6.1.4.1.232.1.2.6.1)
--        cpqSeOptRomTable             (1.3.6.1.4.1.232.1.2.6.2)
--
--      The ROM group contains a description of the system ROM and a table
--      providing option ROM information.  The option ROM table contains
--      entries specifying the starting address and size of the each option
--      ROM in the system.
--
--      Implementation of the ROM group is mandatory for all agents
--      supporting the Standard Equipment MIB.
--
-- ****************************************************************************


    cpqSeSysRomVer OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "System ROM version information."
        ::= { cpqSeRom 1 }


    cpqSeOptRomTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSeOptRomEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A table of option ROM descriptions."
        ::= { cpqSeRom 2 }

    cpqSeOptRomEntry OBJECT-TYPE
        SYNTAX  CpqSeOptRomEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "An option ROM description."
        INDEX   { cpqSeOptRomAddrIndex }
        ::= { cpqSeOptRomTable 1 }

    CpqSeOptRomEntry ::= SEQUENCE {
        cpqSeOptRomAddrIndex       INTEGER,
        cpqSeOptRomSize            INTEGER
    }

    cpqSeOptRomAddrIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..4294967295)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The starting address of the option ROM.

            This value indicates the number of bytes from the start of
            physical memory to the beginning of this option ROM."
        ::= { cpqSeOptRomEntry 1 }

    cpqSeOptRomSize OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The size in bytes of the option ROM."
        ::= { cpqSeOptRomEntry 2 }

    cpqSeBiosRomDataRaw OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (256))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The BIOS ROM data area.  This may be the current contents or
            a copy of the BIOS ROM data area from when the Insight Agent was
            initialized."
        ::= { cpqSeRom 3 }

    cpqSeRedundantSysRomVer OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "System ROM version information for the redundant ROM
            image.  This will be left blank if the system does not
            support a redundant ROM."
        ::= { cpqSeRom 4 }

    cpqSeSmbiosVer OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "SMBIOS version information."
        ::= { cpqSeRom 5 }

    cpqSeMPFwVer OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "The version of Management Processor Firmware."
        ::= { cpqSeRom 6 }

    cpqSeBMCFwVer OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "The version of the manageability firmware."
        ::= { cpqSeRom 7 }

    cpqSeHPVMFwVer OBJECT-TYPE 
        SYNTAX  DisplayString (SIZE (0..255)) 
        ACCESS  read-only 
        STATUS  optional 
        DESCRIPTION 
            "The version of the virtual machine firmware." 
        ::= { cpqSeRom 8 }

-- ****************************************************************************
--   Standard Equipment Keyboard Group
--   =================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--        cpqSeKeyboard Group          (1.3.6.1.4.1.232.1.2.7)
--
--      The keyboard group describes the keyboard attached to the system.
--
--      Implementation of the Keyboard group is mandatory for all agents
--      supporting the Standard Equipment MIB.
--
-- ****************************************************************************

    cpqSeKeyboardDesc OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A description of the keyboard."
        ::= { cpqSeKeyboard 1 }

-- ****************************************************************************
--   Standard Equipment Video Group
--   ==============================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--        cpqSeVideo Group             (1.3.6.1.4.1.232.1.2.8)
--
--      The video group describes the video adapter and display.
--
--      Implementation of the video group is mandatory for all agents
--      supporting the Standard Equipment MIB.
--
-- ****************************************************************************

    cpqSeVideoDesc OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A description of the video system in the computer.  This may
            include the manufacturer, board name, modes supported, etc.."
        ::= { cpqSeVideo 1 }

-- ****************************************************************************
--   Standard Equipment Serial Port Table
--   ====================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--        cpqSeSerialPort Group        (1.3.6.1.4.1.232.1.2.9)
--         cpqSeSerialPortTable        (1.3.6.1.4.1.232.1.2.9.1)
--
--      The serial port group describes the serial ports in the system.
--
--      Implementation of the Serial Port group is mandatory for all agents
--      supporting the Standard Equipment MIB.
--
--
-- ****************************************************************************

    cpqSeSerialPortTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSeSerialPortEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A table of serial port descriptions."
        ::= { cpqSeSerialPort 1 }

    cpqSeSerialPortEntry OBJECT-TYPE
        SYNTAX  CpqSeSerialPortEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A description of a serial port."
        INDEX   { cpqSeSerialPortIndex }
        ::= { cpqSeSerialPortTable 1 }

    CpqSeSerialPortEntry ::= SEQUENCE {
        cpqSeSerialPortIndex       INTEGER,
        cpqSeSerialPortAddr        INTEGER,
        cpqSeSerialPortDesc        DisplayString,
        cpqSeSerialPortHwLocation  DisplayString
    }

    cpqSeSerialPortIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "An index that uniquely specifies this entry."
        ::= { cpqSeSerialPortEntry 1 }

    cpqSeSerialPortAddr OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The I/O port address used by this serial port."
        ::= { cpqSeSerialPortEntry 2 }

    cpqSeSerialPortDesc OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A text description of further information known about the serial
            port.  This may be an empty string if no further information is
            known."
        ::= { cpqSeSerialPortEntry 3 }

    cpqSeSerialPortHwLocation  OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "A text description of the hardware location, on complex
             multi SBB hardware only, for the serial port.
             A NULL string indicates that the hardware location could not
             be determined or is irrelevant."
        ::= { cpqSeSerialPortEntry 4 }

-- ****************************************************************************
--   Standard Equipment Parallel Port Table
--   ======================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--        cpqSeParallel Group          (1.3.6.1.4.1.232.1.2.10)
--         cpqSeParallelPortTable      (1.3.6.1.4.1.232.1.2.10.1)
--
--
--      The parallel port group describes the parallel ports in the system.
--
--      Implementation of the Parallel Port group is mandatory for all agents
--      supporting the Standard Equipment MIB.
--
--
-- ****************************************************************************


    cpqSeParallelPortTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSeParallelPortEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A table of parallel port descriptions."
        ::= { cpqSeParallelPort 1 }

    cpqSeParallelPortEntry OBJECT-TYPE
        SYNTAX  CpqSeParallelPortEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A description of a parallel port."
        INDEX   { cpqSeParallelPortIndex }
        ::= { cpqSeParallelPortTable 1 }

    CpqSeParallelPortEntry ::= SEQUENCE {
        cpqSeParallelPortIndex        INTEGER,
        cpqSeParallelPortAddr         INTEGER,
        cpqSeParallelPortDesc         DisplayString,
        cpqSeParrallelPortHwLocation  DisplayString
    }

    cpqSeParallelPortIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "An index that uniquely specifies this entry."
        ::= { cpqSeParallelPortEntry 1 }

    cpqSeParallelPortAddr OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The I/O port address used by this parallel port."
        ::= { cpqSeParallelPortEntry 2 }

    cpqSeParallelPortDesc OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A text description of further information known about the
            parallel port.  This may be an empty string if no further
            information is known."
        ::= { cpqSeParallelPortEntry 3 }

    cpqSeParrallelPortHwLocation  OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "A text description of the hardware location, on complex
             multi SBB hardware only, for the parallel port.
             A NULL string indicates that the hardware location could not
             be determined or is irrelevant."
        ::= { cpqSeParallelPortEntry 4 }

-- ****************************************************************************
--   Standard Equipment Floppy Disk Table
--   ======================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--        cpqSeFloppyDisk Group        (1.3.6.1.4.1.232.1.2.11)
--         cpqSeFloppyDiskTable        (1.3.6.1.4.1.232.1.2.11.1)
--
--      The floppy disk group describes the floppy disk drives in the system.
--
--      Implementation of the Floppy Disk group is mandatory for all agents
--      supporting the Standard Equipment MIB.
--
-- ****************************************************************************

    cpqSeFloppyDiskTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSeFloppyDiskEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A table of floppy drive descriptions."
        ::= { cpqSeFloppyDisk 1 }

    cpqSeFloppyDiskEntry OBJECT-TYPE
        SYNTAX  CpqSeFloppyDiskEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A floppy drive description."
        INDEX   { cpqSeFloppyDiskIndex }
        ::= { cpqSeFloppyDiskTable 1 }

    CpqSeFloppyDiskEntry ::= SEQUENCE {
        cpqSeFloppyDiskIndex       INTEGER,
        cpqSeFloppyDiskType        INTEGER,
        cpqSeFloppyDiskHwLocation  DisplayString
    }

    cpqSeFloppyDiskIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "An index that uniquely specifies this entry.  If possible, this
            field will map directly to the drive letter (0 for A:, 1 for B:)."
        ::= { cpqSeFloppyDiskEntry 1 }

    cpqSeFloppyDiskType OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            drive360k(2),
            drive1200k(3),
            drive720k(4),
            drive1440k(5),
            drive120mb(6)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The type (capacity) of the floppy drive.  The following values
            are valid:

            other (1)       This floppy drive could not be identified.
            drive360k (2)   This is a 360 kilobyte, 5.25 inch floppy drive.
            drive1200k (3)  This is a 1.2 megabyte, 5.25 inch floppy drive.
            drive720k (4)   This is a 720 kilobyte, 3.5 inch floppy drive.
            drive1440k (5)  This is a 1.44 megabyte, 3.5 inch floppy drive.
            drive120mb(6)   This is a 120 megabyte, 3.5 inch floptical
                            drive."
        ::= { cpqSeFloppyDiskEntry 2 }

    cpqSeFloppyDiskHwLocation  OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "A text description of the hardware location, on complex
             multi SBB hardware only, for the floppy disk.
             A NULL string indicates that the hardware location could not
             be determined or is irrelevant."
        ::= { cpqSeFloppyDiskEntry 3 }

-- ****************************************************************************
--   Standard Equipment Fixed Disk Table
--   ===================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--        cpqSeFixedDisk Group         (1.3.6.1.4.1.232.1.2.12)
--         cpqSeFixedDiskTable         (1.3.6.1.4.1.232.1.2.12.1)
--
--      The fixed disk group describes the fixed disk drives in the system
--      that are accessible through a ST506 compatible interface.
--
--      Implementation of the Fixed Disk group is mandatory for all agents
--      supporting the Standard Equipment MIB.
--
-- ****************************************************************************

    cpqSeFixedDiskTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSeFixedDiskEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A table of ST-506 interface accessible fixed disk descriptions."
        ::= { cpqSeFixedDisk 1 }

    cpqSeFixedDiskEntry OBJECT-TYPE
        SYNTAX  CpqSeFixedDiskEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A fixed disk description."
        INDEX   { cpqSeFixedDiskIndex }
        ::= { cpqSeFixedDiskTable 1 }

    CpqSeFixedDiskEntry ::= SEQUENCE {
        cpqSeFixedDiskIndex              INTEGER,
        cpqSeFixedDiskType               INTEGER,
        cpqSeFixedDiskCyls               INTEGER,
        cpqSeFixedDiskHeads              INTEGER,
        cpqSeFixedDiskSectors            INTEGER,
        cpqSeFixedDiskCapacity           INTEGER,
        cpqSeFixedDiskHwLocation         DisplayString
    }

    cpqSeFixedDiskIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "An index that uniquely specifies this entry.  Each possible
            index value indicates a specific drive as shown in the table
            below:

                fixedDiskIndex   IDE/ESDI Controller  Drive Unit
                =============   ===================  ==========
                    0               Primary             1
                    1               Primary             2
                    2               Secondary           1
                    3               Secondary           2

            Any other index value would be implementation specific."
        ::= { cpqSeFixedDiskEntry 1 }

    cpqSeFixedDiskType OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The drive type."
        ::= { cpqSeFixedDiskEntry 2 }

    cpqSeFixedDiskCyls OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The number of cylinders on the drive."
        ::= { cpqSeFixedDiskEntry 3 }

    cpqSeFixedDiskHeads OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The number of heads on the drive."
        ::= { cpqSeFixedDiskEntry 4 }

    cpqSeFixedDiskSectors OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The number of sectors per track on the drive."
        ::= { cpqSeFixedDiskEntry 5 }

    cpqSeFixedDiskCapacity OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The capacity of the drive in megabytes."
        ::= { cpqSeFixedDiskEntry 6 }

    cpqSeFixedDiskHwLocation  OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "A text description of the hardware location, on complex
             multi SBB hardware only, for the fixed disk.
             A NULL string indicates that the hardware location could not
             be determined or is irrelevant."
        ::= { cpqSeFixedDiskEntry 7 }

-- ****************************************************************************
--   Standard Equipment PCI Group
--   ============================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--        cpqSePci Group               (1.3.6.1.4.1.232.1.2.13)
--
--
--      The PCI group provides a set of tables and variables that detail the
--      configuration information about the PCI bus architecture.  The
--      Peripheral Component Interconnect (PCI)  local bus is a 32 or 64-bit
--      high performance bus intended to be  used to interconnect highly
--      integrated peripheral controller components, peripheral add-in boards,
--      and processor/memory sub-systems.
--
--      Implementation of the cpqSePci group is optional.
--      Support for the cpqSePci group is MANDATORY for all systems that
--      contain a PCI bus.
-- ****************************************************************************



-- ****************************************************************************
--   Standard Equipment PCI Slot Table
--   =================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--        cpqSePci Group               (1.3.6.1.4.1.232.1.2.13)
--         cpqSePciSlotTable           (1.3.6.1.4.1.232.1.2.13.1)
--
-- ****************************************************************************

    cpqSePciSlotTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSePciSlotEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A list of PCI slot information entries."
        ::= { cpqSePci 1}

    cpqSePciSlotEntry OBJECT-TYPE
        SYNTAX  CpqSePciSlotEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A description of a PCI slot."
        INDEX   { cpqSePciSlotBusNumberIndex , cpqSePciSlotDeviceNumberIndex}
        ::= { cpqSePciSlotTable 1 }

    CpqSePciSlotEntry ::= SEQUENCE {
        cpqSePciSlotBusNumberIndex      INTEGER,
        cpqSePciSlotDeviceNumberIndex   INTEGER,
        cpqSePciPhysSlot                INTEGER,
        cpqSePciSlotSubSystemID         DisplayString,
        cpqSePciSlotBoardName           DisplayString,
        cpqSePciSlotWidth               INTEGER,
        cpqSePciSlotSpeed               INTEGER,
        cpqSePciSlotExtendedInfo        INTEGER,
        cpqSePciSlotType                INTEGER,
        cpqSePciSlotCurrentMode         INTEGER,
        cpqSePciMaxSlotSpeed            INTEGER,
        cpqSePciXMaxSlotSpeed           INTEGER,
        cpqSePciCurrentSlotSpeed        INTEGER,
        cpqSePciHwLocation              DisplayString,
        cpqSePciSlotIOCTablePtr         INTEGER,
        cpqSePciSlotHeaderType          INTEGER,
        cpqSePciIsSlot0Embedded         INTEGER
    }

    cpqSePciSlotBusNumberIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The PCI  bus number for this device."
        ::= { cpqSePciSlotEntry 1 }

    cpqSePciSlotDeviceNumberIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number that uniquely identifies this device on its PCI bus."
        ::= { cpqSePciSlotEntry 2 }

    cpqSePciPhysSlot OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The physical PCI slot number of this device.  Embedded devices
               will return 0 for this variable."
        ::= { cpqSePciSlotEntry 3 }

    cpqSePciSlotSubSystemID OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (7))
        ACCESS  read-only
        STATUS  mandatory 
        DESCRIPTION
            "Uniquely identifies the board configured in this slot. A zero
            length ID indicates the Subsystem ID is not supported and the
            (Device ID/Vendor ID) should be used for identification purposes.
            An ID of all 0xFFh indicates an empty slot."
        ::= { cpqSePciSlotEntry 4 }

    cpqSePciSlotBoardName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The product name (or other suitable description) of this PCI
             board. This field may be empty if no descriptive information
             is known about the board."
        ::= { cpqSePciSlotEntry 5 }

    cpqSePciSlotWidth OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            unknown(2),
            thirtyTwoBit(3),
            sixtyFourBit(4),
            oneTwentyEightBit(5),
            x1(6),
            x2(7),
            x4(8),
            x8(9),
            x12(10),
            x16(11),
            x32(12)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The maximum data width supported by this PCI slot."
        ::= { cpqSePciSlotEntry 6 }

    cpqSePciSlotSpeed OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            unknown(2),
            thirtyThreeMHz(3),
            sixtySixMHz(4)
            }
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The maximum speed supported by this PCI slot."
        ::= { cpqSePciSlotEntry 7 }

    cpqSePciSlotExtendedInfo OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The PCI Extended Slot Information.

            This is a set of flags indicating extended features for the
            PCI slot.  Each bit has the following meaning when it is
            set (1):

                Bit  0:     Extended SCSI PCI Slot
                Bit  1:     PCI-X capable
                Bits 2-31:  reserved (set to 0)

            NOTE:   bit 31 is the most significant bit, bit 0 is the least
                    significant."
        ::= { cpqSePciSlotEntry 8 }

    cpqSePciSlotType OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            unknown(2),
            pci(3),
            pci66(4),
            pcix(5),
            pciexpress(6)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The type of PCI the slot.

            This indicates the capability of the slot, not the currently
            operating mode."
        ::= { cpqSePciSlotEntry 9 }

    cpqSePciSlotCurrentMode OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            unknown(2),
            pci(3),
            pci66(4),
            pcix(5)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The current operating mode of PCI/PCI-X slot.

            This indicates the current operating mode of the device in the
            slot.  If the slot is empty, this value would be unknown."
        ::= { cpqSePciSlotEntry 10 }

    cpqSePciMaxSlotSpeed OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The maximum speed in megahertz supported by this PCI slot.  If
            the slot also supports PCI-X, this value indicates the maximum
            speed of the slot when a non-PCI-X adapter is used.

            An entry of 0 indicates the speed is unknown."
        ::= { cpqSePciSlotEntry 11 }

    cpqSePciXMaxSlotSpeed OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The maximum speed in megahertz supported by this PCI-X slot.

            An entry of 0 indicates the speed is unknown.  An entry
            of -1 indicates the slot does not support PCI-X."
        ::= { cpqSePciSlotEntry 12 }

    cpqSePciCurrentSlotSpeed OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The current speed in megahertz of the adapter in this PCI
            or PCI-X slot.

            An entry of 0 indicates the speed is could not be determined or
            the slot is empty."
        ::= { cpqSePciSlotEntry 13 }

    cpqSePciHwLocation  OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "A text description of the hardware location, on complex
             multi SBB hardware only, for the Peripheral Component
             Interconnect (PCI)  bus.
             A NULL string indicates that the hardware location could not
             be determined or is irrelevant."
        ::= { cpqSePciSlotEntry 14 }

    cpqSePciSlotIOCTablePtr OBJECT-TYPE
        SYNTAX  INTEGER(0..19)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Index for the I/O Chassis in cpqSePCISlotIOCTablePtr where this PCI slot is physically located."
        ::= { cpqSePciSlotEntry 15 }

    cpqSePciSlotHeaderType OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This represents header type byte of a PCI device"
        ::= { cpqSePciSlotEntry 16 }

    cpqSePciIsSlot0Embedded OBJECT-TYPE
        SYNTAX  INTEGER {
            true(1),
            false(2)
        }
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This OID indicates whether PCI slot 0 is embedded in the machine or not."
        ::= { cpqSePciSlotEntry 17 }


-- ****************************************************************************
--   Standard Equipment PCI Function Table
--   =====================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--        cpqSePci Group               (1.3.6.1.4.1.232.1.2.13)
--         cpqSePciFunctTable          (1.3.6.1.4.1.232.1.2.13.2)
--
-- ****************************************************************************

    cpqSePciFunctTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSePciFunctEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A list of PCI function information entries."
        ::= { cpqSePci 2}

    cpqSePciFunctEntry OBJECT-TYPE
        SYNTAX  CpqSePciFunctEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A description of the functions in each PCI slot."
        INDEX   { cpqSePciFunctBusNumberIndex, cpqSePciFunctDeviceNumberIndex,
                  cpqSePciFunctIndex  }
        ::= { cpqSePciFunctTable 1 }

    CpqSePciFunctEntry ::= SEQUENCE {
        cpqSePciFunctBusNumberIndex     INTEGER,
        cpqSePciFunctDeviceNumberIndex  INTEGER,
        cpqSePciFunctIndex              INTEGER,
        cpqSePciFunctClassCode          OCTET STRING,
        cpqSePciFunctClassDescription   DisplayString,
        cpqSePciFunctDeviceID           INTEGER,
        cpqSePciFunctVendorID           INTEGER,
        cpqSePciFunctRevID              INTEGER,
        cpqSePciFunctIntLine            INTEGER,
        cpqSePciFunctDevStatus          INTEGER,
        cpqSePciFunctHwLocation         DisplayString
    }

    cpqSePciFunctBusNumberIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The PCI  bus number for this device function."
        ::= { cpqSePciFunctEntry 1 }

    cpqSePciFunctDeviceNumberIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The device index for this function."
        ::= { cpqSePciFunctEntry 2 }

    cpqSePciFunctIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..7)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
             " The unique index that specifies this function."
        ::= { cpqSePciFunctEntry 3 }

 
    cpqSePciFunctClassCode OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE(0..3))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The class code register as defined in the PCI Local
             Bus Specification in the following format:
                      Octet        Register
                      -----        --------
                        1          Programming Interface
                        2          Sub-class code
                        3          Base class code"
        ::= { cpqSePciFunctEntry 4 }

    cpqSePciFunctClassDescription OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(0..80))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A text string which describes the PCI Base Class and
             Sub Class to which this device belongs. This field
             may empty if no descriptive information is known about
             this function's class."
        ::= { cpqSePciFunctEntry 5 }

    cpqSePciFunctDeviceID OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This variable identifies this particular device.  This
             identifier is allocated by the component manufacturer."
        ::= { cpqSePciFunctEntry 6 }

    cpqSePciFunctVendorID OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This variable identifies the component manufacturer.  Valid
             identifiers are assigned by the PCI SIG."
        ::= { cpqSePciFunctEntry 7 }

    cpqSePciFunctRevID OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This variable is a vendor defined extension to the device ID and
              specifies a device specific revision identifier."
        ::= { cpqSePciFunctEntry 8}

    cpqSePciFunctIntLine OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
           "This variable specifies which input of the system interrupt
            controller(s) the device's interrupt pin is connected to.
            A value of 0ffh means unknown or no connection."
        ::= { cpqSePciFunctEntry 9}

    cpqSePciFunctDevStatus OBJECT-TYPE
        SYNTAX  INTEGER {
                unknown(1),
                enabled(2),
                disabled(3)
                }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
             "The status of the device described by this function.
              Some PCI devices, such as embedded devices, have the
              potential of being present but disabled. "
        ::= { cpqSePciFunctEntry 10 }

    cpqSePciFunctHwLocation  OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "A text description of the hardware location, on complex 
             multi SBB hardware only, for the Peripheral Component
             Interconnect (PCI)  bus.
             A NULL string indicates that the hardware location could not
             be determined or is irrelevant."
        ::= { cpqSePciFunctEntry 11 }

-- ****************************************************************************
--   Standard Equipment PCI Base Memory Table
--   ============================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--        cpqSePci Group               (1.3.6.1.4.1.232.1.2.13)
--         cpqSePciMemoryTable         (1.3.6.1.4.1.232.1.2.13.3)
--
-- ****************************************************************************
    cpqSePciMemoryTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSePciMemoryEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A list of PCI base memory entries"
        ::= { cpqSePci 3}

    cpqSePciMemoryEntry OBJECT-TYPE
        SYNTAX  CpqSePciMemoryEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A description of the base memory usage in each function"
        INDEX   { cpqSePciMemoryBusNumberIndex, cpqSePciMemoryDeviceNumberIndex,
                  cpqSePciMemoryFunctionIndex,  cpqSePciMemoryIndex  }
        ::= { cpqSePciMemoryTable 1 }

    CpqSePciMemoryEntry ::= SEQUENCE {
        cpqSePciMemoryBusNumberIndex     INTEGER,
        cpqSePciMemoryDeviceNumberIndex  INTEGER,
        cpqSePciMemoryFunctionIndex      INTEGER,
        cpqSePciMemoryIndex              INTEGER,
        cpqSePciMemoryBaseAddr           INTEGER,
        cpqSePciMemoryType               INTEGER,
        cpqSePciMemorySize               INTEGER,
        cpqSePciMemoryHwLocation         DisplayString
    }

    cpqSePciMemoryBusNumberIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The PCI  bus number for this memory entry."
        ::= { cpqSePciMemoryEntry 1 }

    cpqSePciMemoryDeviceNumberIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The device index for this memory entry"
        ::= { cpqSePciMemoryEntry 2 }

    cpqSePciMemoryFunctionIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..7) 
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
             " The unique index that specifies the function associated
               with this memory entry."
        ::= { cpqSePciMemoryEntry 3 }

    cpqSePciMemoryIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..6)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
             " The unique index that specifies this memory entry. "
        ::= { cpqSePciMemoryEntry 4 }

    cpqSePciMemoryBaseAddr OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
             "Base address of this memory usage entry."
        ::= { cpqSePciMemoryEntry 5 }

    cpqSePciMemoryType OBJECT-TYPE
        SYNTAX  INTEGER {
                unknown(1),
                io(2),
                memory-mapped(3),
                exp-rom(4)
                }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
             "The type of memory this entry describes.  This variable
              is used to determine if this memory entry maps into
              memory, expansion rom or I/O space."
        ::= { cpqSePciMemoryEntry 6 }

    cpqSePciMemorySize OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
             "This variable specifies how much address space this function
              requires.  A value of 0 will be returned if the agent cannot
              obtain this information."
        ::= { cpqSePciMemoryEntry 7 }

    cpqSePciMemoryHwLocation  OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "A text description of the hardware location, on complex
             multi SBB hardware only, for the Peripheral Component
             Interconnect (PCI)  bus.
             A NULL string indicates that the hardware location could not
             be determined or is irrelevant."
        ::= { cpqSePciMemoryEntry 8 }

-- ****************************************************************************
-- Standard Equipment PC Card Group
-- ========================================
--
-- The compaq enterprise            (1.3.6.1.4.1.232)
--      cpqStdEquipment Group       (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group       (1.3.6.1.4.1.232.1.2)
--        cpqSePCCard Group         (1.3.6.1.4.1.232.1.2.14)
--         cpqSePCCardSlotTable     (1.3.6.1.4.1.232.1.2.14.1)
--
--  The PC Card Group provides a set of tables and variables that detail the
--  configuration information about the PC Card slot architecture. The PC
--  Card Slots are connected via a dedicated bridge off the PCI local bus
--  which allows 16-bit and/or 32-bit expansion slots.
--
--  Implementation of the cpqSePCCard group is optional for desktop and
--  server platforms but mandatory for portables.
-- ****************************************************************************

    cpqSePCCardSlotTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSePCCardSlotEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A list of PC Card slot information entries."
      ::= { cpqSePCCard 1}

    cpqSePCCardSlotEntry OBJECT-TYPE
        SYNTAX  CpqSePCCardSlotEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A PC Card slot description table entry.
             A table entry is defined for each PC Card Slot in the
             current system configuration."
        INDEX   { cpqSePCCardSlotIndex}
        ::= { cpqSePCCardSlotTable 1 }

    CpqSePCCardSlotEntry ::= SEQUENCE {
            cpqSePCCardSlotIndex            INTEGER,
            cpqSePCCardCondition            INTEGER,
            cpqSePCCardPhysLocation         DisplayString,
            cpqSePCCardSlotType             INTEGER,
            cpqSePCCardSlotWidth            INTEGER,
            cpqSePCCardSlotThermalCapacity  INTEGER,
            cpqSePCCardSlotThermalSensor    INTEGER,
            cpqSePCCardSlotPowerState       INTEGER,
            cpqSePCCardStatus               INTEGER,
            cpqSePCCardDeviceInfo           DisplayString,
            cpqSePCCardProductInfo          DisplayString,
            cpqSePCCardSerialNumber         DisplayString,
            cpqSePCCardAssetTag             DisplayString
        }

    cpqSePCCardSlotIndex OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Defines the logical PC Card slot number for this PC Card Slot.
            In addition, the slot number serves as the index into the
            PC Card data table.  Typical index ranges will be either 1 to
            4 (for 4 slots) or 1 to 2 (for 2 slots).  (Un)Docking may
            cause the supported index range to change dynamically."
        ::= { cpqSePCCardSlotEntry 1 }

    cpqSePCCardCondition OBJECT-TYPE
        SYNTAX  INTEGER {
            unknown(1),
            ok(2),
            degraded(3),
            failed(4)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Defines the overall condition of the PC Card.
            The supported values are defined as follows:

               unknown(1)
                    The current condition is unknown for the PC Card or PC Card Slot.

               ok(2)
                    PC Card operations are normal.
                    No user action required.

               degraded (3)
                    PC Card operations have degraded.
                    Consult the cpqSePCCardStatus field for recommended actions.

               failed (4)
                    PC Card operations have failed.
                    Consult the cpqSePCCardStatus field for recommended actions."
        ::= { cpqSePCCardSlotEntry 2 }


    cpqSePCCardPhysLocation OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(0..40))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Defines the user level PC Card Slot location description.
            Text strings supported are:
                - System Unit Top Slot,
                - System Unit Bottom Slot,
                - Docking Station Top Slot,
                - Docking Station Bottom Slot."
        ::= { cpqSePCCardSlotEntry 3 }

    cpqSePCCardSlotType OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Defines the PC Card Slot capabilities.
            This is a bit mapped value defined by DMI Mobile Supplement for the System Slots Group,
            Slot Type. Bits of interest for PC Card support are:
                Bit 6 - PCMCIA slot (if set),
                Bit 13 - 16 bit PC Card capable (if set),
                Bit 14 - CardBus PC Card capable (if set),
                Bit 15 - ZV Port capable (if set),
                Bit 16 - Modem Ring Resume capable (if set), 
            All other bits should be zero (reset) for PC Card slots."
        ::= { cpqSePCCardSlotEntry 4 }

    cpqSePCCardSlotWidth OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            unknown(2),
            width8bit(3),
            width16bit(4),
            width32bit(5),
            width64bit(6),
            width128bit(7)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Defines the maximum bus width for this PC Card Slot.
            The supported values are defined as follows:

                Other (1)
                    Value is not in defined list.

                Unknown (2)
                    Actual value is not known.

                width 8 bit (3)
                    Bus is 8 bits wide.

                width 16 bit (4)
                    Bus is 16 bits wide.

                width 32 bit (5)
                    Bus is 32 bits wide.

                width 64 bit (6)
                    Bus is 64 bits wide.

                width 128 bit (7)
                    Bus is 128 bits wide."
        ::= { cpqSePCCardSlotEntry 5 }


    cpqSePCCardSlotThermalCapacity OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Defines the maximum thermal dissipation capacity (milliwatts)
            for this PC Card Slot.  A value of zero indicates the thermal
            capacity is unknown.  A non-zero value indicates the thermal
            capacity in milliwatts."
        ::= { cpqSePCCardSlotEntry 6 }

    cpqSePCCardSlotThermalSensor OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Defines the Thermal Sensor ID that monitors this PC Card Slot.
            A value of zero indicates that a sensor is not present or
            unknown for this slot.  A non-zero value indicates the sensor
            ID as defined by the platform firmware."
        ::= { cpqSePCCardSlotEntry 7 }

    cpqSePCCardSlotPowerState OBJECT-TYPE
        SYNTAX  INTEGER {
            unknown(1),
            on(2),
            off(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Defines the current power state (On/Off) for this PC Card Slot.
            The supported values are defined as follows:

                unknown (1)
                  Current power state is unknown.

                on (2)
                  Power is currently on.

                off (3)
                  Power is currently off."
        ::= { cpqSePCCardSlotEntry 8 }

    cpqSePCCardStatus OBJECT-TYPE
        SYNTAX  INTEGER {
            unknown(1),
            ok(2),
            thermalDegraded(3),
            thermalFailure(4)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Defines the operating status for the card in this PC Card Slot.
            The supported values are defined as follows:

                unknown (1)
                    The current status is not known for the PC Card or
                    PC Card Slot.

                ok (2)
                    PC Card operations are normal.
                    No user action required.

                thermalDegraded (3)
                    PC Card operations have degraded due to unsafe thermal
                    conditions.
                    Recommended Actions include: 
                        Discontinue the use of the PC Card as soon as
                        possible.  If a Modem or LAN card then close
                        all communication applications/links.   If a
                        Memory, ATA, or SCSI device then close all
                        open/related files.  Remove PC Card from slot
                        after use is discontinued, if possible.

                thermalFailure (4)
                    PC Card operations have failed due to unsafe thermal
                    conditions.  The PC Card will automatically be powered
                    off to protect itself and the system.
                    Recommended Actions include:
                        Discontinue the use of the PC Card immediately.
                        If a Modem or LAN card then close all communication applications/links.
                        If a Memory, ATA, or SCSI device then close all open/related files.
                        Remove PC Card from slot after use is discontinued, if possible."
        ::= { cpqSePCCardSlotEntry 9 }

    cpqSePCCardDeviceInfo OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(0..80))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Defines the PC Card Manufacturer / Device information for
            the card in this PC Card Slot.  The returned string data is
            read from the PC Card's onboard Card Information Structure
            (CIS)."
      ::= { cpqSePCCardSlotEntry 10 }

    cpqSePCCardProductInfo OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(0..80))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Defines the PC Card Model / Part Number information for
            the card in this PC Card Slot.  The returned string data
            is read from the PC Card's onboard Card Information
            Structure (CIS)."
        ::= { cpqSePCCardSlotEntry 11 }

    cpqSePCCardSerialNumber OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(0..80))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Defines the PC Card Serial Number information for the
            card in this PC Card Slot.   The returned string data is
            read from the PC Card's onboard Card Information Structure
            (CIS)."
        ::= { cpqSePCCardSlotEntry 12 }

    cpqSePCCardAssetTag OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(0..80))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Defines the PC Card Asset Tag information for the card in
            this PC Card Slot.   The returned string data is read from
            the PC Card's onboard Card Information Structure (CIS)."
        ::= { cpqSePCCardSlotEntry 13 }

-- ****************************************************************************
--   Standard Equipment USB Port Table
--   ====================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--        cpqSeUSBPort Group           (1.3.6.1.4.1.232.1.2.15)
--         cpqSeUSBPortTable           (1.3.6.1.4.1.232.1.2.15.1)
--
--      The cpqSeUSBPort group lists the USB ports in the system.
--
--      Implementation of the cpqSeUSBPort group is optional.
--      Support for the cpqSeUSBPort group is MANDATORY for all systems that
--      contain a USB bus.
--
-- ****************************************************************************

    cpqSeUSBPortTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSeUSBPortEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A table of USB port descriptions."
        ::= { cpqSeUSBPort 1 }

    cpqSeUSBPortEntry OBJECT-TYPE
        SYNTAX  CpqSeUSBPortEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A description of a USB port."
        INDEX   { cpqSeUSBPortIndex }
        ::= { cpqSeUSBPortTable 1 }

    CpqSeUSBPortEntry ::= SEQUENCE {
        cpqSeUSBPortIndex       INTEGER,
        cpqSeUSBPortType        INTEGER,
        cpqSeUSBPortHwLocation  DisplayString
    }

    cpqSeUSBPortIndex OBJECT-TYPE
        SYNTAX  INTEGER (1..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "An index that uniquely specifies this entry."
        ::= { cpqSeUSBPortEntry 1 }


    cpqSeUSBPortType OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            usbPort(2)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The port type.
             The supported values are defined as follows:

             other (1)
                 USB port data is not available.

             usbPort (2)
                 The port is a USB Port."
        ::= { cpqSeUSBPortEntry 2 }

    cpqSeUSBPortHwLocation  OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "A text description of the hardware location, on complex
             multi SBB hardware only, for the USB port.
             A NULL string indicates that the hardware location could not
             be determined or is irrelevant."
        ::= { cpqSeUSBPortEntry 3 }

-- ****************************************************************************
--   Standard Equipment Cell Table
--   =============================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--        cpqSeCell                    (1.3.6.1.4.1.232.1.2.16)
--
--      A cell is equivalent to a single board computer.
--
--
-- ****************************************************************************

    cpqSeCellTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSeCellEntry
        ACCESS  not-accessible
        STATUS  optional
        DESCRIPTION
            "A list of cells in the partition."
        ::= { cpqSeCell 1 }

    cpqSeCellEntry OBJECT-TYPE
        SYNTAX  CpqSeCellEntry
        ACCESS  not-accessible
        STATUS  optional
        DESCRIPTION
            "A description of a cell in the system."
        INDEX   { cpqSeCellUnitIndex }
        ::= { cpqSeCellTable 1 }

    CpqSeCellEntry ::= SEQUENCE {
        cpqSeCellUnitIndex                   INTEGER,
        cpqSeCellCabinetNumber               INTEGER,
        cpqSeCellCellNumber                  INTEGER,
        cpqSeCellIOCTablePtr                 INTEGER,
        cpqSeCellPDHCFirmwareRevision        DisplayString,
        cpqSeCellSysFwVersion                DisplayString,
        cpqSeCellBootInhibited               TruthValue,
        cpqSeCellToScanBusConnectionStatus   INTEGER,
        cpqSeCellHasCoreIO                   TruthValue,
        cpqSeCellBoardSpeed                  INTEGER,
        cpqSeCellPresent                     TruthValue,
        cpqSeCellHasPower                    TruthValue,
        cpqSeCellReadyForReconfig            TruthValue,
        cpqSeCellTotalMemory                 INTEGER,
        cpqSeCellLEDState                    INTEGER, 
        cpqSeCellState                       INTEGER,
        cpqSeCellCLMRequestPercentage        INTEGER,
        cpqSeCellCLMRequestSize              INTEGER,
        cpqSeCellCLMAllocatedSize            INTEGER,
        cpqSeCellInterleaveAllocatedSize     INTEGER,
        cpqSeCellHasInterleaveMem            INTEGER,
        cpqSeCellSerialNumber                DisplayString,
        cpqSeCellCLMCondition                INTEGER
    }

    cpqSeCellUnitIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..15)
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This is a number that uniquely specifies the cell."
        ::= { cpqSeCellEntry 1 }

    cpqSeCellCabinetNumber OBJECT-TYPE
        SYNTAX  INTEGER (0..1)
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This value represents the cabinet that the cell belongs to."
        ::= { cpqSeCellEntry 2 }

    cpqSeCellCellNumber OBJECT-TYPE
        SYNTAX  INTEGER (0..7)
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This value is cell/slot number that is unique across the cabinet."
        ::= { cpqSeCellEntry 3 }

    cpqSeCellIOCTablePtr OBJECT-TYPE
        SYNTAX  INTEGER (0..19)
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "Table index for the I/O chassis which is connected to this cell."
        ::= { cpqSeCellEntry 4 }

    cpqSeCellPDHCFirmwareRevision OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "HP SAL Revision"
        ::= { cpqSeCellEntry 5 }

    cpqSeCellSysFwVersion OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This is the revision of system firmware on the cell board"
        ::= { cpqSeCellEntry 6 }

    cpqSeCellBootInhibited OBJECT-TYPE
        SYNTAX  TruthValue
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This value indicates whether the cell is active."
        ::= { cpqSeCellEntry 7 }

    cpqSeCellToScanBusConnectionStatus OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This bitmap represents the state of cell to scan 
               bus connection/RIO cable state.

             if bit 6 is set to 1, Cable port swapped.
             if bit 5 is set to 1, Cable ID mismatched.
             if bit 4 is set to 1, Output Cable parity error.
             if bit 3 is set to 1, Output Cable detached.
             if bit 2 is set to 1, Input Cable parity error.
             if bit 1 is set to 1, Input Cable detached.
             if bit 0 is set to 1, Connection valid."
        ::= { cpqSeCellEntry 8 }

    cpqSeCellHasCoreIO OBJECT-TYPE
        SYNTAX  TruthValue
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This value indicates whether the cell has core I/O attached to it."
        ::= { cpqSeCellEntry 9 }

    cpqSeCellBoardSpeed  OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This value represents the speed of the cell board/FSB ratio"
        ::= { cpqSeCellEntry 10 }

    cpqSeCellPresent OBJECT-TYPE
        SYNTAX  TruthValue
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This value represents whether there is a cell in the slot"
        ::= { cpqSeCellEntry 11 }

    cpqSeCellHasPower OBJECT-TYPE
        SYNTAX  TruthValue
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This value represents whether the cell has power"
        ::= { cpqSeCellEntry 12 }

    cpqSeCellReadyForReconfig OBJECT-TYPE
        SYNTAX  TruthValue
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This value represents whether the cell is ready for reconfiguration"
        ::= { cpqSeCellEntry 13 }

    cpqSeCellTotalMemory OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This value represents total memory in the cell"
        ::= { cpqSeCellEntry 14 }

    cpqSeCellLEDState OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-write
        STATUS  optional
        DESCRIPTION
            "This value represents state of the cell LED.
             This is a bit-mapped value defined as follows.
             Bit 31..30 = 00, LED 3 is Off
                        = 01, LED 3 is On
                        = 10, LED 3 is Blinking
                        = 11, For LED 3 future use

             Bit 29..27 = 000, LED 3 is Red
                        = 001, LED 3 is Yellow
                        = 010, LED 3 is Green
                        = 011, LED 3 is Blue
                        = 100, For LED 3 future use
                        = 101, For LED 3 future use
                        = 110, For LED 3 future use
                        = 111, For LED 3 future use

             Bit 26..24 = 000, LED 3 indicates Power
                        = 001, LED 3 indicates Run
                        = 010, LED 3 indicates Attention
                        = 011, LED 3 indicates Fault
                        = 100, For LED 3 future use
                        = 101, For LED 3 future use
                        = 110, For LED 3 future use
                        = 111, For LED 3 future use

             Bit 23..22 = 00, LED 2 is Off
                        = 01, LED 2 is On
                        = 10, LED 2 is Blinking
                        = 11, For LED 2 future use

             Bit 21..19 = 000, LED 2 is Red
                        = 001, LED 2 is Yellow
                        = 010, LED 2 is Green
                        = 011, LED 2 is Blue
                        = 100, For LED 2 future use
                        = 101, For LED 2 future use
                        = 110, For LED 2 future use
                        = 111, For LED 2 future use

             Bit 18..16 = 000, LED 2 indicates Power
                        = 001, LED 2 indicates Run
                        = 010, LED 2 indicates Attention
                        = 011, LED 2 indicates Fault
                        = 100, For LED 2 future use
                        = 101, For LED 2 future use
                        = 110, For LED 2 future use
                        = 111, For LED 2 future use

             Bit 15..14 = 00, LED 1 is Off
                        = 01, LED 1 is On
                        = 10, LED 1 is Blinking
                        = 11, For LED 1 future use

             Bit 13..11 = 000, LED 1 is Red
                        = 001, LED 1 is Yellow
                        = 010, LED 1 is Green
                        = 011, LED 1 is Blue
                        = 100, For LED 1 future use
                        = 101, For LED 1 future use
                        = 110, For LED 1 future use
                        = 111, For LED 1 future use

             Bit 10..8  = 000, LED 1 indicates Power
                        = 001, LED 1 indicates Run
                        = 010, LED 1 indicates Attention
                        = 011, LED 1 indicates Fault
                        = 100, For LED 1 future use
                        = 101, For LED 1 future use
                        = 110, For LED 1 future use
                        = 111, For LED 1 future use

             Bit 7..6   = 00, LED 0 is Off
                        = 01, LED 0 is On
                        = 10, LED 0 is Blinking
                        = 11, For LED 0 future use

             Bit 5..3   = 000, LED 0 is Red
                        = 001, LED 0 is Yellow
                        = 010, LED 0 is Green
                        = 011, LED 0 is Blue
                        = 100, For LED 0 future use
                        = 101, For LED 0 future use
                        = 110, For LED 0 future use
                        = 111, For LED 0 future use

             Bit 2..0   = 000, LED 0 indicates Power
                        = 001, LED 0 indicates Run
                        = 010, LED 0 indicates Attention
                        = 011, LED 0 indicates Fault
                        = 100, For LED 0 future use
                        = 101, For LED 0 future use
                        = 110, For LED 0 future use
                        = 111, For LED 0 future use "
        ::= { cpqSeCellEntry 15 }

    cpqSeCellState OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-write
        STATUS  optional
        DESCRIPTION
            "This value represents state of the cell"
        ::= { cpqSeCellEntry 16 }

    cpqSeCellCLMRequestPercentage OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional 
        DESCRIPTION
            "The requested percentage of CLM memory to be configured in the cell."
        ::= { cpqSeCellEntry 17 }

    cpqSeCellCLMRequestSize OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "The size of requested CLM memory in the cell in kilobytes."
        ::= { cpqSeCellEntry 18 }

    cpqSeCellCLMAllocatedSize OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "The size of allocated CLM memory in the cell in kilobytes."
        ::= { cpqSeCellEntry 19 }

    cpqSeCellInterleaveAllocatedSize OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "The size of allocated interleaved memory in the cell
             in kilobytes."
        ::= { cpqSeCellEntry 20 }

    cpqSeCellHasInterleaveMem OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "When set indicates that there is an interleaved memory
             configured in the cell."
        ::= { cpqSeCellEntry 21 }

    cpqSeCellSerialNumber OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This is the cell board serial number."
        ::= { cpqSeCellEntry 22 }

    cpqSeCellCLMCondition OBJECT-TYPE
        SYNTAX  INTEGER {
            unknown(1),
            ok(2),
            degraded(3),
            failed(4)
            }
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
             "The CLM (Cell Local Memory) settings condition of this cell."
       ::= { cpqSeCellEntry 23 }


-- ****************************************************************************
--   Standard Equipment I/O Chassis Table
--   ==================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--         cpqSeIOCTable               (1.3.6.1.4.1.232.1.2.17)
--
--      An I/O chassis contains PCI devices on the system
--
--
-- ****************************************************************************

    cpqSeIOCTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSeIOCEntry
        ACCESS  not-accessible
        STATUS  optional
        DESCRIPTION
            "A list of I/O chassis in the partition."
        ::= { cpqSeIOC 1 }

    cpqSeIOCEntry OBJECT-TYPE
        SYNTAX  CpqSeIOCEntry
        ACCESS  not-accessible
        STATUS  optional
        DESCRIPTION
            "A description of an I/O chassis in the system."
        INDEX   { cpqSeIOCUnitIndex }
        ::= { cpqSeIOCTable 1 }

    CpqSeIOCEntry ::= SEQUENCE {
        cpqSeIOCUnitIndex           INTEGER,
        cpqSeIOCCabinetNumber       INTEGER,
        cpqSeIOCBayNumber           INTEGER,
        cpqSeIOCIOCNumber           INTEGER,
        cpqSeIOCPowerState          INTEGER,
        cpqSeIOCLEDState            INTEGER
    }

    cpqSeIOCUnitIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..19)
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This is a number that uniquely specifies the I/O chassis."
        ::= { cpqSeIOCEntry 1 }

    cpqSeIOCCabinetNumber OBJECT-TYPE
        SYNTAX  INTEGER (0..3)
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This value represents the cabinet that the I/O chassis belongs to."
        ::= { cpqSeIOCEntry 2 }

    cpqSeIOCBayNumber OBJECT-TYPE
        SYNTAX  INTEGER (0..2)
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This value indicates the bay in the cabinet where the I/O chassis resides."
        ::= { cpqSeIOCEntry 3 }

    cpqSeIOCIOCNumber OBJECT-TYPE
        SYNTAX  INTEGER (0..1)
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This is the I/O chassis number that is unique across the bay."
        ::= { cpqSeIOCEntry 4 }

    cpqSeIOCPowerState OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This value indicates I/O chassis power state"
        ::= { cpqSeIOCEntry 5 }

    cpqSeIOCLEDState OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-write
        STATUS  optional
        DESCRIPTION
            "This value represents the state of a IO Chassis LED.
             This is a bit-mapped value defined as follows.
             Bit 31..30 = 00, LED 3 is Off
                        = 01, LED 3 is On
                        = 10, LED 3 is Blinking
                        = 11, For LED 3 future use

             Bit 29..27 = 000, LED 3 is Red
                        = 001, LED 3 is Yellow
                        = 010, LED 3 is Green
                        = 011, LED 3 is Blue
                        = 100, For LED 3 future use
                        = 101, For LED 3 future use
                        = 110, For LED 3 future use
                        = 111, For LED 3 future use

             Bit 26..24 = 000, LED 3 indicates Power
                        = 001, LED 3 indicates Run
                        = 010, LED 3 indicates Attention
                        = 011, LED 3 indicates Fault
                        = 100, For LED 3 future use
                        = 101, For LED 3 future use
                        = 110, For LED 3 future use
                        = 111, For LED 3 future use

             Bit 23..22 = 00, LED 2 is Off
                        = 01, LED 2 is On
                        = 10, LED 2 is Blinking
                        = 11, For LED 2 future use

             Bit 21..19 = 000, LED 2 is Red
                        = 001, LED 2 is Yellow
                        = 010, LED 2 is Green
                        = 011, LED 2 is Blue
                        = 100, For LED 2 future use
                        = 101, For LED 2 future use
                        = 110, For LED 2 future use
                        = 111, For LED 2 future use

             Bit 18..16 = 000, LED 2 indicates Power
                        = 001, LED 2 indicates Run
                        = 010, LED 2 indicates Attention
                        = 011, LED 2 indicates Fault
                        = 100, For LED 2 future use
                        = 101, For LED 2 future use
                        = 110, For LED 2 future use
                        = 111, For LED 2 future use

             Bit 15..14 = 00, LED 1 is Off
                        = 01, LED 1 is On
                        = 10, LED 1 is Blinking
                        = 11, For LED 1 future use

             Bit 13..11 = 000, LED 1 is Red
                        = 001, LED 1 is Yellow
                        = 010, LED 1 is Green
                        = 011, LED 1 is Blue
                        = 100, For LED 1 future use
                        = 101, For LED 1 future use
                        = 110, For LED 1 future use
                        = 111, For LED 1 future use

             Bit 10..8  = 000, LED 1 indicates Power
                        = 001, LED 1 indicates Run
                        = 010, LED 1 indicates Attention
                        = 011, LED 1 indicates Fault
                        = 100, For LED 1 future use
                        = 101, For LED 1 future use
                        = 110, For LED 1 future use
                        = 111, For LED 1 future use

             Bit 7..6   = 00, LED 0 is Off
                        = 01, LED 0 is On
                        = 10, LED 0 is Blinking
                        = 11, For LED 0 future use

             Bit 5..3   = 000, LED 0 is Red
                        = 001, LED 0 is Yellow
                        = 010, LED 0 is Green
                        = 011, LED 0 is Blue
                        = 100, For LED 0 future use
                        = 101, For LED 0 future use
                        = 110, For LED 0 future use
                        = 111, For LED 0 future use

             Bit 2..0   = 000, LED 0 indicates Power
                        = 001, LED 0 indicates Run
                        = 010, LED 0 indicates Attention
                        = 011, LED 0 indicates Fault
                        = 100, For LED 0 future use
                        = 101, For LED 0 future use
                        = 110, For LED 0 future use
                        = 111, For LED 0 future use "
        ::= { cpqSeIOCEntry 6 }

-- ****************************************************************************
--   Standard Equipment Partition Structure
--   ======================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--         cpqSePartition              (1.3.6.1.4.1.232.1.2.18)
--
--      A partition can have many cells spread across cabinets.
--
--
-- ****************************************************************************

    cpqSePartitionTotalCPU OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This is the number of logical CPUs in the partition. Zero will be returned
             if the value can not be determined."
        ::= { cpqSePartition 1 }

    cpqSePartitionAvailableCellSlots OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This is the number of available cell slots in the partition.
             Zero will be returned if the value can not be determined."
        ::= { cpqSePartition 2 }

    cpqSePartitionInstalledCells OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This is the number of installed cells in the partition. Zero
             will be returned if the value can not be determined."
        ::= { cpqSePartition 3 }

    cpqSePartitionPoweredOnCells OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This denotes the number of powered on cells in the partition.
             Zero will be returned if the value can not be determined."
        ::= { cpqSePartition 4 }

    cpqSePartitionReadyForReconfigCells OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This represents the cells that are ready for reconfiguration.
             Zero will be returned if the value can not be determined."
        ::= { cpqSePartition 5 }

    cpqSePartitionMemInterleavingType OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This represents memory interleaving type for the partition.
             Zero will be returned if the value can not be determined."
        ::= { cpqSePartition 6}

    cpqSePartitionName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This represents the partition name."
        ::= { cpqSePartition 7}

    cpqSePartitionCoreCell OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "Index to cpqSeCellTablePtr for core cell in the partition."
        ::= { cpqSePartition 8}

    cpqSePartitionCoreCellCabinet OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "Index to cpqSeCellTablePtr for core cell in the cabinet."
        ::= { cpqSePartition 9}

    cpqSePartitionCLMRequestPercentage OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "The requested percentage of CLM memory to be configured in the
             partition."
        ::= { cpqSePartition 10}

    cpqSePartitionCLMRequestSize OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "The size of requested CLM memory in the partition in kilobytes."
        ::= { cpqSePartition 11}

    cpqSePartitionCLMAllocatedSize OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "The size of allocated CLM memory in the partition in
             kilobytes."
        ::= { cpqSePartition 12}

    cpqSePartitionInterleaveAllocatedSize OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "The size of allocated interleaved memory in the partition
             in kilobytes."
        ::= { cpqSePartition 13}

    cpqSePartitionHasInterleaveMem OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "When set, it indicates that there is an interleaved memory
             configured in the partition."
        ::= { cpqSePartition 14}

    cpqSePartitionNumber OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This represents the logical partition number of the current
             partition in the complex."
        ::= { cpqSePartition 15}

-- ****************************************************************************
--   Standard Equipment Cabinet Table
--   =============================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--         cpqSeCabinetTable           (1.3.6.1.4.1.232.1.2.19)
--
--      A cabinet contains many cells and/or I/O chassis
--
--
-- ****************************************************************************

    cpqSeCabinetTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSeCabinetEntry
        ACCESS  not-accessible
        STATUS  optional
        DESCRIPTION
            "A list of cabinets that contain cells in the partition."
        ::= { cpqSeCabinet 1 }

    cpqSeCabinetEntry OBJECT-TYPE
        SYNTAX  CpqSeCabinetEntry
        ACCESS  not-accessible
        STATUS  optional
        DESCRIPTION
            "A description of a cabinet in the system."
        INDEX   { cpqSeCabinetUnitIndex }
        ::= { cpqSeCabinetTable 1 }

    CpqSeCabinetEntry ::= SEQUENCE {
        cpqSeCabinetUnitIndex    INTEGER,
        cpqSeCabinetCPULED       TruthValue,
        cpqSeCabinetIOXLED       TruthValue,
        cpqSeCabinetTypeNum      INTEGER,
        cpqSeCabinetLED          INTEGER
    }

    cpqSeCabinetUnitIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..3)
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This is a number that uniquely specifies the cabinet."
        ::= { cpqSeCabinetEntry 1 }

    cpqSeCabinetCPULED OBJECT-TYPE
        SYNTAX  TruthValue
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This value represents the on/off state of compute cabinet LED."
        ::= { cpqSeCabinetEntry 2 }

    cpqSeCabinetIOXLED OBJECT-TYPE
        SYNTAX  TruthValue
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This value represents the on/off state of IOX cabinet LED."
        ::= { cpqSeCabinetEntry 3 }

    cpqSeCabinetTypeNum OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This value represents type and number of a compute or IOX cabinet.
             Bit 31..16 = 0x0000, type of cabinet is Thin Boy
             Bit 31..16 = 0x0001, type of cabinet is Fat Boy
             Bit 31..16 = 0x0002, type of cabinet is Dome Lite
             Bit 31..16 = 0x0003, type of cabinet is Key Stone
             Bit 31..16 = 0x0004, type of cabinet is Matter Horn
             Bit 31..16 = 0x0080, type of cabinet is IOX
             Bit 15..0, represents the compute cabinet number."
        ::= { cpqSeCabinetEntry 4 }

    cpqSeCabinetLED OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-write
        STATUS  optional
        DESCRIPTION
            "This value represents the state of a cabinet LED.
             This is a bit-mapped value defined as follows.
             Bit 31..30 = 00, LED 3 is Off
                        = 01, LED 3 is On
                        = 10, LED 3 is Blinking
                        = 11, For LED 3 future use

             Bit 29..27 = 000, LED 3 is Red
                        = 001, LED 3 is Yellow
                        = 010, LED 3 is Green
                        = 011, LED 3 is Blue
                        = 100, For LED 3 future use
                        = 101, For LED 3 future use
                        = 110, For LED 3 future use
                        = 111, For LED 3 future use

             Bit 26..24 = 000, LED 3 indicates Power
                        = 001, LED 3 indicates Run
                        = 010, LED 3 indicates Attention
                        = 011, LED 3 indicates Fault
                        = 100, For LED 3 future use
                        = 101, For LED 3 future use
                        = 110, For LED 3 future use
                        = 111, For LED 3 future use

             Bit 23..22 = 00, LED 2 is Off
                        = 01, LED 2 is On
                        = 10, LED 2 is Blinking
                        = 11, For LED 2 future use

             Bit 21..19 = 000, LED 2 is Red
                        = 001, LED 2 is Yellow
                        = 010, LED 2 is Green
                        = 011, LED 2 is Blue
                        = 100, For LED 2 future use
                        = 101, For LED 2 future use
                        = 110, For LED 2 future use
                        = 111, For LED 2 future use

             Bit 18..16 = 000, LED 2 indicates Power
                        = 001, LED 2 indicates Run
                        = 010, LED 2 indicates Attention
                        = 011, LED 2 indicates Fault
                        = 100, For LED 2 future use
                        = 101, For LED 2 future use
                        = 110, For LED 2 future use
                        = 111, For LED 2 future use

             Bit 15..14 = 00, LED 1 is Off
                        = 01, LED 1 is On
                        = 10, LED 1 is Blinking
                        = 11, For LED 1 future use

             Bit 13..11 = 000, LED 1 is Red
                        = 001, LED 1 is Yellow
                        = 010, LED 1 is Green
                        = 011, LED 1 is Blue
                        = 100, For LED 1 future use
                        = 101, For LED 1 future use
                        = 110, For LED 1 future use
                        = 111, For LED 1 future use

             Bit 10..8  = 000, LED 1 indicates Power
                        = 001, LED 1 indicates Run
                        = 010, LED 1 indicates Attention
                        = 011, LED 1 indicates Fault
                        = 100, For LED 1 future use
                        = 101, For LED 1 future use
                        = 110, For LED 1 future use
                        = 111, For LED 1 future use

             Bit 7..6   = 00, LED 0 is Off
                        = 01, LED 0 is On
                        = 10, LED 0 is Blinking
                        = 11, For LED 0 future use

             Bit 5..3   = 000, LED 0 is Red
                        = 001, LED 0 is Yellow
                        = 010, LED 0 is Green
                        = 011, LED 0 is Blue
                        = 100, For LED 0 future use
                        = 101, For LED 0 future use
                        = 110, For LED 0 future use
                        = 111, For LED 0 future use

             Bit 2..0   = 000, LED 0 indicates Power
                        = 001, LED 0 indicates Run
                        = 010, LED 0 indicates Attention
                        = 011, LED 0 indicates Fault
                        = 100, For LED 0 future use
                        = 101, For LED 0 future use
                        = 110, For LED 0 future use
                        = 111, For LED 0 future use "
        ::= { cpqSeCabinetEntry 5 }

-- ****************************************************************************
--   Standard Equipment Complex Structure
--   ====================================
--
-- The compaq enterprise                             (1.3.6.1.4.1.232)
--      cpqStdEquipment Group                        (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group                        (1.3.6.1.4.1.232.1.2)
--         cpqSeComplex                              (1.3.6.1.4.1.232.1.2.20)
--           cpqSeComplexCellSlotStatusTable         (1.3.6.1.4.1.232.1.2.20.7)
--
--
--      A complex can have at most 4 cabinets
--
--
-- ****************************************************************************

    cpqSeComplexUUID OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This is the complex UUID."
        ::= { cpqSeComplex 1 }

    cpqSeComplexTotalCabinet OBJECT-TYPE
        SYNTAX  INTEGER (0..4)
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This is the total number of cabinets in the complex.
             Zero will be returned if the value can not be determined."
        ::= { cpqSeComplex 2 }

    cpqSeComplexComputeCabinet OBJECT-TYPE
        SYNTAX  INTEGER (0..2)
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This is the number of compute cabinets in the complex."
        ::= { cpqSeComplex 3 }

    cpqSeComplexIOXCabinet OBJECT-TYPE
        SYNTAX  INTEGER (0..1)
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This denotes the number of IOX cabinets in the complex."
        ::= { cpqSeComplex 4 }

    cpqSeComplexName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This represents the complex name."
        ::= { cpqSeComplex 5 }

    cpqSeComplexLockedProperty OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "Bit 31 - Indicates that there is a locked IPMI property when set.
             Bit 7:0 - Contains the property number currently locked."
        ::= { cpqSeComplex 6 }

    cpqSeComplexCellSlotStatusTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSeComplexCellSlotStatusEntry
        ACCESS  not-accessible
        STATUS  optional
        DESCRIPTION
            "A table of cell slot status in a complex."
        ::= { cpqSeComplex 7 }

    cpqSeComplexCellSlotStatusEntry OBJECT-TYPE
        SYNTAX  CpqSeComplexCellSlotStatusEntry
        ACCESS  not-accessible
        STATUS  optional
        DESCRIPTION
            "A cell slot status description."
        INDEX   { cpqSeComplexCellSlotStatusIndex }
        ::= { cpqSeComplexCellSlotStatusTable 1 }

    CpqSeComplexCellSlotStatusEntry ::= SEQUENCE {
        cpqSeComplexCellSlotStatusIndex       INTEGER,
        cpqSeComplexCellSlotStatusCabinetNo   INTEGER,
        cpqSeComplexCellSlotStatusSlotNo      INTEGER,
        cpqSeComplexCellSlotStatus            INTEGER,
        cpqSeComplexCellSlotPartitionNo       INTEGER,
        cpqSeComplexCellSlotPartitionName     DisplayString
    }

    cpqSeComplexCellSlotStatusIndex OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "The table index of cell slot status in a complex.

            This value is a unique index for a row in the table of complex
            cell slot status."
        ::= { cpqSeComplexCellSlotStatusEntry 1 }

    cpqSeComplexCellSlotStatusCabinetNo OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "The cabinet number of this cell slot."
        ::= { cpqSeComplexCellSlotStatusEntry 2 }

    cpqSeComplexCellSlotStatusSlotNo OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "The number of this cell slot."
        ::= { cpqSeComplexCellSlotStatusEntry 3 }

    cpqSeComplexCellSlotStatus OBJECT-TYPE
        SYNTAX  INTEGER {
            unknown(1),
            active(2),
            inactive(3),
            assigned-powered-off(4),
            free-powered-on(5),
            free-powered-off(6),
            empty(7)
            }
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "The status of this cell slot."
        ::= { cpqSeComplexCellSlotStatusEntry 4 }

    cpqSeComplexCellSlotPartitionNo OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "The partition number this cell is assigned."
        ::= { cpqSeComplexCellSlotStatusEntry 5 }

    cpqSeComplexCellSlotPartitionName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "The partition this cell belongs to."
        ::= { cpqSeComplexCellSlotStatusEntry 6 }

-- ****************************************************************************
--   Standard Equipment LED Table
--   ============================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--         cpqSeLED                    (1.3.6.1.4.1.232.1.2.21)
--
--      This is a generic table of LEDs in the system
--
-- ****************************************************************************

    cpqSeLEDTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSeLEDEntry
        ACCESS  not-accessible
        STATUS  optional
        DESCRIPTION
            "A list of LEDs in the system."
        ::= { cpqSeLED 1 }

    cpqSeLEDEntry OBJECT-TYPE
        SYNTAX  CpqSeLEDEntry
        ACCESS  not-accessible
        STATUS  optional
        DESCRIPTION
            "An entry of an LED in the system."
        INDEX   { cpqSeLEDIndex }
        ::= { cpqSeLEDTable 1 }

    CpqSeLEDEntry ::= SEQUENCE {
        cpqSeLEDIndex            INTEGER,
        cpqSeLEDState            INTEGER,
        cpqSeLEDStateDuration    INTEGER,
        cpqSeLEDLocationType     INTEGER,
        cpqSeLEDDescription      DisplayString,
        cpqSeLEDHardwareLocation DisplayString
    }

    cpqSeLEDIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This is a number that uniquely identifies the LED."
        ::= { cpqSeLEDEntry 1 }

    cpqSeLEDState OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-write
        STATUS  optional
        DESCRIPTION
            "This value represents the state of an LED.
             Bit 31..24 = ON-duration time in unit of 0.1 sec
             Bit 23..16 = OFF-duration time in unit of 0.1 sec
             Bit 15..8 = 0, LED state is OFF
                       = 1, LED state is ON
                       = 2, LED state is BLINKING
             Bit 7..0 = 0, invalid color value
                      = 1, LED color is Brown
                      = 2, LED color is Red
                      = 3, LED color is Orange
                      = 4, LED color is Yellow
                      = 5, LED color is Green
                      = 6, LED color is Blue
                      = 7, LED color is Violet
                      = 8, LED color is Gray
                      = 9, LED color is White "
        ::= { cpqSeLEDEntry 2 }

    cpqSeLEDStateDuration OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-write
        STATUS  optional
        DESCRIPTION
            "This is the duration of an LED state in seconds. "
        ::= { cpqSeLEDEntry 3 }

    cpqSeLEDLocationType OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "This value indicates whether an LED is internal or external.
             0 = External
             1 = Internal "
        ::= { cpqSeLEDEntry 4 }

    cpqSeLEDDescription OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "Description of the LED entry."
        ::= { cpqSeLEDEntry 5 }

    cpqSeLEDHardwareLocation OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "Description of the location of an LED entry."
        ::= { cpqSeLEDEntry 6 }
        
-- ****************************************************************************
--   Standard Equipment USB Device Group
--   ====================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqStdEquipment Group          (1.3.6.1.4.1.232.1)
--       cpqSeComponent Group          (1.3.6.1.4.1.232.1.2)
--        cpqSeUSBDevice Group           (1.3.6.1.4.1.232.1.2.22)
--
--      The cpqSeUSBDevice group lists the USB Devices in the system.
--
--      Implementation of the cpqSeUSBDevice group is optional.
--      Support for the cpqSeUSBDevice group is MANDATORY for all systems that
--      contain a USB bus.
--
-- ****************************************************************************

    cpqSeUSBDeviceType  OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "Attached USB device type."
        ::= { cpqSeUSBDevice 1 }

    cpqSeUSBDeviceName  OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "Attached USB device name."
        ::= { cpqSeUSBDevice 2 }
        

-- ****************************************************************************
--  Standard Equipment MIB Trap Definitions
--  =======================================
--
--  The SNMP trap messages must not be bigger than 484 octets (bytes).
--
--  Trap support in an SNMP agent implementation is optional.  An SNMP
--  agent implementation may support all, some, or none of the traps.
--  If traps are supported, The user should be provided with the option of
--  disabling traps.
-- **************************************************************************
-- Deprecated in 7.20 trap 1005 is the replacement
    cpqSeCpuThresholdPassed TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSeCpuSlot, cpqSeCpuSocketNumber}
        DESCRIPTION
            "This trap is sent when an internal CPU error threshold has been
            passed on a particular CPU causing it to go degraded. This trap
            will be sent when cpqSeCpuThreshPassed transitions from false to
            true."

        --#TYPE "CPU error threshold passed (1001)"
        --#SUMMARY "CPU internal corrected errors have passed a set threshold."
        --#ARGUMENTS {}
        --#SEVERITY MINOR
        --#TIMEINDEX 99
        --#STATE OPERATIONAL

        ::= 1001

    cpqSePCCardThermalDegraded TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSePCCardDeviceInfo,
                     cpqSePCCardProductInfo, cpqSePCCardSlotIndex }
        DESCRIPTION
            "This trap is sent when the PC Card Slot Thermal Sensor threshold has been
            exceeded for safe operations thereby causing degraded operations. This trap
            will be sent when cpqSePCCardStatus transitions from Normal (1) to Thermal
            Degraded (2).
            The manufacturer and product information strings as well as the slot number
            for the degraded PC Card is provided as parameters for this trap."
        --#TYPE "PC Card Thermal Degraded Status (1002)"
        --#SUMMARY "Safe PC Card %d Thermal operating conditions exceeded."
        --#ARGUMENTS {4}
        --#SEVERITY MAJOR
        --#TIMEINDEX 99
        --#STATE DEGRADED
        ::= 1002


    cpqSePCCardThermalFailure TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSePCCardDeviceInfo,
                     cpqSePCCardProductInfo, cpqSePCCardSlotIndex }
        DESCRIPTION
            "This trap is sent when the PC Card Slot Thermal Sensor threshold has been
            exceeded for degraded operations thereby causing failed operations.
            This trap will be sent when cpqSePCCardStatus transitions from Thermal Degraded
            (2) to Thermal Failure (3).
            The manufacturer and product information strings as well as the slot number
            for the failed PC Card is provided as parameters for this trap."
        --#TYPE "PC Card Thermal Failure Status (1003)"
        --#SUMMARY "Degraded PC Card %d Thermal operating conditions exceeded."
        --#ARGUMENTS {4}
        --#SEVERITY CRITICAL
        --#TIMEINDEX 99
        --#STATE NONOPERATIONAL
        ::= 1003

    cpqSePCCardThermalSafe TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSePCCardSlotIndex }
        DESCRIPTION
            "This trap is sent when the PC Card Slot Thermal Sensor threshold has been
            crossed which restored the thermal status to normal operations. This trap will be sent
            when cpqSePCCardStatus transitions from Thermal Degraded (2) or Thermal Failure
            (3) to Normal (1).
            The number of the recovered PC Card slot is provided as a parameter for this trap."
        --#TYPE "PC Card Thermal Safe Operations Status (1004)"
        --#SUMMARY "Degraded/Failed PC Card %d Thermal conditions restored to Safe operations."
        --#ARGUMENTS {2}
        --#SEVERITY INFORMATIONAL
        --#TIMEINDEX 99
        --#STATE OPERATIONAL
        ::= 1004

-- Updated for 7.20 trap replaced 1001
    cpqSe2CpuThresholdPassed TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSeCpuSlot, cpqSeCpuSocketNumber,
                cpqSeCpuSpeed, cpqSeCpuExtSpeed, cpqSeCpuCacheSize}
        DESCRIPTION
            "This trap is sent when an internal CPU error threshold has been
            passed on a particular CPU causing it to go degraded. This trap
            will be sent when cpqSeCpuThreshPassed transitions from false to
            true."

        --#TYPE "CPU error threshold passed (1005)"
        --#SUMMARY "CPU internal corrected errors have passed a set threshold."
        --#ARGUMENTS {}
        --#SEVERITY MINOR
        --#TIMEINDEX 99
        --#STATE OPERATIONAL

        ::= 1005

cpqSeCpuStatusChange TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES { sysName, cpqHoTrapFlags, cpqSeCpuUnitIndex,
                    cpqSeCpuSlot, cpqSeCpuName, cpqSeCpuSpeed,
                    cpqSeCpuStep, cpqSeCpuStatus,
                    cpqSeCpuExtSpeed, cpqSeCpuSocketNumber, 
                    cpqSeCpuHwLocation}
        DESCRIPTION
            "This trap is sent when CPU status changed.

             CPU can be brought down to Stop state and removed
             from O.S Active set or Brought back to Running state
             and made member of O.S Active set.

             User Action: None."

        --#TYPE "Processor Monitor Event Trap"
        --#SUMMARY "Processor in Slot %d status change to %d"
        --#ARGUMENTS {4, 8}
        --#SEVERITY MAJOR
        --#TIMEINDEX 99

        ::= 1006

cpqSeCpuPowerPodstatusChange TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES { sysName, cpqHoTrapFlags, cpqSeCpuUnitIndex,
                    cpqSeCpuSlot, cpqSeCpuName, cpqSeCpuSpeed,
                    cpqSeCpuStep, cpqSeCpuPowerpodStatus,
                    cpqSeCpuExtSpeed, cpqSeCpuSocketNumber,
                    cpqSeCpuHwLocation}
        DESCRIPTION
            "This Trap is sent if CPU Power Pod status changes.

             User Action: None."

        --#TYPE "Processor Monitor Event Trap"
        --#SUMMARY "Processor in Slot %d Power supply status is %d"
        --#ARGUMENTS {4, 8}
        --#SEVERITY MAJOR
        --#TIMEINDEX 99

        ::= 1007
        
    cpqSeUSBStorageDeviceAttached TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqSeUSBDeviceType, cpqSeUSBDeviceName }
        DESCRIPTION
            "This trap is sent when a USB storage device has been attached "
            
        --#TYPE "USB storage device attached (1008)"
        --#SUMMARY "A USB storage device has been attached to the system."
        --#ARGUMENTS {}
        --#SEVERITY INFORMATIONAL
        --#TIMEINDEX 99
        --#STATE OPERATIONAL
        
        ::= 1008

    cpqSeUSBStorageDeviceRemoved TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqSeUSBDeviceType, cpqSeUSBDeviceName }
        DESCRIPTION
	    "This trap is sent when a attached USB storage device is removed "
	    
        --#TYPE "USB storage device removed (1009)"
        --#SUMMARY "A USB storage device has been removed from the system."
        --#ARGUMENTS {}
        --#SEVERITY INFORMATIONAL
        --#TIMEINDEX 99
        --#STATE OPERATIONAL
        
        ::= 1009        

END
