DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5656 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event MC: MCA to BINIT escalation not supported by PAL'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event MC: MCA to BINIT escalation not supported by PAL: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Cannot escalate an MCA to BINIT.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5657 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event MC: Get PAL features failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event MC: Get PAL features failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='SFW failed to get the feature set from PAL.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5658 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event MC: Previous PAL rendezvous failed; rebooting'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event MC: Previous PAL rendezvous failed; rebooting: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='PAL Failed to rendezvous the processors during a MCA.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5659 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event MC: Set PAL features failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event MC: Set PAL features failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='SFW failed to get the feature set from PAL.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5677 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event MC: Monarch failed in slave rendezvous'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event MC: Monarch failed in slave rendezvous: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='SFW s MCA Handler has failed to rendezvous all the slaves Data: Return from the rendezvous call.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5679 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event MC_RENDEZVOUS: Rendezvous vector out of range'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event MC_RENDEZVOUS: Rendezvous vector out of range: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A bad rendezvous vector has been registered.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5682 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event MC_RENDEZVOUS: No MC monarch'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event MC_RENDEZVOUS: No MC monarch: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='No Machine Check Monarch exists, exiting MC Rendezvous.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5683 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event MC_RENDEZVOUS: No wakeup registered'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event MC_RENDEZVOUS: No wakeup registered: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The OS has not registered a wake-up mechanism for rendezvous.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5684 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event MC_RENDEZVOUS: MCA escalation not supported by PAL'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event MC_RENDEZVOUS: MCA escalation not supported by PAL: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='PAL call failed to set the BINIT escalation bit'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5685 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event MC_RENDEZVOUS: Get PAL features failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event MC_RENDEZVOUS: Get PAL features failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The PAL call PAL_GET_FEATURES has failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5686 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event MC_RENDEZVOUS: Set PAL features failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event MC_RENDEZVOUS: Set PAL features failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The PAL call PAL_SET_FEATURES has failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5692 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Internal Firmware Programming Error from the EFI portion of the firmware'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Internal Firmware Programming Error from the EFI portion of the firmware: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An internal SAL_ABI firmware error was encountered. This is usually caused by a bad parameter passed to a function, corrupt memory, corrupt malloc, corrupt firmware tree or something similar. The data field contains the IP address of the'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='function that encountered the error.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5696 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event memory extender loading order error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event memory extender loading order error: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Memory extenders have not been loaded in the correct order.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5698 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Inconsistency in the length of the ESI table'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Inconsistency in the length of the ESI table: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The length field within the ESI (Extensible SAL Interface) table does not agree with the product of the entry_count field and the size of each entry. Data Field: computed value of the length based on entry_count and size of the entries.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5700 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The computed checksum for ESI Table incorrect.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The computed checksum for ESI Table incorrect.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The computed checksum for the ESI (Extensible SAL Interface) table is not zero as expected. EFI is halting. Data Field: the computed checksum.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5701 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event ESI Table contains an unsupported entry type.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event ESI Table contains an unsupported entry type.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='EFI found an unsupported entry type within the ESI (Extensible SAL Interface) Table. Data Field: unknown type.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5704 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A GUID was larger than the expected 128 bits.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A GUID was larger than the expected 128 bits.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='EFI was attempting to output a GUID in the EFI_GUID_HALF1 and EFI_GUID_HALF2 events which was larger than 128 bits. The data field contains the actual length of the GUID in bytes.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5708 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event EFI is halting'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event EFI is halting: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='EFI is halting. Look for the cause of the halt in preceding events. Data Field: the  halt  (0x0F) major change in system state code.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5711 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event chipspare not supported on quad'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event chipspare not supported on quad: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This code will be sent when FW detects a rank installed in the system that doesn t support chipspare. The data field is used to indicate the rank that the x8 DIMMs are installed. It is in the format 0x00000000XDXCXBXA or 0x00000000YBYAXBXA'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='where X and Y are the number of the rank.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5712 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event EFI internal error detected resulting in execution of ASSERT macro'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event EFI internal error detected resulting in execution of ASSERT macro: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='EFI has detected an internal error. The actual error is unspecified by this event. Examine previous events and console output for possible explanations.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5713 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event EFI has executed the  break  shell command.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event EFI has executed the  break  shell command.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='EFI has executed the  break  shell command. EFI is halting. The  break  command is currently implemented as an infinite loop to halt EFI.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5714 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event EFI USB HCD interrupt service has detected the host controller is hung'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event EFI USB HCD interrupt service has detected the host controller is hung: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The EFI USB interrupt service has detected the host controller is hung. EFI is halting.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5715 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The EFI/SAL handoff structure s version does not match EFI expectations'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The EFI/SAL handoff structure s version does not match EFI expectations: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The EFI/SAL handoff structure s version does not match EFI expectations. EFI is halting. Look for EFI_SAL_HANDOFF_VER_EXPECTED to provide EFI s expected value. Data Field: Actual value of the version in the structure.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5717 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unable to obtain access to all RTC SAL services'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unable to obtain access to all RTC SAL services: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='EFI is unable to obtain access to all the RTC (Real Time Clock) SAL services. This means that EFI is unable to fully interact with the RTC. EFI is halting. Data Field: Return status from internal EFI function.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5718 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unable to obtain access to all SAL timer services'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unable to obtain access to all SAL timer services: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='EFI is unable to obtain access to all the SAL timer services. This means that EFI is unable to fully interact with the timer. EFI is halting. Data Field: Return status from internal EFI function.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5719 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event EFI unable to start the periodic timer'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event EFI unable to start the periodic timer: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='EFI is unable to start the periodic timer. This timer interrupts EFI periodically to process time sensitive events. EFI is halting. Data Field: Return status for internal EFI function.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5720 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event No I/O port space region found in the MDT'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event No I/O port space region found in the MDT: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='EFI did not find an I/O port space region in the MDT. EFI is halting.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5721 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event EFI reached an unimplemented section of code'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event EFI reached an unimplemented section of code: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='EFI reached an unimplemented section of code. EFI is halting. Data Field: Unique identifier indicating the location reached within the code.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5722 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event EFI unable to read current speedy boot settings'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event EFI unable to read current speedy boot settings: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='EFI was unable to read the current speedy boot settings. The speedy boot settings are stored within the BMC. EFI will use a default value of 0 and continue booting. The speedy boot functionality is also accessed via the boot test EFI shell'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='command and via the OS. These other accesses will likely fail. Data Field: Return status from internal EFI function..  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5723 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unpermitted SAL callback attempted'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unpermitted SAL callback attempted: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A SAL Callback was attempted. This is not permitted. EFI is halting. Data Field: index of the function that was being called.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5724 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event EFI unable to determine frequency base of the CPU interval timer'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event EFI unable to determine frequency base of the CPU interval timer: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='While attempting to calibrate the EFI stall timer, system firmware is unable to determine the frequency of the CPU interval timer. System firmware will assume 800 MHz for the purpose of the stall timer calibration and continue boot. Data'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='Field: error status code (should be 0xFFFFFFFD).  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5725 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event EFI system events already initialized'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event EFI system events already initialized: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The EFI system events have already been initialized. This is unexpected. EFI is continuing. Data Field: the current value of the system event entry point.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5726 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unable to create internal virtualization event while initializing IPMI events'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unable to create internal virtualization event while initializing IPMI events: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='EFI was unable to create an internal virtualization event while initializing EFI s System Events (IPMI events). This internal event is not an IPMI event; rather it serves as a trigger for EFI to virtualize the System Event facility when going'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='virtual. EFI will likely halt. Data Field: return status from internal EFI function.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5728 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event There was an error creating or initializing the FPGA node in firmware'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event There was an error creating or initializing the FPGA node in firmware: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error was detected while initializing the FPGA node and services asociated with the PDH.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5729 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error creating the pdh ioconfig node or attaching the service to it.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error creating the pdh ioconfig node or attaching the service to it.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware encountered an error when creating the ioconfig node as a child of the pdh node.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5730 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error ecnountered setting up the dillon_pdh node or service.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error ecnountered setting up the dillon_pdh node or service.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System firmware was unable to correctly set up the pdh arbiter node as a child of the pdh node, or was unable to locate and attach the pdh arbiter service to the node. The status is returned in the data field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5731 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The PDH component encountered an error dealing with a property on a node.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The PDH component encountered an error dealing with a property on a node.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The PDH service was unable to either get or set the property specified in the data field as an ascii message.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5732 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error creating the acpi_hw node.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error creating the acpi_hw node.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='PDH encountered an error creating the ACPI Hardware Node in the device tree or installing its properties.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5733 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error encountered creating or initializing the ipmi node'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error encountered creating or initializing the ipmi node: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The PDH service encountered an error while creating the ipmi node or adding properties to it. The status is in the data field.'

