DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8141 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A CPU module has reported overtemp, so will be powered off in 1 minute.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A CPU module has reported overtemp, so will be powered off in 1 minute.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CPU module s temperature has exceed the high temperature threshold. As a result of this event, an irrevocable 2 minute timer will begin. At the end of 2 minutes, the offending CPU module will be powered off by the Cell hardware. The Cell'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='must be powered off then on using the MP s PE command before the CPU module will be powered again.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8143 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An error occurred while updating the PDHC firmware.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An error occurred while updating the PDHC firmware.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while updating the PDHC firmware. More specific details of the update error may be displayed by the Firmware Update utility running on the MP.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8147 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Boot is disabled because the cell type does not match the System FW ROM type.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Boot is disabled because the cell type does not match the System FW ROM type.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The cell type (IPF or PA) does not match System FW type. The cell type is detected based on information stored in CPU modules  FRUID EEPROMs. The System FW type is determined based on data that is embedded in the System FW ROM image. This is'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='checked each time Cell power transitions from off to on, and each time the System FW is updated. Following the detection of this mismatch, the Cell will not be allowed to boot until the problem has been resolved.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8149 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The PDHC has waited an abnormally long time for PDH bus access.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The PDHC has waited an abnormally long time for PDH bus access.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This event is emitted after the PDHC has waited longer than a maximum expected time for the PDH arbiter to grant it control of the PDH bus. The PDHC will continue waiting for contol of the PDH bus until the arbiter grants it control, or the'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='Cell is powered off using the MP s PE command. While waiting for the PDH bus, the PDHC will NOT perform its normal duties such as monitoring the Cell status, and passing messages from the system to the MP, and the PDHC heartbeat will not  '
DEFine MSGACTion Name=(*,40)
ACTION=ANNOTATE TEXT='blink." '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8151 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The PDHC has waited an abnormally long time to obtain the PDH semaphore.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The PDHC has waited an abnormally long time to obtain the PDH semaphore.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This event is emitted after the PDHC has waited longer than a maximum expected time to obtain control of the PDH bus semaphore. The PDHC will continue waiting for contol of the PDH bus semaphore until System FW relinquishes control of the'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='semaphore, or the Cell is powered off using the MP s PE command. While waiting for the PDH bus semaphore, the PDHC will NOT perform its normal duties such as monitoring the Cell status, and passing messages from the system to the MP, and the  '
DEFine MSGACTion Name=(*,40)
ACTION=ANNOTATE TEXT='PDHC heartbeat will not blink. The data field contains debug data that may be useful for developers. Data_byte[0] = last value read from PDHC s address for the microSemaphore register. Data_byte[1] = boolean indicator (1=set,0=not_set) of  '
DEFine MSGACTion Name=(*,50)
ACTION=ANNOTATE TEXT='whether the PDHC s flag is set. Data_byte[2] = boolean indicator (1=set,0=not_set) of whether the System FW s flag is set." '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8153 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An error occurred while transmitting an IPMI message in the BMC2HOST direction.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An error occurred while transmitting an IPMI message in the BMC2HOST direction.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This event indicates that an error occurred while transmitting an IPMI message in the BMC2HOST direction. The data field contains more detailed information about the source of the error. Data Bytes 0 & 1 form a 16-bit IPMI error indicator that'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='has the following values and meanings: 1 - IPMI_HOST_BUSY_TIMEOUT - The PDHC could not put a message in the BMC2HOST hardware message queue for over 10 seconds, so the pending message(s) were dropped. 2 - IPMI_INVALID_MSG_SIZE - The MP sent an  '
DEFine MSGACTion Name=(*,40)
ACTION=ANNOTATE TEXT='IPMI message response that has an embedded size indicator that is less than 4 bytes or greater than the size of the message data. The poorly formed message response will be dropped. 3 - IPMI_BMC2HOST_Q_FULL - The BMC2HOST message queue in the  '
DEFine MSGACTion Name=(*,50)
ACTION=ANNOTATE TEXT='PDHC is full, so a message response from the MP has been dropped." '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8154 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event EFI unable to read initial debug level from the BMC'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event EFI unable to read initial debug level from the BMC: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='EFI was unable to read the initial debug level from the BMC token. EFI will continue with an unknown value for the debug level. Data Field: Return status from internal EFI function.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8156 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A XBC port was unexpectedly found to not be landmined.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A XBC port was unexpectedly found to not be landmined.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A XBC port was unexpectedly found to not be landmined. The data field consists of the XBC number (32:43) and the port number (44:55).'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8159 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An invalid number of XBC ports were landmined in the system.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An invalid number of XBC ports were landmined in the system.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The number of landmined XBC ports was not within the allowable range. There is a minimum number of landmined ports because some ports are always unused. There is a maximum number of landmined ports because there is a limit to the number of'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='broken links allowed in a system. The data field shows the number of landmined ports found  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8184 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The backplane was not recognized as one that contains fabric'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The backplane was not recognized as one that contains fabric: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Data field contains the backplane type found. During Intra SKD Routing, the backplane type detected was either a Medel backplane or was unrecognized. The backplane could therefore not be routed. This is a firmware sanity check. Data Field:'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='system type  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8186 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Writing the XIN Error Mask Register to zero failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Writing the XIN Error Mask Register to zero failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Prior to initializing the CC to XBC link, the XIN error mask should be zeroed out to prevent spurious errors from interferring with the link initialization. This write to zero out the error mask failed. Data Field: (cell << 56) | return'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='status  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8187 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Dumping error info. Read status of the Primary Mode Register'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Dumping error info. Read status of the Primary Mode Register: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Coherency Controller s (CC) XIN link did not initialize properly. The data field contains the return status from an attempted read of the CC Primary Error Mode CSR. (0 = SUCCESS)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8188 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Data read from the CC Primary Mode CSR'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Data read from the CC Primary Mode CSR: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Coherency Controller s (CC) XIN link did not initialize properly. The data field contains the data read from the CC Primary Error Mode CSR.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8189 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Dumping error info. Read status of the CC Error Mask Register'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Dumping error info. Read status of the CC Error Mask Register: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Coherency Controller s (CC) XIN link did not initialize properly. The data field contains the return status from an attempted read of the CC Primary Error Mode CSR. (0 = SUCCESS)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8190 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Data read from the CC Error Mask CSR'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Data read from the CC Error Mask CSR: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Coherency Controller s (CC) XIN link did not initialize properly. The data field contains the data read from the CC Error Mask CSR.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8194 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The link could not be crossed upon first attempt'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The link could not be crossed upon first attempt: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The neighbor s port connected to the link being crossed is not routable. This was the first attempt to cross the link, PDC will now look for another link it can cross. DATA: (xbcNum << 32 ) | (port << 44)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8195 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed reading an XBC forward progress register'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed reading an XBC forward progress register: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Fabric read error. Data field: (XBC number << 32 | return status)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8198 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Could not find an adjacent XBC due to broken fabric links'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Could not find an adjacent XBC due to broken fabric links: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Too many crossbar links are broken. Cell cannot boot, halting. Data field: XBC number << 32'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8199 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The run-time verification of a programming assumption has failed.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The run-time verification of a programming assumption has failed.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='For debug purposes, many assumptions made by the PM developer(s) are checked at run-time. If this event log is seen, it will either indicate that the hardware is in a unknown state that is not handled by the PM, or that a programming bug has'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='been found. For developer debug purposes, the data field describes where in the code that the error was detected. Data Bytes[0-1]: The line number within the source code file where the error was detected. Data Bytes[2-7]: The first 6 characters  '
DEFine MSGACTion Name=(*,40)
ACTION=ANNOTATE TEXT='of the source code file name." '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8200 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An unknown error has been detected by the PDHC firmware.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An unknown error has been detected by the PDHC firmware.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An unknown error has been detected by the PM firmware. For developer debug purposes, the data field describes where in the code that the error was detected. Data Bytes[0-1]: The line number within the source code file where the error was'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='detected. Data Bytes[2-7]: The first 6 characters of the source code file name.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8202 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Data field contains data meant for firmware debug only.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Data field contains data meant for firmware debug only.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This event is a tool to aid in the debugging and testing of firmware.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8205 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Testing of correctable errors injected from the CC has failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Testing of correctable errors injected from the CC has failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failed link testing to ensure that SBE and LPE errors are detected properly by the XBC. The XBC did not detect any errors. Data field indicates the return status: (1 = err detected, 0 = no err detected, -1 = XBC accesses failed)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8206 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A cabinet has been configured using an invalid cabinet number'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A cabinet has been configured using an invalid cabinet number: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The data field contains the cabinet number that is invalid'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8207 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cells trying to join a PD are at incompatible firmware revisions'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cells trying to join a PD are at incompatible firmware revisions: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The cell indicated in the data field is at a different firmware revision than the reporting cell. This is determined by evaluating the checksums of the 2 rom images.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8212 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An attempt to write to a device on the PM s I2C bus has failed.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An attempt to write to a device on the PM s I2C bus has failed.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An attempt to write to a device on the PM s I2C bus has failed. The Data field contains information that can identify the exact device that has failed. Refer to the UGUY ERS for a mapping of I2C device addresses to devices. Data Bytes[0-1]:'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='Reserved Data Bytes[2-3]: I2C Device Address Data Bytes[4-5]: Starting Word Address Data Bytes[6-7]: Size of attempted access (in bytes).  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8214 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An attempt to read from a device on the PM s I2C bus has failed.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An attempt to read from a device on the PM s I2C bus has failed.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An attempt to read from a device on the PM s I2C bus has failed. This event is only emitted when the PM is reading a BPS s. The Data field contains information that can identify the exact device that has failed. Refer to the UGUY ERS for a'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='mapping of I2C device addresses to devices. Data Bytes[0-1]: Reserved Data Bytes[2-3]: I2C Device Address (to convert to BPS slot number subtract 1 and divide by 2) Data Bytes[4-5]: Starting Word Address Data Bytes[6-7]: Size of attempted  '
DEFine MSGACTion Name=(*,40)
ACTION=ANNOTATE TEXT='access (in bytes)." '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8216 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An error was encountered updating the cell info structure in ICM'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An error was encountered updating the cell info structure in ICM: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error was encountered trying to obtain the data required for the cell information structure in ICM. The data field is an ASCII message that indicates the information that was not found.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8218 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An error was encountered pointing the slave cell consoles to the diva'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An error was encountered pointing the slave cell consoles to the diva: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error was encountered establishing the slave cells use of the diva console.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8219 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An error was encountered trying to relocate a slave cells registry'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An error was encountered trying to relocate a slave cells registry: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error was encountered trying to relocate the registry on a slave cell to point to the core cells main memory strucutres.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8220 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Complex Profile Group C CRC didn t match the expected value'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Complex Profile Group C CRC didn t match the expected value: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Calculuated CRC for the group C Partition Profile did not match the stored value. The expected value and the actual value will be emmited in 2 sequential chassis codes.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8238 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failure to identify a core cell during Global MCA.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failure to identify a core cell during Global MCA.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Not able to find a core cell in the PD during a global MCA error processing.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8239 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unexpected fabric firmware error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unexpected fabric firmware error: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An unexpected error occurred while initializing the fabric. The firmware is not able to analyze this error. Clues to the cause of this error may be found in the IPMI forward progress log (FPL) either shortly before or after this log entry'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='occurred. The FPL is available from the management processor using the  sl  command. HP-UX also saves these logs in the /var/stm/logs/os directory, and they can be viewed using the slview utility.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8240 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Internal firmware programming error in the PMI handler.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Internal firmware programming error in the PMI handler.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An internal firmware error was encountered. This is usually caused by a bad parameter passed to a function, corrupt memory, corrupt malloc tables or something similar. The data field contains the IP address of the function that encountered the'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='error.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8243 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event During a Cell On Line Add inconsistent number of cells discovered'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event During a Cell On Line Add inconsistent number of cells discovered: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='During the on line addition of a cell the partition adding the cell has determined inconsistent data as to which cell is being added. The cell addition will be aborted and the partition will resume execution without the new cell.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8257 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error reading source cell port on XBC during data traversability test'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error reading source cell port on XBC during data traversability test: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while reading the routing from the source cell s port on the source XBC. Data Field: (source cell << 56 | source XBC << 32)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8269 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPUs of different maximum core frequencies are installed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPUs of different maximum core frequencies are installed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='CPU s of mixed maximum core frequencies are installed'

