DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12069 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event SFW detected an error while writing to stable store flash.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event SFW detected an error while writing to stable store flash.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while writing to stable store flash. Data field is unused.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12091 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PCI interlock open with PCI power applied.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PCI interlock open with PCI power applied.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='PCI interlock has been opened with PCI slot power on. The datafield can be decoded as follows (where byte 0 is the rightmost byte): byte offset 2:PCI slot number byte offset 5: IO Chassis number byte offset 6: IO Bay number byte offset 7:'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='Cabinet number   '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12101 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Fault detected on low drop out regulator on I/O backplane.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Fault detected on low drop out regulator on I/O backplane.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The specified low dropout regulator on the IO backplane is reporting a fault. The specified power rail is reporting a fault. The number in the slot field of the physical location is the rail number that caused the fault. Rails are: 4 = LDO'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='2.5v for Esca 0, 5 = LDO 2.5v for Esca 1, 1.5v, 7 = Other backplane 2.5v, 8 = Other backplane 1.2v  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12102 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Fault detected on low drop out regulator on main backplane.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Fault detected on low drop out regulator on main backplane.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The specified low dropout regulator on the main backplane is reporting a fault. The number in the slot field of the physical location is the rail number that caused the fault. Rails are: 0 = SysBP xb0 1.5v, 1 = SysBp xb1 1.5v, 2 = SysBp'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='switched 3.3v, 3 = SysBp LDO xb0 2.5v, 4 = SysBp xb1 LDO 2.5v, 5 = SysBp LDO 1.5v br0, 6 = SysBp LDO 1.5v br1  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12103 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Fault detected hot swap controller of specified core IO.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Fault detected hot swap controller of specified core IO.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The hot swap controller for the specified core IO is reporting fault.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12109 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An error occurred while retrieving the crossbar chip number.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An error occurred while retrieving the crossbar chip number.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while retrieving the crossbar chip number. Data Field: cell number << 56 | port number << 44 | return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12119 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event One or more of the cells are not configured for Cell-Local Memory (CLM) mode'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event One or more of the cells are not configured for Cell-Local Memory (CLM) mode: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='For most workloads, the system performance may be degraded if CLM mode is not enabled for all of the cells in a partition. Windows Server 2003 contains additional support to optimize for CLM systems, increasing the performance compared to an'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='interleaved configuration.   '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12120 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Double DRAM chip sparing events have been invoked.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Double DRAM chip sparing events have been invoked.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Corrected memory errors have been detected. Double DRAM chip sparing events have been invoked.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12121 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A platform error was detected by the firmware/hardware, and corrected by using a spare channel.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A platform error was detected by the firmware/hardware, and corrected by using a spare channel.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A error occurred in the crossbar controller and was corrected by the hardware.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12127 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A platform error was detected by the firmware/hardware, and corrected by using a spare channel.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A platform error was detected by the firmware/hardware, and corrected by using a spare channel.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A platform error was detected by the firmware/hardware, and corrected by using a spare channel. The error occurred between the crossbar chips on the backplane(s).'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12128 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A platform error was detected by the firmware/hardware, and corrected by using a spare channel.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A platform error was detected by the firmware/hardware, and corrected by using a spare channel.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A platform error was detected by the firmware/hardware, and corrected by using a spare channel. The error occurred between the cell controller and the IO controller.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12129 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Multiple platform errors were detected and corrected by the firmware/hardware.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Multiple platform errors were detected and corrected by the firmware/hardware.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Multiple platform errors were detected and corrected by the firmware/hardware. The errors occurred between the cell controller and the backplane.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12130 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Multiple platform errors were detected and corrected by the firmware/hardware.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Multiple platform errors were detected and corrected by the firmware/hardware.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Multiple platform errors were detected and corrected by the firmware/hardware. The errors occurred between the crossbar chips on the backplane(s).'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12131 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Multiple platform errors were detected and corrected by the firmware/hardware.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Multiple platform errors were detected and corrected by the firmware/hardware.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Multiple platform errors were detected and corrected by the firmware/hardware. The errors occurred between the cell controller and the IO controller.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12132 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The server ID does not match the cabinet type.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The server ID does not match the cabinet type.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The server identification information does not match the cabinet type. The server will not power on until this condition is resolved.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12135 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Duplicate DIMM serial numbers have been detected. Data field gives physical location of DIMM. Check for other events specifying other DIMMs with same serial number.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Duplicate DIMM serial numbers have been detected. Data field gives physical location of DIMM. Check for other events specifying other DIMMs with same serial number.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Duplicate DIMM serial numbers have been detected. Data field gives physical location of DIMM. Check for other events specifying other DIMMs with same serial number.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12143 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The MP has lost lan communication with the UPS.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The MP has lost lan communication with the UPS.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The MP has lost communications with the UPS via SNMP over the LAN'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12144 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The MP has re-gained lan communication with the UPS.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The MP has re-gained lan communication with the UPS.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The MP lan communications with the UPS have been restored.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12149 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An unrecoverrable processor interrupt occured while in IPF firmware. The data value is the processor IFA.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An unrecoverrable processor interrupt occured while in IPF firmware. The data value is the processor IFA.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An unrecoverrable processor interrupt occured while in IPF firmware. The data value is the processor IFA.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12150 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An unrecoverable processor interrupt occured while in IPF firmware. The event data is the processor ISR.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An unrecoverable processor interrupt occured while in IPF firmware. The event data is the processor ISR.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An unrecoverable processor interrupt occured while in IPF firmware. The event data is the processor ISR.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12153 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Double chip sparing has been invoked'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Double chip sparing has been invoked: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System firmware has detected and corrected memory errors. Double chip sparing has been invoked to help mitigate this condition.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12155 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event External clock cable has been removed from the CPU cabinet. The data field contains the physical location of the cabinet.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event External clock cable has been removed from the CPU cabinet. The data field contains the physical location of the cabinet.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='External clock cable has been removed from the CPU cabinet. The data field contains the physical location of the cabinet.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12156 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event System Fabric encountered a link error after opening up the fabric link.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event System Fabric encountered a link error after opening up the fabric link.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System Fabric encountered a link error after opening up the fabric link'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12157 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Fatal errors are present on a cell s link to the fabric. Data Field: (crossbar port 44) | (crossbar 32) | 1'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Fatal errors are present on a cell s link to the fabric. Data Field: (crossbar port 44) | (crossbar 32) | 1: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Fatal errors are present on a cell s link to the fabric. Data Field: (crossbar port << 44) | (crossbar << 32) | 1'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12159 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event System firmware encountered fabric problems. Data Field: (crossbar port 44) | (crossbar 32)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event System firmware encountered fabric problems. Data Field: (crossbar port 44) | (crossbar 32): &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System firmware encountered fabric problems. Data Field: (crossbar port << 44) | (crossbar << 32)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12160 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Fatal errors are present on a cell s link to the fabric. Data Field: (crossbar port 44) | (crossbar 32)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Fatal errors are present on a cell s link to the fabric. Data Field: (crossbar port 44) | (crossbar 32): &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Fatal errors are present on a cell s link to the fabric. Data Field: (crossbar port << 44) | (crossbar << 32)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12161 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The operating system has recovered from a PCI error.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The operating system has recovered from a PCI error.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A PCI error occurred, but the OS recovered.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12162 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The operating system has recovered from a PCI error.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The operating system has recovered from a PCI error.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A PCI error occurred, but the operating system recovered.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12163 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The operating system has recovered from a PCI error.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The operating system has recovered from a PCI error.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A PCI error occurred, but the operating system recovered'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12164 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The request to power on, either via MP user interface, power button, or other, was denied by the Enclosure Manager.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The request to power on, either via MP user interface, power button, or other, was denied by the Enclosure Manager.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The request to power on, either via MP user interface, power button, or other, was denied by the Enclosure Manager.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12165 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The blade has been forced to power-on, either via the MP user interface or the power button. The blade did not negotiate with the enclosure to insure that there was sufficient power for this action.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The blade has been forced to power-on, either via the MP user interface or the power button. The blade did not negotiate with the enclosure to insure that there was sufficient power for this action.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The blade has been forced to power-on, either via the MP user interface or the power button. The blade did not negotiate with the enclosure to insure that there was sufficient power for this action.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12168 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The MP has repeatedly tried to communicate with the enclosure manager and has not received any response.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The MP has repeatedly tried to communicate with the enclosure manager and has not received any response.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The MP has repeatedly tried to communicate with the enclosure manager and has not received any response'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12193 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event This is an internal SW error. See Cause/Action .'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event This is an internal SW error. See Cause/Action .: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This is an internal SW error'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12194 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event This is an internal SW error. See Cause/Action.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event This is an internal SW error. See Cause/Action.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This is an internal SFW error'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12195 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event This is an internal SW error. See Cause/Action.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event This is an internal SW error. See Cause/Action.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This is an internal SFW error'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12196 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event This is an internal SW error. See Cause/Action.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event This is an internal SW error. See Cause/Action.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This is an internal SFW error'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12199 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The complex profiles between cells in a partition do not match. Data field is unused, earlier events will give more detail.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The complex profiles between cells in a partition do not match. Data field is unused, earlier events will give more detail.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='There are miscompares in the complex profiles between cells in a partition. Data field is unused, earlier events will give more detail.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12204 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An I/O device is missing from the Core I/O'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An I/O device is missing from the Core I/O: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An I/O device is missing from the Core I/O. Internal peripherals may be not accessible.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 12207 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event fPars PMI handler was unable to Notify a CPU s new owner after a migrate.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event fPars PMI handler was unable to Notify a CPU s new owner after a migrate.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An fPar s GPE_EN bits are not set up to handle receiving a CPU migrate. This event is emitted 2 times, the Data field is different each time. 1. Data field: Address of GPE block 2. Data field: bits 31:0 Virtual GPE_EN register (lower byte)'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='bits 63:32 Enable bits needed for successful migrate  '

