DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9750 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Windows: Predictive Failure in Memory (Warning)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Windows: Predictive Failure in Memory (Warning): &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='ECC (Error Checking and Correcting) memory is designed to detect and correct single-bit errors that occasionally occur in computer systems. This memory module is currently correcting many single bit errors.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9751 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Windows: Predictive Failure in Memory (Critical)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Windows: Predictive Failure in Memory (Critical): &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='ECC (Error Checking and Correcting) memory is designed to detect and correct single-bit errors that occasionally occur in computer systems. This memory module is currently correcting many single bit errors.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9753 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A rope parity error occurred'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A rope parity error occurred: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A error occurred on the bus connecting the PCI card to the system bus.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9754 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PCI card inaccessible due to bus error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PCI card inaccessible due to bus error: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A PCI card has been marked as  fatal  by the operating system due to a bus error. The LBA has been isolated by the operating system due to an error which occured in a device(s) connected to that LBA.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9755 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PCI card inaccessible due to device error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PCI card inaccessible due to device error: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A PCI card has been marked as  fatal  by the operating system due to a device error.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9768 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event error reading bmc first boot token'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event error reading bmc first boot token: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware tried to read the first boot token an got a failure. The data field contains the token number that FW tried to read. This is a stop boot condition'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9769 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event a rendezvousing cell is non PA architecture and thus incompatible.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event a rendezvousing cell is non PA architecture and thus incompatible.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='monarch PA cell has detected that a cell it is attempting to rendezvous into its PD is not a PA cell and is thus incompatible.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9774 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event failed to write the XBC error log clear register'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event failed to write the XBC error log clear register: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A XBC error could not be cleared due to a write failure. The data field indicates the type of error: (XBC Port Num << 56) | (XBC Num << 32) | error status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9775 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error encounted while reading the XBC CSR Error Status Register'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error encounted while reading the XBC CSR Error Status Register: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failed to read the XBC Global CSR Error Status register. Data Field: (XBC Port Num << 56) | (XBC Num << 32) | error status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9776 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The XBC CSR Low Severity error was not cleared'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The XBC CSR Low Severity error was not cleared: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The XBC CSR Low Severity error was not cleared or more errors remain. Data Field: (XBC Port Num << 56) | (XBC Num << 32) | contents of the XBC CSR Error Status Register'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9777 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The XBC CSR High Severity error was not cleared'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The XBC CSR High Severity error was not cleared: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The XBC CSR High Severity error was not cleared or more errors remain. Data Field: (XBC Port Num << 56) | (XBC Num << 32) | contents of the XBC CSR Error Status Register'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9778 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error encounted while reading the XBC Port Error Status Register'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error encounted while reading the XBC Port Error Status Register: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failed to read the XBC Port Error Status register. Data Field: (XBC Port Num << 56) | (XBC Num << 32) | error status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9780 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to read the XBC CSR Error Status register'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to read the XBC CSR Error Status register: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failed to read the XBC Global CSR Error Status register. Data Field: (XBC Port Num << 56) | error status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9781 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to copy the XBC CSR Error Symbol01 Block'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to copy the XBC CSR Error Symbol01 Block: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware failed to copy the XBC CSR Error symbol 01 registers into a data structure on the stack. Data Field: address where the register contents are being copied'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9782 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to copy the XBC CSR Error Symbol23 Block'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to copy the XBC CSR Error Symbol23 Block: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware failed to copy the XBC CSR Error symbol 23 registers into a data structure on the stack. Data Field: address where the register contents are being copied'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9783 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to reset the XBC Low Severity Error Log State'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to reset the XBC Low Severity Error Log State: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware was unable to reset the XBC CSR Low Severity error log state. Data Field: (XBC Port Num << 56) | (XBC Num << 32) | error status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9784 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to clear the XBC Low Severity Log Symbol 01'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to clear the XBC Low Severity Log Symbol 01: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The XBC Low Severity error logs were not cleared. Data Field: (XBC Port Num << 56) | (XBC Num << 32) | number of failed clear attempts'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9785 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Could not determine if there is a new XBC CSR Low Severity error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Could not determine if there is a new XBC CSR Low Severity error: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Reading the XBC CSR Error Status register failed. Data field: (XBC Port Num << 56) | (XBC Num << 32) | error status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9786 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to read the XBC CSR Low Severity Error Log State'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to read the XBC CSR Low Severity Error Log State: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failed to read a XBC Global scratch register that indicates if new, unlogged errors have been encountered. Data field: (XBC Port Num << 56) | (XBC Num << 32) | error status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9787 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to reset the XBC Low Severity Error Log State'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to reset the XBC Low Severity Error Log State: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware was unable to reset the XBC CSR Low Severity error log state. Data Field: (XBC Port Num << 56) | (XBC Num << 32) | error status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9788 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Could not determine if there is a new XBC CSR High Severity error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Could not determine if there is a new XBC CSR High Severity error: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Reading the XBC CSR Error Status register failed. Data field: (XBC Port Num << 56) | (XBC Num << 32) | error status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9789 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to read the XBC CSR High Severity Error Log State'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to read the XBC CSR High Severity Error Log State: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failed to read a XBC Global scratch register that indicates if new, unlogged errors have been encountered. Data field: (XBC Port Num << 56) | (XBC Num << 32) | error status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9801 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An error occurred while enabling hashing in the platform cache'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An error occurred while enabling hashing in the platform cache: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while enabling hashing in the platform cache. The data field contains the status.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9827 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The XBC CSR is not a valid CSR address'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The XBC CSR is not a valid CSR address: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A write to an invalid XBC CSR address was attempted. The write will not be allowed. The severity of this result will be determined by the calling function. Data Field: XBC CSR address that was attempted'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9832 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event It indicates loss of cell connectivity in the partition.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event It indicates loss of cell connectivity in the partition.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='It indicates loss of cell connectivity in the partition during a global MCA processing.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9849 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error building cell-level FW device tree'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error building cell-level FW device tree: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error status of building the cell-level firmware device tree'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9867 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU deconfigured during FSB interface initialization'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU deconfigured during FSB interface initialization: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error has occurred during CPU FSB interface initialization. The datafield contains a 32-bit error number and 32-bits of additional error information. The CPU will be deconfigured.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9868 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU deconfigured due to error obtaining parameters from PAL'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU deconfigured due to error obtaining parameters from PAL: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error has occurred while obtaining CPU parameters from the CPU abstraction layer. The datafield contains a 32-bit error number and 32-bits of additional error information. The CPU will be deconfigured.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9869 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU deconfigured due to failure retrieving icache parameters from PAL'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU deconfigured due to failure retrieving icache parameters from PAL: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while getting CPU icache parameters from the CPU abstraction layer. The datafield contains a 32-bit error number and 32-bits of additional error information. The CPU will be deconfigured if this error occurs during system'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='boot.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9870 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU deconfigured during initialization process'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU deconfigured during initialization process: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while obtaining CPU dcache parameters from the CPU abstraction layer. The datafield contains a 32-bit error number and 32-bits of additional error information. The CPU will be deconfigured if error occurs during system boot.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9871 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU deconfigured during dcache init'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU deconfigured during dcache init: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while initializing the CPU cache to a known state. The datafield contains a 32-bit error number and 32-bits of additional error information. The CPU will be deconfigured.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9872 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU deconfigured due to internal error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU deconfigured due to internal error: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while enabling CPU cache error monitoring. The datafield contains a 32-bit error number and 32-bits of additional error information. The CPU will be deconfigured.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9873 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU deconfigured due to machine check'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU deconfigured due to machine check: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while enabling some machine error check traps on a CPU. The datafield contains a 32-bit error number and 32-bits of additional error information. The CPU will be deconfigured.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9874 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU deconfigured due to error while disabling machine check'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU deconfigured due to error while disabling machine check: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while disabling maching error check traps on a CPU. The datafield contains a 32-bit error number and 32-bits of additional error information. The CPU will be deconfigured.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9875 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU deconfigured due to failure in late self tests'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU deconfigured due to failure in late self tests: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred during the serialized CPU late selftests. The datafield contains a 32-bit error number and 32-bits of additional error information. The CPU will be deconfigured.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9876 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU deconfigured while enabling L2 shared cache'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU deconfigured while enabling L2 shared cache: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while enabling the CPU L2 shared cache. The datafield contains a 32-bit error number and 32-bits of additional error information. The CPU will be deconfigured.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9877 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU deconfigured while retrieving default values from PAL'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU deconfigured while retrieving default values from PAL: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error while getting default values for programmable CPU internal registers from the CPU abstraction layer. The datafield contains a 32-bit error number and 32-bits of additional error information. The CPU will be deconfigured.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9878 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU deconfigured getting an address for a CPU internal register within a buffer from the CPU abstraction layer'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU deconfigured getting an address for a CPU internal register within a buffer from the CPU abstraction layer: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while getting an address for a CPU internal register within a buffer from the CPU abstraction layer. The datafield contains a 32-bit error number and 32-bits of additional error information. The CPU will be deconfigured.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9879 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU deconfigured while getting an address for a CPU internal register within a buffer from the CPU abstraction layer'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU deconfigured while getting an address for a CPU internal register within a buffer from the CPU abstraction layer: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while programming CPU internal registers with final configuration values. The datafield contains a 32-bit error number and 32-bits of additional error information. The CPU will be deconfigured.'

