Updated HP Message Records

---

This folder (\CPQEM\UPDATED) contains message record files that have been
changed or updated since the last release of the integration module.

The directory contains the complete files with the included changes, and the readme.txt
details specifically what changed in each file.

You can delete all the message records that are in the updated files, then reapply the 
entire file, or you can edit the message records and make the changes below.

The REMOVE files are provided if the user simply wants to remove the previous versions
of the message records and install the new ones.

For example, execute 'cautil -f cpqfca3_remove.txt' to remove the old message records
before running 'cautil -f cpqfca3.txt' to install the updated ones.  

Note: Any customizations should be saved before removing the currently installed
message records.  Executing the REMOVE files will also delete any customization
that has been added by the user.

---------------------------------------------------------------------------

Installation Script for the Updates:

Executing LOADUPDATES.BAT will automatically remove the current message records 
defined and load the updated versions of these message records.  

Note: Do not execute this script until you have saved any customized actions, 
otherwise the customizations will be lost.





CPQHEALTH9.TXT

Message records for trap 6054 and 6055 were updated.

#-----------------------------
# Definiton for trap 6054
#-----------------------------
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6054*'
       MSGNODE=*
       DEScription='HP - Fault Tolerant Power Supply redundancy restored.'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fault Tolerant Power Supply redundancy restored on Chassis &(26:)'
       SEVerity=I
       ATTRIB=default
       COLOR=blue

CHANGED TO:

#-----------------------------
# Definiton for trap 6054
#-----------------------------
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6054*'
       MSGNODE=*
       DEScription='HP - Fault Tolerant Power Supply redundancy restored.'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fault Tolerant Power Supply redundancy restored on Chassis &26'
       SEVerity=I
       ATTRIB=default
       COLOR=blue



#-----------------------------
# Definiton for trap 6055
#-----------------------------
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6055*'
       MSGNODE=*
       DEScription='HP - Fault Tolerant Fan redundancy restored.'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fault Tolerant Fan redundancy restored on Chassis &(26:)'
       SEVerity=I
       ATTRIB=default
       COLOR=blue

CHANGED TO:

#-----------------------------
# Definiton for trap 6055
#-----------------------------
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6055*'
       MSGNODE=*
       DEScription='HP - Fault Tolerant Fan redundancy restored.'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fault Tolerant Fan redundancy restored on Chassis &26'
       SEVerity=I
       ATTRIB=default
       COLOR=blue

----------

