#* **************************************************************************
#*
#*                  Insight Integration for CA Unicenter
#*
#*      Copyright 1996,2003 Hewlett-Packard Development Company, L.P.
#*
#*      Hewlett-Packard Company shall not be liable for technical or
#*      editorial errors or omissions contained herein. The information in
#*      this document is provided "as is" without warranty of any kind and
#*      is subject to change without notice. The warranties for HP products
#*      are set forth in the express limited warranty statements
#*      accompanying such products. Nothing herein should be construed as
#*      constituting an additional warranty.
#*
#*      Confidential computer software. Valid license from HP required for
#*      possession, use or copying. Consistent with FAR 12.211 and 12.212,
#*      Commercial Computer Software, Computer Software Documentation, and
#*      Technical Data for Commercial Items are licensed to the U.S.
#*      Government under vendor's standard commercial license.
#*
#* **************************************************************************
#*                                                                        
#* PROPRIETARY NOTE:                                                      
#*     This document contains information confidential and proprietary to 
#*     Hewlett-Packard and shall not be reproduced or transferred to other
#*     documents or disclosed to others or used for any purpose other than 
#*     that for which it was obtained without the expressed written consent
#*     of Hewlett-Packard Company.
#*                                                                        
#* **************************************************************************

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3002 * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Spare Drive Array Status: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Spare Drive Array status: OTHER'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3002 * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Spare Drive Array Status: INVALID'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Spare Drive Array status: INVALID'
       SEVERITY=E
       ATTRIB=default
       COLOR=RED

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3002 * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Spare Drive Array Status: FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Spare Drive Array has FAILED'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3002 * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Spare Drive Array Status: INACTIVE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Spare Drive Array has become INACTIVE'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion NAME=(*,20)
        ACTION=ANNOTATE TEXT='This alarm signifies that the spare is in a ready state.  This alarm is typically issued if you install or replace a spare drive in a drive array. It is issued after you replace a failed spare drive with a new one.'
DEFine MSGACTion NAME=(*,30)
        ACTION=ANNOTATE TEXT='This alarm may also occur when a drive fails and the spare becomes active, the failed drive is replaced, and the spare eventually becomes inactive again.'
DEFine MSGACTion NAME=(*,40)
        ACTION=ANNOTATE TEXT='In fault tolerant configurations, when a drive fails and a spare drive is available, the storage subsystem begins building data onto that spare.'
DEFine MSGACTion NAME=(*,50)
        ACTION=ANNOTATE TEXT='If the failed drive is replaced before restoration has completed, the process halts, and the data is restored to the replacement drive instead.'
DEFine MSGACTion NAME=(*,60)
        ACTION=ANNOTATE TEXT='If the failed drive is replaced after the build process is complete, the system reconstructs the data to the replacement drive, and the spare will revert to its original inactive state. This keeps a spare drive available.'
DEFine MSGACTion NAME=(*,70)
        ACTION=ANNOTATE TEXT='If you have installed or replaced a failed drive in the drive array, then this alarm is to be expected.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3002 * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - Spare Drive Array Status: BUILDING'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Spare Drive Array is BUILDING'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion NAME=(*,20)
        ACTION=ANNOTATE TEXT='This alarm is issued when a spare drive is brought online to replace a failed drive, and the drive array subsystem begins to build data onto the spare.'
DEFine MSGACTion NAME=(*,30)
        ACTION=ANNOTATE TEXT='In fault tolerant configurations, when a spare drive is available, the storage subsystem begins building data onto that spare.'
DEFine MSGACTion NAME=(*,40)
        ACTION=ANNOTATE TEXT='If the failed drive is replaced before restoration has completed, the process halts, and the data is restored to the replacement drive instead.'
DEFine MSGACTion NAME=(*,50)
        ACTION=ANNOTATE TEXT='If the failed drive is replaced after the build process is complete, the system reconstructs the data to the replacement drive, and the spare reverts to its original inactive state. This keeps a spare drive available.'
DEFine MSGACTion NAME=(*,60)
        ACTION=ANNOTATE TEXT='When a spare drive is available, this alarm is usually issued after the Drive Array Physical Drive Status Change - Failed alarm.  This alarm indicates that a drive has failed.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3002 * * * * * * 6*'
       MSGNODE=*              
       DEScription='HP - Spare Drive Array Status: ACTIVE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Spare Drive Array is ACTIVE'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion NAME=(*,20)
        ACTION=ANNOTATE TEXT='A physical drive failed. The array successfully restored data onto a spare. That spare drive has now become active and replaces the failed drive.'
DEFine MSGACTion NAME=(*,30)
        ACTION=ANNOTATE TEXT='In fault tolerant configurations, when a spare drive is available, the storage subsystem begins building data onto that spare.'
DEFine MSGACTion NAME=(*,40)
        ACTION=ANNOTATE TEXT='If the failed drive is replaced before restoration has completed, the process halts, and the data is restored to the replacement drive instead. '
DEFine MSGACTion NAME=(*,50)
        ACTION=ANNOTATE TEXT='If the failed drive is replaced after the build process is complete, the system reconstructs the data to the replacement drive, and the spare will revert to its original inactive state. This keeps a spare drive available.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3003 * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Physical Drive Array Status: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Physical Drive Array status: OTHER' 
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3003 * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Physical Drive Array Status: OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Physical Drive Array is OK' 
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3003 * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Physical Drive Array Status: FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Physical Drive Array has FAILED' 
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3003 * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Physical Drive Array Status: Predictive Failure'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Physical Drive Array: Predictive Failure' 
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The S.M.A.R.T. hard drive or HP specific hard drive predicts imminent failure. The device or client issuing this alarm has a drive that exceeded one or more factory preset thresholds for functional degradation.'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='As a result of normal wear and tear, the operation of a hard drive may gradually deteriorate. If certain thresholds are exceeded, the drive may not perform to specified levels, and may be subject to hardware failure sometime in the future.'
DEFine MSGACTion NAME=(*,40)
       ACTION=ANNOTATE TEXT='Drives that exceed these thresholds need to be replaced, although true catastrophic failure has not yet occurred.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3004 * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Factory Threshold Physical Drive Array Status: FALSE' 
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Factory Threshold Drive Array physical drive is within its limits'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3004 * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Factory Threshold Physical Drive Array Status: TRUE' 
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Factory Threshold Drive Array physical drive has been exceeded'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3005 * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - 4MB Array Accelerator Write Cache Status: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - 4MB Array Accelerator Write Cache status: OTHER'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3005 * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - 4MB Array Accelerator Write Cache Status: INVALID'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - 4MB Array Accelerator Write Cache is INVALID'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3005 * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - 4MB Array Accelerator Write Cache Status: ENABLED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - 4MB Array Accelerator Write Cache is ENABLED'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3005 * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - 4MB Array Accelerator Write Cache Status: TEMPORARILY DISABLED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - 4MB Array Accelerator Write Cache is TEMPORARILY DISABLED'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3005 * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - 4MB Array Accelerator Write Cache Status: PERMANENTLY DISABLED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - 4MB Array Accelerator Write Cache is PERMANENTLY DISABLED'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3006 * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - 4MB Array Accelerator Write Cache Bad Data Status: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - 4MB Array Accelerator Write Cache bad data status: OTHER'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3006 * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - 4MB Array Accelerator Write Cache Bad Data Status: NONE NO DATA LOSS'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - 4MB Array Accelerator Write Cache is OK NO DATA LOSS'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3006 * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - 4MB Array Accelerator Write Cache Bad Data Status: POSSIBLE DATA LOSS'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - 4MB Array Accelerator Write Cache may possibly losing power, if data was being stored in the accelerator, it has been lost'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3007 * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - 4MB Array Accelerator Write Cache Battery Status: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - 4MB Array Accelerator Write Cache battery status: OTHER'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3007 * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - 4MB Array Accelerator Write Cache Battery Status: OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - 4MB Array Accelerator Write Cache battery is OK'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3007 * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - 4MB Array Accelerator Write Cache Battery Status: RECHARGING'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - 4MB Array Accelerator Write Cache battery is RECHARGING'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3007 * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - 4MB Array Accelerator Write Cache Battery Status: FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - 4MB Array Accelerator Write Cache battery has FAILED'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3007 * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - 4MB Array Accelerator Write Cache Battery Status: DEGRADED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - 4MB Array Accelerator Write Cache battery is DEGRADED'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
 
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3007 * * * * * * 6*'
       MSGNODE=*
       DEScription='HP - 4MB Array Accelerator Write Cache Battery Status: NOT PRESENT'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - 4MB Array Accelerator Write Cache battery is NOT PRESENT'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue