DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8243 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event During a Cell On Line Add inconsistent number of cells discovered'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event During a Cell On Line Add inconsistent number of cells discovered: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='During the on line addition of a cell the partition adding the cell has determined inconsistent data as to which cell is being added. The cell addition will be aborted and the partition will resume execution without the new cell.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8257 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error reading source cell port on XBC during data traversability test'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error reading source cell port on XBC during data traversability test: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while reading the routing from the source cell s port on the source XBC. Data Field: (source cell << 56 | source XBC << 32)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8269 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPUs of different maximum core frequencies are installed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPUs of different maximum core frequencies are installed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='CPU s of mixed maximum core frequencies are installed'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8271 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The RVL CC-Togo link initialization workaround (PS221) failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The RVL CC-Togo link initialization workaround (PS221) failed: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Concorde-Togo link initialization is having an intermittent failure. The data field contains the number of initialization sequences that failed before being successful.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8643 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PDC failed clearing the OLA steering bit in the Dillon microstatus reg.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PDC failed clearing the OLA steering bit in the Dillon microstatus reg.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='PDC failed clearing the OLA steering bit in the Dillon microstatus register. Data field contains the physical location of the cell with the failure. This can only happen on an OLA cell and will cause that cell to reset and not to join the'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='existing partition.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8648 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Fabric Discovery could not initialize the local cell s XBC link'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Fabric Discovery could not initialize the local cell s XBC link: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Fabric Discovery s final attempt to initialize the local cell s CC to Crossbar Chip (XBC) link has failed. This cell cannot talk to the fabric. Data: link init state bit read from the CC Link State register'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8652 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Internal firmware programming error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Internal firmware programming error: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An internal firmware error was encountered. This is usually caused by a bad parameter passed to a function, corrupt memory, corrupt malloc tables or something similar. The data field contains the physical address that failed mapping to a'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='virtual address  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8676 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error writing the XIN init disable register.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error writing the XIN init disable register.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failure while writing the XBC CSR containing the link status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8677 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error reading the XIN init state register.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error reading the XIN init state register.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failure while reading the XBC CSR containing the link status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8679 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event intermittent failure while retrying the CC to XBC link init'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event intermittent failure while retrying the CC to XBC link init: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Fabric Discovery s attempt to initialize the local cell s CC to XBC link has failed. The link initialization sequence has an intermittent problem.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8690 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Initialization of a PCI node in the firmware device tree failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Initialization of a PCI node in the firmware device tree failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='error code'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8691 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An error was encountered while scanning the PCI bus.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An error was encountered while scanning the PCI bus.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='error code'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8692 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An error was encountered initializing the PCI bridge'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An error was encountered initializing the PCI bridge: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='error code'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8693 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An error was encountered initializing the PCI IO map.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An error was encountered initializing the PCI IO map.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='pfa'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8694 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An error was encountered creating the PCI MMIO map'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An error was encountered creating the PCI MMIO map: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='pfa'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8709 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event There was an error initializing the SBA node'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event There was an error initializing the SBA node: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='error code'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8710 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event There was an error discovering the SBA'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event There was an error discovering the SBA: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='error code'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8711 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An error was encountered while resetting the SBA'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An error was encountered while resetting the SBA: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='error code'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8712 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event There was an error initializing the IO link'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event There was an error initializing the IO link: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error was detected in the link berween the CC and the I/O controller.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8713 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event There is a problem initializing the REO cable'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event There is a problem initializing the REO cable: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='cable status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8714 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The IO chassis discovered was powered off'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The IO chassis discovered was powered off: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Identified the cell number that is connected to the chassis.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8715 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event There was an error initializing the LBA'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event There was an error initializing the LBA: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='error code'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8716 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event There was an error querying the LBA width'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event There was an error querying the LBA width: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='error code'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8717 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event There was an error with the LBA phase'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event There was an error with the LBA phase: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='error code'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8718 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event There was an error clearing the LBA'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event There was an error clearing the LBA: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='error code'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8719 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event There was an error with the LBA log'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event There was an error with the LBA log: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='error code'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8720 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event There was an error discovering the LBA'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event There was an error discovering the LBA: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='error code'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8721 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event There was an error configuring the LBA'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event There was an error configuring the LBA: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='error code'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8722 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event There was an error scanning the PCI bus'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event There was an error scanning the PCI bus: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='error code'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8723 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event There was an error configuring PCI space through the LBA'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event There was an error configuring PCI space through the LBA: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='error code'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8747 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Firmware was unable to find a suitable block of main memory to relocate ROM'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Firmware was unable to find a suitable block of main memory to relocate ROM: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A Firmware tries to find a main memory block large enough meeting alignment requirements.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8756 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The Options service received an NVRAM allocation error.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The Options service received an NVRAM allocation error.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Options service received an error when attempting to allocate an NVRAM storage block. Either an error was returned from the call, or the call returned successfully yet an invalid address was returned.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8758 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event SAL errlog access timeout'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event SAL errlog access timeout: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Access to SAL error log procedure timed out because the log facility was busy processing a request from another CPU. Data field indicates the SAL procedure ID.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8761 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The Dillon IPR is not cleared after a MAX_RD_CLR_IPR_TRIES on a cell.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The Dillon IPR is not cleared after a MAX_RD_CLR_IPR_TRIES on a cell.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Dillon IPR is not cleared after a MAX_RD_CLR_IPR_TRIES on a cell. The Data Filed in the Cell number. See the next Chassis Code to see the MAX_RD_CLR_IPR_TRIES'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8762 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Indicated the Dillon IPR is not cleared after a number of PDC attemps.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Indicated the Dillon IPR is not cleared after a number of PDC attemps.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Indicated the Dillon IPR is not cleared after a number of PDC attemps. The Data Field contens the MAX_RD_CLR_IPR_TRIES. Please look at the previous Chassis Code to see the Cell number.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8768 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The echelon given in the data field is not fully populated.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The echelon given in the data field is not fully populated.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='One or more dimms are missing from the echelon given in the data field. The dimms may not be installed or firmware was not able to detect the dimms.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8771 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Attempted to read the port state from an illegal port number'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Attempted to read the port state from an illegal port number: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The code that reads the port state (landmine vs. healthy) expects a XBC internal port number, it received bogus data. The port state cannot be read. Data Field: (port << 44) | (xbc num << 32)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8772 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Attempted to write the port state for an illegal port'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Attempted to write the port state for an illegal port: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The code that writes the port state (landmine vs. healthy) expects a XBC internal port number, it received bogus data. The port state cannot be read. Data Field: (port << 44) | (xbc num << 32)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8784 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The main backplane is reporting the LPM status as fault.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The main backplane is reporting the LPM status as fault.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The main backplane is reporting the LPM status as fault.'

