DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9876 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU deconfigured while enabling L2 shared cache'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU deconfigured while enabling L2 shared cache: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while enabling the CPU L2 shared cache. The datafield contains a 32-bit error number and 32-bits of additional error information. The CPU will be deconfigured.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9877 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU deconfigured while retrieving default values from PAL'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU deconfigured while retrieving default values from PAL: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error while getting default values for programmable CPU internal registers from the CPU abstraction layer. The datafield contains a 32-bit error number and 32-bits of additional error information. The CPU will be deconfigured.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9878 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU deconfigured getting an address for a CPU internal register within a buffer from the CPU abstraction layer'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU deconfigured getting an address for a CPU internal register within a buffer from the CPU abstraction layer: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while getting an address for a CPU internal register within a buffer from the CPU abstraction layer. The datafield contains a 32-bit error number and 32-bits of additional error information. The CPU will be deconfigured.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9879 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU deconfigured while getting an address for a CPU internal register within a buffer from the CPU abstraction layer'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU deconfigured while getting an address for a CPU internal register within a buffer from the CPU abstraction layer: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while programming CPU internal registers with final configuration values. The datafield contains a 32-bit error number and 32-bits of additional error information. The CPU will be deconfigured.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9896 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Not enough error free memory to run late sefltests'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Not enough error free memory to run late sefltests: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='There was not enough error free memory in the system to run the late selftests.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10060 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The left cell latch is open.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The left cell latch is open.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The left cell ejector on the specified cell is open.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10061 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Right ejector latch is open'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Right ejector latch is open: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The right ejector latch on the specified cell board is open.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10062 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The optical emitters on the cell latch sensors are not functioning'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The optical emitters on the cell latch sensors are not functioning: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The optical emitters on the cell latch sensors are not functioning.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10063 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The vrm on the specified cell is reporting a voltage fault.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The vrm on the specified cell is reporting a voltage fault.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The specifed vrm is reporting a fault.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10064 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The vrm on the specified cell is reporting a temperature fault.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The vrm on the specified cell is reporting a temperature fault.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The specifed vrm is reporting a fault.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10065 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The rail on a cell is reporting a fault.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The rail on a cell is reporting a fault.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The specifed vrm is reporting a fault.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10068 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A I/O backplane vrm is reporting a voltage fault.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A I/O backplane vrm is reporting a voltage fault.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The specifed vrm is reporting a fault.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10069 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A I/O backplane power brick is reporting a voltage fault.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A I/O backplane power brick is reporting a voltage fault.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The specifed vrm is reporting a fault.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10070 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A I/O backplane vrm is reporting a temperature fault.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A I/O backplane vrm is reporting a temperature fault.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The specifed vrm is reporting a fault.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10071 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A I/O backplane power brick is reporting a temperature fault.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A I/O backplane power brick is reporting a temperature fault.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The specifed vrm is reporting a fault.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10072 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A I/O backplane vrm rail is reporting a fault.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A I/O backplane vrm rail is reporting a fault.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The specifed vrm is reporting a fault.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10073 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A I/O backplane power brick is reporting a rail fault.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A I/O backplane power brick is reporting a rail fault.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The specifed vrm is reporting a fault.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10077 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Power for a cell has been shut off due to open ejector latches.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Power for a cell has been shut off due to open ejector latches.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='N/a'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10103 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The specified system backplane vrm is reporting a module voltage fault.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The specified system backplane vrm is reporting a module voltage fault.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='n/a'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10104 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The specified system backplane vrm is reporting a temperature fault.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The specified system backplane vrm is reporting a temperature fault.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='n/a'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10105 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The specifed system backplane rail is reporting a fault'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The specifed system backplane rail is reporting a fault: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='n/a'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10115 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Master MP failure. Slave MP has taken control'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Master MP failure. Slave MP has taken control: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The master mp has failed. The slave has taken over management of the cabinet.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10116 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The NVRAM service was unable to satisfy an NVRAM allocation reques'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The NVRAM service was unable to satisfy an NVRAM allocation reques: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The NVRAM service was unable to satisfy an NVRAM allocation request.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10132 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The RTC not updating its internal time registers'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The RTC not updating its internal time registers: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The RTC seems to not be updating its internal time registers. The cell cannot boot without the RTC.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10159 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Uncorrectable PAA fault on MX2'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Uncorrectable PAA fault on MX2: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An uncorrectable PAA fault has occurred on the MX2 module and PAA firmware has halted. The system will continue to run without PAA firmware.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10351 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The maximum memory supported by this system has been exceeded.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The maximum memory supported by this system has been exceeded.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The maximum memory supported by this system has been exceeded. The data field contains the amount of memory supported by the system.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10361 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A command to the memory buffer chip failed to complete.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A command to the memory buffer chip failed to complete.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A command to the memory buffer chip failed to complete.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10489 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Input power to the specified UPS has failed.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Input power to the specified UPS has failed.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Input power to the specified UPS has failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10490 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Input power to the specified UPS has been restored.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Input power to the specified UPS has been restored.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Input power to the specified UPS has been restored.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10492 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event At least one processor has an inconsistant setting for multi-thread enablement.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event At least one processor has an inconsistant setting for multi-thread enablement.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware has detected that the tread enablement settings are not consistant on all cpus in the partition. The offending CPU is reported in the data field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10495 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event UPS power exhausted. The system is being powered down.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event UPS power exhausted. The system is being powered down.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The system is being powered down as UPS power is exhausted.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10623 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The checksum update for the PDT has failed.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The checksum update for the PDT has failed.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The checksum update for the PDT has failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10625 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The checksum in the memory area of NVM is bad.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The checksum in the memory area of NVM is bad.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The checksum in the memory area of NVM is bad. Memory NVM will be cleared.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10626 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Checksum calculation failed.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Checksum calculation failed.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Checksum calculation failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10628 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Both SAL s copy and BMC copy of the token specified in the data field is bad.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Both SAL s copy and BMC copy of the token specified in the data field is bad.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The BMC copy and SAL copy of the token specified in the data field has been initialized from the default value for the token due to an IPMI error and SAL NVM error.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10629 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Incompatible I/O Backplane or I/O cables installed.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Incompatible I/O Backplane or I/O cables installed.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Detected incompatibility between the cell board and the I/O backplane and/or I/O backplane cables.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10779 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The CPU modules have been installed in an illegal configuration on the cell board'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The CPU modules have been installed in an illegal configuration on the cell board: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The CPU modules have been installed in an illegal configuration on the cell board.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10780 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Invalid CPU terminator installed on the cell board.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Invalid CPU terminator installed on the cell board.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An invalid CPU terminator card is installed on the cell board. The data field indicates the physical location of the offending socket.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10814 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Significant numbers of corrected memory errors have been detected on the memory subsystem'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Significant numbers of corrected memory errors have been detected on the memory subsystem: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Significant numbers of corrected memory errors have been detected on the memory subsystem'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10822 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Over-temperature condition detected on a processor'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Over-temperature condition detected on a processor: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Over-temperature condition detected on a processor'

