DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5073 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event NVRAM test fail'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event NVRAM test fail: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='NVM has failed test. The system will halt'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5076 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Interrupt vector out of range'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Interrupt vector out of range: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A interrupt vector has been requested out of the acceptible range. Data: Vector Number.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5077 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Pal proc error getting pal copy info'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Pal proc error getting pal copy info: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The PAL Copy Info call has failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5078 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Pal proc error copying pal to memory'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Pal proc error copying pal to memory: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error coping PAL to memory'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5079 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Boot pal proc failure'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Boot pal proc failure: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A PAL Proc has failed. This will halt the processor. Data: Local CPU Number'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5080 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Console device failure'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Console device failure: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A console device has failed. Data: Physical Addr of device that failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5081 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Platform interface device failure'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Platform interface device failure: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A console device has failed. Data: Physical Addr of device that failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5082 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event platform scratch RAM test failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event platform scratch RAM test failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Platfrom Scratch RAM has failed the test.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5083 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU rendezvous failure'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU rendezvous failure: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CPU has failed to meeet rendezvous. Data: Local CPU Number'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5084 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error extracting sal_b from rom'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error extracting sal_b from rom: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='SFW could not extract SAL_B from the ROM'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5085 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Scratch RAM bad'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Scratch RAM bad: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Platform Scratch RAM has failed test.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5087 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event IPMI System Event Log (SEL) is full'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event IPMI System Event Log (SEL) is full: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='IPMI SEL full '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5091 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Slave wakeup before vector registered'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Slave wakeup before vector registered: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='No wakeup vector registered for processor Data: Local CPU Number'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5092 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU failed rendezvous handler'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU failed rendezvous handler: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Slave Rendezvous handler has failed. Data: Local CPU Number.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5098 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error building SMBIOS Tables'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error building SMBIOS Tables: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='SFW failed to build the SMBIOS tables'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5100 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Trap nest limit exceeded'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Trap nest limit exceeded: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The trap nesting limit has been exceeded. Data: Vector Number'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5101 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Trap not serviced'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Trap not serviced: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A trap has been requested and not serviced. Data: Vector Number'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5102 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Trap taken'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Trap taken: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A trap has been taken. Data: Number of the vector taken.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5103 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Uncleared interrupt'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Uncleared interrupt: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='At least one interrupt was not cleared. Data: The highest pending interrupt number'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5104 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unexpected external interrupt'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unexpected external interrupt: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An unexpected external interrupt has occurred. Data: External Interrupt Number'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5105 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Interrupt before redirection table set up'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Interrupt before redirection table set up: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An interrupt has occurred before setting up the IVT. Data: Interrupt Number'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5106 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU unexpected MCA'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU unexpected MCA: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An unexpected MCA has occurred before MCA s are unmasked. Data: Local CPU Number.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5107 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unexpected trap'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unexpected trap: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An unexpected trap has occurred. The trap number is either invalid or the requested trap has not been registered. Data: Trap Number'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5108 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU unknown boot error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU unknown boot error: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='SFW has detected an unknown error.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5118 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CC errors PAL failure'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CC errors PAL failure: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='SFW has detected a PAL Failure'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5119 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Expected MC vector unregistered'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Expected MC vector unregistered: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Expected Machine Check Vector not registered'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5121 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event INIT initiated'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event INIT initiated: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This is the equivalent of a TOC event in the PA RISC Architecture. On IPF systems, this event is called an INIT. This event can be triggered by the  tc  command from the MP, or from the button labeled  TOC  :wor  Transfer of Control  on the'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='Management card or bezel of the system. There are also other causes of an INIT generated by software. Data: Local CPU Number  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5123 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Expected I/O host bridge is missing '
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Expected I/O host bridge is missing : &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An I/O host bridge is missing. Firmware will continue boot and display the following EFI warning,  Unexpected hardware I/O configuration.  Data Field: Physical location of the missing I/O host bridge.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5124 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event LBA has unexpected number of I/O slots'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event LBA has unexpected number of I/O slots: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware detected an unexpected number of I/O slots connected to an I/O host bridge. Firmware display the following EFI warning message,  Unexpected hardware I/O configuration.  Data Field: Physical location of the I/O host bridge.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5125 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event I/O rope width does not match expected value'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event I/O rope width does not match expected value: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware found an I/O controller rope of unexpected width. Firmware will configure the I/O host bridge connected to the rope and display the following EFI warning message,  Unexpected hardware I/O configuration.  Data Field: Physical location'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='of the I/O host bridge connected to the rope.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5127 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Found unexpected I/O host bridge'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Found unexpected I/O host bridge: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware found an unexpected I/O host bridge. Firmware will configure the I/O host bridge and display the following EFI warning message,  Unexpected hardware I/O configuration.  Data Field: Physical location of the unexpected I/O host bridge.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5130 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PCI clock DLL error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PCI clock DLL error: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An I/O host bridge s bus frequency DLL circuit failed. Firmware will deconfigure the failed I/O host bridge and display the following EFI warning message,  Failed I/O slot(s) deconfigured.  Data Field: Physical location of the I/O host'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='bridge.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5131 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PCI hot plug controller failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PCI hot plug controller failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An I/O host bridge s hot-plug controller has failed. Firmware will deconfigure the I/O host bridge and display the following EFI warning message,  Failed I/O slot(s) deconfigured.  Data Field: Physical location of the I/O hostbridge.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5132 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Found unknown I/O rope width'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Found unknown I/O rope width: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware attempts to configure an I/O controller rope to an unsupported width. Firmware will deconfigure any I/O host bridge connected to the rope. Data Field: Physical location of the failed rope.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5133 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event I/O LBA clear error failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event I/O LBA clear error failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='During I/O host bridge configuration, firmware found a persistent error condition. Firmware will deconfigure the I/O host bridge and display the following EFI warning message,  Failed I/O slot(s) deconfigured.  Data Field: Physical location of'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='the I/O hostbridge.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5136 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event I/O host bridge inaccessible because rope reset failed to complete'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event I/O host bridge inaccessible because rope reset failed to complete: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An I/O host bridge is inaccessible because an I/O controller rope reset failed to complete. Firmware will deconfigure the I/O host bridge and display the following EFI warning message,  Failed I/O slot(s) deconfigured.  Data Field: Physical'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='location of the I/O host bridge.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5137 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Insufficient power to turn on PCI slot'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Insufficient power to turn on PCI slot: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='There is insufficient power. Firmware will not power on a hot-plug I/O slot. In addition, firmware will display the following EFI warning message,  Failed I/O slot(s) deconfigured.  Date Field: Physical location of the I/O slot.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5138 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PCI bus walk unknown error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PCI bus walk unknown error: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware encountered an unexpected error while attempting to configure an I/O host bridge s I/O devices. Firmware will continue boot but will not configure the I/O devices connected to the specified I/O host bridge. Such I/O devices will not'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='be usable as console nor boot devices but might be usable by the O/S. Data Field: Physical location of the I/O host bridge.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5139 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PCI bus walk resources exceeded'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PCI bus walk resources exceeded: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The total resource requirement from the I/O devices connected to an I/O host bridge exceeds the resource limit of the I/O host bridge. Firmware will continue boot but will not configure the I/O devices connected to the specified I/O host'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='bridge. In addition, firmware will display the following EFI warning message,  Insufficient resources to assign to one or more I/O devices.  Such I/O devices will not be usable as console nor boot devices but might be usable by the O/S. Data  '
DEFine MSGACTion Name=(*,40)
ACTION=ANNOTATE TEXT='Field: Physical location of the I/O host bridge." '

