#* **************************************************************************
#*
#*                  Insight Integration for CA Unicenter
#*
#*      Copyright 1996,2003 Hewlett-Packard Development Company, L.P.
#*
#*      Hewlett-Packard Company shall not be liable for technical or
#*      editorial errors or omissions contained herein. The information in
#*      this document is provided "as is" without warranty of any kind and
#*      is subject to change without notice. The warranties for HP products
#*      are set forth in the express limited warranty statements
#*      accompanying such products. Nothing herein should be construed as
#*      constituting an additional warranty.
#*
#*      Confidential computer software. Valid license from HP required for
#*      possession, use or copying. Consistent with FAR 12.211 and 12.212,
#*      Commercial Computer Software, Computer Software Documentation, and
#*      Technical Data for Commercial Items are licensed to the U.S.
#*      Government under vendor's standard commercial license.
#*
#* **************************************************************************
#*                                                                        
#* PROPRIETARY NOTE:                                                      
#*     This document contains information confidential and proprietary to 
#*     Hewlett-Packard and shall not be reproduced or transferred to other
#*     documents or disclosed to others or used for any purpose other than 
#*     that for which it was obtained without the expressed written consent
#*     of Hewlett-Packard Company.
#*                                                                        
#* **************************************************************************

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16016 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Physical Drive Status Change: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Physical Drive Status Change: OTHER (Chassis: &26, Time: &31, Bus: &36, Bay: &41, Model: &51 &52, S/N: &57, Firmware: &62, Failure Code: &67)'
       SEVerity=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16016 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Physical Drive Status Change: UNCONFIGURED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Physical Drive Status Change: UNCONFIGURED (Chassis: &26, Time: &31, Bus: &36, Bay: &41, Model: &51 &52, S/N: &57, Firmware: &62, Failure Code: &67)'
       SEVerity=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16016 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Physical Drive Status Change: OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Physical Drive Status Change: OK (Chassis: &26, Time: &31, Bus: &36, Bay: &41, Model: &51 &52, S/N: &57, Firmware: &62, Failure Code: &67)'
       SEVerity=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16016 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Physical Drive Status Change: THRESHOLD EXCEEDED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Physical Drive Status Change: THRESHOLD EXCEEDED (Chassis: &26, Time: &31, Bus: &36, Bay: &41, Model: &51 &52, S/N: &57, Firmware: &62, Failure Code: &67)'
       SEVerity=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16016 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Physical Drive Status Change: PREDICTIVE FAILURE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Physical Drive Status Change: PREDICTIVE FAILURE (Chassis: &26, Time: &31, Bus: &36, Bay: &41, Model: &51 &52, S/N: &57, Firmware: &62, Failure Code: &67)'
       SEVerity=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16016 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 6*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Physical Drive Status Change: FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Physical Drive Status Change: FAILED (Chassis: &26, Time: &31, Bus: &36, Bay: &41, Model: &51 &52, S/N: &57, Firmware: &62, Failure Code: &67)'
       SEVerity=E
       ATTRIB=default
       COLOR=red


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: OTHER (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: INVALID'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: INVALID (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: ENABLED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: ENABLED (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=S
       ATTRIB=default
       COLOR=green


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4 * * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED - Error Code: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED  - Error Code: OTHER (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Other - Indicates that the instrument agent does not recognize the error code.  You may need to update your software.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4 * * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED - Error Code: INVALID'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED  - Error Code: INVALID (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Invalid - Indicates that write cache operations are currently configured and enabled for at least one logical drive.  No write cache errors have occurred.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4 * * * * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED - Error Code: BAD CONFIG'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED  - Error Code: BAD CONFIG (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Bad Configuration - Indicates that write cache operations are temporarily disabled.  The Array Accelerator board was configured for a different controller.  This error could be caused if boards were switched from one system to another.'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='Rerun the EISA Configuration Utility and ensure that the board has been properly configured for this system.  Note: If data from another system was stored on the board, rerunning EISA Configuration will cause the data to be lost.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4 * * * * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED - Error Code: LOW BATTERY'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED  - Error Code: LOW BATTERY (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Low Battery Power - Indicates that write cache operations are temporarily disabled due to insufficient battery power.  Please view the Battery Status object instance for more information.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4 * * * * * * * * * * * * * * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED - Error Code: DISABLE ISSUED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED  - Error Code: DISABLE ISSUED (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Disable Command Issued - Indicates that write cache operations are temporarily disabled.  The device driver issues this command when the server is taken down.  This condition should not exist when the system regains power.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4 * * * * * * * * * * * * * * * * * * * 6*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED - Error Code: NO RESOURCES'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED  - Error Code: NO RESOURCES (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='No Resources Available - Indicates that write cache operations are temporarily disabled.  The controller does not have sufficient resources to perform write cache operations.'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='Once the operation that requires the resources has completed, this condition will clear and write cache operations will resume.  For example, when a replaced drive is being rebuilt, there will not be sufficient resources.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4 * * * * * * * * * * * * * * * * * * * 7*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED - Error Code: NOT CONNECTED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED  - Error Code: NOT CONNECTED (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Board Not Connected - Indicates that write cache operations are temporarily disabled.  The Array Accelerator board has been configured but is not currently attached to the controller. Check the alignment of the board and connections.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4 * * * * * * * * * * * * * * * * * * * 8*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED - Error Code: BAD MIRROR DATA'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED  - Error Code: BAD MIRROR DATA (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Bad Mirror Data - Indicates that write cache operations have been permanently disabled.  The Array Accelerator board stores mirrored copies of all data.'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='If data exists on the board when the system is first powered up, the board performs a data compare test between the mirrored copies. If the data does not match, an error has occurred. Data may have been lost. Your board may need servicing.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4 * * * * * * * * * * * * * * * * * * * 9*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED - Error Code: READ FAILURE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED  - Error Code: READ FAILURE (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Read Failure - Indicates that write cache operations have been permanently disabled.  The Array Accelerator board stores mirror copies of all data.  While reading the data from the board, memory parity errors have occurred.'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='Both copies were corrupted and cannot be retrieved.  Data has been lost, and you should service the board.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4 * * * * * * * * * * * * * * * * * * * 10*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED - Error Code: WRITE FAILURE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED  - Error Code: WRITE FAILURE (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Write Failure - Indicates that write cache operations have been permanently disabled.  This error occurs when an unsuccessful attempt was made to write data to the Array Accelerator board.'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='Data could not be written to write cache memory in duplicate due to the detection of parity errors.  This error does not indicate data loss.  You should service the Array Accelerator board.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4 * * * * * * * * * * * * * * * * * * * 11*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED - Error Code: CONFIG COMMAND'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED  - Error Code: CONFIG COMMAND (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Config Command - Indicates that write cache operations have been permanently disabled.  The configuration of the logical drives has changed.  You need to reconfigure the Array Accelerator board.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4 * * * * * * * * * * * * * * * * * * * 12*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED - Error Code: EXPAND IN PROGRESS'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED  - Error Code: EXPAND IN PROGRESS (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Expand In Progress - Indicates that cache operations are temporarily disabled due to an expand of a logical drive.  When the expand operation completes, the accelerator will be enabled.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4 * * * * * * * * * * * * * * * * * * * 13*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED - Error Code: SNAPSHOT IN PROGRESS'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED  - Error Code: SNAPSHOT IN PROGRESS (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Snapshot In Progress - Indicates that cache operations are temporarily disabled due to a snapshot operation that is queued up or in progress.  When the snapshot operation completes, the accelerator will be enabled.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4 * * * * * * * * * * * * * * * * * * * 14*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED - Error Code: REDUNDANT LOW BATTERY'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED  - Error Code: REDUNDANT LOW BATTERY (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Redundant Low Battery - Indicates that cache operations are temporarily disabled.  The redundant controller has insufficient cache battery power.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4 * * * * * * * * * * * * * * * * * * * 15*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED - Error Code: REDUNDANT SIZE MISMATCH'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED  - Error Code: REDUNDANT SIZE MISMATCH (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Redundant Size Mismatch - Indicates that cache operations are temporarily disabled.  The cache sizes on the redundant controllers do not match.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4 * * * * * * * * * * * * * * * * * * * 16*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED - Error Code: REDUNDANT CACHE FAILURE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED  - Error Code: REDUNDANT CACHE FAILURE (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Redundant Cache Failure - Indicates that cache operations are temporarily disabled.  The cache on the redundant controller has failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4 * * * * * * * * * * * * * * * * * * * 17*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED - Error Code: EXCESSIVE ECC ERRORS'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: TEMPORARILY DISABLED  - Error Code: EXCESSIVE ECC ERRORS (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Excessive ECC Errors - Indicates that write cache operations have been permanently disabled.  The number of cache lines experiencing excessive ECC errors has reached a preset limit.'



DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5 * * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED - Error Code: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED  - Error Code: OTHER (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Other - Indicates that the instrument agent does not recognize the error code.  You may need to update your software.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5 * * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED - Error Code: INVALID'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED  - Error Code: INVALID (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Invalid - Indicates that write cache operations are currently configured and enabled for at least one logical drive.  No write cache errors have occurred.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5 * * * * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED - Error Code: BAD CONFIG'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED  - Error Code: BAD CONFIG (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Bad Configuration - Indicates that write cache operations are temporarily disabled.  The Array Accelerator board was configured for a different controller.  This error could be caused if boards were switched from one system to another.'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='Rerun the EISA Configuration Utility and ensure that the board has been properly configured for this system.  Note: If data from another system was stored on the board, rerunning EISA Configuration will cause the data to be lost.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5 * * * * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED - Error Code: LOW BATTERY'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED  - Error Code: LOW BATTERY (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Low Battery Power - Indicates that write cache operations are temporarily disabled due to insufficient battery power.  Please view the Battery Status object instance for more information.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5 * * * * * * * * * * * * * * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED - Error Code: DISABLE ISSUED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED  - Error Code: DISABLE ISSUED (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Disable Command Issued - Indicates that write cache operations are temporarily disabled.  The device driver issues this command when the server is taken down.  This condition should not exist when the system regains power.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5 * * * * * * * * * * * * * * * * * * * 6*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED - Error Code: NO RESOURCES'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED  - Error Code: NO RESOURCES (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='No Resources Available - Indicates that write cache operations are temporarily disabled.  The controller does not have sufficient resources to perform write cache operations.'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='Once the operation that requires the resources has completed, this condition will clear and write cache operations will resume.  For example, when a replaced drive is being rebuilt, there will not be sufficient resources.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5 * * * * * * * * * * * * * * * * * * * 7*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED - Error Code: NOT CONNECTED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED  - Error Code: NOT CONNECTED (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Board Not Connected - Indicates that write cache operations are temporarily disabled.  The Array Accelerator board has been configured but is not currently attached to the controller. Check the alignment of the board and connections.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5 * * * * * * * * * * * * * * * * * * * 8*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED - Error Code: BAD MIRROR DATA'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED  - Error Code: BAD MIRROR DATA (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Bad Mirror Data - Indicates that write cache operations have been permanently disabled.  The Array Accelerator board stores mirrored copies of all data.'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='If data exists on the board when the system is first powered up, the board performs a data compare test between the mirrored copies. If the data does not match, an error has occurred. Data may have been lost. Your board may need servicing.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5 * * * * * * * * * * * * * * * * * * * 9*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED - Error Code: READ FAILURE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED  - Error Code: READ FAILURE (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Read Failure - Indicates that write cache operations have been permanently disabled.  The Array Accelerator board stores mirror copies of all data.  While reading the data from the board, memory parity errors have occurred.'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='Both copies were corrupted and cannot be retrieved.  Data has been lost, and you should service the board.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5 * * * * * * * * * * * * * * * * * * * 10*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED - Error Code: WRITE FAILURE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED  - Error Code: WRITE FAILURE (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Write Failure - Indicates that write cache operations have been permanently disabled.  This error occurs when an unsuccessful attempt was made to write data to the Array Accelerator board.'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='Data could not be written to write cache memory in duplicate due to the detection of parity errors.  This error does not indicate data loss.  You should service the Array Accelerator board.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5 * * * * * * * * * * * * * * * * * * * 11*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED - Error Code: CONFIG COMMAND'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED  - Error Code: CONFIG COMMAND (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Config Command - Indicates that write cache operations have been permanently disabled.  The configuration of the logical drives has changed.  You need to reconfigure the Array Accelerator board.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5 * * * * * * * * * * * * * * * * * * * 12*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED - Error Code: EXPAND IN PROGRESS'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED  - Error Code: EXPAND IN PROGRESS (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Expand In Progress - Indicates that cache operations are temporarily disabled due to an expand of a logical drive.  When the expand operation completes, the accelerator will be enabled.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5 * * * * * * * * * * * * * * * * * * * 13*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED - Error Code: SNAPSHOT IN PROGRESS'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED  - Error Code: SNAPSHOT IN PROGRESS (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Snapshot In Progress - Indicates that cache operations are temporarily disabled due to a snapshot operation that is queued up or in progress.  When the snapshot operation completes, the accelerator will be enabled.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5 * * * * * * * * * * * * * * * * * * * 14*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED - Error Code: REDUNDANT LOW BATTERY'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED  - Error Code: REDUNDANT LOW BATTERY (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Redundant Low Battery - Indicates that cache operations are temporarily disabled.  The redundant controller has insufficient cache battery power.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5 * * * * * * * * * * * * * * * * * * * 15*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED - Error Code: REDUNDANT SIZE MISMATCH'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED  - Error Code: REDUNDANT SIZE MISMATCH (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Redundant Size Mismatch - Indicates that cache operations are temporarily disabled.  The cache sizes on the redundant controllers do not match.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5 * * * * * * * * * * * * * * * * * * * 16*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED - Error Code: REDUNDANT CACHE FAILURE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED  - Error Code: REDUNDANT CACHE FAILURE (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Redundant Cache Failure - Indicates that cache operations are temporarily disabled.  The cache on the redundant controller has failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16017 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5 * * * * * * * * * * * * * * * * * * * 17*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED - Error Code: EXCESSIVE ECC ERRORS'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Status Change: PERMANENTLY DISABLED  - Error Code: EXCESSIVE ECC ERRORS (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Excessive ECC Errors - Indicates that write cache operations have been permanently disabled.  The number of cache lines experiencing excessive ECC errors has reached a preset limit.'



DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16018*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Bad Data'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Bad Data (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &46, Total Memory: &51)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that the agent has detected an Array Accelerator Cache Board that has lost battery power.  If data was being stored in the accelerator memory when the system lost power, that data has been lost. Verify that no data has been lost.'




DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16019*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Accelerator Board Battery Failed'
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Accelerator Board Battery Failed (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &46, Total Memory: &51)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that the agent has detected a battery failure associated with the Array Accelerator Cache Board.  User Action: Replace the Accelerator Cache Board.'



DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16020 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Controller Status Change: OTHER'
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Controller Status Change: OTHER (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16020 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Controller Status Change: OK'
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Controller Status Change: OK (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16020 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Controller Status Change: FAILED'
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Controller Status Change: FAILED (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16020 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Controller Status Change: OFFLINE'
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Controller Status Change: OFFLINE (Chassis: &26, Time: &31, Box I/O Slot: &36, S/N: &51, Total Memory: &56)'
       SEVerity=E
       ATTRIB=default
       COLOR=red


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16021 * * * * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Host Controller Status Change: OTHER'
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Host Controller Status Change: OTHER (Slot: &26, World Wide Name: &41 &42 &43 &44 &45)'
       SEVerity=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The agent is unable to determine the status of the host controller.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16021 * * * * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Host Controller Status Change: OK'
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Host Controller Status Change: OK (Slot: &26, World Wide Name: &41 &42 &43 &44 &45)'
       SEVerity=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16021 * * * * * * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Host Controller Status Change: FAILED'
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Host Controller Status Change: FAILED (Slot: &26, World Wide Name: &41 &42 &43 &44 &45)'
       SEVerity=E
       ATTRIB=default
       COLOR=red


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16021 * * * * * * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Host Controller Status Change: SHUTDOWN'
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Host Controller Status Change: SHUTDOWN (Slot: &26, World Wide Name: &41 &42 &43 &44 &45)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Indicates that the host controller has been shutdown.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16021 * * * * * * * * * * * * * * * * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Host Controller Status Change: LOOP DEGRADED'
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Host Controller Status Change: LOOP DEGRADED (Slot: &26, World Wide Name: &41 &42 &43 &44 &45)'
       SEVerity=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Indicates that the fibre channel connection is degraded.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16021 * * * * * * * * * * * * * * * * * * * * * 6*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Host Controller Status Change: LOOP FAILED'
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Host Controller Status Change: LOOP FAILED (Slot: &26, World Wide Name: &41 &42 &43 &44 &45)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Indicates that the fibre channel connection is failed.'
