#* **************************************************************************
#*
#*                  Insight Integration for CA Unicenter
#*
#*      Copyright 1996,2003 Hewlett-Packard Development Company, L.P.
#*
#*      Hewlett-Packard Company shall not be liable for technical or
#*      editorial errors or omissions contained herein. The information in
#*      this document is provided "as is" without warranty of any kind and
#*      is subject to change without notice. The warranties for HP products
#*      are set forth in the express limited warranty statements
#*      accompanying such products. Nothing herein should be construed as
#*      constituting an additional warranty.
#*
#*      Confidential computer software. Valid license from HP required for
#*      possession, use or copying. Consistent with FAR 12.211 and 12.212,
#*      Commercial Computer Software, Computer Software Documentation, and
#*      Technical Data for Commercial Items are licensed to the U.S.
#*      Government under vendor's standard commercial license.
#*
#* **************************************************************************
#*                                                                        
#* PROPRIETARY NOTE:                                                      
#*     This document contains information confidential and proprietary to 
#*     Hewlett-Packard and shall not be reproduced or transferred to other
#*     documents or disclosed to others or used for any purpose other than 
#*     that for which it was obtained without the expressed written consent
#*     of Hewlett-Packard Company.
#*                                                                        
#* **************************************************************************

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6001 * * * * * * ?*'
       MSGNODE=*
       DEScription='HP - A Bad Memory chip error detected'
       TYPE=MSG
DEFine MSGACTion NAME=(*,5)
       ACTION=sendkeep TEXT='HP - Bad Memory Chip has been detected by the error correcting memory'
       SEVerity=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6002 * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - correctable memory log status: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,5)
       ACTION=sendoper TEXT='HP - correctable memory log status: OTHER'
       SEVerity=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6002 * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - correctable memory log status: NOT SUPPORTED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,5)
       ACTION=sendoper TEXT='HP - correctable memory log status: NOT SUPPORTED'
       SEVerity=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6002 * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - correctable memory log status: DISABLED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,5)
       ACTION=sendoper TEXT='HP - correctable memory log status: DISABLED'
       SEVerity=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6002 * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - correctable memory log status: ENABLED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,5)
       ACTION=sendkeep TEXT='HP - correctable memory log status: ENABLED'
       SEVerity=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6003*'
       MSGNODE=*
       DEScription='HP - The System Temp Exceeded Operating Limits'
       TYPE=MSG
DEFine MSGACTion NAME=(*,5)
       ACTION=sendkeep TEXT='HP - Systems Temperature has exceeded its operating limits'
       SEVerity=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6004 * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - System Temp is Outside normal operating range: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,5)
       ACTION=sendoper TEXT='HP - System Temperature is outside normal operating range: OTHER'
       SEVerity=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6004 * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - System Temp is Outside normal operating range: CONTINUE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,5)
       ACTION=sendkeep TEXT='HP - System Temperature is outside normal operating range, but will continue'
       SEVerity=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6004 * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - System Temp is Outside normal operating range: SHUTDOWN'
       TYPE=MSG
DEFine MSGACTion NAME=(*,5)
       ACTION=sendkeep TEXT='HP - System Temperature is outside normal operating range and the system shutdown'
       SEVerity=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6005*'
       MSGNODE=*
       DEScription='HP - The System Temp Returned to normal'
       TYPE=MSG
DEFine MSGACTion NAME=(*,5)
       ACTION=sendkeep TEXT='HP - Systems Temperature has returned to normal operating range'
       SEVerity=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6006 * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - System Fan is operating status: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,5)
       ACTION=sendoper TEXT='HP - System Fan is operating: OTHER'
       SEVerity=S
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6006 * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - System Fan is operating status: CONTINUE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,5)
       ACTION=sendkeep TEXT='HP - System Fan thermal condition has degraded but will CONTINUE'
       SEVerity=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6006 * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - System Fan is operating status: SHUTDOWN'
       TYPE=MSG
DEFine MSGACTion NAME=(*,5)
       ACTION=sendkeep TEXT='HP - System Fan thermal condition has degraded and will SHUTDOWN'
       SEVerity=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6007*'
       MSGNODE=*
       DEScription='HP - Systems Optional fan is not operating properly'
       TYPE=MSG
DEFine MSGACTion NAME=(*,5)
       ACTION=sendkeep TEXT='HP - Systems Optional fan is not operating properly'
       SEVerity=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6008*'
       MSGNODE=*
       DEScription='HP - Any Previous System fans'
       TYPE=MSG
DEFine MSGACTion NAME=(*,5)
       ACTION=sendkeep TEXT='HP - Any previous NON-operational system fans have returned to normal'
       SEVerity=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6009*'
       MSGNODE=*
       DEScription='HP - Processor Fan'
       TYPE=MSG
DEFine MSGACTion NAME=(*,5)
       ACTION=sendkeep TEXT='HP - Processor Fan is not operating normally'
       SEVerity=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6010*'
       MSGNODE=*
       DEScription='HP - previous non-operational processor fans'
       TYPE=MSG
DEFine MSGACTion NAME=(*,5)
       ACTION=sendkeep TEXT='HP - Any previous NON-operational processor fans have returned to normal operation'
       SEVerity=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6011*'
       MSGNODE=*
       DEScription='HP - ASR System Feature'
       TYPE=MSG
DEFine MSGACTion NAME=(*,5)
       ACTION=sendkeep TEXT='HP - A system that has been shut down by the ASR feature is operational again'
       SEVerity=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6012*'
       MSGNODE=*
       DEScription='HP - A System Thermal Shutdown'
       TYPE=MSG
DEFine MSGACTion NAME=(*,5)
       ACTION=sendkeep TEXT='HP - A system that had a thermal shutdown has become operational'
       SEVerity=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6013*'
       MSGNODE=*
       DEScription='HP - Power On Self Test Errors'
       TYPE=MSG
DEFine MSGACTion NAME=(*,5)
       ACTION=sendkeep TEXT='HP - One or more Power On Self Test errors have occurred during reboot'
       SEVerity=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6014*'
       MSGNODE=*
       DEScription='HP - Server power supply has degraded'
       TYPE=MSG
DEFine MSGACTion NAME=(*,5)
       ACTION=sendkeep TEXT='HP - Server power supply has become degraded'
       SEVerity=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6015*'
       MSGNODE=*
       DEScription='HP - Bad memory chip detected by Error Correcting Memory'
       TYPE=MSG
DEFine MSGACTion NAME=(*,5)
       ACTION=sendkeep TEXT='HP - Bad memory chip detected by Error Correcting Memory (Total Errors &26)'
       SEVerity=W
       ATTRIB=default
       COLOR=orange

