DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8906 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An Error occurred trying to notify the MP of the attempted reset.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An Error occurred trying to notify the MP of the attempted reset.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while trying to notify the MP that a reset is about to occure (QPartitionReleaseBIB command). The status is in the data field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8924 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error Data tied to a previous Error Assert event'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error Data tied to a previous Error Assert event: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A software error has occurred. Data field consists of data pertinent to the error. Lab involvement is indicated.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8926 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed disabling the XIN link for a single cell medel'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed disabling the XIN link for a single cell medel: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A fabric access error occurred while trying to disable the CC to CC link on a single cell Medel system. This cell will halt. Data field: error status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8930 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error while getting the XBC Semaphore'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error while getting the XBC Semaphore: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='While updating the Port State register, the cell could not get the XBC semaphore. Data field is: (Port Num << 44 | XBC num << 32 | return status). Where return status is: (0 Success; -1 Access Failure; -2 Semaphore Owned By Another, -3'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='Semaphore Already Owned; -4 XBC Key Contention)  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8931 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error releasing the XBC Semaphore'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error releasing the XBC Semaphore: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='While updating the Port State register, the cell could not get the XBC semaphore. Data field is: (Port Num << 44 | XBC num << 32 | return status). Where return status is: (0 Success; -1 Generic Failure)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8936 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unexpected fabric firmware error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unexpected fabric firmware error: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An unexpected error occurred while initializing the fabric. The firmware is not able to analyze this error. Clues to the cause of this error may be found in the IPMI forward progress log (FPL) either shortly before or after this log entry'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='occurred. The FPL is available from the management processor using the  sl  command. HP-UX also saves these logs in the /var/stm/logs/os directory, and they can be viewed using the slview utility.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8939 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The CC s XIN link was found to be already initialized'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The CC s XIN link was found to be already initialized: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='While attempting to initialize the XIN link, it was found to already be initialized. A firmware assertion has failed. The link will not be re-initialized and processing should continue as normal. However, the system could be confused at this'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='point.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8940 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cell has been disabled by the PDHC because no CPU modules were found.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cell has been disabled by the PDHC because no CPU modules were found.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The PDHC FW could not detect any CPU modules on its Cell board, so it is holding the Cell in reset.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8941 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cell has been disabled by PDHC FW because the CPU modules are not compatible.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cell has been disabled by PDHC FW because the CPU modules are not compatible.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Cell has been disabled by PDHC FW because the CPU modules are not compatible. Compatibility is determined based on data stored in the Scratch/FRUID EEPROM on each CPU module. The CPU module partition compatibility byte for each CPU module'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='must be identical.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8942 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cell has been disabled because of invalid data in a CPU module Scratch EEPROM.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cell has been disabled because of invalid data in a CPU module Scratch EEPROM.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Cell has been disabled because of invalid data in a CPU module Scratch EEPROM. PDHC FW checksums the FRUID data stored in each CPU module s Scratch EEPROM. If a checksum fails, the Cell is held in reset and will not boot. The data field'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='identifies the CPU module that failed.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8954 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The Cell Battery voltage level low warning'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The Cell Battery voltage level low warning: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The battery voltage level is low for the cell. This indicates that the NVRAM will not be saved if the power is removed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8959 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error while copying the XBC routing to the local port'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error while copying the XBC routing to the local port: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='There was an error while copying the routing for the XBC to the local XBC port. The cell will reset. Data: (XBC port << 44) | (XBC num << 32) | return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8960 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A read after write of a XBC CSR failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A read after write of a XBC CSR failed: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The read immediately after a write while copying routing registers failed. Data: whether or not the XBC Key was enabled'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8962 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Couldn t release the Semaphore while writing routing states.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Couldn t release the Semaphore while writing routing states.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failed to release a XBC Semaphore while marking each XBC in the complex to indicate that routing has completed. Data: (XBC num << 32) | return value'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8964 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Couldn t write the XBC s forward progress register'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Couldn t write the XBC s forward progress register: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Writing this XBC s forward progress register failed. Data: (XBC num << 32) | return value'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8965 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Couldn t access the XBC semaphore registers.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Couldn t access the XBC semaphore registers.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failed to get a XBC Semaphore while marking each XBC in the complex to indicate that routing has completed. Skipping this XBC. Data: (XBC num << 32) | return value'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8966 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Couldn t determine the complex fabric topology'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Couldn t determine the complex fabric topology: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Reading this XBC s topology register failed. Data Field: (xbc num << 32) | return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8968 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error checking a cell to cell link during traversability tests'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error checking a cell to cell link during traversability tests: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Could not check the traversability between two cells on an XBCless platform. Data field: return status (1 = SUCCESS, 0 = FALSE, -1 = FAILURE)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8969 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An error occurred while traversing the cell to cell link.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An error occurred while traversing the cell to cell link.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Could not check the traversability between two cells on an XBCless platform. Data field: return status (1 = SUCCESS, 0 = FALSE, -1 = FAILURE)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8970 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error reading the local cell s XIN link state'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error reading the local cell s XIN link state: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='While checking traversability of a 2 cell back to back system, there was an error reading the local cell s XIN block. Data Field: return status (1 or -1)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8971 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error reading the remote cell s XIN link state register'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error reading the remote cell s XIN link state register: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='While checking traversability of a 2 cell back to back system, there was an error reading the local cell s XIN block. Data Field: return status (1 or -1)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8972 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The XIN link is not connected to the target cell.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The XIN link is not connected to the target cell.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Could not traverse to the target cell. The XIN link is either not initialized, or is not connected to the target cell. However, the target cell is designated to be within the partition. Data Field: target cell << 56 | XIN link state register'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8973 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The XIN link is not connected to the target cell.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The XIN link is not connected to the target cell.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Could not traverse to the target cell. The XIN link is either not initialized, or is not connected to the target cell. However, the target cell is designated to be within the partition. Data Field: target cell << 56 | XIN link state register'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8974 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error reading the XIN_LINK_STATE register while disabling the link'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error reading the XIN_LINK_STATE register while disabling the link: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error reading the XIN_LINK_STATE register of the CC. This occurred while verifying that the link had been disabled. Data Field: cell being read << 56 | return status from the CSR read.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8975 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error reading the XIN_LINK_STATE register'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error reading the XIN_LINK_STATE register: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failure while reading the XBC CSR containing the link status. This occurred while attempting the retry process to get XBC to CC link initialized. Data Field: link init status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8976 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unexpected fabric firmware error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unexpected fabric firmware error: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An unexpected error occurred while initializing the fabric. The firmware is not able to analyze this error. Clues to the cause of this error may be found in the IPMI forward progress log (FPL) either shortly before or after this log entry'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='occurred. The FPL is available from the management processor using the  sl  command. HP-UX also saves these logs in the /var/stm/logs/os directory, and they can be viewed using the slview utility.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8979 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The CPU is performance or functionally restricted'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The CPU is performance or functionally restricted: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The CPU that just completed self tests is functionally or performace restricted. The data field contains the Self Test State Parameter. The 2-bit state field (bits 1..0) can have the following values when this event is displayed: 01 -'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='Performance Restricted - cpu still functions 10 - Functionally Restricted - cpu doesn t function properly  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8981 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The RTC was found to be invalid and has been cleared'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The RTC was found to be invalid and has been cleared: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The RTC was found to be invalid and has been cleared'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8982 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Status indicates that the Late Self Tests did not actually run'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Status indicates that the Late Self Tests did not actually run: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System firmware requested that Late Self Tests be run by PAL, but PAL returned that the tests did not actually run on the processor. The data field indicates the status word returned by PAL.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8983 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A fabric walk failed while updating the cell state'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A fabric walk failed while updating the cell state: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An attempt to update the cell state has failed due to a fabric crossbar failure. The cell number being updated in in bits 63:56, while the traversable cell set (those cells connected to the fabric) is returned in bits 31:0'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8984 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Could not reset the cell due to failure updating cell state'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Could not reset the cell due to failure updating cell state: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failed to reset a cell due to an error setting the cell s state. The cell will not be reset with the other cells in the PD. The cell number is reported in the data field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9000 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event DRAM failure on DIMM XX, deallocte rank'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event DRAM failure on DIMM XX, deallocte rank: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='SFW has detected that a DRAM is failing on the DIMM specified by the physical location. The rank the failing DIMM is part of will be deallocated.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9019 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event System Clocks are not valid'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event System Clocks are not valid: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Internal CPU clocks are not valid when compared with the real time clock. The data field contains the hex value of the elapsed time. If this value is off a small percentage from the expected value (which is given in the next chassis code), the'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='event is emitted.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9020 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cell Online Addition failed due to fabric access error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cell Online Addition failed due to fabric access error: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Could not traverse the fabric to the cell being added. Data field: (chosen cell << 56) | return status, where -1 = failure'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9021 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Fabric found a bad XBC port on a reboot. Attempting to route around it.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Fabric found a bad XBC port on a reboot. Attempting to route around it.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A XBC port was found to be unhealthy on this reboot. This cell will attempt to route around it. Data field: (local Cell << 56) | (local internal Port << 44) | (local XBC << 32) | XBC internal port number being routed around.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9022 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Could not access an internal firmware table while rerouting XBC port'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Could not access an internal firmware table while rerouting XBC port: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error getting the XBC port s expected neighbor from a firmware table. Data field: 0 (SUCCESS) or -1 (FAILURE)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9038 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cell/Partition to be reset because PDC couldn t read PDH memory'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cell/Partition to be reset because PDC couldn t read PDH memory: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Either PDC is going to halt the cell or reset the partition because PDC was unable to access the PDH memory of either its local cell or another cell in the partition. The data field contains the error return value from PDC function'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='IsHCellCpuDeconfig().  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9039 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cell/Partition to be reset because PDC couldn t read PDH memory'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cell/Partition to be reset because PDC couldn t read PDH memory: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Either PDC is going to halt the cell or reset the partition because PDC was unable to access the PDH memory of either its local cell or another cell in the partition. The data field contains the error return value from PDC function'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='SleepAndWakeupCountersGet().  '

