#* **************************************************************************
#*
#*                  Insight Integration for CA Unicenter
#*
#*      Copyright 1996,2003 Hewlett-Packard Development Company, L.P.
#*
#*      Hewlett-Packard Company shall not be liable for technical or
#*      editorial errors or omissions contained herein. The information in
#*      this document is provided "as is" without warranty of any kind and
#*      is subject to change without notice. The warranties for HP products
#*      are set forth in the express limited warranty statements
#*      accompanying such products. Nothing herein should be construed as
#*      constituting an additional warranty.
#*
#*      Confidential computer software. Valid license from HP required for
#*      possession, use or copying. Consistent with FAR 12.211 and 12.212,
#*      Commercial Computer Software, Computer Software Documentation, and
#*      Technical Data for Commercial Items are licensed to the U.S.
#*      Government under vendor's standard commercial license.
#*
#* **************************************************************************
#*                                                                        
#* PROPRIETARY NOTE:                                                      
#*     This document contains information confidential and proprietary to 
#*     Hewlett-Packard and shall not be reproduced or transferred to other
#*     documents or disclosed to others or used for any purpose other than 
#*     that for which it was obtained without the expressed written consent
#*     of Hewlett-Packard Company.
#*                                                                        
#* **************************************************************************

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3010 * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Drive Array physical drive: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Drive Array physical drive status: OTHER'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3010 * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Drive Array physical drive: OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Drive Array physical drive is OK'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3010 * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Drive Array physical drive: FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Drive Array physical drive has FAILED'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3010 * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Drive Array physical drive: PREDICTIVE FAILURE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Drive Array physical drive: PREDICTIVE FAILURE'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The S.M.A.R.T. hard drive or HP specific hard drive predicts imminent failure. The device or client issuing this alarm has a drive that exceeded one or more factory preset thresholds for functional degradation.'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='As a result of normal wear and tear, the operation of a hard drive may gradually deteriorate. If certain thresholds are exceeded, the drive may not perform to specified levels, and may be subject to hardware failure sometime in the future.'
DEFine MSGACTion NAME=(*,40)
       ACTION=ANNOTATE TEXT='Drives that exceed these thresholds need to be replaced, although true catastrophic failure has not yet occurred.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3011 * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Drive Array physical drive factory threshold changed: TRUE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Drive Array physical drive factory threshold has been exceeded'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3011 * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Drive Array physical drive factory threshold changed: FALSE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Drive Array physical drive factory threshold is within its limits'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3012 * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - 4MB Array Accelerator Write Cache changed: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - 4MB Array Accelerator Write Cache status: OTHER'
       SEVERITY=I
       ATTRIB=DEFAULT
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3012 * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - 4MB Array Accelerator Write Cache changed: INVALID'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - 4MB Array Accelerator Write Cache has become INVALID'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3012 * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - 4MB Array Accelerator Write Cache changed: ENABLED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - 4MB Array Accelerator Write Cache is ENABLED'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3012 * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - 4MB Array Accelerator Write Cache changed: TEMPORARILY DISABLED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - 4MB Array Accelerator Write Cache is TEMPORARILY DISABLED'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3012 * * * * * * * * * * * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - 4MB Array Accelerator Write Cache changed: PERMANENTLY DISABLED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - 4MB Array Accelerator Write Cache is PERMANENTLY DISABLED'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3013 * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - 4MB Array Accelerator Write Cache Battery Status: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - 4MB Array Accelerator Write Cache battery status: OTHER'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3013 * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - 4MB Array Accelerator Write Cache Battery Status: OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - 4MB Array Accelerator Write Cache battery is OK'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3013 * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - 4MB Array Accelerator Write Cache Battery Status: POSSIBLE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - 4MB Array Accelerator Write Cache board lost battery power: Data loss Possible'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3014 * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - 4MB Array Accelerator Write Cache Battery Status: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - 4MB Array Accelerator Write Cache Battery status: OTHER'
       SEVERITY=I
       ATTRIB=DEFAULT
       COLOR=BLUE

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3014 * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - 4MB Array Accelerator Write Cache Battery Status: OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - 4MB Array Accelerator Write Cache battery is OK'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3014 * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - 4MB Array Accelerator Write Cache Battery Status: RECHARGING'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - 4MB Array Accelerator Write Cache battery is RECHARGING'
       SEVERITY=I
       ATTRIB=default
       COLOR=BLUE

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3014 * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - 4MB Array Accelerator Write Cache Battery Status: FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - 4MB Array Accelerator Write Cache battery has FAILED'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3014 * * * * * * * * * * * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - 4MB Array Accelerator Write Cache Battery Status: DEGRADING'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - 4MB Array Accelerator Write Cache battery: DEGRADED'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3014 * * * * * * * * * * * * * * * * 6*'
       MSGNODE=*
       DEScription='HP - 4MB Array Accelerator Write Cache Battery Status: NOT PRESENT'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - 4MB Array Accelerator Write Cache battery: NOT PRESENT'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
