#* **************************************************************************
#*
#*                  Insight Integration for CA Unicenter
#*
#*      Copyright 1996,2003 Hewlett-Packard Development Company, L.P.
#*
#*      Hewlett-Packard Company shall not be liable for technical or
#*      editorial errors or omissions contained herein. The information in
#*      this document is provided "as is" without warranty of any kind and
#*      is subject to change without notice. The warranties for HP products
#*      are set forth in the express limited warranty statements
#*      accompanying such products. Nothing herein should be construed as
#*      constituting an additional warranty.
#*
#*      Confidential computer software. Valid license from HP required for
#*      possession, use or copying. Consistent with FAR 12.211 and 12.212,
#*      Commercial Computer Software, Computer Software Documentation, and
#*      Technical Data for Commercial Items are licensed to the U.S.
#*      Government under vendor's standard commercial license.
#*
#* **************************************************************************
#*                                                                        
#* PROPRIETARY NOTE:                                                      
#*     This document contains information confidential and proprietary to 
#*     Hewlett-Packard and shall not be reproduced or transferred to other
#*     documents or disclosed to others or used for any purpose other than 
#*     that for which it was obtained without the expressed written consent
#*     of Hewlett-Packard Company.
#*                                                                        
#* **************************************************************************


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 12001*'
       MSGNODE=*
       DEScription='HP - A/C line power connected to a UPS failed'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - The A/C line power connected to a UPS has failed (Approximately &16 minutes of power remaining)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 12002*'
       MSGNODE=*
       DEScription='HP - A/C line power connected to a UPS ok' 
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - The A/C line power connected to a UPS has returned'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 12003*'
       MSGNODE=*
       DEScription='HP - UPS software is initiated a graceful server shutdown'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - UPS software has initiated a graceful server shutdown'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 12004*'
       MSGNODE=*
       DEScription='HP - system shutdown by the UPS software is operational'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - System that has been shutdown by the UPS software has just become operational'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 12005*'
       MSGNODE=*
       DEScription='HP - UPS low battery power status'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - the UPS is reporting low battery power and may lose power'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 12006*'
       MSGNODE=*
       DEScription='HP - The A/C line connected to UPS failed'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - The A/C line power connected to a UPS has failed (Approximately &26 minutes of power remaining)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 12007*'
       MSGNODE=*
       DEScription='HP - The A/C line connected to UPS returned'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - The A/C line power connected to a UPS has returned'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 12008*'
       MSGNODE=*
       DEScription='HP - The UPS software is initiating a server shutdown'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - the UPS software is initiating a graceful server shutdown'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 12009*'
       MSGNODE=*
       DEScription='HP - The UPS software shutdown has become operational'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - system shutdown initiated by UPS software is now operational'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 12010*'
       MSGNODE=*
       DEScription='HP - The UPS may lose power and shutdown'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - UPS is reporting low battery power and may lose power'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 12011*'
       MSGNODE=*
       DEScription='HP - The UPS is reporting an overload condition'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - the UPS is reporting an overload condition'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 12012*'
       MSGNODE=*
       DEScription='HP - The UPS is reporting low battery power'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - the UPS is reporting low battery power'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 12013*'
       MSGNODE=*
       DEScription='HP - Generic UPS Critical Alarm'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Generic UPS Critical Alarm: &26 &27 &28 &29 &30 &31 &32 &33 &34 &35 &36 &37 &38 &39 &40 &41 &42 &43 &44 &45 &46'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 12014*'
       MSGNODE=*
       DEScription='HP - UPS Informational Alarm'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - UPS Informational Alarm: &26 &27 &28 &29 &30 &31 &32 &33 &34 &35 &36 &37 &38 &39 &40 &41 &42 &43 &44 &45 &46'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
