DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10116 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Lockset 2 Unlocked (10116)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Lockset 2 Unlocked (10116)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting lockset 2 has been unlocked.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10117 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Lockset 2 Failed To Lock (10117)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Lockset 2 Failed To Lock (10117)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting lockset 2 has failed to lock.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10118 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Lockset 2 Error (10118)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Lockset 2 Error (10118)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting an error with lockset 2.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10119 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Lockset 2 Locked (10119)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Lockset 2 Locked (10119)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting lockset 2 has been locked.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10134 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Lockset 2 Normal (10134)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Lockset 2 Normal (10134)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting lockset 2 is normal.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10135 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Lockset 2 Normal (10135)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Lockset 2 Normal (10135)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting lockset 2 is normal.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20001 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - UPS Input Voltage Below Minimum (20001)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - UPS Input Voltage Below Minimum (20001)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting input voltage below minimum threshold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20002 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - UPS Input Voltage Above Maximum (20002)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - UPS Input Voltage Above Maximum (20002)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting input voltage above maximum threshold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20003 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - UPS Input Voltage Normal (20003)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - UPS Input Voltage Normal (20003)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting input voltage is out of range. Recommendations: 1. Check to make sure the UPS is plugged into an outlet supplied with utility power. 2. If the UPS remains on battery for an extended period of time it will not be able'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='to sustain the load.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20011 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - UPS Output Voltage Below Minimum (20011)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - UPS Output Voltage Below Minimum (20011)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting output voltage below minimum threshold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20012 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - UPS Output Voltage Above Maximum (20012)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - UPS Output Voltage Above Maximum (20012)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting output voltage above maximum threshold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21020 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - UPS Output Voltage Normal (21020)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - UPS Output Voltage Normal (21020)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting output voltage is out of Range. Recommendations: 1. Initiate a UPS self test. 2. If this error persists contact technical support.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20014 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - UPS Output Overload (20014)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - UPS Output Overload (20014)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting an overload condition. Recommendations: 1. Reduce the load on the UPS by moving some of the load to another UPS. 2. Consider moving to a larger UPS to support the current load.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20015 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - UPS Output Overload Cleared (20015)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - UPS Output Overload Cleared (20015)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting an overload condition. Recommendations: 1. Reduce the load on the UPS by moving some of the load to another UPS. 2. Consider moving to a larger UPS to support the current load.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21055 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - UPS Battery Low (21055)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - UPS Battery Low (21055)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting low battery. Recommendations: 1. Check to make sure the UPS is plugged into an outlet supplied with utility power. 2. When utility power is restored, charge the battery to it s full capacity. If the battery level'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='continues to decrease, the UPS will not be able to sustain the output load!  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21056 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - UPS Battery Low Cleared (21056)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - UPS Battery Low Cleared (21056)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting low battery. Recommendations: 1. Check to make sure the UPS is plugged into an outlet supplied with utility power. 2. When utility power is restored, charge the battery to it s full capacity. If the battery level'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='continues to decrease, the UPS will not be able to sustain the output load!  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20022 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - UPS Depleted Battery (20022)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - UPS Depleted Battery (20022)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is a depleted battery.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20023 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - UPS Battery Level Normal (20023)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - UPS Battery Level Normal (20023)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting low battery. Recommendations: 1. Check to make sure the UPS is plugged into an outlet supplied with utility power. 2. When utility power is restored, charge the battery to it s full capacity. If the battery level'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='continues to decrease, the UPS will not be able to sustain the output load!  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21063 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - UPS On Battery (21063)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - UPS On Battery (21063)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting on battery condition. Recommendations: 1. Check to make sure the UPS is plugged into an outlet supplied with utility power. If the UPS remains on battery for an extended time it will not be able to sustain the output'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='load!  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20032 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - UPS On Bypass (20032)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - UPS On Bypass (20032)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is being bypassed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21029 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - UPS On Buck (21029)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - UPS On Buck (21029)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting an On Buck condition due to the following. 1. Utility power has increased above recommended utility input levels. Recommendation: 1. Contact an electrician.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21031 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - UPS On Boost (21031)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - UPS On Boost (21031)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting an On Boost condition due to the following. 1. Utility power has dropped below recommended utility input levels. Recommendation: 1. Contact an electrician.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21064 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - UPS On Utility Power (21064)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - UPS On Utility Power (21064)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting on battery condition. Recommendations: 1. Check to make sure the UPS is plugged into an outlet supplied with utility power. If the UPS remains on battery for an extended time it will not be able to sustain the output'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='load!  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20101 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - UPS Temperature Low (20101)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - UPS Temperature Low (20101)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting temperature blow minimum threshold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20102 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - UPS Temperature High (20102)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - UPS Temperature High (20102)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting temperature above maximum threshold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20103 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - UPS Temperature Normal (20103)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - UPS Temperature Normal (20103)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting temperature is out of range. Recommendations: 1. Check to make sure the UPS is in a well ventilated area. 2. Lower the ambient temperature in the area where the UPS is located.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20111 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - UPS Internal Failure (20111)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - UPS Internal Failure (20111)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting a general UPS failure. Recommendations: 1. Initiate a UPS self test. 2. If this error persists contact technical support.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20112 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - UPS Internal Failure Cleared (20112)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - UPS Internal Failure Cleared (20112)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting a general UPS failure. Recommendations: 1. Initiate a UPS self test. 2. If this error persists contact technical support.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20121 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - UPS Battery Failure (20121)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - UPS Battery Failure (20121)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting a battery failure. Recommendations: 1. Initiate a UPS self test. 2. If this error persists contact technical support. 3. Your battery may need to be replaced. The UPS may not be capable of supporting it s load if'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='utility power fails!  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20122 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - UPS Battery Failure Cleared (20122)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - UPS Battery Failure Cleared (20122)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting a battery failure. Recommendations: 1. Initiate a UPS self test. 2. If this error persists contact technical support. 3. Your battery may need to be replaced. The UPS may not be capable of supporting it s load if'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='utility power fails!  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20131 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - UPS Diagnostic Test Failed (20131)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - UPS Diagnostic Test Failed (20131)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting a diagnostic test failed. Recommendations: 1. Your battery may need to be replaced. 2. If this error persists contact technical support. 3. The UPS may not be capable of supporting it s load if utility power fails!'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20132 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - UPS Diagnostic Test Succeeded (20132)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - UPS Diagnostic Test Succeeded (20132)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting a diagnostic test failed. Recommendations: 1. Your battery may need to be replaced. 2. If this error persists contact technical support. 3. The UPS may not be capable of supporting it s load if utility power fails!'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20141 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - Input Under Or Over Frequency (20141)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Input Under Or Over Frequency (20141)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Input (Utility) fault: measured input frequency is outside of either the upper or lower frequency limit specification for normal operation.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20142 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - Input Frequency Normal (20142)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Input Frequency Normal (20142)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Measured input frequency is normal'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 29998 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - DC Start Occurred (29998)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - DC Start Occurred (29998)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The UPS has been started on battery when AC input power is not present. This alarm is used to record the date and time of this event.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 29999 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - DC Start Occurred Cleared (29999)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - DC Start Occurred Cleared (29999)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The UPS has been started on utility while AC input power is present.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20161 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - Bypass Not Available (20161)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Bypass Not Available (20161)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting bypass not avaliable. Recommendations: 1. Initiate a UPS self test. 2. If this error persists contact technical support.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20162 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - Bypass Not Available Cleared (20162)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Bypass Not Available Cleared (20162)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting bypass not avaliable. Recommendations: 1. Initiate a UPS self test. 2. If this error persists contact technical support.'

