DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9420 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Power has been removed from AC input B1.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Power has been removed from AC input B1.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Power is no longer being supplied to input B1 on the cabinet specified in the data field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9428 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to disable the XIN link during a failed link init'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to disable the XIN link during a failed link init: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failed to disable the XIN link init CSR on a XBCless system. Cell will halt. Data field: return status (0 = SUCCESS, -1 = FAILURE), -1 is expected for this event.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9430 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error copying the routing registers to the local port'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error copying the routing registers to the local port: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error writing the XBC port s routing registers. The cell will reboot. Data Field: XBC port << 44 | XBC num << 32 | return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9431 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error while reading the remote CC s XIN Error Mask register'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error while reading the remote CC s XIN Error Mask register: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Could not read the XIN error mask regisiter on the CC. Data Field: cell number and return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9432 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error clearing the init packet received bit in the XIN error mask'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error clearing the init packet received bit in the XIN error mask: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Could not write the XIN error mask regisiter on the CC. Data Field: cell number and return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9433 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to read the XBC s Port Status register'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to read the XBC s Port Status register: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='While testing link traversability, a XBC CSR could not be read. Data Field: Port Number << 44 | XBC Number << 32 | return value'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9438 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PDHC has detected the PDH battery low warning.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PDHC has detected the PDH battery low warning.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Battery-Low interrupt was signaled in the Interrupt Pending Register in Dillon (PDH) by the hardware. PDHC is merely reporting the problem.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9440 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event FW will not handoff to the OS_MCA handler for this MCA event'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event FW will not handoff to the OS_MCA handler for this MCA event: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This means that the system FW MCA handler is not going to handoff to the OS_MCA handler.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9441 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Resetting the partition because couldn t access PDH memory'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Resetting the partition because couldn t access PDH memory: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='When returning from other software, like when returning from ISL, PDC is trying to make sure that all of the slave processors in the partition are asleep; however, this event ID indicates that we were unable to access PDH memory of a cell that'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='is supposed to be part of our partition. The data field contains the error return status from a function called SleepAndWakeupCountersGet().  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9442 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Resetting the partition because a processor was not in expected state'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Resetting the partition because a processor was not in expected state: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='When returning to PDC from other software, like returning from ISL, PDC tries to verify that all the slave processors are in the expected state (ie that all slave processors are asleep); however, this event ID indicates that at least one'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='processor active in the partition was not asleep. So, PDC is going to reset the partition. The data field of this Event ID is the global CPU number of the first CPU in the partition not found in the expected state.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9445 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Halting the cell because a cell couldn t access its own PDH memory'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Halting the cell because a cell couldn t access its own PDH memory: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='PDC could not access one of its own data structures on the local cell. The cell will be halted. The data field contains the return status from the PDC function that encountered the error.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9448 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The NVRAM block table maintained by System Firmware is corrupt'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The NVRAM block table maintained by System Firmware is corrupt: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Unused'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9450 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Resetting cell because processor couldn t access it s own PDH memory'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Resetting cell because processor couldn t access it s own PDH memory: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The cell will be reset because it was unable to access PDH memory on its own cell. While trying to move all the slave processors on the cell to the  late boot sleep , the monarch tried to write the sleep timeout to PDH memory on its own cell,'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='but encountered an error in doing so. The data field contains a PDC return status.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9460 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event All CPUs were deconfigured and have now been reconfigured.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event All CPUs were deconfigured and have now been reconfigured.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='All CPUs have been determined to be manually deconfigured in NVM during boot. This may only happen when switching from single core CPU deconfiguration to multi-core CPU deconfiguration in product qualification testing. As a recovery, NVM'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='settings have been changed to reconfigure all CPUs.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9461 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A failure has occurred trying to get the number of CPU cores per module.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A failure has occurred trying to get the number of CPU cores per module.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A failure has occurred trying to determine the number of CPU cores per module. Depending upon the situation, either the cell will be halted or the entire partition will be reset.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9465 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Couldn t read the topology from the XBC register'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Couldn t read the topology from the XBC register: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='While writing the remote routing, the local XBC could not be accessed to determine the topology. Look for additional chassis codes to determine what will happen as a result of this failure. Data field: return status, either SUCCESS (0) or'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='(-1)  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9466 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Attempt to update Cell Static Routing has failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Attempt to update Cell Static Routing has failed: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failed to route around a broken link on cell reboot. Data Field: PDC return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9468 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to read the XBC CSR that containes the number of failed links'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to read the XBC CSR that containes the number of failed links: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Could not read the XBC register that contains the number of links that are currently broken on the complex. Data Field: (XBC Num << 32) | PDC return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9469 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to read the XBC CSR that containes the number of failed links'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to read the XBC CSR that containes the number of failed links: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Could not read the XBC register that contains the number of links that are currently broken on the complex. Data Field: (XBC Num << 32) | PDC return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9470 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to write the XBC CSR that containes the number of failed links'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to write the XBC CSR that containes the number of failed links: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Could not write the XBC register that contains the number of links that are currently broken on the complex. Data Field: (XBC Num << 32) | PDC return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9471 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to read the XBC CSR that containes the number of failed links'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to read the XBC CSR that containes the number of failed links: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Could not read the XBC register that contains the number of links that are currently broken on the complex. Data Field: (XBC Num << 32) | PDC return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9472 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to write the XBC CSR that containes the number of failed links'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to write the XBC CSR that containes the number of failed links: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Could not write the XBC register that contains the number of links that are currently broken on the complex. Data Field: (XBC Num << 32) | PDC return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9473 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event This cell encountered too many broken crossbar links'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event This cell encountered too many broken crossbar links: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Too many broken crossbar links were found. This cell will have no connectivity to other cells in the complex. It will attempt a fabricless boot, except in a few configurations. Data Field: (XBC Num << 32) | number of broken links'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9474 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to read the XBC CSR that containes the number of failed links'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to read the XBC CSR that containes the number of failed links: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Could not read the XBC register that contains the number of links that are currently broken on the complex. Data Field: PDC return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9475 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to write the XBC CSR that containes the number of failed links'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to write the XBC CSR that containes the number of failed links: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Could not write the XBC register that contains the number of links that are currently broken on the complex. Data Field: (XBC Num << 32) | PDC return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9476 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to read the XBC CSR that marks the port route arounds'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to read the XBC CSR that marks the port route arounds: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Could not read the XBC register that marks the ports that have been routed around. Data Field: (XBC Num << 32) | PDC return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9477 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Could not traverse the PIOB route to the remote XBC'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Could not traverse the PIOB route to the remote XBC: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The PIOB route to the remote XBC was not traversable. The cell will halt. Data Field: (XBC Num << 32) | PDC return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9479 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to release the XBC semaphore after landmining a remote XBC port'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to release the XBC semaphore after landmining a remote XBC port: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Could not release the remote XBC s semaphore. Cell will halt. Data Field: (XBC Num << 32) | PDC return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9480 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to do a broadcast write to the XBC Remote Routing registers'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to do a broadcast write to the XBC Remote Routing registers: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failed to complete a broadcast write to an XBC. Data Field: (XBC Num << 32) | PDC return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9481 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to read a XBC Remote Routing register'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to read a XBC Remote Routing register: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failed to complete a read to the built-in port of a XBC. Data Field: (XBC Num << 32) | PDC return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9482 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to write a XBC Remote Routing register'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to write a XBC Remote Routing register: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failed to complete a write to the local cell s port of the XBC. Data Field: (XBC Port << 44) | (XBC Num << 32) | PDC return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9484 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The link between the CC and SBA failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The link between the CC and SBA failed: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The link between the CC and SBA failed meaning that I/O is not available to the reporting cell.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9485 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The SBA failed and the cell has no I/O'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The SBA failed and the cell has no I/O: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error was detected in the SBA and the reporting cell has no I/O.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9486 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The system firmware had an error with the structured error handling mechanism.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The system firmware had an error with the structured error handling mechanism.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The structured exception handling within the system firmware failed during I/O initialization.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9487 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Not enough malloc resources for I/O structure error handlig.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Not enough malloc resources for I/O structure error handlig.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='There is not enough malloc resources for the I/O structure exception handling. I/O on the reported cell is not available.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9488 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unable to create entry for I/O structure error handling.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unable to create entry for I/O structure error handling.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error creating the structure for housing the I/O structured exception handling services and data. I/O is lost on the reporting cell.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9489 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unable to bind services for I/O structure exception handling.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unable to bind services for I/O structure exception handling.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Unable to bind the I/O structure exception handling to the internal data structures.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9490 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error initializing the I/O structure exception handling services.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error initializing the I/O structure exception handling services.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error detected while initializing the I/O structure exception handling services.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9491 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error initializing structured I/O exception data structures.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error initializing structured I/O exception data structures.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error initializing the I/O structure exception handling data structures.'

