#* **************************************************************************
#*
#*                  Insight Integration for CA Unicenter
#*
#*      Copyright 1996,2003 Hewlett-Packard Development Company, L.P.
#*
#*      Hewlett-Packard Company shall not be liable for technical or
#*      editorial errors or omissions contained herein. The information in
#*      this document is provided "as is" without warranty of any kind and
#*      is subject to change without notice. The warranties for HP products
#*      are set forth in the express limited warranty statements
#*      accompanying such products. Nothing herein should be construed as
#*      constituting an additional warranty.
#*
#*      Confidential computer software. Valid license from HP required for
#*      possession, use or copying. Consistent with FAR 12.211 and 12.212,
#*      Commercial Computer Software, Computer Software Documentation, and
#*      Technical Data for Commercial Items are licensed to the U.S.
#*      Government under vendor's standard commercial license.
#*
#* **************************************************************************
#*                                                                        
#* PROPRIETARY NOTE:                                                      
#*     This document contains information confidential and proprietary to 
#*     Hewlett-Packard and shall not be reproduced or transferred to other
#*     documents or disclosed to others or used for any purpose other than 
#*     that for which it was obtained without the expressed written consent
#*     of Hewlett-Packard Company.
#*                                                                        
#* **************************************************************************

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16004 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Accelerator Board Status: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Fibre Channel Accelerator Board Status: OTHER'
       SEVerity=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16004 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Accelerator Board Status: INVALID'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Accelerator Board Status: INVALID'
       SEVerity=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The status of the FCA accelerator device is invalid, indicating that an Array Accelerator board has not been installed in this system or is not configured.'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='This state can also be reached if all the logical drives have had the accelerator disabled even though it is still installed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16004 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Accelerator Board Status: ENABLED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Fibre Channel Accelerator Board Status: ENABLED'
       SEVerity=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16004 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Accelerator Board Status: TEMPORARILY DISABLED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Accelerator Board Status: TEMPORARILY DISABLED'
       SEVerity=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The FCA Accelerator on the drive array controller has been temporarily disabled, due to one of the following reasons:'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='The accelerator is holding data, and is configured for a different Drive Array Controller. Make sure the accelerator is installed on the original controller;'
DEFine MSGACTion NAME=(*,40)
       ACTION=ANNOTATE TEXT='Battery charge level is below 75 percent; Sufficient resources to perform posted reads or writes are not available. This may be due to a current rebuilding process;' 
DEFine MSGACTion NAME=(*,50)
       ACTION=ANNOTATE TEXT='The accelerator has failed or has been detached from the controller; The accelerator is temporarily disabled when an expansion is taking place;'
DEFine MSGACTion NAME=(*,60)
       ACTION=ANNOTATE TEXT='The host operating system has temporarily disabled posted reads and/or writes.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16004 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Accelerator Board Status: PERMANENTLY DISABLED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Accelerator Board Status: PERMANENTLY DISABLED'
       SEVerity=E
       ATTRIB=default
       COLOR=red



DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16005*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Accelerator Board Bad Data'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Accelerator Board Bad Data: Accelerator Board lost Battery Power'
       SEVerity=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The Management Agent has detected an Array Accelerator Cache Board that has lost battery power.  If data was being stored in the accelerator memory when the server lost power, that data has been lost.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16006*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Accelerator Board: BATTERY FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Accelerator Board: BATTERY FAILED'
       SEVerity=E
       ATTRIB=default
       COLOR=red



DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16007 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Controller Status: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Fibre Channel Array Controller Status: OTHER'
       SEVerity=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16007 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Controller Status: OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Fibre Channel Array Controller Status: OK'
       SEVerity=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16007 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Controller Status: FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Controller Status: FAILED'
       SEVerity=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16007 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Controller Status: OFFLINE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Array Controller Status: OFFLINE'
       SEVerity=E
       ATTRIB=default
       COLOR=red



DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16008 * * * * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Tape Controller Status Change: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Tape Controller Status Change: OTHER'
       SEVerity=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16008 * * * * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Tape Controller Status Change: OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Tape Controller Status Change OK'
       SEVerity=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16008 * * * * * * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Tape Controller Status Change: OFFLINE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Tape Controller Status Change: OFFLINE'
       SEVerity=E
       ATTRIB=default
       COLOR=red



DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16009 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Tape Library Status: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Tape Library Status: OTHER'
       SEVerity=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16009 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Tape Library Status: OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Tape Library Status: OK'
       SEVerity=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16009 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Tape Library Status: DEGRADED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Tape Library Status: DEGRADED'
       SEVerity=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16009 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Tape Library Status: FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Tape Library Status: FAILED'
       SEVerity=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16009 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - Tape Library Status: OFFLINE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Tape Library Status: OFFLINE'
       SEVerity=W
       ATTRIB=default
       COLOR=orange



DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16010 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Tape Library Door Status: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Tape Library Door Status: OTHER'
       SEVerity=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16010 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Tape Library Door Status: Not Supported'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Tape Library Door Status: Not Supported'
       SEVerity=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16010 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Tape Library Door Status: Closed'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Tape Library Door Status: Closed'
       SEVerity=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16010 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Tape Library Door Status: Open'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Tape Library Door Status: Open'
       SEVerity=I
       ATTRIB=default
       COLOR=blue



DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16011 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Fiber Channel Tape Drive Status: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Fiber Channel Tape Drive Status: OTHER'
       SEVerity=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16011 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Fiber Channel Tape Drive Status: OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Fiber Channel Tape Drive Status: OK'
       SEVerity=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16011 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Fiber Channel Tape Drive Status: DEGRADED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Fiber Channel Tape Drive Status: DEGRADED'
       SEVerity=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16011 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Fiber Channel Tape Drive Status: FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Fiber Channel Tape Drive Status: FAILED'
       SEVerity=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16011 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - Fiber Channel Tape Drive Status: OFFLINE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Fiber Channel Tape Drive Status: OFFLINE'
       SEVerity=W
       ATTRIB=default
       COLOR=orange



DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16012*'
       MSGNODE=*
       DEScription='HP - Tape Drive Cleaning Required'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Tape Drive Cleaning is Required'
       SEVerity=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16013*'
       MSGNODE=*
       DEScription='HP - Tape Drive Cleaning Tape needs replacing'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Tape Drive Cleaning Tape needs replacement'
       SEVerity=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16014*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Array Controller Status: ACTIVE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Fibre Channel Array Controller Status: ACTIVE (Chassis Name: &26, FCACntrlBoxIOSlot: &36)'
       SEVerity=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The Storage Agent has detected that a backup array controller in a duplexed pair has switched over to the active role.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16015 * * * * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Host Controller Status Change: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Host Controller Status Change: OTHER (Slot: &26)'
       SEVerity=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16015 * * * * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Host Controller Status Change: OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Host Controller Status Change: OK (Slot: &26)'
       SEVerity=S
       ATTRIB=default
       COLOR=GREEN

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16015 * * * * * * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Host Controller Status Change: FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Host Controller Status Change: FAILED (Slot: &26)'
       SEVerity=E
       ATTRIB=default
       COLOR=RED

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16015 * * * * * * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Host Controller Status Change: SHUTDOWN'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Host Controller Status Change: SHUTDOWN (Slot: &26)'
       SEVerity=W
       ATTRIB=default
       COLOR=ORANGE

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16015 * * * * * * * * * * * * * * * * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Host Controller Status Change: LOOP DEGRADED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Host Controller Status Change: LOOP DEGRADED (Slot: &26)'
       SEVerity=W
       ATTRIB=default
       COLOR=ORANGE

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16015 * * * * * * * * * * * * * * * * * * * * * 6*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Host Controller Status Change: LOOP FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Host Controller Status Change: LOOP FAILED (Slot: &26)'
       SEVerity=E
       ATTRIB=default
       COLOR=RED
