DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9040 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cell/Partition to be reset because PDC couldn t read PDH memory'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cell/Partition to be reset because PDC couldn t read PDH memory: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Either PDC is going to halt the cell or reset the partition because PDC was unable to access the PDH memory of either its local cell or another cell in the partition. The data field contains the error return value from PDC function'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='PdhGetHCellStructAddr().  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9041 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cell/Partition to be reset because PDC couldn t read PDH memory'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cell/Partition to be reset because PDC couldn t read PDH memory: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Either PDC is going to halt the cell or reset the partition because PDC was unable to access the PDH memory of either its local cell or another cell in the partition. The data field contains the error return value from PDC function'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='HasCpuCompletedWakeupTask().  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9042 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cell/Partition to be reset because PDC couldn t read PDH memory'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cell/Partition to be reset because PDC couldn t read PDH memory: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Either PDC is going to halt the cell or reset the partition because PDC was unable to access the PDH memory of either its local cell or another cell in the partition. The data field contains the error return value from PDC function'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='PdhGetHCellStructAddr().  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9043 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A reset for reconfiguration will be performed soon on the cell.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A reset for reconfiguration will be performed soon on the cell.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='There is a need to reset the cell for reconfiguration, but it cannot be done yet because the cell has not reported at BIB. The Reset is being scheduled to be performed later.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9045 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The Partition Profile specifies the wrong architecture type'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The Partition Profile specifies the wrong architecture type: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='When processing the complex profile, the an unexpected  Architecture Type  was specified in the PA/IA Arch field. The actual data found is displayed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9046 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cell/Partition is about to be reset because PDC is unable to access CPU data'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cell/Partition is about to be reset because PDC is unable to access CPU data: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='While trying to determine whether or not a particular processor has completed the task for which it was awakened, PDC was unable to access the deconfig byte information about the target processor. A processor should always be able to access'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='this data in PDH memory for any processor on its own cell and for any processor on a cell that is alive in the partition. Therefore, PDC is either going to halt the cell or reset the partition because of this problem. The data field contains  '
DEFine MSGACTion Name=(*,40)
ACTION=ANNOTATE TEXT='the PDC error return status from IsHCellCpuDeconfig()." '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9047 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cell/Partition is about to be reset because PDC is unable to access CPU data'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cell/Partition is about to be reset because PDC is unable to access CPU data: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='While trying to determine whether or not a particular processor has completed the task for which it was awakened, PDC was unable to access the CPU s sleep and wakeup counters for the target processor. A processor should always be able to'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='access this data in PDH memory for any processor on its own cell and for any processor on a cell that is alive in the partition. Therefore, PDC is either going to halt the cell or reset the partition because of this problem. The data field  '
DEFine MSGACTion Name=(*,40)
ACTION=ANNOTATE TEXT='contains the PDC error return status from SleepAndWakeupCountersGet()." '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9049 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cell/Partition about to be reset because PDC is unable to access CPU data'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cell/Partition about to be reset because PDC is unable to access CPU data: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='While trying to determine whether or not a particular processor has completed the task for which it was awakened, PDC was unable to access the CPU s forward progress state (ie PST state) for the target processor. A processor should always be'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='able to access this data in PDH memory for any processor on its own cell and for any processor on a cell that is alive in the partition. Therefore, PDC is either going to halt the cell or reset the partition because of this problem. The data  '
DEFine MSGACTion Name=(*,40)
ACTION=ANNOTATE TEXT='field contains the PDC error return status from CpuFpSet()." '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9051 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cell/Partition is about to be reset because PDC is unable to access CPU data'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cell/Partition is about to be reset because PDC is unable to access CPU data: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='While trying to determine whether or not a particular processor has completed the task for which it was awakened, PDC was unable to access the CPU s Forward Progress State (ie PST state) for the target processor. A processor should always be'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='able to access this data in PDH memory for any processor on its own cell and for any processor on a cell that is alive in the partition. Therefore, PDC is either going to halt the cell or reset the partition because of this problem. The data  '
DEFine MSGACTion Name=(*,40)
ACTION=ANNOTATE TEXT='field contains the PDC error return status from CpuFpSet()." '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9052 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PDC is unable to branch to other software via the Page Zero location'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PDC is unable to branch to other software via the Page Zero location: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='At a certain point in PDC boot, all of the processors in the partition except the PD monarch are put into a sleep, and they remain there until they are awakened by the PD monarch, at which time they read an architected location in Page Zero to'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='find out where to branch to. This gives the OS a mechanism by which to bring processors under its control and have it executing OS code. This chassis log is sent if and when a problem is detected by PDC regarding the contents in the Page Zero  '
DEFine MSGACTion Name=(*,40)
ACTION=ANNOTATE TEXT='location. This means that PDC cannot branch to the location logged in the Page Zero location. So, PDC sends this chassis log and then the processor returns to sleep. The data field is unused." '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9084 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event New for MtWhatever: BOOT_BAD_CPU_ORDER'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event New for MtWhatever: BOOT_BAD_CPU_ORDER: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Data Field contains the value used to determine a valid order.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9364 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PDC couldn t access a data structure in PDH memory'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PDC couldn t access a data structure in PDH memory: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='While trying to get the sleep counter and the wakeup counter for a particular processor, which is kept in a data structure in PDH memory, PDC was unable to determine the address to the data structure on the remote cell. PDC is supposed to be'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='able to calculate addresses to anything in PDH memory on other cells in the partition. The data field contains the PDC error return status from a function called PdhGetHCellStructAddr().  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9365 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PDC couldn t access a data structure in PDH memory'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PDC couldn t access a data structure in PDH memory: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error occurred accessing a PDC data structure. Depending upon the situation the cell or entire partition will be reset. The data field contains the return status for the function that encountered the error.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9367 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cell about to be halted because PDC couldn t determine relocated address of code'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cell about to be halted because PDC couldn t determine relocated address of code: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='PDC is about to halt the cell because PDC was unable to determine the GNI address of the SlaveDispatcher function of PDC relocated to memory by PDC. The data field contains the error return value from the function'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='GetGniCodeAddrFromRomCodeAddr().  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9368 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Halting cell because a CPU didn t complete the task for which it was awakened'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Halting cell because a CPU didn t complete the task for which it was awakened: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='PDC is about to halt the cell because at least one of the processors didn t complete the task for which they were awakened and then return to sleep. The data field contains an error return status.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9370 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cell about to be halted because PDC couldn t determine relocated address of code'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cell about to be halted because PDC couldn t determine relocated address of code: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='PDC is about to halt the cell because PDC was unable to determine the GNI address of the CpuFpSet() function of PDC relocated to memory by PDC. The data field contains the error return value from the function GetGniCodeAddrFromRomCodeAddr().'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9371 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cell about to be halted because CPU couldn t change its CPU FP (PST) state'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cell about to be halted because CPU couldn t change its CPU FP (PST) state: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='PDC is about to halt the cell because one or more of the slaves were unable to change their CPU FP state in PDH memory on the local cell. The data field contains an error return status.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9372 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Partition about to be reset because PDC couldn t get address to a structure'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Partition about to be reset because PDC couldn t get address to a structure: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='PDC was trying to move the cell monarchs on each of the non-core cells into the Dispatcher, but in order to do that, the PD monarch needs to be able to read the CPU number of the cell monarch on each of the non-core cells, which is kept in a'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='data structure on each of the cells. PDC was unable to get the address to the CELL_CPU_STATE structure in PDH memory in a cell in the partition. The data field is the error return status from the PDC function called PdhGetHCellStructAddr().  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9373 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Resetting a partition because a CPU didn t complete the task it was awakened for'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Resetting a partition because a CPU didn t complete the task it was awakened for: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='PDC is about to reset the partitionl because at least one of the processors didn t complete the task for which they were awakened and then return to sleep. The data field contains the error return status from the PDC function'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='CheckSingleSlave().  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9375 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Resetting partition because PDC couldn t determine relocated address of code'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Resetting partition because PDC couldn t determine relocated address of code: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='PDC is about to reset the partition because it is unable to determine the GNI address for the CpuFpSet() function for one or more of the cells in the partition. The data field contains the error return status from'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='GetGniCodeAddrFromRomCodeAddr().  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9376 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Resetting partition because a CPU was unable to change its CPU FP state'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Resetting partition because a CPU was unable to change its CPU FP state: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='PDC is about to reset the partition because one or more of the processors were unable to successfully modify their CPU FP State (aka their PST state). The data field contains the error return status from the CpuFpSet() function.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9379 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU Dual Core Initialization Failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU Dual Core Initialization Failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='MX2 initialization failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9380 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Second CPU in Pair has been disabled'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Second CPU in Pair has been disabled: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A cpu that is attached to a cpu that is slated for deconfiguration is being deconfigured as well.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9382 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Virtualzing Dual Core Registers Failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Virtualzing Dual Core Registers Failed: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='FW failed to virtualize the mx2 interposer.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9383 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Virtualizing Dual Core Interposer has failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Virtualizing Dual Core Interposer has failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='FW has failed to virtualize the mx2 interposer.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9385 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Install PMI Handler Failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Install PMI Handler Failed: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Installation of the FW PMI handler has failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9388 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cell failed compatability checks.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cell failed compatability checks.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Cell and or cpus have failed compatability checks.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9389 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PDH space not available after release from reset.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PDH space not available after release from reset.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='PDH space not available after release from reset.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9390 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event MPON failed to release.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event MPON failed to release.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='MPON failed to release.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9391 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Dillon failed to reset.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Dillon failed to reset.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Dillon failed to reset.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9392 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event DMD clock is not running.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event DMD clock is not running.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='DMD clock is not running.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9394 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event All cpus on the Cell are scheduled to be deconfigured'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event All cpus on the Cell are scheduled to be deconfigured: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='All possible CPUs on a cell have been scheduled for deconfiguration.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9403 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A read error occurred while dumping the routing registers'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A read error occurred while dumping the routing registers: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A read error occurred while dumping the XBC port routing registers during boot. This cell will attempt fabricless boot. Data field: (XBC port << 48) | (XBC num << 32) | error status reg'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9412 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to disable the CC to CC link'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to disable the CC to CC link: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='After cell rendezvous for a 2 cell Medel, only one cell made it into the partition. Disabling the link failed. The cell will reset for reconfig. Data Field: return status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9417 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Power has been removed from AC input A0.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Power has been removed from AC input A0.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Power is no longer being supplied to input A0 on the cabinet specified in the data field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9418 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Power has been removed from AC input A1.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Power has been removed from AC input A1.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Power is no longer being supplied to input A1 on the cabinet specified in the data field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9419 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Power has been removed from AC input B0.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Power has been removed from AC input B0.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Power is no longer being supplied to input B0 on the cabinet specified in the data field.'

