DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5776 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event EFI unable to modify system state to  running '
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event EFI unable to modify system state to  running : &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='EFI is unable to modify the system state from  booting  to  running . This is done as part of Exit Boot Services. The system will not be able to enter a sleep mode. Data Field: For errors, this data is zero. For warnings, this data indicates'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='the current system state as: 0 Error 1 booting 2 running 3 attention 4 fault 5 booting + attention  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5777 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event /options settings for CPUBusConfigValue aren t compatible with PAL'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event /options settings for CPUBusConfigValue aren t compatible with PAL: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='CPUBusConfigValue setting in options as been compared with what is reported by PAL as settable and CPUBusConfigValue is specifying at least one bit that is not supported by this version of PAL using the Get Processor Bus Dependent'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='Configuration Features. This chassis code is emmitted in pairs, the first data field contains the PAL expected values; the second data field contains the requested setting from options.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5778 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The Get Processor Bus Dependent Configuration Features PAL call failed.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The Get Processor Bus Dependent Configuration Features PAL call failed.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware was unable to correctly issue the Get Processor Bus Dependent Configuration Features command.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5779 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event memory DIMM pair mismatch'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event memory DIMM pair mismatch: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A pair of DIMMs installed in the system are mismatched, and that pair of DIMMs will not be used. The data field indicates which pair of DIMMs are mismatched in the format 0x000000000000XBXA where X is the number of the rank that is'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='mismatched.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5784 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event EFI unable to initialize internal library'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event EFI unable to initialize internal library: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='EFI is unable to initialize internal library. This collection of internal services is required for much of EFI s functionality. EFI is halting.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5785 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event EFI unable to initialize security system'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event EFI unable to initialize security system: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='EFI is unable to initialize the security system. The privilege level of the system may or may not be Admin. It is likely certain EFI facilities will be unavailable. EFI will continue booting but security may be compromised. Data Field: Return'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='status from internal EFI function.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5786 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event EFI detected invalid internal privilege level'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event EFI detected invalid internal privilege level: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='EFI detected an invalid value for its internal privilege level. This value is stored within SAL. EFI will continue but system security may be compromised. Data Field: The invalid privilege level.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5787 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event EFI detected invalid privilege level when setting password'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event EFI detected invalid privilege level when setting password: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='EFI detected an invalid privilege level when setting a BMC password. Only the levels of Admin (0x30) and User (0x20) are permitted. Data Field: the invalid privilege level.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5788 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event EFI MDT table is bad'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event EFI MDT table is bad: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='SFW has determined that the Memory Data Table (MDT) table is invalid.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5790 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Processor has incompatible fixed core ratio'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Processor has incompatible fixed core ratio: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Processor has incompatible fixed core ratio. Data: Local CPU Number.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5791 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event All processors slated for compatibility deconfiguration'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event All processors slated for compatibility deconfiguration: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Data: A bitmask for which CPUs are slated to be deconfigured'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5793 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An unexpected or invalid value was read from a crossbar remote route table.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An unexpected or invalid value was read from a crossbar remote route table.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while reading a crossbar remote route table, or an unxpected/invalid value was read from the table. The data field consists of the crossbar ID (32:43), the port number of which the table was read (44:55), and the return'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='status of the read call (0:32).  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5794 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error reading the PORT[n]_NEIGHBOR_INFO XBC CSR.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error reading the PORT[n]_NEIGHBOR_INFO XBC CSR.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while trying to read the PORT[n]_NEIGHBOR_INFO crossbar CSR. The data field consists of the crossbar ID (32:43) and port number (44:55) for which the CSR was read.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5795 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event memory DIMM quad mis-match'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event memory DIMM quad mis-match: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A quad of DIMMs installed in the system are mismatched, and that quad of DIMMs will not be used. The data field indicates which quad of DIMMs are mismatched in the format 0x00000000XDXCXBXA where X is the number of the rank that is'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='mismatched.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5796 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Firmware detected excessive errors on the DIMM.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Firmware detected excessive errors on the DIMM.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The DIMM at the physical location given by the data field had excessive errors and has been marked as  FAILED  by firmware.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5797 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The OE (output enable) bit was not set for a XBC port.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The OE (output enable) bit was not set for a XBC port.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A XBC port was expected to be functional, but its OE bit was not set. The data field consists of the contents of the port_status CSR (0:31), the XBC number (32:43), and the port number (44:55).'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5798 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An error occurred while trying to read the PORT_STATUS CSR for a XBC port.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An error occurred while trying to read the PORT_STATUS CSR for a XBC port.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Unable to read the PORT_STATUS CSR for a XBC port. The data field consists of the contents of the PORT_STATUS CSR (0:31), the XBC number (32:43), and the port number (44:55).'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5799 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A XBC port was unexpectedly found to be landmined.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A XBC port was unexpectedly found to be landmined.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A XBC port was unexpectedly found to be landmined. The data field consists of the XBC number (32:43) and the port number (44:55).'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5800 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPUs running at different speeds were detected during rendezvous'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPUs running at different speeds were detected during rendezvous: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Reporting cell tried to rendezvous with a cell with processors that are running at a different speed. The data field lists the offending cell'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5802 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The link between the local CC and the local XBC is unexpectedly not initialized.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The link between the local CC and the local XBC is unexpectedly not initialized.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The link between the local CC and the local XBC is unexpectedly not initialized. The data field is the XIN_LINK_STATE CC CSR value.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5803 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An invalid XBC number was given.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An invalid XBC number was given.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A value that was expected to be a XBC number was found to be an invalid XBC number. The data field is the invalid XBC number.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5804 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An invalid XBC port number was given.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An invalid XBC port number was given.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A value that was expected to be a valid XBC port number was found to be invalid. The data field is the XBC number (33:44) and the invalid XBC port number (44:55).'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5805 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A bad parameter was passed to the LED function in the utilities component'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A bad parameter was passed to the LED function in the utilities component: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A bad parameter was passed to the utilities fuction that manipulates the LED on replacable parts. The offending parameter is displayed in the data field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5806 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An unexpected neighbor type was read from a XBC PORT_NEIGHBOR_INFO CSR.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An unexpected neighbor type was read from a XBC PORT_NEIGHBOR_INFO CSR.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A neighbor type read from a XBC PORT_NEIGHBOR_INFO CSR was different than the expected neighbor type. The data field contains the expected type (32:63) and the actual neighbor type (0:31).'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5807 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A given XBC port is not a valid XBC-CC port.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A given XBC port is not a valid XBC-CC port.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A XBC port number was unexpectedly found to not be a valid XBC-CC port. The data field consists of the XBC number (32:43) and the port number (44:55).'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5808 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A XBC port was unexpectedly found to be an invalid XBC-XBC port.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A XBC port was unexpectedly found to be an invalid XBC-XBC port.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A XBC port was unexpectedly found to be an invalid XBC-XBC port. The data field consists of the XBC number (32:43) and the port number (44:55).'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5809 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The XBC neighbor chip number does not match the expected value for this topology'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The XBC neighbor chip number does not match the expected value for this topology: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The XBC neighbor chip number does not match the expected value for this topology. The data field contains the expected neighbor chip number (32:63) and the actual neighbor chip number (0:31).'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5810 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The XBC neighbor port number does not match the expected value for this topology'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The XBC neighbor port number does not match the expected value for this topology: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The XBC neighbor port number does not match the expected value for this topology. The data field contains the expected neighbor port number (32:63) and the actual neighbor port number (0:31).'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5811 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Write through to BMC token failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Write through to BMC token failed: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A write to a BMC token has failed. This is a stop boot condition. Data: Upper 32 bits, BMC failure return code. Lower 32 bits, BMC token number that failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5812 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Utilities reported an error while trying to manipulate the LED'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Utilities reported an error while trying to manipulate the LED: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The utilities system reported an error while trying to carry out the command to turn on, flash or turn off the LED. The status returned by the command is displayed in the data field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5813 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Duplicate Cpu Ids were dectected within a cell.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Duplicate Cpu Ids were dectected within a cell.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='2 cpus think that they have the same ID within the cell. Typically this would mean that PAL reported the same cpu id for more than 1 cpu on a bus. The cpuid is in the data field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5823 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event OS crashdump started (D700)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event OS crashdump started (D700): &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='OS crashdump started (D700)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5824 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event OS legacy PA hex fault code (Bxxx)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event OS legacy PA hex fault code (Bxxx): &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='OS legacy PA hex fault code (Bxxx). Possible I/O error or system panic'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5825 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event OS dump status (EFxx)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event OS dump status (EFxx): &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='OS dump status (EFxx). Report on the success/failure of the writing of the dump. EF00 = success (followed by either EF0A = successful dump with sync, or EF09 = successful dump without sync), EFFF = a general error, EFFE = dump path assertion'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='failure, EFFD = no dump was taken by default, choice or failure, EFFC = dump was aborted by user.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5827 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Setting processor response timeout failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Setting processor response timeout failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='SFW has failed to set the processor timeout value via a PAL call. Data: PAL call return value.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5832 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unable to validate blank password during EFI security initialization'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unable to validate blank password during EFI security initialization: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='During EFI security initialization, the attempt to determine what privilege level a blank password provides, failed. Most likely this indicates the BMC has failed. EFI assumes that the BMC has failed and will attempt to continue booting. Some'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='EFI functionality may be unavailable. Data Field: Return status from internal EFI function.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5833 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unable to enter Guest mode during EFI security initialization'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unable to enter Guest mode during EFI security initialization: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='As part of normal security initialization, EFI attempted to issue a close session to the BMC (I.e. force the BMC to GUEST mode). This attempt failed. EFI is unable to initialize the security system. EFI will continue but security may be'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='compromised. Data Field: Return status from internal EFI function.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5834 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unable to increase privilege during EFI security initialization'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unable to increase privilege during EFI security initialization: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='As part of normal security initialization, EFI attempted to issue an open session to the BMC in order to raise the privilege level to the highest permitted by a blank password. This attempt failed. EFI is unable to initialize the security'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='system. Data Field: Return status from internal EFI function.  '

