#* **************************************************************************
#*
#*                  Insight Integration for CA Unicenter
#*
#*      Copyright 1996,2003 Hewlett-Packard Development Company, L.P.
#*
#*      Hewlett-Packard Company shall not be liable for technical or
#*      editorial errors or omissions contained herein. The information in
#*      this document is provided "as is" without warranty of any kind and
#*      is subject to change without notice. The warranties for HP products
#*      are set forth in the express limited warranty statements
#*      accompanying such products. Nothing herein should be construed as
#*      constituting an additional warranty.
#*
#*      Confidential computer software. Valid license from HP required for
#*      possession, use or copying. Consistent with FAR 12.211 and 12.212,
#*      Commercial Computer Software, Computer Software Documentation, and
#*      Technical Data for Commercial Items are licensed to the U.S.
#*      Government under vendor's standard commercial license.
#*
#* **************************************************************************
#*                                                                        
#* PROPRIETARY NOTE:                                                      
#*     This document contains information confidential and proprietary to 
#*     Hewlett-Packard and shall not be reproduced or transferred to other
#*     documents or disclosed to others or used for any purpose other than 
#*     that for which it was obtained without the expressed written consent
#*     of Hewlett-Packard Company.
#*                                                                        
#* **************************************************************************

#
# FCA trap 16022
#

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16022*'
       MSGNODE=*
       DEScription='HP - External Array Logical Drive Status Change (16022)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Array Logical Drive Status Change (Varbinds: &(22:))'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The trap variables were sent in the alarm, but they could not be properly parsed for information.  The variable information is displayed as part of the message.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16022 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - External Array Logical Drive Status Change: OTHER (16022)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Array Logical Drive Status Change: OTHER (Chassis: &26, Time: &31, Box Index: &36, Drv Index: &41, OS Name: &51, Fault Tolerance: &56, Size: &61)'
       SEVerity=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that the agent has detected a change in the status of an external array logical drive.  Fault Tolerance: other(1), none(2), mirroring(3), dataGuard(4), distribDataGuard(5), advancedDataGuard(7).'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16022 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - External Array Logical Drive Status Change: OK (16022)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Array Logical Drive Status Change: OK (Chassis: &26, Time: &31, Box Index: &36, Drv Index: &41, OS Name: &51, Fault Tolerance: &56, Size: &61)'
       SEVerity=S
       ATTRIB=default
       COLOR=green
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that the agent has detected a change in the status of an external array logical drive.  Fault Tolerance: other(1), none(2), mirroring(3), dataGuard(4), distribDataGuard(5), advancedDataGuard(7).'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16022 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - External Array Logical Drive Status Change: FAILED (16022)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Array Logical Drive Status Change: FAILED (Chassis: &26, Time: &31, Box Index: &36, Drv Index: &41, OS Name: &51, Fault Tolerance: &56, Size: &61)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that the agent has detected a change in the status of an external array logical drive.  Fault Tolerance: other(1), none(2), mirroring(3), dataGuard(4), distribDataGuard(5), advancedDataGuard(7).'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16022 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - External Array Logical Drive Status Change: UNCONFIGURED (16022)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Array Logical Drive Status Change: UNCONFIGURED (Chassis: &26, Time: &31, Box Index: &36, Drv Index: &41, OS Name: &51, Fault Tolerance: &56, Size: &61)'
       SEVerity=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that the agent has detected a change in the status of an external array logical drive.  Fault Tolerance: other(1), none(2), mirroring(3), dataGuard(4), distribDataGuard(5), advancedDataGuard(7).'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='Insure that all of the drive switches are properly set and that the Configuration Utility has been run.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16022 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - External Array Logical Drive Status Change: RECOVERING (16022)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Array Logical Drive Status Change: RECOVERING (Chassis: &26, Time: &31, Box Index: &36, Drv Index: &41, OS Name: &51, Fault Tolerance: &56, Size: &61)'
       SEVerity=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that the agent has detected a change in the status of an external array logical drive.  Fault Tolerance: other(1), none(2), mirroring(3), dataGuard(4), distribDataGuard(5), advancedDataGuard(7).'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='Indicates that the logical drive is using Interim Recovery Mode.  In Interim Recovery Mode, at least one physical drive has failed, but the logical drive fault tolerance mode lets the drive continue to operate with no data loss.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16022 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 6*'
       MSGNODE=*
       DEScription='HP - External Array Logical Drive Status Change: READY FOR REBUILD (16022)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Array Logical Drive Status Change: READY FOR REBUILD (Chassis: &26, Time: &31, Box Index: &36, Drv Index: &41, OS Name: &51, Fault Tolerance: &56, Size: &61)'
       SEVerity=S
       ATTRIB=default
       COLOR=green
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that the agent has detected a change in the status of an external array logical drive.  Fault Tolerance: other(1), none(2), mirroring(3), dataGuard(4), distribDataGuard(5), advancedDataGuard(7).'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='Indicates that the logical drive is ready for Automatic Data Recovery.  The physical drive that failed has been replaced, but the logical drive is still operating in Interim Recovery Mode.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16022 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 7*'
       MSGNODE=*
       DEScription='HP - External Array Logical Drive Status Change: REBUILDING (16022)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Array Logical Drive Status Change: REBUILDING (Chassis: &26, Time: &31, Box Index: &36, Drv Index: &41, OS Name: &51, Fault Tolerance: &56, Size: &61)'
       SEVerity=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that the agent has detected a change in the status of an external array logical drive.  Fault Tolerance: other(1), none(2), mirroring(3), dataGuard(4), distribDataGuard(5), advancedDataGuard(7).'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='Indicates that the logical drive is currently doing Automatic Data Recovery.  During Automatic Data Recovery, fault tolerance algorithms restore data to the replacement drive.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16022 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 8*'
       MSGNODE=*
       DEScription='HP - External Array Logical Drive Status Change: WRONG DRIVE (16022)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Array Logical Drive Status Change: WRONG DRIVE (Chassis: &26, Time: &31, Box Index: &36, Drv Index: &41, OS Name: &51, Fault Tolerance: &56, Size: &61)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that the agent has detected a change in the status of an external array logical drive.  Fault Tolerance: other(1), none(2), mirroring(3), dataGuard(4), distribDataGuard(5), advancedDataGuard(7).'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='Indicates that the wrong physical drive was replaced after a physical drive failure.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16022 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 9*'
       MSGNODE=*
       DEScription='HP - External Array Logical Drive Status Change: BAD CONNECT (16022)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Array Logical Drive Status Change: BAD CONNECT (Chassis: &26, Time: &31, Box Index: &36, Drv Index: &41, OS Name: &51, Fault Tolerance: &56, Size: &61)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that the agent has detected a change in the status of an external array logical drive.  Fault Tolerance: other(1), none(2), mirroring(3), dataGuard(4), distribDataGuard(5), advancedDataGuard(7).'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16022 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 10*'
       MSGNODE=*
       DEScription='HP - External Array Logical Drive Status Change: OVERHEATING (16022)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Array Logical Drive Status Change: OVERHEATING (Chassis: &26, Time: &31, Box Index: &36, Drv Index: &41, OS Name: &51, Fault Tolerance: &56, Size: &61)'
       SEVerity=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that the agent has detected a change in the status of an external array logical drive.  Fault Tolerance: other(1), none(2), mirroring(3), dataGuard(4), distribDataGuard(5), advancedDataGuard(7).'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='Indicates that the storage box that contains the logical drive is overheating.  The array is still functioning, but should be shutdown.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16022 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 11*'
       MSGNODE=*
       DEScription='HP - External Array Logical Drive Status Change: SHUTDOWN (16022)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Array Logical Drive Status Change: SHUTDOWN (Chassis: &26, Time: &31, Box Index: &36, Drv Index: &41, OS Name: &51, Fault Tolerance: &56, Size: &61)'
       SEVerity=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that the agent has detected a change in the status of an external array logical drive.  Fault Tolerance: other(1), none(2), mirroring(3), dataGuard(4), distribDataGuard(5), advancedDataGuard(7).'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='Indicates that the storage box that contains the logical drive has overheated.  The logical drive is no longer functioning.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16022 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 12*'
       MSGNODE=*
       DEScription='HP - External Array Logical Drive Status Change: EXPANDING (16022)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Array Logical Drive Status Change: EXPANDING (Chassis: &26, Time: &31, Box Index: &36, Drv Index: &41, OS Name: &51, Fault Tolerance: &56, Size: &61)'
       SEVerity=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that the agent has detected a change in the status of an external array logical drive.  Fault Tolerance: other(1), none(2), mirroring(3), dataGuard(4), distribDataGuard(5), advancedDataGuard(7).'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='This alarm indicates that the logical drive is currently performing Automatic Data Expansion.  This alarm may be issued if you have used the Array Configuration Utility to expand a drive array.'
DEFine MSGACTion NAME=(*,40)
       ACTION=ANNOTATE TEXT='Once Automatic Data Expansion is successfully completed, the FCA Logical Drive Status Change - OK alarm is also issued.  No further action is required at this time.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16022 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 13*'
       MSGNODE=*
       DEScription='HP - External Array Logical Drive Status Change: NOT AVAILABLE (16022)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Array Logical Drive Status Change: NOT AVAILABLE (Chassis: &26, Time: &31, Box Index: &36, Drv Index: &41, OS Name: &51, Fault Tolerance: &56, Size: &61)'
       SEVerity=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that the agent has detected a change in the status of an external array logical drive.  Fault Tolerance: other(1), none(2), mirroring(3), dataGuard(4), distribDataGuard(5), advancedDataGuard(7).'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='This alarm may be issued if you have used the Array Configuration Utility to expand a logical drive and the new configuration frees additional disk space. If this free space is configured into another logical drive it will be set to Not Available.'
DEFine MSGACTion NAME=(*,40)
       ACTION=ANNOTATE TEXT='Once the expansion process is complete, the logical drive that was Not Available will transition to a state of OK and the FCA Logical Drive Status Change - OK alarm will be issued.'
DEFine MSGACTion NAME=(*,50)
       ACTION=ANNOTATE TEXT='During the period of time that the logical drive is in a state of Not Available, the operating system may not allow the logical drive to become a useable part of the operating system disk subsystem.'
DEFine MSGACTion NAME=(*,60)
       ACTION=ANNOTATE TEXT='After the logical drive has transitioned to OK, use the operating system specific mechanism to enable the new logical disk into the operating system disk subsystem.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16022 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 14*'
       MSGNODE=*
       DEScription='HP - External Array Logical Drive Status Change: QUEUED FOR EXPANSION (16022)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Array Logical Drive Status Change: QUEUED FOR EXPANSION (Chassis: &26, Time: &31, Box Index: &36, Drv Index: &41, OS Name: &51, Fault Tolerance: &56, Size: &61)'
       SEVerity=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that the agent has detected a change in the status of an external array logical drive.  Fault Tolerance: other(1), none(2), mirroring(3), dataGuard(4), distribDataGuard(5), advancedDataGuard(7).'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16022 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 15*'
       MSGNODE=*
       DEScription='HP - External Array Logical Drive Status Change: HARD ERROR (16022)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Array Logical Drive Status Change: HARD ERROR (Chassis: &26, Time: &31, Box Index: &36, Drv Index: &41, OS Name: &51, Fault Tolerance: &56, Size: &61)'
       SEVerity=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that the agent has detected a change in the status of an external array logical drive.  Fault Tolerance: other(1), none(2), mirroring(3), dataGuard(4), distribDataGuard(5), advancedDataGuard(7).'

#
# Trap 16023 assumes a model name (cpqFcTapeDriveModel) of 1 word and a location name (cpqFcTapeDriveLocation)
# of 1 word.  If these are not matched, the first message record below is displayed.  The allocated spots for 
# model name and location can be modified to allow for more words in each.
#

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16023*'
       MSGNODE=*
       DEScription='HP - External Tape Drive Status Change'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Tape Drive Status Change (Varbinds: &(22:))'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The trap variables were sent in the alarm, but they could not be properly parsed for information.  The variable information is displayed as part of the message.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16023 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - External Tape Drive Status Change: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Tape Drive Status Change: OTHER (Controller Index: &26, Bus: &31, SCSI ID: &36, LUN: &41)'
       SEVerity=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16023 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - External Tape Drive Status Change: OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Tape Drive Status Change: OK (Controller Index: &26, Bus: &31, SCSI ID: &36, LUN: &41)'
       SEVerity=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16023 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - External Tape Drive Status Change: DEGRADED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Tape Drive Status Change: DEGRADED (Controller Index: &26, Bus: &31, SCSI ID: &36, LUN: &41)'
       SEVerity=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16023 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - External Tape Drive Status Change: FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Tape Drive Status Change: FAILED (Controller Index: &26, Bus: &31, SCSI ID: &36, LUN: &41)'
       SEVerity=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16023 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - External Tape Drive Status Change: OFFLINE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Tape Drive Status Change: OFFLINE (Controller Index: &26, Bus: &31, SCSI ID: &36, LUN: &41)'
       SEVerity=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16023 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 6*'
       MSGNODE=*
       DEScription='HP - External Tape Drive Status Change: MISSING WAS OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Tape Drive Status Change: MISSING WAS OK (Controller Index: &26, Bus: &31, SCSI ID: &36, LUN: &41)'
       SEVerity=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16023 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 7*'
       MSGNODE=*
       DEScription='HP - External Tape Drive Status Change: MISSING WAS OFFLINE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Tape Drive Status Change: MISSING WAS OFFLINE (Controller Index: &26, Bus: &31, SCSI ID: &36, LUN: &41)'
       SEVerity=W
       ATTRIB=default
       COLOR=orange

#
# FCA trap 16024
#

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16024*'
       MSGNODE=*
       DEScription='HP - External Tape Drive Cleaning Required'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Tape Drive Cleaning is Required (Controller Index: &26, Bus: &31, SCSI ID: &36, LUN: &41)'
       SEVerity=W
       ATTRIB=default
       COLOR=orange

#
# FCA trap 16025
#

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16025*'
       MSGNODE=*
       DEScription='HP - External Tape Drive Cleaning Tape needs replacing'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Tape Drive Cleaning Tape needs replacement (Controller Index: &26, Bus: &31, SCSI ID: &36, LUN: &41)'
       SEVerity=W
       ATTRIB=default
       COLOR=orange
