#* **************************************************************************
#*
#*                  Insight Integration for CA Unicenter
#*
#*      Copyright 1996,2003 Hewlett-Packard Development Company, L.P.
#*
#*      Hewlett-Packard Company shall not be liable for technical or
#*      editorial errors or omissions contained herein. The information in
#*      this document is provided "as is" without warranty of any kind and
#*      is subject to change without notice. The warranties for HP products
#*      are set forth in the express limited warranty statements
#*      accompanying such products. Nothing herein should be construed as
#*      constituting an additional warranty.
#*
#*      Confidential computer software. Valid license from HP required for
#*      possession, use or copying. Consistent with FAR 12.211 and 12.212,
#*      Commercial Computer Software, Computer Software Documentation, and
#*      Technical Data for Commercial Items are licensed to the U.S.
#*      Government under vendor's standard commercial license.
#*
#* **************************************************************************
#*                                                                        
#* PROPRIETARY NOTE:                                                      
#*     This document contains information confidential and proprietary to 
#*     Hewlett-Packard and shall not be reproduced or transferred to other
#*     documents or disclosed to others or used for any purpose other than 
#*     that for which it was obtained without the expressed written consent
#*     of Hewlett-Packard Company.
#*                                                                        
#* **************************************************************************

#
# Trap ID 1 from v22etrp.mib
#

DEFine MSGREcord MSGID='* SNMPTRAP: * * *1588 * * 6 1 * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Switch Fault Alert'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Switch Fault: Switch OK'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='A swFault is generated whenever the power-on startup (POST) diagnostics detects a fault with the switch.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *1588 * * 6 1 * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Switch Fault Alert'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Switch Fault: Central Memory Fault'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='A swFault is generated whenever the power-on startup (POST) diagnostics detects a fault with the switch.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *1588 * * 6 1 * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Switch Fault Alert'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Switch Fault: Embedded Port Fault'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='A swFault is generated whenever the power-on startup (POST) diagnostics detects a fault with the switch.'


#
# Trap ID 2 from v22etrp.mib
#


DEFine MSGREcord MSGID='* SNMPTRAP: * * *1588 * * 6 2 * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Sensor Scan'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Sensor Scan - Status: Unknown, Index: &21, Type: &26, Value: &31, Information: &(36:)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='A swSensorScn is generated whenever an environment sensor changes its operational state. For instance, a fan stops working.  Type may have the following values: temperature(1), fan(2), power-supply(3).'
DEFine MSGACTion Name=(*,30)
       ACTION=ANNOTATE TEXT='The varbinds will contain corresponding instance of the sensor status, sensor index, sensor type, sensor value (reading) and sensor information. Note that the sensor information contains the type of sensor and its number in textual format.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *1588 * * 6 2 * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Sensor Scan'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Sensor Scan - Status: Faulty, Index: &21, Type: &26, Value: &31, Information: &(36:)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='A swSensorScn is generated whenever an environment sensor changes its operational state. For instance, a fan stops working.  Type may have the following values: temperature(1), fan(2), power-supply(3).'
DEFine MSGACTion Name=(*,30)
       ACTION=ANNOTATE TEXT='The varbinds will contain corresponding instance of the sensor status, sensor index, sensor type, sensor value (reading) and sensor information. Note that the sensor information contains the type of sensor and its number in textual format.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *1588 * * 6 2 * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Sensor Scan'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Sensor Scan - Status: Below-Min, Index: &21, Type: &26, Value: &31, Information: &(36:)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='A swSensorScn is generated whenever an environment sensor changes its operational state. For instance, a fan stops working.  Type may have the following values: temperature(1), fan(2), power-supply(3).'
DEFine MSGACTion Name=(*,30)
       ACTION=ANNOTATE TEXT='The varbinds will contain corresponding instance of the sensor status, sensor index, sensor type, sensor value (reading) and sensor information. Note that the sensor information contains the type of sensor and its number in textual format.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *1588 * * 6 2 * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Sensor Scan'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Sensor Scan - Status: Nominal, Index: &21, Type: &26, Value: &31, Information: &(36:)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='A swSensorScn is generated whenever an environment sensor changes its operational state. For instance, a fan stops working.  Type may have the following values: temperature(1), fan(2), power-supply(3).'
DEFine MSGACTion Name=(*,30)
       ACTION=ANNOTATE TEXT='The varbinds will contain corresponding instance of the sensor status, sensor index, sensor type, sensor value (reading) and sensor information. Note that the sensor information contains the type of sensor and its number in textual format.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *1588 * * 6 2 * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Sensor Scan'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Sensor Scan - Status: Above-Max, Index: &21, Type: &26, Value: &31, Information: &(36:)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='A swSensorScn is generated whenever an environment sensor changes its operational state. For instance, a fan stops working.  Type may have the following values: temperature(1), fan(2), power-supply(3).'
DEFine MSGACTion Name=(*,30)
       ACTION=ANNOTATE TEXT='The varbinds will contain corresponding instance of the sensor status, sensor index, sensor type, sensor value (reading) and sensor information. Note that the sensor information contains the type of sensor and its number in textual format.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *1588 * * 6 2 * * * * * * 6*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Sensor Scan'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Sensor Scan - Status: Absent, Index: &21, Type: &26, Value: &31, Information: &(36:)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='A swSensorScn is generated whenever an environment sensor changes its operational state. For instance, a fan stops working.  Type may have the following values: temperature(1), fan(2), power-supply(3).'
DEFine MSGACTion Name=(*,30)
       ACTION=ANNOTATE TEXT='The varbinds will contain corresponding instance of the sensor status, sensor index, sensor type, sensor value (reading) and sensor information. Note that the sensor information contains the type of sensor and its number in textual format.'


#
# Trap ID 3 from v22etrp.mib
#


DEFine MSGREcord MSGID='* SNMPTRAP: * * *1588 * * 6 3 * * * * * * 0*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Port Scan'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Port Scan - Port Index &21 changed to state Unknown'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='A swFCPortScn is generated whenever an FC_Port changes its operational state. For instance, the FC_Port goes from on-line to offline. The port index can have a value from 1-16, where index1 = port0, index2 = port1, etc.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *1588 * * 6 3 * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Port Scan'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Port Scan - Port Index &21 changed to state Online'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='A swFCPortScn is generated whenever an FC_Port changes its operational state. For instance, the FC_Port goes from on-line to offline. The port index can have a value from 1-16, where index1 = port0, index2 = port1, etc.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *1588 * * 6 3 * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Port Scan'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Port Scan - Port Index &21 changed to state Offline'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='A swFCPortScn is generated whenever an FC_Port changes its operational state. For instance, the FC_Port goes from on-line to offline. The port index can have a value from 1-16, where index1 = port0, index2 = port1, etc.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *1588 * * 6 3 * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Port Scan'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Port Scan - Port Index &21 changed to state Testing'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='A swFCPortScn is generated whenever an FC_Port changes its operational state. For instance, the FC_Port goes from on-line to offline. The port index can have a value from 1-16, where index1 = port0, index2 = port1, etc.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *1588 * * 6 3 * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Port Scan'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Port Scan - Port Index &21 changed to state Faulty'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='A swFCPortScn is generated whenever an FC_Port changes its operational state. For instance, the FC_Port goes from on-line to offline. The port index can have a value from 1-16, where index1 = port0, index2 = port1, etc.'


#
# Trap ID 4 from v22etrp.mib
#


DEFine MSGREcord MSGID='* SNMPTRAP: * * *1588 * * 6 4*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Switch Event Alert'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Switch Event - Index: &16, Time: &21 &22 &23, Level: &28, Count: &33, Description: &(38:)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap is generated when an event whose level at or below swEventTrapLevel occurs.  A firmware event has been logged.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *1588 * * 6 4 * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Switch Event Alert'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Switch Event - Level: Critical, Index: &16, Time: &21 &22 &23, Count: &33, Description: &(38:)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap is generated when an event whose level at or below swEventTrapLevel occurs.  A firmware event has been logged.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *1588 * * 6 4 * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Switch Event Alert'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Switch Event - Level: Error, Index: &16, Time: &21 &22 &23, Count: &33, Description: &(38:)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap is generated when an event whose level at or below swEventTrapLevel occurs.  A firmware event has been logged.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *1588 * * 6 4 * * * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Switch Event Alert'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Switch Event - Level: Warning, Index: &16, Time: &21 &22 &23, Count: &33, Description: &(38:)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap is generated when an event whose level at or below swEventTrapLevel occurs.  A firmware event has been logged.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *1588 * * 6 4 * * * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Switch Event Alert'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Switch Event - Level: Informational, Index: &16, Time: &21 &22 &23, Count: &33, Description: &(38:)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap is generated when an event whose level at or below swEventTrapLevel occurs.  A firmware event has been logged.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *1588 * * 6 4 * * * * * * * * * * * * * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Switch Event Alert'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Switch Event - Level: Debug, Index: &16, Time: &21 &22 &23, Count: &33, Description: &(38:)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap is generated when an event whose level at or below swEventTrapLevel occurs.  A firmware event has been logged.'

#
# Trap ID 5 from v22etrp.mib
#

DEFine MSGREcord MSGID='* SNMPTRAP: * * *1588 * * 6 5*'
       MSGNODE=*
       DEScription='HP - Fabric Watch Trap'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fabric Watch Trap - Class/Area: &16, Threshold Index: &21, Varbinds: &(12:)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap is sent by Fabric Watch to notify of an event. Variables: swFwClassAreaIndex: Integer 1-51, swFwThresholdIndex: Integer, swFwName: String, swFwLabel: String, swFwLastEventVal: Integer,'
DEFine MSGACTion Name=(*,30)
       ACTION=ANNOTATE TEXT='swFwLastEventTime: String, swFwLastEvent: started(1), changed(2), exceeded(3), below(4), above(5), inBetween(6), swFwLastState: swFwInformative(1), swFwNormal(2), swFwFaulty(3)'

#
#DEFine MSGREcord MSGID='* SNMPTRAP: * * *1588 * * 6 5*'
#       MSGNODE=*
#       DEScription='HP - Fabric Watch Trap'
#       TYPE=MSG
#DEFine MSGACTion NAME=(*,10)
#       ACTION=sendkeep TEXT='HP - Fabric Watch Trap - Threshold &26 in Class/Area &16 at #index &21 has generated event &46 with &36 on &41. This event is &51'
#       SEVERITY=W
#       ATTRIB=default
#       COLOR=orange
#DEFine MSGACTion Name=(*,20)
#       ACTION=ANNOTATE TEXT='This trap is sent by Fabric Watch to notify of an event. #Variables: swFwClassAreaIndex, swFwThresholdIndex, swFwName, swFwLabel,	#swFwLastEventVal, swFwLastEventTime, swFwLastEvent, swFwLastState.'
#

#
# Trap ID 6 from v22etrp.mib
#

DEFine MSGREcord MSGID='* SNMPTRAP: * * *1588 * * 6 6*'
       MSGNODE=*
       DEScription='HP - Fibre Channel Switch Track Changes Alert'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fibre Channel Switch Track Changes Alert: &(16:)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap is sent for tracking login/logout/config changes.'


