--MibName=cpqSystemInfo
-- ****************************************************************************
--
--                           System Information
--         Management Information Base for SNMP Network Management
--
--
--      Copyright 1992,2003 Hewlett-Packard Development Company, L.P.
--
--      Hewlett-Packard Company shall not be liable for technical or
--      editorial errors or omissions contained herein. The information in
--      this document is provided "as is" without warranty of any kind and
--      is subject to change without notice. The warranties for HP products
--      are set forth in the express limited warranty statements
--      accompanying such products. Nothing herein should be construed as
--      constituting an additional warranty.
--
--      Confidential computer software. Valid license from HP required for
--      possession, use or copying. Consistent with FAR 12.211 and 12.212,
--      Commercial Computer Software, Computer Software Documentation, and
--      Technical Data for Commercial Items are licensed to the U.S.
--      Government under vendor's standard commercial license.
--
--      Refer to the READMIB.RDM file for more information about the
--      organization of the information in the Compaq Enterprise.
--
--      The Compaq Enterprise number is 232.
--      The ASN.1 prefix to, and including the Compaq Enterprise is:
--           1.3.6.1.4.1.232
--
-- ****************************************************************************

CPQSINFO-MIB DEFINITIONS ::= BEGIN

    IMPORTS
        compaq                  FROM CPQHOST-MIB
        DisplayString           FROM RFC1213-MIB
        OBJECT-TYPE             FROM RFC-1212
        sysName                 FROM RFC1213-MIB
        cpqHoTrapFlags          FROM CPQHOST-MIB
        TRAP-TYPE               FROM RFC-1215;


  compaq              OBJECT IDENTIFIER ::= { enterprises 232 }
    cpqSystemInfo       OBJECT IDENTIFIER ::= { compaq 2 }
    cpqSiMibRev         OBJECT IDENTIFIER ::= { cpqSystemInfo 1 }
    cpqSiComponent      OBJECT IDENTIFIER ::= { cpqSystemInfo 2 }

    cpqSiInterface      OBJECT IDENTIFIER ::= { cpqSiComponent 1 }
    cpqSiAsset          OBJECT IDENTIFIER ::= { cpqSiComponent 2 }
    cpqSiSecurity       OBJECT IDENTIFIER ::= { cpqSiComponent 3 }
    cpqSiSystemBoard    OBJECT IDENTIFIER ::= { cpqSiComponent 4 }
    cpqSiBoardRev       OBJECT IDENTIFIER ::= { cpqSiComponent 5 }
    cpqSiRackServer     OBJECT IDENTIFIER ::= { cpqSiComponent 6 }
    cpqSiVideo          OBJECT IDENTIFIER ::= { cpqSiComponent 7 }
    cpqSiMonitor        OBJECT IDENTIFIER ::= { cpqSiComponent 8 }
    cpqSiHotPlugSlot    OBJECT IDENTIFIER ::= { cpqSiComponent 9 }
    cpqSiSystemBattery  OBJECT IDENTIFIER ::= { cpqSiComponent 10 }
    cpqSiDockingStation OBJECT IDENTIFIER ::= { cpqSiComponent 11 }
    cpqSiFru            OBJECT IDENTIFIER ::= { cpqSiComponent 12 }
    cpqSiRackEnclosure  OBJECT IDENTIFIER ::= { cpqSiComponent 13 }

    cpqSiOsCommon       OBJECT IDENTIFIER ::= { cpqSiInterface 4 }

-- ****************************************************************************
--   System Information MIB Revision
--   ===============================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSystemInfo Group            (1.3.6.1.4.1.232.2)
--       cpqSiMibRev Group             (1.3.6.1.4.1.232.2.1)
--
--    Implementation of the MibRev group is mandatory for all Insight Agents
--    supporting the System Information MIB.
--
--     An Agent conforming to this document will return a
--     cpqSiMibRevMajor of one (1) and a cpqSiMibRevMinor of twenty-four (24).
--
--
-- ****************************************************************************

    cpqSiMibRevMajor OBJECT-TYPE
        SYNTAX  INTEGER (1..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The major revision level of the MIB.

            A change in the major revision level represents a major change
            in the architecture of the MIB.  A change in the major revision
            level may indicate a significant change in the information
            supported and/or the meaning of the supported information,
            correct interpretation of data may require a MIB document with
            the same major revision level."
        ::= { cpqSiMibRev 1 }

    cpqSiMibRevMinor OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The minor revision level of the MIB.

            A change in the minor revision level may represent some minor
            additional support, no changes to any pre-existing information
            has occurred."
        ::= { cpqSiMibRev 2 }

    cpqSiMibCondition OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            ok(2),              -- default
            degraded(3),
            failed(4)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The overall condition.

            This object represents the overall status of the server
            information represented by this MIB."
        ::= { cpqSiMibRev 3 }

-- ****************************************************************************
--   System Information Common
--   =========================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSystemInfo Group            (1.3.6.1.4.1.232.2)
--       cpqSiComponent Group          (1.3.6.1.4.1.232.2.2)
--        cpqSiInterface Group         (1.3.6.1.4.1.232.2.2.1)
--         cpqSiOsCommon Group         (1.3.6.1.4.1.232.2.2.1.4)
--
--
--  Implementation of the cpqSiOsCommon group is mandatory for all
--  Insight Agents that support the System Information MIB.
--
-- ****************************************************************************

    cpqSiOsCommonPollFreq OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "The Insight Agent's polling frequency.

            The frequency, in seconds, at which the Insight Agent requests
            information from the device driver.  A frequency of zero (0)
            indicates that the Insight Agent retrieves the information upon
            request of a management station, it does not poll the device
            driver at a specific interval.

            If the poll frequency is zero (0) all attempts to write to this
            object will fail.  If the poll frequency is non-zero,
            setting this value will change the polling frequency of the
            Insight Agent.  Setting the poll frequency to zero (0) will
            always fail, an agent may also choose to fail any request to
            change the poll frequency to a value that would severely impact
            system performance."
        ::= { cpqSiOsCommon 1 }


-- ****************************************************************************
--   System Information Common Module Table
--   ======================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSystemInfo Group            (1.3.6.1.4.1.232.2)
--       cpqSiComponent Group          (1.3.6.1.4.1.232.2.2)
--        cpqSiInterface Group         (1.3.6.1.4.1.232.2.2.1)
--         cpqSiOsCommon Group         (1.3.6.1.4.1.232.2.2.1.4)
--          cpqSiOsCommonModuleTable   (1.3.6.1.4.1.232.2.2.1.4.2) deprecated
--
-- ****************************************************************************

    cpqSiOsCommonModuleTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSiOsCommonModuleEntry
        ACCESS  not-accessible
        STATUS  deprecated
        DESCRIPTION
            "A table of software modules that provide an interface to the
            device this MIB describes."
        ::= { cpqSiOsCommon 2 }

    cpqSiOsCommonModuleEntry OBJECT-TYPE
        SYNTAX  CpqSiOsCommonModuleEntry
        ACCESS  not-accessible
        STATUS  deprecated
        DESCRIPTION
            "A description of a software module that provides an interface
            to the device this MIB describes."
        INDEX   { cpqSiOsCommonModuleIndex }
        ::= { cpqSiOsCommonModuleTable 1 }

        CpqSiOsCommonModuleEntry ::= SEQUENCE {
            cpqSiOsCommonModuleIndex       INTEGER,
            cpqSiOsCommonModuleName        DisplayString,
            cpqSiOsCommonModuleVersion     DisplayString,
            cpqSiOsCommonModuleDate        OCTET STRING,
            cpqSiOsCommonModulePurpose     DisplayString
        }

    cpqSiOsCommonModuleIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "A unique index for this module description."
        ::= { cpqSiOsCommonModuleEntry 1 }

    cpqSiOsCommonModuleName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The module name."
        ::= { cpqSiOsCommonModuleEntry 2 }

    cpqSiOsCommonModuleVersion OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..5))
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The module version in XX.YY format.

            Where XX is the major version number and YY is the minor version
            number.  This field will be a null (size 0) string if the agent
            cannot provide the module version."
        ::= { cpqSiOsCommonModuleEntry 3 }

    cpqSiOsCommonModuleDate OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (7))
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The module date.

             field  octets  contents                  range
             =====  ======  =======                  =====
               1      1-2   year                      0..65536
               2       3    month                     1..12
               3       4    day                       1..31
               4       5    hour                      0..23
               5       6    minute                    0..59
               6       7    second                    0..60
                            (use 60 for leap-second)


            This field will be set to year = 0 if the agent cannot provide
            the module date.  The hour, minute, and second field will be set
            to zero (0) if they are not relevant.  The year field is set
            with the most significant octet first."
        ::= { cpqSiOsCommonModuleEntry 4 }

    cpqSiOsCommonModulePurpose OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The purpose of the module described in this entry."
        ::= { cpqSiOsCommonModuleEntry 5 }

-- ****************************************************************************
--   System Information Asset Group
--   ==============================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSystemInfo Group            (1.3.6.1.4.1.232.2)
--       cpqSiComponent Group          (1.3.6.1.4.1.232.2.2)
--        cpqSiAsset Group             (1.3.6.1.4.1.232.2.2.2)
--
--  The cpqSiAsset group contains the serial numbers of any hardware
--  that supports asset management.
--
--  Implementation of the cpqSiAsset group is mandatory for all Insight
--  Agents that support the System Information MIB.
--
-- ****************************************************************************

    cpqSiSysSerialNum OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The serial number of the system unit.

            The string will be empty if the system does not report the
            serial number function."
        ::= { cpqSiAsset 1 }

    cpqSiFormFactor OBJECT-TYPE
        SYNTAX  INTEGER {
            unknown(1),
            portable(2),
            laptop(3),
            desktop(4),
            tower(5),
            mini-tower(6),
            rack-mount(7)
            }
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "The form factor of the system. Setting this variable to
             unknown will fail."
        ::= { cpqSiAsset 2 }

    cpqSiAssetTag OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "The customer changeable identifier that is set to the system
            serial number at the time of manufacture.

            The string will be empty if the system does not report this
            function."
        ::= { cpqSiAsset 3 }

     cpqSiOwnershipTag OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..79))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This is a customer changeable identifier that will be
            displayed by ROM at POST.  This is an 80 byte standard
            ASCII character string and is Administrator Password
            protected.

            An example could be:
              Property of Hewlett-Packard Company

            The string should be NULL terminated.  This item will be
            empty if the system does not report this function."
        ::= { cpqSiAsset 4 }

    cpqSiSysServiceNum OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The service number of the system unit.

            The string will be empty if the system does not report the
            system service number."
        ::= { cpqSiAsset 5 }

    cpqSiSysProductId OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The product id string of the system unit.

            The string will be empty if the system does not report the
            product id."
        ::= { cpqSiAsset 6 }


-- ****************************************************************************
--   System Information Security Group
--   =================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSystemInfo Group            (1.3.6.1.4.1.232.2)
--       cpqSiComponent Group          (1.3.6.1.4.1.232.2.2)
--        cpqSiSecurity Group          (1.3.6.1.4.1.232.2.2.3)
--
--  The Security group describes how the security features on your
--  computer are currently configured.
--
--  Implementation of the security group is mandatory for all agents that
--  support the System Information MIB.
--
-- ****************************************************************************

    cpqSiPowerOnPassword OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            disabled(2),
            enabled(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The state of the power on password feature."
        ::= { cpqSiSecurity 1 }

    cpqSiNetServerMode OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            disabled(2),
            enabled(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The state of the network server mode feature."
        ::= { cpqSiSecurity 2 }

    cpqSiQuickLockPassword OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            disabled(2),
            enabled(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The state of the quicklock password feature."
        ::= { cpqSiSecurity 3 }

    cpqSiQuickBlank OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            disabled(2),
            enabled(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The state of the quick blank screen feature."
        ::= { cpqSiSecurity 4 }

    cpqSiDisketteBootControl OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            disabled(2),
            enabled(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The state of the diskette boot control feature."
        ::= { cpqSiSecurity 5 }

    cpqSiSerialPortAControl OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            disabled(2),
            enabled(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The state of the access control for the primary serial port
            interface embedded in the system board."
        ::= { cpqSiSecurity 6 }

    cpqSiSerialPortBControl OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            disabled(2),
            enabled(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The state of the access control for the secondary serial port
            interface embedded in the system board."
        ::= { cpqSiSecurity 7 }

    cpqSiParallelPortControl OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            disabled(2),
            enabled(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The state of the access control for the parallel port interface
            embedded in the system board."
        ::= { cpqSiSecurity 8 }

    cpqSiFloppyDiskControl OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            disabled(2),
            enabled(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The state of the access control for the floppy diskette
            interface embedded in the system board."
        ::= { cpqSiSecurity 9 }

    cpqSiFixedDiskControl OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            disabled(2),
            enabled(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The state of the access control for the fixed disk interface
            embedded in the system board."
        ::= { cpqSiSecurity 10 }

    cpqSiHoodRemovedTime OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Last detection of hood removed by Smart Hood Sensor."

        ::= { cpqSiSecurity 11 }

    cpqSiHoodSensorConfiguration OBJECT-TYPE
        SYNTAX  INTEGER {
                other(1),
                disabled(2),
                notifyUser(3),
                adminPasswordProtected(4)
                }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This is the current configuration of the Smart Cover
             sensor.

             The following values are currently defined:

             other(1)
               Smart Cover sensor is not supported on this system or cannot
               be determined by the Insight Agent.  You may need to upgrade
               your software.

             disabled(2)
               Smart Cover sensor will not detect a hood removal and
               cpqSiHoodRemovedTime will not be updated.

             notifyUser(3)
               Smart Cover sensor will detect a hood removal and will display
               a message at POST for the user.

             adminPasswordProtected(4)
               Smart Cover sensor will detect a hood removal and will display
               a message at POST for the user to enter the Admin Password.
               The system will not boot until proper password is entered."
         ::= { cpqSiSecurity 12 }


    cpqSiSmartCoverLockStatus OBJECT-TYPE
        SYNTAX  INTEGER {
                other(1),
                unlocked(2),
                locked(3)
             }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This is the current status of the Smart Cover
             Lock. The following values are currently defined:

             other(1)
               Smart Cover Lock is not supported on this system or cannot
               be determined by the Insight Agent.  You may need to upgrade
               your software.

             unlocked(2)
               Smart Cover Lock is not locked.  The status will be set to
               unlocked due to one of the following:
                  1. The system hood is removed, or
                  2. There is no administrator password set, or
                  3. The administrator manually sets status to unlock.

             locked(3)
               Smart Cover Lock is locked. The administrator password is
               required to unlock the hood."
         ::= { cpqSiSecurity 13 }

    cpqSiUSBPortControl OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            disabled(2),
            enabled(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The state of the access control for the Universal
            Serial Bus interface(s) embedded in the system
            board."
        ::= { cpqSiSecurity 14 }

-- ****************************************************************************
--   System Information System Board Group
--   =====================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSystemInfo Group            (1.3.6.1.4.1.232.2)
--       cpqSiComponent Group          (1.3.6.1.4.1.232.2.2)
--        cpqSiSystemBoard Group       (1.3.6.1.4.1.232.2.2.4)
--
--  The cpqSiSystemBoard group describe features of your computer
--  system board.
--
--  Implementation of the cpqSiSystemBoard group is mandatory for all agents
--  that support the System Information MIB.
--
-- ****************************************************************************

    cpqSiProductId OBJECT-TYPE
        SYNTAX  INTEGER  (1..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The machine product ID.

            This value indicates the product type of the system board
            in this system.  The value 127 will be given if the machine ID
            cannot be determined.  A value of 127 will also be used for the
            special case of a machine containing neither EISA nor ISA slots."
        ::= { cpqSiSystemBoard 1 }

    cpqSiProductName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The machine product name.

            The name of the machine used in this system."
        ::= { cpqSiSystemBoard 2 }

    cpqSiAuxiliaryInput OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            disabled(2),
            enabled(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The state of the auxiliary input (pointing) device."
        ::= { cpqSiSystemBoard 4 }

-- ****************************************************************************
--   System Information Memory Module Table
--   ======================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSystemInfo Group            (1.3.6.1.4.1.232.2)
--       cpqSiComponent Group          (1.3.6.1.4.1.232.2.2)
--        cpqSiSystemBoard Group       (1.3.6.1.4.1.232.2.2.4)
--         cpqSiMemModuleTable         (1.3.6.1.4.1.232.2.2.4.5)
--          cpqSiMemModuleEntry        (1.3.6.1.4.1.232.2.2.4.5.1)
--
-- ****************************************************************************


    cpqSiMemModuleTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSiMemModuleEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A table of memory module descriptions."
        ::= { cpqSiSystemBoard 5 }

    cpqSiMemModuleEntry OBJECT-TYPE
        SYNTAX  CpqSiMemModuleEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A memory module description."
        INDEX   { cpqSiMemBoardIndex , cpqSiMemModuleIndex }
        ::= { cpqSiMemModuleTable 1 }

    CpqSiMemModuleEntry ::= SEQUENCE {
        cpqSiMemBoardIndex            INTEGER,
        cpqSiMemModuleIndex           INTEGER,
        cpqSiMemModuleSize            INTEGER,
        cpqSiMemModuleType            INTEGER,
        cpqSiMemModuleSpeed           INTEGER,              -- deprecated
        cpqSiMemModuleTechnology      INTEGER,
        cpqSiMemModuleManufacturer    DisplayString,
        cpqSiMemModulePartNo          DisplayString,
        cpqSiMemModuleDate            OCTET STRING,
        cpqSiMemModuleSerialNo        DisplayString,
        cpqSiMemModuleECCStatus       INTEGER,
        cpqSiMemModuleHwLocation      DisplayString,
        cpqSiMemModuleFrequency       INTEGER,
        cpqSiMemModuleCellTablePtr    INTEGER,
        cpqSiMemModuleCellStatus      INTEGER,
        cpqSiMemModulePartNoMfgr      DisplayString,
        cpqSiMemModuleSerialNoMfgr    DisplayString
    }

    cpqSiMemBoardIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The slot in which the memory board or cartridge is installed.

            A value of 0 indicates memory installed directly on the
            system board."
        ::= { cpqSiMemModuleEntry 1 }

    cpqSiMemModuleIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The memory module number."
        ::= { cpqSiMemModuleEntry 2 }

    cpqSiMemModuleSize OBJECT-TYPE
        SYNTAX  INTEGER (0..2147483647)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Module memory size in kilobytes.  A kilobyte of memory is
            defined as 1024 bytes.

            A size of 0 indicates the module is not present."
        ::= { cpqSiMemModuleEntry 3 }

    cpqSiMemModuleType OBJECT-TYPE
        SYNTAX  INTEGER {
                other(1),
                board(2),
                cpqSingleWidthModule(3),
                cpqDoubleWidthModule(4),
                simm(5),
                pcmcia(6),
                compaq-specific(7),
                dimm(8),
                smallOutlineDimm(9),
                rimm(10),
                srimm(11)
             }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Type of memory module installed.  The value other(1) will be
             given if the type is not known.  The value board(2) will be
             given if the memory module is permanently mounted (not modular)
             on a system board or memory expansion board."
        ::= { cpqSiMemModuleEntry 4 }

    cpqSiMemModuleSpeed OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "Module memory speed in nanoseconds.  The value zero (0) will
             be given if the module speed cannot be determined."
        ::= { cpqSiMemModuleEntry 5 }

    cpqSiMemModuleTechnology OBJECT-TYPE
        SYNTAX  INTEGER {
                other(1),
                fastPageMode(2),
                edoPageMode(3),
                burstEdoPageMode(4),
                synchronous(5),
                rdram(6)
             }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Technology type of memory module installed.  The value other(1)
             will be given if the technology is not known."
        ::= { cpqSiMemModuleEntry 6 }

    cpqSiMemModuleManufacturer OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
             "The memory module's manufacturer name.

              This field will be a null (size 0) string if the manufacturer
              name is not available."
        ::= { cpqSiMemModuleEntry 7 }

    cpqSiMemModulePartNo OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
             "The memory module's manufacturer part number.

              This field will be a null (size 0) string if the manufacturer
              part number is not available."
        ::= { cpqSiMemModuleEntry 8 }

    cpqSiMemModuleDate OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (7))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
             "The memory module date of manufacture.

             field  octets  contents                  range
             =====  ======  ======================    ========
               1     1-2    year                      0..65536
               2       3    month                     1..12
               3       4    day                       1..31
               4       5    hour                      0..23
               5       6    minute                    0..59
               6       7    second                    0..60
                           (use 60 for leap-second)

             This field will be set to year = 0 if the date of manufacture
             is not available.  The hour, minute, and second fields will
             always be set to 0."
        ::= { cpqSiMemModuleEntry 9 }

    cpqSiMemModuleSerialNo OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
             "The memory module's serial number.

              This field will be a null (size 0) string if the serial number
              is not available."
        ::= { cpqSiMemModuleEntry 10 }

    cpqSiMemModuleECCStatus OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            ok(2),
            degraded(3),
            degradedModuleIndexUnknown(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
             "This provides the current status of the correctable memory
              errors for this memory module.

              The following status values are supported:

                 other(1):
                   ECC is not supported on this memory module.

                 ok(2):
                   The correctable error count is below threshold.

                 degraded(3):
                   The correctable error count has exceeded threshold.

                 degradedModuleIndexUnknown(4):
                   The correctable error count has exceeded threshold.
                   The module index not available."
        ::= { cpqSiMemModuleEntry 11 }

    cpqSiMemModuleHwLocation OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "A text description of the hardware location, on complex
             multi SBB hardware only, for the memory module.
             A NULL string indicates that the hardware location could not
             be determined or is irrelevant."
        ::= { cpqSiMemModuleEntry 12 }


    cpqSiMemModuleFrequency OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The memory module frequency in MHz.  The value zero (0) will
             be given if the module frequency cannot be determined."
        ::= { cpqSiMemModuleEntry 13 }

    cpqSiMemModuleCellTablePtr OBJECT-TYPE
        SYNTAX  INTEGER (0..15)
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "Index for the cell in cpqSeCellTable where the memory board is
             installed."
        ::= { cpqSiMemModuleEntry 14 }

    cpqSiMemModuleCellStatus OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            ok(2),
            deconfigured(3)
        }
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
             "This provides the current status for this memory module.

              The following status values are supported:

                 other(1):
                   the system is not cellular

                 ok(2):
                   The memory module is active

                 deconfigured(3):
                   The memory module is not ready"
        ::= { cpqSiMemModuleEntry 15 }


    cpqSiMemModulePartNoMfgr OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
             "The memory module's manufacturer's part number.

              This field will be a null (size 0) string if the manufacturer
              part number is not available."
        ::= { cpqSiMemModuleEntry 16 }

    cpqSiMemModuleSerialNoMfgr OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
             "The memory module's manufacturer's serial number.

              This field will be a null (size 0) string if the manufacturer
              serial number is not available."
        ::= { cpqSiMemModuleEntry 17 }

-- ****************************************************************************
--   System Information System Board Group
--   =====================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSystemInfo Group            (1.3.6.1.4.1.232.2)
--       cpqSiComponent Group          (1.3.6.1.4.1.232.2.2)
--        cpqSiSystemBoard Group       (1.3.6.1.4.1.232.2.2.4)
--
--
-- ****************************************************************************

    cpqSiSystemId OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The System ID.

            This value indicates the system ID of the system board
            in this system.  This ID replaces the product ID used in
            older machines (cpqSiProductId).  A value of 7Eh for the
            cpqSiProductId indicates that the cpqSiSystemId should be
            used to identify the system.  A value of zero (0)
            indicates that the system ID function is not supported on this
            machine.  In this case, the cpqSiProductId should be used to
            identify the system."
        ::= { cpqSiSystemBoard 6 }

    cpqSiSystemCpuId OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The System ID : CPU Component.

            This value indicates the CPU type of the system board
            in this system.  A value of zero (0) indicates that the CPU
            type cannot be determined."
        ::= { cpqSiSystemBoard 7 }

    cpqSiFlashRomSupport OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            notSupported(2),
            supported(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This value indicates if this system supports flash upgradable
            system ROM."
        ::= { cpqSiSystemBoard 8 }

    cpqSiQuickTestRomDate OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (7))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This value indicates the date of the current quick test ROM
            image.

             field  octets  contents                  range
             =====  ======  =======                  =====
               1      1-2   year                      0..65536
               2       3    month                     1..12
               3       4    day                       1..31
               4       5    hour                      0..23
               5       6    minute                    0..59
               6       7    second                    0..60
                            (use 60 for leap-second)


            This field will be set to year = 0 if quick test ROM is not
            present.  The hour, minute, and second field will be set
            to zero (0) if they are not relevant.  The year field is set
                   with the most significant octet first."
        ::= { cpqSiSystemBoard 9 }

    cpqSiReboot OBJECT-TYPE
        SYNTAX  INTEGER {
                notAvailable(1),
                available(2),
                defaultOnlyAvailable(3),
                rebootToCpqUtils(2693),
                rebootToDefault(8115),
                autoShutdown(9037)
                }
        ACCESS  read-write
        STATUS  deprecated
        DESCRIPTION
            "This object may contain the following values:
                 notAvailable(1)
                      the system does not support the reboot functionality.
                      Setting this object to notAvailable(1) has no effect.

                 available(2)
                      the system supports the both reboot to functionalities.
                      Setting this object to available(2) has no effect.

                 defaultOnlyAvailable(3)
                      the system supports the only the default reboot functionality.
                      Setting this object to available(3) has no effect.

                 rebootToCpqUtils(2693)
                      the system will reboot to the System Utilities if
                      the reboot functionality is available.  If possible,
                      the agent will attempt to gracefully shutdown the
                      operating system before performing the reboot.
                      If this functionality is unavailable on this system
                      then all sets will have no effect.

                 rebootToDefault(8115)
                      the system will reboot and allow the default boot
                      process to occur if the reboot functionality is
                      available.  If possible, the agent will attempt to
                      gracefully shutdown the operating system before
                      performing the reboot.  If this functionality is
                      unavailable on this system then all sets will have
                      no effect.

                 autoShutdown(9037)
                      If possible, the agent will attempt to gracefully
                      shutdown the operating system. The agent will not
                      preform a reboot.

                        "

        ::= { cpqSiSystemBoard 10 }


-- ****************************************************************************
--   System Information Processor Microcode Patch Table
--   ==================================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSystemInfo Group            (1.3.6.1.4.1.232.2)
--       cpqSiComponent Group          (1.3.6.1.4.1.232.2.2)
--        cpqSiSystemBoard Group       (1.3.6.1.4.1.232.2.2.4)
--         cpqSiProcMicroPatchTable    (1.3.6.1.4.1.232.2.2.4.11)
--          cpqSiProcMicroPatchEntry   (1.3.6.1.4.1.232.2.2.4.11.1)
--
-- ****************************************************************************

    cpqSiProcMicroPatchTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSiProcMicroPatchEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "This table lists the set of processor microcode patches that
            the system ROM contains. During post, the ROM will apply the
            appropriate patches to the CPU microcode. Scan this table to
            ensure that a patch is being applied to a processor."
        ::= { cpqSiSystemBoard 11 }

    cpqSiProcMicroPatchEntry OBJECT-TYPE
        SYNTAX  CpqSiProcMicroPatchEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "An entry describing one microcode patch contained in the system
            ROM."
        INDEX   { cpqSiProcMicroPatchIndex }
        ::= { cpqSiProcMicroPatchTable 1 }

    CpqSiProcMicroPatchEntry ::= SEQUENCE {
        cpqSiProcMicroPatchIndex   INTEGER,
        cpqSiProcMicroPatchId      INTEGER,
        cpqSiProcMicroPatchDate    OCTET STRING,
        cpqSiProcMicroPatchFamily  OCTET STRING }

    cpqSiProcMicroPatchIndex OBJECT-TYPE
        SYNTAX  INTEGER (1..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Index into the microcode patch table."
        ::= { cpqSiProcMicroPatchEntry 1 }

    cpqSiProcMicroPatchId OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The ID of this particular CPU microcode patch."
        ::= { cpqSiProcMicroPatchEntry 2 }

    cpqSiProcMicroPatchDate OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (7))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This value indicates the date of this CPU microcode patch.

             field  octets  contents                  range
             =====  ======  =======                  =====
               1      1-2   year                      0..65536
               2       3    month                     1..12
               3       4    day                       1..31
               4       5    hour                      0..23
               5       6    minute                    0..59
               6       7    second                    0..60
                            (use 60 for leap-second)

                 NOTE: Year is stored in packed BCD. The most significant
                 part is in the second octet. For example:
                   1995 would be stored as 0x95 0x19.

            The hour, minute, and second field will be set to zero (0)
            if they are not relevant.  The year field is set with the
            most significant octet first."
        ::= { cpqSiProcMicroPatchEntry 3 }

    cpqSiProcMicroPatchFamily OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (3))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The valid family/model/step of the processor that this CPU
            microcode patch applies to.

             field  octets  contents                  range
             =====  ======  =======                  =====
               1       1    CPU Step                  0..255
               2       2    CPU Model                 0..255
               3       3    CPU Family                0..255 "
        ::= { cpqSiProcMicroPatchEntry 4 }


-- ****************************************************************************
--   System Information System Board Group
--   =====================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSystemInfo Group            (1.3.6.1.4.1.232.2)
--       cpqSiComponent Group          (1.3.6.1.4.1.232.2.2)
--        cpqSiSystemBoard Group       (1.3.6.1.4.1.232.2.2.4)
--
--
-- ****************************************************************************

    cpqSiPowerMgmtStatus OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            disabled(2),
            enabled(3)
            }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION
            "The state of power management."
        ::= { cpqSiSystemBoard 12 }


    cpqSiRebootFlags OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "The Reboot Flags.

            This is a collection of flags used to indicate the re-boot
            options available. This integer is a bitmap, with each bit
            indicating the availability of an option. If the bit is set
            to 1, the option is available; otherwise it is not. Multiple
            options are allowed.

            NOTE:   bit 31 is the most significant bit, bit 0 is the least
                    significant.


            Status   This is a collection of flags.  Each bit has the
                     following meaning when it is on (1):

                     Bit 31:     Execute Set
                     Bit 30-6:   RESERVED
                     Bit 5:      Boot to ROM Based Setup
                     Bit 4:      RESERVED
                     Bit 3:      Boot to OS
                     Bit 2:      Boot to Utils
                     Bit 1:      Warm Boot
                     Bit 0:      Cold Boot"



        ::= { cpqSiSystemBoard 13 }

    cpqSiMemErrorIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Placeholder for memory module number for ECC traps.
            Represents the number of the memory module for which an ECC status
            change has occurred. Set to 65535 if module number not available."
        ::= { cpqSiSystemBoard 14 }

    cpqSiMemECCCondition OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            ok(2),
            degraded(3)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This provides the current condition of the correctable memory
             errors for the entire memory.

             The following status values are supported:

             other(1) :
               ECC is not supported.

             ok(2)    :
               The correctable error count is below threshold.

             degraded(3) :
               The correctable error count has exceeded threshold."

        ::= { cpqSiSystemBoard 15 }

    cpqSiMemConfigChangeData OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..383))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Text string for the memory configuration change trap."
        ::= { cpqSiSystemBoard 16 }

    cpqSiServerSystemId OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..8))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
             "A Server System ID.

             This value is used to uniquely identify systems via a unique
             ID on systems that do not support the EISA bus."
        ::= { cpqSiSystemBoard 17 }

-- ****************************************************************************
--   System Information Board Revision Group
--   =======================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSystemInfo Group            (1.3.6.1.4.1.232.2)
--       cpqSiComponent Group          (1.3.6.1.4.1.232.2.2)
--        cpqSiBoardRev Group          (1.3.6.1.4.1.232.2.2.5)
--
--  The cpqSiBoardRev group describes the board revision information.
--
--  Implementation of the cpqSiBoardRev group is mandatory for all
--  agents that support the System Information MIB in a system that
--  supports the board revision feature.
--
-- ****************************************************************************

    cpqSiCurRevDate OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (8))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The current board revision configuration date in MM/DD/YY
            format.  This is the date that the EISA Configuration Utility
            was used to define the current configuration.  This value will
            contain 'N/A' if this system does not support this feature."
        ::= { cpqSiBoardRev 1 }

    cpqSiPrevRevDate OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (8))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The previous board revision configuration date in MM/DD/YY
            format.  This is the date that the EISA Configuration Utility
            was used to define the previous configuration.  This value will
            contain 'N/A' if this system does not support this feature."
        ::= { cpqSiBoardRev 2 }

-- ****************************************************************************
--    System Information Board Revision Table
--   ========================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSystemInfo Group            (1.3.6.1.4.1.232.2)
--       cpqSiComponent Group          (1.3.6.1.4.1.232.2.2)
--        cpqSiBoardRev Group          (1.3.6.1.4.1.232.2.2.5)
--         cpqSiBoardRevTable          (1.3.6.1.4.1.232.2.2.5.3)
--
-- ****************************************************************************

    cpqSiBoardRevTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSiBoardRevEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A table of board revision descriptions."
        ::= { cpqSiBoardRev 3 }

    cpqSiBoardRevEntry OBJECT-TYPE
        SYNTAX  CpqSiBoardRevEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A board revision description."
        INDEX   { cpqSiBoardRevSlotIndex, cpqSiBoardRevIndex }
        ::= { cpqSiBoardRevTable 1 }

    CpqSiBoardRevEntry ::= SEQUENCE {
        cpqSiBoardRevSlotIndex   INTEGER,
        cpqSiBoardRevIndex       INTEGER,
        cpqSiBoardRevId          DisplayString,
        cpqSiBoardRevCur         DisplayString,
        cpqSiBoardRevPrev        DisplayString,
        cpqSiBoardRevHwLocation  DisplayString
    }

    cpqSiBoardRevSlotIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The slot in which the board described in this entry resides.
             Zero (0) indicates the system board."
        ::= { cpqSiBoardRevEntry 1 }

    cpqSiBoardRevIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number that uniquely specifies which board in a specific slot
            is described in this entry.  Zero (0) indicates the main board
            in this slot.  Any other number indicates a daughter board or a
            component of the main board."
        ::= { cpqSiBoardRevEntry 2 }

    cpqSiBoardRevId OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..16))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A description of the board type.  The defined types are:

            Type
            ==============
            System Board
            Processor n     (n = the processor number)
            Memory n        (n = the memory board number)
            Slot n          (n = the slot the board occupies)

            Other types may be defined at a later date."
        ::= { cpqSiBoardRevEntry 3 }

    cpqSiBoardRevCur OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..8))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The current revision for the board described in this entry.
            This value will be N/A if there is no current revision
            information."
        ::= { cpqSiBoardRevEntry 4 }

    cpqSiBoardRevPrev OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..8))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The revision for the board described in this entry prior to the
            current configuration.  This value will be N/A if there is no
            previous revision information."
        ::= { cpqSiBoardRevEntry 5 }

    cpqSiBoardRevHwLocation OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "A text description of the hardware location, on complex
             multi SBB hardware only, for the board.
             A NULL string indicates that the hardware location could not
             be determined or is irrelevant."
        ::= { cpqSiBoardRevEntry 6 }

-- ****************************************************************************
--   System Information Firmware Revision Table
--   ==========================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSystemInfo Group            (1.3.6.1.4.1.232.2)
--       cpqSiComponent Group          (1.3.6.1.4.1.232.2.2)
--        cpqSiBoardRev Group          (1.3.6.1.4.1.232.2.2.5)
--         cpqSiFirmwareRevTable       (1.3.6.1.4.1.232.2.2.5.4)
--
-- ****************************************************************************

    cpqSiFirmwareRevTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSiFirmwareRevEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A table of firmware revision descriptions."
        ::= { cpqSiBoardRev 4 }

    cpqSiFirmwareRevEntry OBJECT-TYPE
        SYNTAX  CpqSiFirmwareRevEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A firmware revision description."
        INDEX   { cpqSiFirmwareRevIndex }
        ::= { cpqSiFirmwareRevTable 1 }

    CpqSiFirmwareRevEntry ::= SEQUENCE {
        cpqSiFirmwareRevIndex          INTEGER,
        cpqSiFirmwareRevDesc           DisplayString,
        cpqSiFirmwareRevString         DisplayString,
        cpqSiFirmwareRevCellTablePtr   INTEGER
    }

    cpqSiFirmwareRevIndex OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Locally-unique index for this entry."
        ::= { cpqSiFirmwareRevEntry 1 }

    cpqSiFirmwareRevDesc OBJECT-TYPE
        SYNTAX  DisplayString
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Description, e.g. SRM console, ARC console, System BIOS, etc."
        ::= { cpqSiFirmwareRevEntry 2 }

    cpqSiFirmwareRevString OBJECT-TYPE
        SYNTAX  DisplayString
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Version number, possibly of the form Vx.y or Vx.y-z."
        ::= { cpqSiFirmwareRevEntry 3 }

    cpqSiFirmwareRevCellTablePtr OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "Index for the cell in cpqSeCellTable where this firmware is located"
        ::= { cpqSiFirmwareRevEntry 4 }

-- ****************************************************************************
--   System Information Firmware Configuration Table
--   ===============================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSystemInfo Group            (1.3.6.1.4.1.232.2)
--       cpqSiComponent Group          (1.3.6.1.4.1.232.2.2)
--        cpqSiBoardRev Group          (1.3.6.1.4.1.232.2.2.5)
--         cpqSiFirmwareCfgTable       (1.3.6.1.4.1.232.2.2.5.5)
--
-- ****************************************************************************

    cpqSiFirmwareCfgTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSiFirmwareCfgEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "Table of soft switches and symbols maintained by the
             firmware.  May be operating system and/or option-specific
             and will certainly be system-specific.  This list is
             intended to be easily extensible and support arbitrary
             datatypes.  It includes such switches as powerup options,
             default dump device, etc.
             Note - the string comparison for svrFwSymbolName is case
             insensitive."
        ::= { cpqSiBoardRev 5 }

    cpqSiFirmwareCfgEntry OBJECT-TYPE
        SYNTAX  CpqSiFirmwareCfgEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "Each entry represents one variable or symbol maintained by
             or stored by some instance of firmware in the system."
        INDEX   { cpqSiFirmwareCfgName }
        ::= { cpqSiFirmwareCfgTable 1 }

    CpqSiFirmwareCfgEntry ::= SEQUENCE {
        cpqSiFirmwareCfgName     DisplayString,
        cpqSiFirmwareCfgValue    DisplayString
    }

    cpqSiFirmwareCfgName OBJECT-TYPE
        SYNTAX  DisplayString
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The firmware configuration symbol name as visible from the
             console."
        ::= { cpqSiFirmwareCfgEntry 1 }

    cpqSiFirmwareCfgValue OBJECT-TYPE
        SYNTAX  DisplayString
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The firmware configuration symbol value.  Null if none
             or unknown."
        ::= { cpqSiFirmwareCfgEntry 2 }


-- ****************************************************************************
--   System Information Ups Shutdown Group
--   =====================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSystemInfo Group            (1.3.6.1.4.1.232.2)
--       cpqSiComponent Group          (1.3.6.1.4.1.232.2.2)
--        cpqSiRackServer Group        (1.3.6.1.4.1.232.2.2.6)
--
--  The cpqSiRackServer group describes this system's role in a rack
--  family.
--
--  Implementation of the cpqSiRackServer group is mandatory for all
--  agents that support the System Information MIB in a system that
--  supports Rack Server features.
--
-- ****************************************************************************

    cpqSiRackServerShutdownRole OBJECT-TYPE
        SYNTAX  INTEGER {
                other(1),
                master(2),
                slave(3)
                }
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "This entry describes this system's role in a rack-mounted
             uninterruptible power supply family. The master both
             communicates with the UPS and derives its power from the
             UPS.  The slave derives its power from the UPS, but does
             not communicate with it."
        ::= { cpqSiRackServer 1 }

    cpqSiRackServerMasterName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..48))
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "This entry describes the name of the master server in a
             rack-mounted uninterruptible power supply family. A slave
             system would communicate with this server to derive UPS
             status."
        ::= { cpqSiRackServer 2 }


-- ****************************************************************************
--   System Information Video Group
--   ==============================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSystemInfo Group            (1.3.6.1.4.1.232.2)
--       cpqSiComponent Group          (1.3.6.1.4.1.232.2.2)
--        cpqSiVideo Group             (1.3.6.1.4.1.232.2.2.7)
--
--  The Video group describes the manageable video displays that are
--  attached to the system.
--
--  Implementation of the video group is mandatory for all agents that
--  support the System Information MIB when a manageable video display
--  is in the system.
--
-- ****************************************************************************

    cpqSiVideoEdidRaw OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (128))
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The raw value returned from the video EDID function."
        ::= { cpqSiVideo 1 }

    cpqSiVideoDesc OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The manufacturer and model description of the video display."
        ::= { cpqSiVideo 2 }

    cpqSiVideoSerialNumber OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..32))
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The serial number of the video display."
        ::= { cpqSiVideo 3 }

    cpqSiVideoManufactureDate OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (7))
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The date of manufacture of the video display in the following
             format:

             field  octets  contents                  range
             =====  ======  =======                  =====
               1      1-2   year                      0..65536
               2       3    month                     1..12
               3       4    day                       1..31
               4       5    hour                      0..23
               5       6    minute                    0..59
               6       7    second                    0..60
                            (use 60 for leap-second)

            This field will be set to year = 0 if the agent cannot provide
            the date.  The date information that is given resolves to a year
            and week, so the hour, minute, and second field will be set to 0,
            the month and day fields will give the monday of the week of
            manufacture."
        ::= { cpqSiVideo 4 }

    cpqSiVideoHeight OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The maximum image height of the video display in centimeters"
        ::= { cpqSiVideo 5 }

    cpqSiVideoWidth OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The maximum image width of the video display in centimeters"
        ::= { cpqSiVideo 6 }


    cpqSiVideoMaxHorPixel OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The number of horizontal pixels in the highest resolution video
             mode supported."
        ::= { cpqSiVideo 7 }


    cpqSiVideoMaxVertPixel OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The number of vertical pixels in the highest resolution video
             mode supported."
        ::= { cpqSiVideo 8 }


    cpqSiVideoMaxRefreshRate OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The video refresh rate in Hz of the highest resolution video
             mode supported."
        ::= { cpqSiVideo 9 }

-- ****************************************************************************
--   System Information Monitor Group
--   ================================
--
--   The compaq enterprise             (1.3.6.1.4.1.232)
--      cpqSystemInfo Group            (1.3.6.1.4.1.232.2)
--       cpqSiComponent Group          (1.3.6.1.4.1.232.2.2)
--        cpqSiMonitor Group           (1.3.6.1.4.1.232.2.2.8)
--
--   The Monitor group describes all manageable video displays
--   that are attached to the system.
--
--   Implementation of the monitor group is mandatory for all agents that
--   support the Compaq System Information MIB when a manageable
--   video display is in the system.
--
-- ****************************************************************************

    cpqSiMonitorOverallCondition OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            ok(2),
            degraded(3),
            failed(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This value specifies the overall condition of the system's
             monitor(s).

             The following conditions are supported:

             other(1)
               The monitor does not support fault reporting or condition is
               unknown.

             ok(2)
               The monitor is operating OK.

             degraded(3)
               The monitor has detected a fault.  The monitor is still useable
               but action should be taken to return the monitor to ok.

             failed(4)
               The monitor has detected a fault.  The monitor will not
               be useable. Action should be taken to replace the monitor."
        ::= { cpqSiMonitor 1 }


-- ****************************************************************************
--   System Information Monitor Group
--   ================================
--
--   The compaq enterprise             (1.3.6.1.4.1.232)
--      cpqSystemInfo Group            (1.3.6.1.4.1.232.2)
--       cpqSiComponent Group          (1.3.6.1.4.1.232.2.2)
--        cpqSiMonitor Group           (1.3.6.1.4.1.232.2.2.8)
--         cpqSiMonitorTable           (1.3.6.1.4.1.232.2.2.8.2)
--          cpqSiMonitorEntry          (1.3.6.1.4.1.232.2.2.8.2.1)
--
--   The Monitor Table describes all manageable video displays
--   that are attached to the system.
--
-- ****************************************************************************

    cpqSiMonitorTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSiMonitorEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A table of all video monitor descriptions connected to this
            system."
        ::= {  cpqSiMonitor 2 }

    cpqSiMonitorEntry OBJECT-TYPE
        SYNTAX  CpqSiMonitorEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A video monitor description."
        INDEX   { cpqSiMonitorIndex }
        ::= { cpqSiMonitorTable 1 }

        CpqSiMonitorEntry ::= SEQUENCE {
                 cpqSiMonitorIndex                  INTEGER,
                 cpqSiMonitorEdidRaw                OCTET STRING,
                 cpqSiMonitorDesc                   DisplayString,
                 cpqSiMonitorSerialNumber           DisplayString,
                 cpqSiMonitorManufactureDate        OCTET STRING,
                 cpqSiMonitorHeight                 INTEGER,
                 cpqSiMonitorWidth                  INTEGER,
                 cpqSiMonitorMaxHorPixel            INTEGER,
                 cpqSiMonitorMaxVertPixel           INTEGER,
                 cpqSiMonitorMaxRefreshRate         INTEGER,
                 cpqSiMonitorManufacturer           DisplayString,
                 cpqSiMonitorThermalCondition       INTEGER,
                 cpqSiMonitorOperationalCondition   INTEGER,
                 cpqSiMonitorStatus                 INTEGER
        }

    cpqSiMonitorIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..15)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A unique index for each video display connected to the system."

       ::= { cpqSiMonitorEntry 1 }

    cpqSiMonitorEdidRaw OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (128))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The raw value returned from the video EDID function."
        ::= { cpqSiMonitorEntry 2 }

    cpqSiMonitorDesc OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The manufacturer and model description of the video display."
        ::= { cpqSiMonitorEntry 3 }

    cpqSiMonitorSerialNumber OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..32))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The serial number of the video display."
        ::= { cpqSiMonitorEntry 4 }

    cpqSiMonitorManufactureDate OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (7))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The date of manufacture of the video display in the following
             format:

             field  octets  contents                  range
             =====  ======  =======                  =====
               1      1-2   year                      0..65536
               2       3    month                     1..12
               3       4    day                       1..31
               4       5    hour                      0..23
               5       6    minute                    0..59
               6       7    second                    0..60
                            (use 60 for leap-second)

            This field will be set to year = 0 if the agent cannot provide
            the date.  The date information that is given resolves to a year
            and week, so the hour, minute, and second field will be set to 0,
            the month and day fields will give the monday of the week of
            manufacture."
        ::= { cpqSiMonitorEntry 5 }

    cpqSiMonitorHeight OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The maximum image height of the video display in centimeters"
        ::= { cpqSiMonitorEntry 6}

    cpqSiMonitorWidth OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The maximum image width of the video display in centimeters"
        ::= { cpqSiMonitorEntry 7 }


    cpqSiMonitorMaxHorPixel OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The number of horizontal pixels in the highest resolution video
             mode supported."
        ::= { cpqSiMonitorEntry 8 }

    cpqSiMonitorMaxVertPixel OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The number of vertical pixels in the highest resolution video mode
             supported."
        ::= { cpqSiMonitorEntry 9 }

    cpqSiMonitorMaxRefreshRate OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The video refresh rate in Hz of the highest resolution video mode
             supported."
        ::= { cpqSiMonitorEntry 10 }

    cpqSiMonitorManufacturer OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The manufacturer of the video display."
        ::= { cpqSiMonitorEntry 11 }

    cpqSiMonitorThermalCondition OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            ok(2),
            degraded(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This provides the condition of the monitor’s internal temperature.

            This value will be one of the following:

            other(1)
              Monitor thermal fault reporting is not supported by this monitor
              or the Insight Agent does not recognize the status.  You may
              need to upgrade your software.

            ok(2)
              The internal temperature is within normal limits.

            degraded(3)
              The internal temperature is outside normal operating range."
        ::= { cpqSiMonitorEntry 12 }

    cpqSiMonitorOperationalCondition OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            ok(2),
            degraded(3),
            failed(4)
           }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
           "This provides the condition of the monitor's operational features.

            This condition value will be one of the following:

            other(1)
              Monitor operational fault reporting is not supported by this
              monitor or the Insight Agent does not recognize the status.
              You may need to upgrade your software.

            ok(2)
              The monitor is operating within normal limits.

            degraded(3)
              The monitor is not functioning within normal operating limits.
              At least one of the operational features has become degraded.

            failed(4)
              The monitor is not functioning within normal operating limits.
              At least one of the operational features has failed causing the
              monitor to not be usable.  The monitor should be replaced."
        ::= { cpqSiMonitorEntry 13 }

    cpqSiMonitorStatus OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            unknown(2),
            ok(3),
            thermalDegraded(4),
            operationalFailure(5)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
           "This provides the status of the monitor's fault reporting features.

            This status value will be one of the following:

            other(1)
              Monitor fault reporting is not supported by this monitor or the
              Insight Agent does not recognize the status. You may need to
              upgrade your software.

            unknown(2)
              The monitor status is unknown because the monitor is
              either in power saving mode or it has been turned off.

            ok(3)
              The monitor is operating within normal limits.

            thermalDegraded(4)
              The monitor's internal temperature is not functioning within
              normal operating limits.

            operationalFailure(5)
              The monitor is not functioning within normal operating limits.
              At least one of the operational features has failed.
              The monitor should be replaced."

        ::= { cpqSiMonitorEntry 14 }


-- ****************************************************************************
--   System Information Hot Plug Slot Group
--   ======================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSystemInfo Group            (1.3.6.1.4.1.232.2)
--       cpqSiComponent Group          (1.3.6.1.4.1.232.2.2)
--        cpqSiHotPlugSlot Group       (1.3.6.1.4.1.232.2.2.9)
--
--  The cpqSiHotPlugSlot group describes the System Information Hot Plug
--  slot information.
--
--  Implementation of the cpqSiHotPlugSlot group is mandatory for all
--  agents that support the System Information MIB.
--
-- ****************************************************************************

    cpqSiHotPlugSlotSupported OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            notSupported(2),
            supported(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This value specifies if this system supports the Hot
            Pluggable Slot feature."
        ::= { cpqSiHotPlugSlot 1 }

    cpqSiHotPlugSlotCondition OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            ok(2),
            degraded(3),
            failed(4)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This value specifies the overall condition of the Hot Plug
            Slot feature.

            The Hot Plug condition is set as follows:

            other(1)
              When Hot Plug Slots are not supported or condition is unknown.

            ok(2)
              If there are no hot plug slots with a condition of degraded
              or failed.

            degraded(3)
              If there are degraded slot entries but none failed.

            failed(4)
              If there are failed slot entries."
        ::= { cpqSiHotPlugSlot 2 }

    cpqSiHotPlugSlotChangeCount OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This value will be incremented each time a hot plug event
            occurs resulting in a change in the hot plug slot table."
        ::= { cpqSiHotPlugSlot 3 }


-- ****************************************************************************
--   System Information Hot Plug Slot Table
--   ======================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSystemInfo Group            (1.3.6.1.4.1.232.2)
--       cpqSiComponent Group          (1.3.6.1.4.1.232.2.2)
--        cpqSiHotPlugSlot Group       (1.3.6.1.4.1.232.2.2.9)
--         cpqSiHotPlugSlotTable       (1.3.6.1.4.1.232.2.2.9.4)
--
--  The cpqSiHotPlugSlot group describes the manageable Hot Plug
--  Slots in the system.  This table will be missing if the system does
--  not support hot plug slots.
--
-- ****************************************************************************

    cpqSiHotPlugSlotTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSiHotPlugSlotEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A list of Hot Plug Slot information entries."
        ::= { cpqSiHotPlugSlot 4 }

    cpqSiHotPlugSlotEntry OBJECT-TYPE
        SYNTAX  CpqSiHotPlugSlotEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A description of a Hot Plug Slot."
        INDEX   { cpqSiHotPlugSlotChassis, cpqSiHotPlugSlotIndex }
        ::= { cpqSiHotPlugSlotTable 1 }

    CpqSiHotPlugSlotEntry ::= SEQUENCE {
        cpqSiHotPlugSlotChassis              INTEGER,
        cpqSiHotPlugSlotIndex                INTEGER,
        cpqSiHotPlugSlotBoardPresent         INTEGER,
        cpqSiHotPlugSlotPowerState           INTEGER,
        cpqSiHotPlugSlotBoardCondition       INTEGER,
        cpqSiHotPlugSlotErrorStatus          INTEGER,
        cpqSiHotPlugSlotHwLocation           DisplayString
    }

    cpqSiHotPlugSlotChassis OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The Chassis where this hot plug slot resides."
        ::= { cpqSiHotPlugSlotEntry 1 }

    cpqSiHotPlugSlotIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The slot within the chassis for this hot plug slot."
        ::= { cpqSiHotPlugSlotEntry 2 }

    cpqSiHotPlugSlotBoardPresent OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            present(2),
            absent(3),
            presentButSuspended(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This value indicates whether a board is present(2) in or
            absent(3) from the slot.  A value of other(1) indicates
            the information could not be obtained."
        ::= { cpqSiHotPlugSlotEntry 3 }

    cpqSiHotPlugSlotPowerState OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            powerOn(2),
            powerOff(3)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This value is set to powerOn(2) when power is being supplied
            to the slot and powerOff(3) when power is not being supplied.
            A value of other(1) indicates the information could not be
            obtained."
        ::= { cpqSiHotPlugSlotEntry 4 }

    cpqSiHotPlugSlotBoardCondition OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            ok(2),
            degraded(3),
            failed(4)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This value specifies the condition of the hot plug slot.

            The hot plug condition is set as follows:

            other(1)
              When the condition could not be determined.

            ok(2)
              The slot is powered up and operating normally.

            degraded(3)
              If the board in the slot is not fully functioning.

            failed(4)
              If the slot is failed for any reason.  See the status code
              for more information on the failure."
        ::= { cpqSiHotPlugSlotEntry 5 }

    cpqSiHotPlugSlotErrorStatus OBJECT-TYPE
        SYNTAX  INTEGER {
            noError(1),
            generalError(2),
            wrongRevision(3),
            wrongBoard(4),
            cannotConfig(5),
            powerFault(6),
            unexpectedPowerLoss(7),
            wrongSpeed(8),
            functionalFailure(9)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This value specifies the status of the hot plug slot.

            The hot plug slot status is set as follows:

            noError(1)
              The slot is operating normally.

            generalError(2)
              A general error occurred.

            wrongRevision(3)
              The revision of the replacement adapter was different from
              the original adapter.

            wrongBoard(4)
              The model of the replacement adapter was different from the
              original adapter.

            cannotConfig(5)
              The adapter could not be configured.

            powerFault(6)
              A power fault occurred for the slot.

            unexpectedPowerLoss(7)
              Power was unexpectedly lost from the slot.

            wrongSpeed(8)
              The adapter cannot be run at the current bus speed.

            functionlFailure(9)
              The adapter is not functioning correctly.  This may
              be caused by a cabling problem."
        ::= { cpqSiHotPlugSlotEntry 6 }

    cpqSiHotPlugSlotHwLocation OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "A text description of the hardware location, on complex
             multi SBB hardware only, for the hot plug slot.
             A NULL string indicates that the hardware location could not
             be determined or is irrelevant."
        ::= { cpqSiHotPlugSlotEntry 7 }

-- ****************************************************************************
--   System Information System Battery Group
--   =======================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSystemInfo Group            (1.3.6.1.4.1.232.2)
--       cpqSiComponent Group          (1.3.6.1.4.1.232.2.2)
--        cpqSiSystemBattery Group     (1.3.6.1.4.1.232.2.2.10)
--
--  The cpqSiSystemBattery group describes information about the system
--  (portable) batteries that are used to power your system.  These
--  are the rechargeable batteries.
--
--
--  Implementation of the cpqSiBattery group is mandatory for all
--  agents that support the System Information MIB.
--
-- ****************************************************************************


    cpqSiSystemBatteryOverallCondition OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            ok(2),
            degraded(3),
            failed(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This value specifies the overall condition of all of the
             system batteries.

             The following conditions are supported:

             other(1)
               The system does not use system batteries or the battery
               condition is unknown.

             ok(2)
               All System Batteries are operating OK.

             degraded(3)
               One or more of the System Batteries has degraded.  The
               degraded battery will continue to function but should be
               replaced.

             failed(4)
               One of more of the System Batteries has failed.  The failed
               battery is no longer usable. Action should be taken to replace
               the battery."
        ::= { cpqSiSystemBattery 1 }


-- ****************************************************************************
--   System Information System Battery Group
--   =======================================
--
--   The compaq enterprise             (1.3.6.1.4.1.232)
--      cpqSystemInfo Group            (1.3.6.1.4.1.232.2)
--       cpqSiComponent Group          (1.3.6.1.4.1.232.2.2)
--        cpqSiSystemBattery Group     (1.3.6.1.4.1.232.2.2.10)
--         cpqSiSystemBatteryTable     (1.3.6.1.4.1.232.2.2.10.2)
--          cpqSiSystemBatteryEntry    (1.3.6.1.4.1.232.2.2.10.2.1)
--
--   The System Battery Table describes asset, physical, and status
--   information about the portable batteries powering your system.
--
-- ****************************************************************************

    cpqSiSysBatteryTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSiSysBatteryEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A table of System Batteries."
        ::= { cpqSiSystemBattery 2 }

    cpqSiSysBatteryEntry OBJECT-TYPE
        SYNTAX  CpqSiSysBatteryEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A system battery description."
        INDEX   { cpqSiSysBatteryIndex }
        ::= { cpqSiSysBatteryTable 1 }

    CpqSiSysBatteryEntry ::= SEQUENCE {
        cpqSiSysBatteryIndex              INTEGER,
        cpqSiSysBatteryModel              DisplayString,
        cpqSiSysBatterySerialNum          DisplayString,
        cpqSiSysBatteryAssetTag           DisplayString,
        cpqSiSysBatteryManufacturer       DisplayString,
        cpqSiSysBatteryDate               OCTET STRING,
        cpqSiSysBatterySmartVersion       DisplayString,
        cpqSiSysBatteryCondition          INTEGER,
        cpqSiSysBatteryStatus             INTEGER,
        cpqSiSysBatteryChemistry          INTEGER,
        cpqSiSysBatteryRemainingCap       INTEGER,
        cpqSiSysBatteryFirmwareRevision   INTEGER,
        cpqSiSysBatteryHardwareRevision   INTEGER,
        cpqSiSysBatteryFullCap            INTEGER,
        cpqSiSysBatteryDesignCap          INTEGER,
        cpqSiSysBatteryHwLocation         DisplayString
    }

    cpqSiSysBatteryIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A unique index for this battery entry."
        ::= { cpqSiSysBatteryEntry 1 }


    cpqSiSysBatteryModel OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The model name for  this battery."
        ::= { cpqSiSysBatteryEntry 2 }

    cpqSiSysBatterySerialNum OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The serial number for this battery."
        ::= { cpqSiSysBatteryEntry 3 }

    cpqSiSysBatteryAssetTag OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This is the customer changeable battery identifier that is set
            to this system battery's serial number at the time of
            manufacture.

            The string will be empty if the battery does support
            this function."
        ::= { cpqSiSysBatteryEntry 4 }

    cpqSiSysBatteryManufacturer OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
           "The battery's manufacturer's name.

            The string will be empty if the battery does support
            this function."
         ::= { cpqSiSysBatteryEntry 5 }


    cpqSiSysBatteryDate OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (7))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The battery's manufacture date.

             field  octets  contents                  range
             =====  ======  =======                  =====
               1      1-2   year                      0..65536
               2       3    month                     1..12
               3       4    day                       1..31
               4       5    hour                      0..23
               5       6    minute                    0..59
               6       7    second                    0..60
                            (use 60 for leap-second)

            This field will be set to year = 0 if the agent cannot provide
            the module date.  The hour, minute, and second field will be set
            to zero (0) if they are not relevant.  The year field is set
            with the most significant octet first.

            The string will be empty if the battery does support
            this function."
        ::= { cpqSiSysBatteryEntry 6 }

    cpqSiSysBatterySmartVersion OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
           "The Smart Battery Data Specification version number supported by this
            battery.

            The string will be empty if the system battery does support
            this function."
         ::= { cpqSiSysBatteryEntry 7 }

    cpqSiSysBatteryCondition OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            ok(2),
            degraded(3),
            failed(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
             "This provides the current condition of this system battery.

              The following status values are supported:

                other(1)
                  The battery does not support condition monitoring or
                  the Insight Agent cannot determine condition.

                ok(2)
                  The battery is operating normally.  No user action is
                  required.

                degraded(3)
                  The battery is degraded.  The battery is still usable
                  but should be replaced.

                failed(4)
                  The battery has failed.  The battery is no longer
                  usable and should be replaced soon."
         ::= { cpqSiSysBatteryEntry 8 }

    cpqSiSysBatteryStatus OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            ok(2),
            capacityDegraded(3),
            chargeFault(4),
            batteryFailure(5)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
             "This provides the current status of the battery.

              The following status values are supported:

                 other(1):
                   This battery does not support status reporting.

                 ok(2):
                   The battery is operating ok.

                   User Action: No action required.

                 capacityDegraded(3):
                   Significant battery degradation has occurred.
                   The battery can no longer be fully recharged.

                   User Action:
                   If using multiple batteries, run the Power
                   Conservation Utility to identify the battery
                   location.  Contact your System Administrator or
                   Authorized Reseller to order a replacement
                   battery.

                 chargeFault(4):
                   One or more batteries are not functioning properly.

                   User Action:
                   Make sure all batteries are operating in the
                   recommended temperature range.  Check for foreign
                   objects in the battery slots.  Remove and reinsert all
                   batteries to resume normal battery operation.
                   Contact your System Administrator or Authorized
                   Reseller if you are still experiencing problems.

                 batteryFailure(5):
                   The battery has failed and must be replaced.

                   User Action:
                   Contact your System Administrator or Authorized
                   Reseller to order a replacement battery.  Recycle your
                   old battery. For proper disposal information, refer
                   to the documentation that came with your computer."

         ::= { cpqSiSysBatteryEntry 9 }

    cpqSiSysBatteryChemistry OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            unknown(2),
            lead-Acid(3),
            nickel-Cadmium(4),
            nickel-Metal-Hydride(5),
            lithium-Ion(6),
            zinc-Air(7),
            lithium-Polymer(8)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
           "The chemistry of the battery."

         ::= { cpqSiSysBatteryEntry 10 }

   cpqSiSysBatteryRemainingCap OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
           "This is a percentage of the battery's remaining capacity
            from its design capacity.

            If this attribute is not supported, 65535 is returned."
        ::= { cpqSiSysBatteryEntry 11 }

    cpqSiSysBatteryFirmwareRevision OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
           "This is the revision level of the firmware on the battery.

            If this attribute is not supported, 255 is returned."
        ::= { cpqSiSysBatteryEntry 12 }

    cpqSiSysBatteryHardwareRevision OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
           "This is the revision level of the hardware on the battery.

            If this attribute is not supported, 255 is returned."
        ::= { cpqSiSysBatteryEntry 13 }

    cpqSiSysBatteryFullCap OBJECT-TYPE
        SYNTAX  INTEGER  (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
           "This is the mWatt-Hours of the battery's Full capacity on
            the current charge.

            If this attribute is not supported, 65535 is returned."
        ::= { cpqSiSysBatteryEntry 14 }

    cpqSiSysBatteryDesignCap OBJECT-TYPE
        SYNTAX  INTEGER  (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "This is the mWatt-Hours of the battery's design capacity as
           specified by the manufacturer.

            If this attribute is not supported, 65535 is returned."
        ::= { cpqSiSysBatteryEntry 15 }

    cpqSiSysBatteryHwLocation OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  optional
        DESCRIPTION
            "A text description of the hardware location, on complex
             multi SBB hardware only, for the battery.
             A NULL string indicates that the hardware location could not
             be determined or is irrelevant."
        ::= { cpqSiSysBatteryEntry 16 }


-- ****************************************************************************
--   System Information Docking Station Group
--   ========================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSystemInfo Group            (1.3.6.1.4.1.232.2)
--       cpqSiComponent Group          (1.3.6.1.4.1.232.2.2)
--        cpqSiDockingStation Group    (1.3.6.1.4.1.232.2.2.11)
--
--  The cpqsiDockingStation group describes the asset information
--  about portable docking stations.
--
--
--  Implementation of the cpqSiDockingStation group is mandatory for all
--  agents that support the System Information MIB.
--
-- ****************************************************************************

    cpqSiDockingStationStatus OBJECT-TYPE
        SYNTAX  INTEGER {
            notSupported(1),
            docked(2),
            undocked(3)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This value specifies the connection of the computer
             system to a docking station.

             The following connection states are supported:

             notSupported(1)
               This system does not interface to a docking station.

             docked(2)
               This system is connected to a docking station.

             undocked(3)
               This system is not connect to a docking station."
        ::= { cpqSiDockingStation 1}

    cpqSiDockingStationSerialNum OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The serial number of the docking station.

            The string will be empty if the docking station does not support a
            serial or the system does not interface to a docking station."
        ::= { cpqSiDockingStation 2 }

    cpqSiDockingStationModel OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The model name of the docking station.

            The string will be empty if the docking station does not report the
            model name or the system does not interface to a docking station."
        ::= { cpqSiDockingStation 3 }

     cpqSiDockingStationAssetTag OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This is a customer changeable identifier that is set to the docking
            station serial number at the time of manufacture.

            The string will be empty if the docking station does not report an
            asset tag or the system does not interface to a docking station."
        ::= { cpqSiDockingStation 4}

-- ****************************************************************************
--   System Information FRU Group
--   ============================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSystemInfo Group            (1.3.6.1.4.1.232.2)
--       cpqSiComponent Group          (1.3.6.1.4.1.232.2.2)
--        cpqSiFru Group               (1.3.6.1.4.1.232.2.2.12)
--
--  The cpqsiFru group describes the Field Replaceable Units in the
--  server system.
--
--
--  Implementation of the cpqSiFru group is mandatory for all
--  Server Agents that support the System Information MIB.
--
-- ****************************************************************************

     cpqSiFruTable OBJECT-TYPE
         SYNTAX SEQUENCE OF CpqSiFruEntry
         ACCESS not-accessible
         STATUS mandatory
         DESCRIPTION
             "Table of Field Replaceable Units of system, providing
              inventory and asset control information.  This table is
              referenced from logical hardware descriptions elsewhere in
              the MIB."
         ::= { cpqSiFru 1 }

     cpqSiFruEntry OBJECT-TYPE
         SYNTAX CpqSiFruEntry
         ACCESS not-accessible
         STATUS mandatory
         DESCRIPTION
             "Each entry represents a Field Replaceable Unit (FRU) of hardware."
         INDEX { cpqSiFruIndex }
         ::= { cpqSiFruTable 1 }

     CpqSiFruEntry  ::=
         SEQUENCE {
             cpqSiFruIndex                INTEGER,
             cpqSiFruType                 INTEGER,
             cpqSiFruDescr                DisplayString,
             cpqSiFruVendor               DisplayString,
             cpqSiFruPartNumber           DisplayString,
             cpqSiFruRevision             DisplayString,
             cpqSiFruFirmwareRevision     DisplayString,
             cpqSiFruSerialNumber         DisplayString,
             cpqSiFruAssetNo              DisplayString,
             cpqSiFruClass                INTEGER,
             cpqSiFruSlotNumber           DisplayString,
             cpqSiFruSubAssemblyNumber    INTEGER,
             cpqSiFruAssemblyNumber       INTEGER,
             cpqSiFruChassisNumber        INTEGER,
             cpqSiFruPositionNumber       INTEGER,
             cpqSiFruCabinetIDNumber      INTEGER,
             cpqSiFruSiteLocation         INTEGER,
             cpqSiFruDiagStatus           INTEGER,
             cpqSiFruExtendedDiagStatus   INTEGER,
             cpqSiFruCellTablePtr         INTEGER,
             cpqSiFruIOCTablePtr          INTEGER,
             cpqSiFruFileId               DisplayString,
             cpqSiFruScanRev              DisplayString
                  }

     cpqSiFruIndex OBJECT-TYPE
         SYNTAX  INTEGER
         ACCESS  read-only
         STATUS  mandatory
         DESCRIPTION
             "A locally-unique index value."
         ::= { cpqSiFruEntry 1 }

     cpqSiFruType OBJECT-TYPE
         SYNTAX  INTEGER {
                     unknown(1) ,
                     other(2) ,
                     motherBoard(3) ,
                     processor(4) ,
                     memoryCard(5) ,
                     memoryModule(6) ,
                     peripheralDevice(7) ,
                     systemBusBridge(8) ,
                     powerSupply(9) ,
                     chassis(10) ,
                     fan(11) ,
                     ioCard(12)
                 }
         ACCESS  read-only
         STATUS  mandatory
         DESCRIPTION
             "General category of the type of FRU that this is."
         ::= { cpqSiFruEntry 2 }

     cpqSiFruDescr OBJECT-TYPE
         SYNTAX  DisplayString
         ACCESS  read-write
         STATUS  mandatory
         DESCRIPTION
             "More detailed description of FRU type, if known."
         ::= { cpqSiFruEntry 3 }

     cpqSiFruVendor OBJECT-TYPE
         SYNTAX  DisplayString
         ACCESS  read-only
         STATUS  mandatory
         DESCRIPTION
             "Manufacturer name or ID."
         ::= { cpqSiFruEntry 4 }

     cpqSiFruPartNumber OBJECT-TYPE
         SYNTAX  DisplayString
         ACCESS  read-only
         STATUS  mandatory
         DESCRIPTION
             "Number by which this unit is orderable."
         ::= { cpqSiFruEntry 5 }

     cpqSiFruRevision OBJECT-TYPE
         SYNTAX  DisplayString
         ACCESS  read-only
         STATUS  mandatory
         DESCRIPTION
             "Version number of this unit. If artwork level is available, it will
             appear as 'Artwork: XXX' following FRU version portion."
         ::= { cpqSiFruEntry 6 }

     cpqSiFruFirmwareRevision OBJECT-TYPE
         SYNTAX  DisplayString
         ACCESS  read-only
         STATUS  mandatory
         DESCRIPTION
             "The revision of the firmware, if any.  Otherwise null."
         ::= { cpqSiFruEntry 7 }

     cpqSiFruSerialNumber OBJECT-TYPE
         SYNTAX  DisplayString
         ACCESS  read-only
         STATUS  mandatory
         DESCRIPTION
             "The serial number of this unit's instance."
         ::= { cpqSiFruEntry 8 }

     cpqSiFruAssetNo OBJECT-TYPE
         SYNTAX  DisplayString
         ACCESS  read-write
         STATUS  mandatory
         DESCRIPTION
             "The asset number for this unit. This string may be limited."
         ::= { cpqSiFruEntry 9 }

     cpqSiFruClass OBJECT-TYPE
         SYNTAX  INTEGER {
                     unknown(1) ,
                     other(2) ,
                     currentBoardInSlot(3) ,
                     priorBoardInSlot(4) ,
                     parentBoard(5) ,
                     priorParentBoard(6) ,
                     priorParentSystem(7)
                 }
         ACCESS  read-only
         STATUS  mandatory
         DESCRIPTION
             "Represents the status category of the unit."
         ::= { cpqSiFruEntry 10 }

     cpqSiFruSlotNumber  OBJECT-TYPE
         SYNTAX  DisplayString
         ACCESS  read-only
         STATUS  mandatory
         DESCRIPTION
            "Physical slot number of FRU."
         ::= { cpqSiFruEntry 11 }

     cpqSiFruSubAssemblyNumber  OBJECT-TYPE
         SYNTAX  INTEGER
         ACCESS  read-only
         STATUS  mandatory
         DESCRIPTION
            "Subassembly containing this FRU.  From FRU V5.0."
         ::= { cpqSiFruEntry  12 }

     cpqSiFruAssemblyNumber  OBJECT-TYPE
         SYNTAX  INTEGER
         ACCESS  read-only
         STATUS  mandatory
         DESCRIPTION
            "Assembly containing this FRU.  From FRU V5.0."
         ::= { cpqSiFruEntry 13 }

     cpqSiFruChassisNumber  OBJECT-TYPE
         SYNTAX  INTEGER
         ACCESS  read-only
         STATUS  mandatory
         DESCRIPTION
            "Chassis containing this FRU.  From FRU V5.0."
         ::= { cpqSiFruEntry 14 }

     cpqSiFruPositionNumber  OBJECT-TYPE
         SYNTAX  INTEGER
         ACCESS  read-only
         STATUS  mandatory
         DESCRIPTION
            "Position in Chassis to help locate FRU.  From FRU V5.0."
         ::= { cpqSiFruEntry 15 }

     cpqSiFruCabinetIDNumber  OBJECT-TYPE
         SYNTAX  INTEGER
         ACCESS  read-only
         STATUS  mandatory
         DESCRIPTION
            "Cabinet number containing this FRU.  From FRU V5.0."
         ::= { cpqSiFruEntry 16 }

     cpqSiFruSiteLocation  OBJECT-TYPE
         SYNTAX  INTEGER
         ACCESS  read-only
         STATUS  mandatory
         DESCRIPTION
            "Site code for system containing this FRU.  From FRU V5.0."
         ::= { cpqSiFruEntry  17 }

     cpqSiFruDiagStatus  OBJECT-TYPE
         SYNTAX  INTEGER {
                     unknown(1),
                     ok(2),
                     degraded(3),
                     failed(4),
                     disabled(5)
                 }
         ACCESS  read-only
         STATUS  mandatory
         DESCRIPTION
            "Use system status values to describe current state of the
            FRU."
         ::= { cpqSiFruEntry 18 }

     cpqSiFruExtendedDiagStatus OBJECT-TYPE
         SYNTAX  INTEGER
         ACCESS  read-only
         STATUS  mandatory
         DESCRIPTION
            "Diagnostic Status value returned by Device Specific
            diagnostics.  Usually through a diagnostic status register
            on the device.  See product manual for bit descriptions."
         ::= { cpqSiFruEntry 19 }

     cpqSiFruCellTablePtr OBJECT-TYPE
         SYNTAX  INTEGER
         ACCESS  read-only
         STATUS  optional
         DESCRIPTION
             "Index for the cell in cpqSeCellTable where this FRU is physically located."
         ::= { cpqSiFruEntry 20 }

     cpqSiFruIOCTablePtr OBJECT-TYPE
         SYNTAX  INTEGER
         ACCESS  read-only
         STATUS  optional
         DESCRIPTION
             "Index for the I/O Chassis in cpqSeIOCTablePtr where this FRU is physically located"
         ::= { cpqSiFruEntry 21 }

    cpqSiFruFileId OBJECT-TYPE
         SYNTAX  DisplayString (SIZE (0..255))
         ACCESS  read-only
         STATUS  optional
         DESCRIPTION
             "This represents the FRU file identifier"
         ::= { cpqSiFruEntry 22 }

    cpqSiFruScanRev  OBJECT-TYPE
         SYNTAX  DisplayString (SIZE (0..255))
         ACCESS  read-only
         STATUS  optional
         DESCRIPTION
            "This represents FRU scan revision"
         ::= { cpqSiFruEntry 23 }

-- ****************************************************************************
--   System Information Rack and Enclosure Group
--   ===========================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSystemInfo Group            (1.3.6.1.4.1.232.2)
--       cpqSiComponent Group          (1.3.6.1.4.1.232.2.2)
--        cpqSiRackEnclosure Group     (1.3.6.1.4.1.232.2.2.13)
--
--  The cpqSiRackEnclosure group indicates the availability of rack and/or
--  enclosure based systems.
--
-- ****************************************************************************

     cpqSiRackEnclosureMgrTable OBJECT-TYPE
         SYNTAX SEQUENCE OF CpqSiRackEnclosureMgrEntry
         ACCESS not-accessible
         STATUS mandatory
         DESCRIPTION
             "Table of possible rack and/or enclosure based systems."
         ::= { cpqSiRackEnclosure 1 }

     cpqSiRackEnclosureMgrEntry OBJECT-TYPE
         SYNTAX CpqSiRackEnclosureMgrEntry
         ACCESS not-accessible
         STATUS mandatory
         DESCRIPTION
             "A entry for a rack and/or enclosure based system."
         INDEX { cpqSiRackEnclosureMgrIndex }
         ::= { cpqSiRackEnclosureMgrTable 1 }

     CpqSiRackEnclosureMgrEntry  ::=
         SEQUENCE {
             cpqSiRackEnclosureMgrIndex               INTEGER,
             cpqSiRackEnclosureMgrType                INTEGER,
             cpqSiRackEnclosureMgrIpAddr              DisplayString,
             cpqSiRackEnclosureMgrWebLink             DisplayString,
             cpqSiRackEnclosureMgrCondition           INTEGER,
             cpqSiRackEnclosureMgrSerialNumber        DisplayString
                  }

     cpqSiRackEnclosureMgrIndex  OBJECT-TYPE
         SYNTAX  INTEGER
         ACCESS  read-only
         STATUS  mandatory
         DESCRIPTION
            "A locally-unique index value."
         ::= { cpqSiRackEnclosureMgrEntry 1 }

     cpqSiRackEnclosureMgrType OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            noEnclosureManagement(2),
            enclosureManagement(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This value specifies the type of enclosure management.

            other(1)
              When the type not be determined.

            noEnclosureManagement(2)
              The server is part of a rack/enclosure managed system, but there
              is no dedicated enclosure manager.

            enclosureManagement(3)
              The server is part of a rack/enclosure managed system with a
              dedicated enclosure manager."
         ::= { cpqSiRackEnclosureMgrEntry 2 }

     cpqSiRackEnclosureMgrIpAddr OBJECT-TYPE
         SYNTAX  DisplayString
         ACCESS  read-only
         STATUS  mandatory
         DESCRIPTION
             "The IP address of the rack enclosure manager.

             The string will be empty if the enclosure does not report the
             information or it could not be determined."
         ::= { cpqSiRackEnclosureMgrEntry 3 }

     cpqSiRackEnclosureMgrWebLink OBJECT-TYPE
         SYNTAX  DisplayString
         ACCESS  read-only
         STATUS  mandatory
         DESCRIPTION
             "The web link to the enclosure managers web based management
             information for the enclosure.

             The string will be empty if the enclosure does not report the
             information or it could not be determined."
         ::= { cpqSiRackEnclosureMgrEntry 4 }

     cpqSiRackEnclosureMgrCondition  OBJECT-TYPE
         SYNTAX  INTEGER {
                     other(1),
                     ok(2),
                     degraded(3),
                     failed(4)
                 }
         ACCESS  read-only
         STATUS  mandatory
         DESCRIPTION
             "The overall condition of the Enclosure Manager.  For more detailed
             status information, follow the cpqSiEnclosureMgrWebLink through
             the Web Management Agent interface.

             other(1)
               This is the default condition for systems when
               cpqSiRackEnclosureMgrType has a value of
               noEnclosureManagement(2).

               When cpqSiRackEnclosureMgrType has a value of
               enclosureManagement(3), this indicates the status of the
               enclosure manager could not be determined.

             ok(2)
               The enclosure manager is in an ok state.  Follow the
               cpqSiRackEnclosureMgrWebLink link in the Web Management Agents
               to manage the enclosure.

             degraded(3)
               The enclosure manager is in a degraded state.  Follow the
               cpqSiRackEnclosureMgrWebLink link in the Web Management Agents
               to manage the enclosure.

             failed(4)
               The enclosure manager is in a failed state.  Follow the
               cpqSiRackEnclosureMgrWebLink link in the Web Management Agents
               to manage the enclosure."
         ::= { cpqSiRackEnclosureMgrEntry 5 }

     cpqSiRackEnclosureMgrSerialNumber OBJECT-TYPE
         SYNTAX  DisplayString
         ACCESS  read-only
         STATUS  mandatory
         DESCRIPTION
             "The serial number of the enclosure containing the enclosure
             manager.

             The string will be empty if the enclosure does not report the
             information or it could not be determined."
         ::= { cpqSiRackEnclosureMgrEntry 6 }


-- ****************************************************************************
--  System Info MIB Trap Definitions
--  ================================
--
--  The SNMP trap messages must not be bigger than 484 octets (bytes).
--
--  Trap support in an SNMP agent implementation is optional.  An SNMP
--  agent implementation may support all, some, or none of the traps.
--  If traps are supported, The user should be provided with the option of
--  disabling traps.
-- **************************************************************************

    cpqSiHoodRemoved TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags }
        DESCRIPTION
           "System hood is removed.

            The hood status has been set to removed.  The
            system's hood is not in a properly installed state. This
            situation may result in improper cooling of the system due
            to air flow changes caused by the missing hood.

            User Action: Replace the cover (hood), ensure the system's cover
            is properly installed. Verify the system is in working order."

        --#TYPE "System hood is removed (2001)"
        --#SUMMARY "Hood is removed from unit."
        --#ARGUMENTS {}
        --#SEVERITY MAJOR
        --#TIMEINDEX 99
        --#STATE DEGRADED

        ::= 2001

    cpqSiMonitorConditionOK TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSiMonitorIndex }
        DESCRIPTION
            "Fault reporting features have returned to within their normal
             operating range for the monitor indicated by cpqSiMonitorIndex.
             The monitor's condition has been set to OK.

             User Action:  None."

        --#TYPE "Monitor Condition OK (2002)"
        --#SUMMARY "The monitor's condition has been set to OK."
        --#ARGUMENTS {}
        --#SEVERITY INFORMATIONAL
        --#TIMEINDEX 99
        --#STATE OPERATIONAL
        ::=  2002


     cpqSiMonitorConditionDegraded TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSiMonitorIndex }
        DESCRIPTION
            "A fault reporting feature has exceeded normal limits for
             the monitor indicated by the cpqSiMonitorIndex. The monitor's
             condition is degraded due to the internal temperature exceeding
             normal operating limits.  The monitor is still useable, but
             action should be taken to return the condition to OK.

             User Action: Physically check for obstructions to air flow around
             the monitor.  Check the thermostat in the room that the system
             occupies.  Allow the monitor to cool by turning off the monitor
             for 5 minutes then turn the monitor back on.  After the monitor
             cools, another alarm indicating an improving condition, such as
             Monitor OK, will be issued."

        --#TYPE "Monitor Condition Degraded (2003)"
        --#SUMMARY "The monitor's condition has been set to degraded."
        --#ARGUMENTS {}
        --#SEVERITY MINOR
        --#TIMEINDEX 99
        --#STATE DEGRADED

       ::=  2003

     cpqSiMonitorConditionFailed TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSiMonitorIndex }
        DESCRIPTION
            "A fault reporting feature has exceeded normal limits in the
             monitor indicated by the cpqSiMonitorIndex. The monitor's
             condition has been set to failed due to an operational feature
             exceeding normal operating limits.  The monitor will not be
             useable and should be replaced.

             User Action: Make a note of the monitor model number and serial
             number.  Replace the monitor.

             Refer to the appropriate Maintenance and Service Guide for
             detailed information on a component replacement."

        --#TYPE "Monitor Condition Failed (2004)"
        --#SUMMARY "The monitor's condition has been set to failed."
        --#ARGUMENTS {}
        --#SEVERITY CRITICAL
        --#TIMEINDEX 99
        --#STATE NONOPERATIONAL

       ::=  2004

     cpqSiCorrMemErrStatusDegraded TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSiMemErrorIndex }
        DESCRIPTION
            "Correctable memory error count has exceeded the threshold for the
             memory module indicated by the 'cpqSiMemErrorIndex' variable.
             The appropriate cpqSiMemModuleECCStatus has been set to degraded.

             User Action: For Desktops, the System Administrator should run
             the F10 Diagnostics on this system and select RAM LONG TEST. If
             it is determined that a module needs replacing, schedule
             maintenance for the system and replace the failed memory module.

             Refer to the appropriate Maintenance and Service Guide for detailed
             information on a component replacement."

        --#TYPE "Excessive Correctable Memory Errors (2005)"
        --#SUMMARY "The Memory Module %d ECC status has been set to degraded."
        --#ARGUMENTS {3}
        --#SEVERITY MINOR
        --#TIMEINDEX 99
        --#STATE DEGRADED

        ::=  2005

     cpqSiCorrMemErrStatusOk TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSiMemErrorIndex }
        DESCRIPTION
            "Correctable memory error count is now below the threshold for the
             memory module indicated by the 'cpqSiMemErrorIndex' variable. The
             appropriate cpqSiMemModuleECCStatus has been set to ok.

             User Action: None."

        --#TYPE "Correctable Memory Errors Count OK (2006)"
        --#SUMMARY "The Memory Module %d ECC status has been set to OK."
        --#ARGUMENTS {3}
        --#SEVERITY INFORMATIONAL
        --#TIMEINDEX 99
        --#STATE OPERATIONAL

       ::=  2006

     cpqSiMemConfigChange TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSiMemConfigChangeData }
        DESCRIPTION
            "A memory configuration change has occurred. CpqSiMemConfigChangeData
             will indicate which memory modules slots have changed.

             User Action: You may want to verify a valid reason for a memory
             configuration to have occurred. If system issuing the alert is
             a Desktop running NT, the memory configuration change information
             is also logged in the NT System Log."

        --#TYPE "Memory modules have changed (2007)"
        --#SUMMARY "The system's memory configuration has changed."
        --#ARGUMENTS {}
        --#SEVERITY INFORMATIONAL
        --#TIMEINDEX 99
        --#STATE OPERATIONAL
       ::=  2007

    cpqSiHotPlugSlotBoardRemoved TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSiHotPlugSlotChassis,
                     cpqSiHotPlugSlotIndex }
        DESCRIPTION
           "Hot Plug Slot Board Removed.

           A Hot Plug Slot Board has been removed from the specified
           chassis and slot.

           User Action: None."

        --#TYPE "Hot Plug Slot Board Removed (2008)"
        --#SUMMARY "Hot Plug Slot Board Removed from Chassis %d, Slot %d."
        --#ARGUMENTS {2, 3}
        --#SEVERITY INFORMATIONAL
        --#TIMEINDEX 99
        --#STATE OPERATIONAL

        ::= 2008

    cpqSiHotPlugSlotBoardInserted TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSiHotPlugSlotChassis,
                     cpqSiHotPlugSlotIndex }
        DESCRIPTION
           "Hot Plug Slot Board Inserted.

           A Hot Plug Slot Board has been inserted into the specified
           chassis and slot.

           User Action: None."

        --#TYPE "Hot Plug Slot Board Inserted (2009)"
        --#SUMMARY "Hot Plug Slot Board Inserted into Chassis %d, Slot %d."
        --#ARGUMENTS {2, 3}
        --#SEVERITY INFORMATIONAL
        --#TIMEINDEX 99
        --#STATE OPERATIONAL

        ::= 2009

    cpqSiHotPlugSlotPowerUpFailed TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSiHotPlugSlotChassis,
                     cpqSiHotPlugSlotIndex, cpqSiHotPlugSlotErrorStatus }
        DESCRIPTION
           "Hot Plug Slot Board Failed Power-Up.

           A Hot Plug Slot Board has failed to power-up in the specified
           chassis and slot.

           User Action: Insure the board and all cables are installed
           correctly and the board type and revision are the same as
           the replaced board."

        --#TYPE "Hot Plug Slot Board Failed (2010)"
        --#SUMMARY "Hot Plug Slot Board Failed in Chassis %d, Slot %d, Error %d."
        --#ARGUMENTS {2, 3, 4}
        --#SEVERITY CRITICAL
        --#TIMEINDEX 99
        --#STATE FAILED

        ::= 2010

    cpqSiSysBatteryFailure  TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSiSysBatteryIndex,
                     cpqSiSysBatterySerialNum }
        DESCRIPTION
           "The battery indicated by cpqSiSysBatteryIndex has failed
           and must be replaced.

           User Action:  Contact your System Administrator or
           Authorized Reseller to order a replacement battery.
           Recycle your old battery. For proper disposal information,
           refer to the documentation that came with your computer."

        --#TYPE "Battery Failure (2011)"
        --#SUMMARY "Battery %d has failed."
        --#ARGUMENTS {2}
        --#SEVERITY MAJOR
        --#TIMEINDEX 99
        --#STATE DEGRADED

        ::= 2011

    cpqSiSysBatteryChargingDegraded TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSiSysBatteryIndex,
                     cpqSiSysBatterySerialNum  }
        DESCRIPTION
            "Significant battery degradation has occurred with battery
            indicated by cpqSiSysBatteryIndex.  The battery can
            no longer be fully recharged.

            User Action: If using multiple batteries, run
            the Power Conservation Utility to identify the
            battery location.  Contact your System Administrator
            or Authorized Reseller to order a replacement
            battery."

        --#TYPE "Battery Charging Degradation (2012)"
        --#SUMMARY "Battery %d has degraded charging capacity."
        --#ARGUMENTS {2}
        --#SEVERITY MAJOR
        --#TIMEINDEX 99
        --#STATE DEGRADED
        ::= 2012


    cpqSiSysBatteryCalibrationError TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSiSysBatteryIndex,
                     cpqSiSysBatterySerialNum  }
        DESCRIPTION
            "Calibration is needed with battery
            indicated by cpqSiSysBatteryIndex.  The battery can
            not correctly indicate capacity.

            User Action: Run the Power Conservation Utility.  Contact
            your System Administrator or Authorized Reseller to
            order a replacement battery."

        --#TYPE "Battery Calibration Error (2013)"
        --#SUMMARY "Battery %d has calibration error."
        --#ARGUMENTS {2}
        --#SEVERITY MAJOR
        --#TIMEINDEX 99
        --#STATE DEGRADED
        ::= 2013

END
