#* **************************************************************************
#*
#*                  Insight Integration for CA Unicenter
#*
#*      Copyright 1996,2003 Hewlett-Packard Development Company, L.P.
#*
#*      Hewlett-Packard Company shall not be liable for technical or
#*      editorial errors or omissions contained herein. The information in
#*      this document is provided "as is" without warranty of any kind and
#*      is subject to change without notice. The warranties for HP products
#*      are set forth in the express limited warranty statements
#*      accompanying such products. Nothing herein should be construed as
#*      constituting an additional warranty.
#*
#*      Confidential computer software. Valid license from HP required for
#*      possession, use or copying. Consistent with FAR 12.211 and 12.212,
#*      Commercial Computer Software, Computer Software Documentation, and
#*      Technical Data for Commercial Items are licensed to the U.S.
#*      Government under vendor's standard commercial license.
#*
#* **************************************************************************
#*                                                                        
#* PROPRIETARY NOTE:                                                      
#*     This document contains information confidential and proprietary to 
#*     Hewlett-Packard and shall not be reproduced or transferred to other
#*     documents or disclosed to others or used for any purpose other than 
#*     that for which it was obtained without the expressed written consent
#*     of Hewlett-Packard Company.
#*                                                                        
#* **************************************************************************

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6016 * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Correctable memory log disabled status: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - correctable memory log status: OTHER'
       SEVerity=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6016 * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Correctable memory log disabled status: NOT SUPPORTED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - correctable memory log status: NOT SUPPORTED'
       SEVerity=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6016 * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Correctable memory log disabled status: DISABLED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - correctable memory log status: DISABLED'
       SEVerity=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Logging of correctable memory errors ceases when the error count exceeds a factory preset value. Continuing to log errors after the preset number is reached affects performance of the system.'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='This alarm indicates a failing or failed memory module. Though this alarm is classified noncritical, an error of this type indicates that a memory component is failing or has failed in the system issuing the alarm.'
DEFine MSGACTion NAME=(*,40)
       ACTION=ANNOTATE TEXT='The system continues to correct any errors it can. Correct the problem as soon as possible. Further degradation of the memory components may occur, and then errors may no longer be correctable; the system may shut down.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6016 * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Correctable memory log disabled status: ENABLED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - correctable memory log status: ENABLED'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6017 * * * * * * * * * * * ?*'
       MSGNODE=*
       DEScription='HP - System Temp has exceeded its operating limits: SHUTDOWN'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - System temperature has exceeded its operating limits and the system will SHUT DOWN'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6018 * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - System Temp degraded status: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - System temperature degraded status: OTHER'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6018 * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - System Temp degraded status: CONTINUE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - System temperature has DEGRADED and will CONTINUE'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='If the temperature continues to rise, expect the hardware to initiate an immediate and unexpected shutdown. The Degraded Action item on the Environment window is set to continue in the event this alarm was issued.'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='You can set the Degraded Action field to SHUT DOWN when this alarm occurs, thus avoiding a catastrophic shutdown. You can also use the System Configuration Utility to set this item.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6018 * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - System Temp degraded status: SHUTDOWN'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - System temperature has DEGRADED and the system will SHUTDOWN'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The temperature status has been set to degraded. The system has been configured to initiate a system shutdown when this alarm is received.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6019 * * * * * * * * * * * ?*'
       MSGNODE=*
       DEScription='HP - System Temp status: NORMAL'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - System temperature has returned to NORMAL operating range'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6020 * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - System Fan status: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - System fan status: OTHER'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6020 * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - System Fan status: CONTINUE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - System fan is NOT operating properly but the system will CONTINUE'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='If the system continues to operate in this degraded condition, expect the hardware to initiate an immediate and unexpected shutdown. The Degraded Action item on the Environment window is set to continue in the event this alarm was issued.'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='You can set the Degraded Action field to SHUT DOWN when this alarm occurs, thus avoiding a catastrophic shutdown. You can also use the System Configuration Utility to set this item.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6020 * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - System Fan status: SHUTDOWN'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - The system fan is not operating properly and the system will SHUTDOWN'
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The temperature status has been set to degraded. The system has been configured to initiate a system shutdown when this alarm is received.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6021 * * * * * * * * * * * ?*'
       MSGNODE=*
       DEScription='HP - System Optional Fan Degraded'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - The system optional fan is not operating properly'
       Severity=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6022 * * * * * * * * * * * ?*'
       MSGNODE=*
       DEScription='HP - Previous non-operational system Fans status: RETURN TO NORMAL'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Any Previous NON-operational System fan has returned to normal operation'
       Severity=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6023 * * * * * * * * * * * ?*'
       MSGNODE=*
       DEScription='HP - Processor Fan status: FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Processor fan is not operating properly - Server will shutdown'
       Severity=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6024 * * * * * * * * * * * ?*'
       MSGNODE=*
       DEScription='HP - Previous NON-operational processor fans status: RETURNED TO NORMAL'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Any Previous NON-operational processor fans have returned to normal operation'
       Severity=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6025 * * * * * * * * * * * ?*'
       MSGNODE=*
       DEScription='HP - System shut down by ASR feature has become operational'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - A system that has been shut down by the ASR feature has become operational'
       Severity=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6026 * * * * * * * * * * * ?*'
       MSGNODE=*
       DEScription='HP - system with a thermal shutdown has become operational'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - A System that had a thermal shutdown has just become operational'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6027 * * * * * * * * * * * ?*'
       MSGNODE=*
       DEScription='HP - Power On Self Test Errors occured'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - One or more Power On Self Test errors have occurred during reboot'
       SEVerity=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='A Power-On error occurred during a reboot of the system. This error may have been noted during the Automatic Server Recovery reboot. The subsystem responsible for the error may also be responsible for the ASR reboot.'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='The error may include uncorrectable memory errors, fatal hard drive and/or controller failures, and system board failures. It may not be possible to view the system issuing the alarm, as the network operating system may have failed to load properly.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6028 * * * * * * * * * * * ?*'
       MSGNODE=*
       DEScription='HP - Systems redundant power supply subsystem degrading'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - The system redundant power supply subsystem has become degraded'
       SEVerity=W
       ATTRIB=default
       COLOR=orange
