#* **************************************************************************
#*
#*                  Insight Integration for CA Unicenter
#*
#*      Copyright 1996,2003 Hewlett-Packard Development Company, L.P.
#*
#*      Hewlett-Packard Company shall not be liable for technical or
#*      editorial errors or omissions contained herein. The information in
#*      this document is provided "as is" without warranty of any kind and
#*      is subject to change without notice. The warranties for HP products
#*      are set forth in the express limited warranty statements
#*      accompanying such products. Nothing herein should be construed as
#*      constituting an additional warranty.
#*
#*      Confidential computer software. Valid license from HP required for
#*      possession, use or copying. Consistent with FAR 12.211 and 12.212,
#*      Commercial Computer Software, Computer Software Documentation, and
#*      Technical Data for Commercial Items are licensed to the U.S.
#*      Government under vendor's standard commercial license.
#*
#* **************************************************************************
#*                                                                        
#* PROPRIETARY NOTE:                                                      
#*     This document contains information confidential and proprietary to 
#*     Hewlett-Packard and shall not be reproduced or transferred to other
#*     documents or disclosed to others or used for any purpose other than 
#*     that for which it was obtained without the expressed written consent
#*     of Hewlett-Packard Company.
#*                                                                        
#* **************************************************************************
#
# Storage System traps from version 5.40 to 6.40 of the management agents


#-------------------------------
# Definition for trap 8026
#-------------------------------

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8026*'
       MSGNODE=*
       DEScription='HP - Storage System Fan Status Change (8026)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Fan Status Change (TrapData: &(26:))'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The agent has detected a change in the Fan Status of a storage system.  The last variable (cpqSsBoxFanStatus) indicates the current fan status. If the fan status is degraded or failed, replace any failed fans.'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='The fan status may be other(1), ok(2), failed(3), noFan(4), or degraded(5).'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8026 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Storage System Fan Status Other (8026)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Fan Status Other (Location: &26 &27, Controller: &32, Box Bus: &37, Box Vendor: &42,  Box Model: &47, Box S/N: &52)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8026 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Storage System Fan Status Ok (8026)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Fan Status Ok (Location: &26 &27, Controller: &32, Box Bus: &37, Box Vendor: &42,  Box Model: &47, Box S/N: &52)'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8026 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Storage System Fan Status Failed (8026)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Fan Status Failed (Location: &26 &27, Controller: &32, Box Bus: &37, Box Vendor: &42,  Box Model: &47, Box S/N: &52)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='One or more storage system fans have failed.  The fan(s) should be replaced immediately to avoid hardware damage.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8026 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Storage System Fan Status NoFan (8026)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Fan Status NoFan (Location: &26 &27, Controller: &32, Box Bus: &37, Box Vendor: &42,  Box Model: &47, Box S/N: &52)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='This unit does not support fan monitoring.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8026 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - Storage System Fan Status Degraded (8026)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Fan Status Degraded (Location: &26 &27, Controller: &32, Box Bus: &37, Box Vendor: &42,  Box Model: &47, Box S/N: &52)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='At least one storage system fan has failed, but there is still sufficient cooling capacity to allow the system to continue. The fan should be replaced.'



#-------------------------------
# Definition for trap 8027
#-------------------------------

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8027*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature Status Change (8027)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Temperature Status Change (TrapData: &(26:))'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The agent has detected a change in the temperature status of a storage system.  The last variable (cpqSsBoxTempStatus) indicates the current temperature status: other(1), ok(2), degraded(3), failed(4), noTemp(5).'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='If the temperature status is degraded or failed, shutdown the storage system as soon as possible.  Insure that the storage system environment is being cooled properly and that no components are overheated.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8027 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature Status Other (8027)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Temperature Status Other (Location: &26 &27, Controller: &32, Box Bus: &37, Box Vendor: &42,  Box Model: &47, Box S/N: &52)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Temperature monitoring is not supported by this system or it is not supported by the driver.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8027 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature Status Ok (8027)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Temperature Status Ok (Location: &26 &27, Controller: &32, Box Bus: &37, Box Vendor: &42,  Box Model: &47, Box S/N: &52)'
       SEVERITY=S
       ATTRIB=default
       COLOR=green
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The temperature is within normal operating range.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8027 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature Status Degraded (8027)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Temperature Status Degraded (Location: &26 &27, Controller: &32, Box Bus: &37, Box Vendor: &42,  Box Model: &47, Box S/N: &52)'
       SEVERITY=W
       ATTRIB=default
       COLOR=Orange
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The temperature is outside of normal operating range. User Action: Shutdown the storage system as soon as possible.  Insure that the storage system environment is being cooled properly and that no components are overheated.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8027 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature Status Failed (8027)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Temperature Status Failed (Location: &26 &27, Controller: &32, Box Bus: &37, Box Vendor: &42,  Box Model: &47, Box S/N: &52)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The temperature could permanently damage the system. The storage system will automatically shutdown if this condition is detected.'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='User Action: Shutdown the storage system as soon as possible.  Insure that the storage system environment is being cooled properly and that no components are overheated.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8027 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature Status NoTemperature (8027)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Temperature Status NoTemperature (Location: &26 &27, Controller: &32, Box Bus: &37, Box Vendor: &42,  Box Model: &47, Box S/N: &52)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='This unit does not support temperature monitoring.'


#-------------------------------
# Definition for trap 8028
#-------------------------------

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8028*'
       MSGNODE=*
       DEScription='HP - Storage System Power Supply Status Change (8028)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Power Supply Status Change (TrapData: &(26:))'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The agent has detected a change in the power supply status of a storage system.  The last variable (cpqSsBoxFltTolPwrSupplyStatus) indicates the current power supply status.'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='Status may be other(1), ok(2), degraded(3), failed(4) or noFaultTolPower(5). User Action: If the power supply status is degraded, take action to restore power or replace the failed power supply.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8028 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Storage System Power Supply Status Other (8028)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Power Supply Status Other (Location: &26 &27, Controller: &32, Box Bus: &37, Box Vendor: &42,  Box Model: &47, Box S/N: &52)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Power Supply monitoring is not supported by this system or it is not supported by the driver.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8028 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Storage System Power Supply Status Ok (8028)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Power Supply Status Ok (Location: &26 &27, Controller: &32, Box Bus: &37, Box Vendor: &42,  Box Model: &47, Box S/N: &52)'
       SEVERITY=S
       ATTRIB=default
       COLOR=green
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The Power Supply is within normal operating range.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8028 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Storage System Power Supply Status Degraded (8028)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Power Supply Status Degraded (Location: &26 &27, Controller: &32, Box Bus: &37, Box Vendor: &42,  Box Model: &47, Box S/N: &52)'
       SEVERITY=W
       ATTRIB=default
       COLOR=Orange
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='One of the power supply units in a fault tolerant power supply has failed. User Action: Take action to restore power or replace the failed power supply.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8028 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Storage System Power Supply Status Failed (8028)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Power Supply Status Failed (Location: &26 &27, Controller: &32, Box Bus: &37, Box Vendor: &42,  Box Model: &47, Box S/N: &52)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8028 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - Storage System Power Supply Status NoFaultTolerantPower (8028)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Power Supply Status NoFaultTolerantPower (Location: &26 &27, Controller: &32, Box Bus: &37, Box Vendor: &42,  Box Model: &47, Box S/N: &52)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='This unit does not support fault tolerant power supply monitoring.'

