DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5474 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CellInfoList is not NULL.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CellInfoList is not NULL.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The CellInfoList is not null and was expected to be. There has been an error in interleaving.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5478 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error in constructing the Memory Descriptor.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error in constructing the Memory Descriptor.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error in constructing the Memory Descriptor.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5479 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unable to update the local memory layout'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unable to update the local memory layout: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Unable to update the local memory layout.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5483 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A required address was not found within a mapped address.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A required address was not found within a mapped address.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A required address was not found within a mapped address in the PDT.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5485 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failure to install a Partition level PDT.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failure to install a Partition level PDT.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failure to install a partition level PDT. Errors prevented it.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5490 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A critical resourse could not be found or is unusable'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A critical resourse could not be found or is unusable: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A critical resouse that is required early in the initialization process either could not be found, or was unusable. The specific resouse is specified in the data field as follows: Platform Paramaters Component not found in FIT: 0xdead0001;'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='SRAM_BASE not found in platform parms: 0xdead0002; SRAM_SIZE not found in Platform Parms: 0xdead0003; firmware framework not found in the fit: 0xdead0004; Framework Segmant not usable: 0xdead0005; bad NVRAM: 0xdead0006; Dillon unusable:  '
DEFine MSGACTion Name=(*,40)
ACTION=ANNOTATE TEXT='0xdead0007; SRAM unusable: 0xdead0008; CPU unusable: 0xdead0009; Options Component Unusable: 0xdead000a; Real Time Clock unusable: DEAD_RTC; Unknown: 0xdead0086" '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5491 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Internal firmware programming error.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Internal firmware programming error.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An internal firmware error was encountered. This is usually caused by a bad parameter passed to a function, corrupt memory, corrupt malloc tables or something similar. The data field contains the IP address of the function that encountered the'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='error.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5492 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event NVRam test failed with a data compare error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event NVRam test failed with a data compare error: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='NVRAM failed with a data compare error. 3 chassis codes will be sent. The first one will have the expected data and the second the actual data and the third one will be the address.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5493 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An NVRam CRC Error was detected'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An NVRam CRC Error was detected: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An NVRAM CRC Error was detected. There will always be 2 chassis codes sent. The first one will give the expected data and the second the actual data.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5494 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The Error Response Mode has been determined'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The Error Response Mode has been determined: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Get Error Response Mode has been called. The first 8 bytes of the response mode string are displayed in the data field and must be converted to ascii from the hex values.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5496 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A semaphore could not be obtained'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A semaphore could not be obtained: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The required semaphore could not be obtained due to errors. The data field contains the IP of the routine trying to obtain the semaphore. A request was placed for more NVRAM to be allocated but NVRAM was full.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5498 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The BLOCK requested in NVRAM has the wrong revision'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The BLOCK requested in NVRAM has the wrong revision: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The NVRAM block requested has an unexpected revision. This chassis code will be emmitted in pairs. The first one will contain the expected revision number, the second will contain the actual revision number.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5499 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The requested NVRAM block was not found.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The requested NVRAM block was not found.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The requested NVRAM block was not found. The ID that was not found is displayed in the data field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5500 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The requested NVRAM block is locked.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The requested NVRAM block is locked.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The block id specified in the data field is locked.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5501 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Firmware tried to unlock a NVRAM block that was already unlocked.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Firmware tried to unlock a NVRAM block that was already unlocked.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware tried to unlock a NVRAM block that was already unlocked. Data field contains the block ID.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5502 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The Header in NVRAM was not found'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The Header in NVRAM was not found: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The header in the NVRAM space was not found.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5503 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The Freelist used for NVM block allocation is corrupt.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The Freelist used for NVM block allocation is corrupt.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Freelist used vor Non-Volatile Memory allocation is corrpt.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5505 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Firmware is preparing to reset for reconfiguration.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Firmware is preparing to reset for reconfiguration.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System firmware has detected a condition that requires the cell to be reset for reconfiguration. The function has been called and is now executing. Data field contains the cell number being reset.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5507 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An error was encountered communicating with utilities during PD rendez.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An error was encountered communicating with utilities during PD rendez.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='During PD rendezvous, system firmware encountered a problem sending commands to the utilities system. This will prevent a fully functional PD from being created.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5509 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Forward Progress is stopping. The Cell or System will not boot further.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Forward Progress is stopping. The Cell or System will not boot further.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System Firmware has determined that cell or system progress must be halted. The data field contains the Instruction Pointer of the function that called for the halt. The second instance of this code being emitted indicates the major state in'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='system change. This code must be emmitted in pairs.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5510 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event No console is available for the DUI to use.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event No console is available for the DUI to use.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The DUI (Developers User Interface) was entered, but there is no console available for the interface.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5511 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error Processing encountered an unrecoverable error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error Processing encountered an unrecoverable error: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='During Error processing and reporting, an error was detected that prevented further processing of errors. The data field contains an ASCII message indicating the problem.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5514 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event System is unable to complete the Reset For Reconfiguration request.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event System is unable to complete the Reset For Reconfiguration request.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System firmware is unable to complete the request to reset the cell for reconfiguration. Typically, are required step has not been performed yet or a needed resource is unavailable.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5515 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The cell is not able to reach all requested cells through the fabric.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The cell is not able to reach all requested cells through the fabric.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The cell was not able to reach all the other cells in its configured set through the fabric. The data field contains the bitmask of actual cells that were reached.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5518 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event LBA has unexpected number of I/O Slots.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event LBA has unexpected number of I/O Slots.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware detected a PCI-to-PCI bridge that exceeds the maximum supported bridge depth. Firmware will not configure I/O devices below the maximum bridge depth. Such I/O devices will not be usable as console nor boot devices but might be usable'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='by the O/S. Data Field: PCI function address of the bridge that exceeded the maximum depth limit. Bits 24..31: segment number Bits 16..23: bus number Bits 11..15: device number Bits 8..10: function number Bits 0..7: reserved (0)  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5521 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Console device failed to connect.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Console device failed to connect.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Debugging event, not for release. This event is no longer used on Everest/xPeak systems but its event ID is still contained in the code base.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5524 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error loading EFI driver.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error loading EFI driver.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Debugging event, not for release. This event is no longer used on Everest/xPeak systems but its event ID is still contained in the code base.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5525 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Copying memory test code failed.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Copying memory test code failed.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This event is unused'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5527 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A remote cell is in an unknown state of PD rendezvous'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A remote cell is in an unknown state of PD rendezvous: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The reporting cell read an unknown state from a remote cell. This chassis code will be emitted in pairs. The first one indicating the cell number in the data field and the second code indicating the state read in the data field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5528 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Multiple Core Cells have been discovered in the same PD'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Multiple Core Cells have been discovered in the same PD: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The reporting Cell thinks that it should be the core cell but has discovered another cell in the same PD that thinks it should be the core cell. This is a serious problem.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5529 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The utilities component encountered an error when sending a command to the MP'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The utilities component encountered an error when sending a command to the MP: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The utilities system firmware component received an error response from the SINC in response to a command being sent. The exact error is displayed in the data field. Typically, this can occure when the SINC cannot talk to the MP.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5530 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error received after issuing the Retrieve Cell Slot State command'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error received after issuing the Retrieve Cell Slot State command: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System Firmware issued the Retrieve Cell Slot State command to the Sync and got an error back. See related chassis code or the specifics of the error.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5546 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event This indicates that all the cpus in the cell did not rendezvous during the MCA.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event This indicates that all the cpus in the cell did not rendezvous during the MCA.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This denotes the fact that all the cpus in the cell did not rendezvous.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5547 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event This indicates that it does not have any access to the PD.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event This indicates that it does not have any access to the PD.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This chassis code indicates that thecell does not have any access to a PD.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5548 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event This indicates the loss of lockstep during the MCA path.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event This indicates the loss of lockstep during the MCA path.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This indicates the cell would not be able to join the other cells in the PD level rendezvous. The data portion represents the cell id of the cell that incurred the loss of lockstep.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5550 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The PD level cell rendezvous failed.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The PD level cell rendezvous failed.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This inicates that some of the cells did not show up during the PD level rendezvous.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5556 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event It stands for diagnosis of catastrophic errors in the PIN block of concorde.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event It stands for diagnosis of catastrophic errors in the PIN block of concorde.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This indicates that catastrophic errors have been found in the PIN block of the concorde. The cell needs to be reset/ halt.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5557 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The cell monarch cpu has failed.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The cell monarch cpu has failed.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This means that the cell monach cpu has not completed the assigned task within the timeout and hence it will be deconfigured.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5558 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event This indicates that the cell missed the rendezvous at the partition level.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event This indicates that the cell missed the rendezvous at the partition level.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This indicates that the cell is too late for the PD level rendezvous. And hence it will not join the other PD cells.'

