--MibName=cpqSm2
-- ****************************************************************************
--
--            Remote Insight/Integrated Lights-Out Information
--         Management Information Base for SNMP Network Management
--
--
--      Copyright 1996,2003 Hewlett-Packard Development Company, L.P.
--
--      Hewlett-Packard Company shall not be liable for technical or
--      editorial errors or omissions contained herein. The information in
--      this document is provided "as is" without warranty of any kind and
--      is subject to change without notice. The warranties for HP products
--      are set forth in the express limited warranty statements
--      accompanying such products. Nothing herein should be construed as
--      constituting an additional warranty.
--
--      Confidential computer software. Valid license from HP required for
--      possession, use or copying. Consistent with FAR 12.211 and 12.212,
--      Commercial Computer Software, Computer Software Documentation, and
--      Technical Data for Commercial Items are licensed to the U.S.
--      Government under vendor's standard commercial license.
--
--      Refer to the READMIB.RDM file for more information about the
--      organization of the information in the Compaq Enterprise.
--
--      The Compaq Enterprise number is 232.
--      The ASN.1 prefix to, and including the Compaq Enterprise is:
--           1.3.6.1.4.1.232
--
-- ****************************************************************************


CPQSM2-MIB DEFINITIONS ::= BEGIN

    IMPORTS
        Counter                 FROM RFC1155-SMI
        IpAddress               FROM RFC1155-SMI
        DisplayString           FROM RFC1213-MIB
        OBJECT-TYPE             FROM RFC-1212
        TRAP-TYPE               FROM RFC-1215
        sysName                 FROM RFC1213-MIB
        compaq                  FROM CPQHOST-MIB
        cpqHoTrapFlags          FROM CPQHOST-MIB;

    compaq              OBJECT IDENTIFIER ::= { enterprises 232 }
    cpqSm2              OBJECT IDENTIFIER ::= { compaq 9 }
    cpqSm2MibRev        OBJECT IDENTIFIER ::= { cpqSm2 1 }
    cpqSm2Component     OBJECT IDENTIFIER ::= { cpqSm2 2 }
    cpqSm2Trap          OBJECT IDENTIFIER ::= { cpqSm2 3 }

    cpqSm2Interface     OBJECT IDENTIFIER ::= { cpqSm2Component 1 }
    cpqSm2Cntlr         OBJECT IDENTIFIER ::= { cpqSm2Component 2 }
    cpqSm2EventLog      OBJECT IDENTIFIER ::= { cpqSm2Component 3 }
    cpqSm2AsyncComm     OBJECT IDENTIFIER ::= { cpqSm2Component 4 }
    cpqSm2Nic           OBJECT IDENTIFIER ::= { cpqSm2Component 5 }

    cpqSm2OsCommon      OBJECT IDENTIFIER ::= { cpqSm2Interface 4 }

-- Object identifiers returned for the sysObjectId from the firmware agent.
-- This loosely matches the cpqSm2CntlrModel enumeration construct.

    cpqSm2Products         OBJECT IDENTIFIER ::= { cpqSm2 4 }
 -- .1.3.6.1.4.1.232.9.4.2
    cpaSm2ProdEisaRemote   OBJECT IDENTIFIER ::= { cpqSm2Products 2 }
 -- .1.3.6.1.4.1.232.9.4.3
   cpqSm2ProdPCIRemote     OBJECT IDENTIFIER ::= { cpqSm2Products 3 }
 -- .1.3.6.1.4.1.232.9.4.4
   cpqSm2ProdRILOE         OBJECT IDENTIFIER ::= { cpqSm2Products 4 }
 -- .1.3.6.1.4.1.232.9.4.5
   cpqSm2ProdiLo           OBJECT IDENTIFIER ::= { cpqSm2Products 5 }
 -- .1.3.6.1.4.1.232.9.4.6
   cpqSm2ProdRILOEII       OBJECT IDENTIFIER ::= { cpqSm2Products 6 }


-- ****************************************************************************
--   Remote Insight/Integrated Lights-Out Information MIB Revision
--   =============================================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSm2 Group                   (1.3.6.1.4.1.232.9)
--       cpqSm2MibRev Group            (1.3.6.1.4.1.232.9.1)
--
--      Implementation of the cpqSm2MibRev group is mandatory for all agents
--      supporting the Remote Insight/Integrated Lights-Out MIB.
--
--      An Insight Agent conforming to this document will return a
--      cpqSm2MibRevMajor of one (1) and a cpqSm2MibRevMinor of six (6).
--
-- ****************************************************************************

    cpqSm2MibRevMajor OBJECT-TYPE
        SYNTAX  INTEGER (1..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The Major Revision level of the MIB.

            A change in the major revision level represents a major change
            in the architecture of the MIB.  A change in the major revision
            level may indicate a significant change in the information
            supported and/or the meaning of the supported information.
            Correct interpretation of data may require a MIB document with
            the same major revision level."
        ::= { cpqSm2MibRev 1 }

    cpqSm2MibRevMinor OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The Minor Revision level of the MIB.

            A change in the minor revision level may represent some minor
            additional support, no changes to any pre-existing information
            has occurred."
        ::= { cpqSm2MibRev 2 }

    cpqSm2MibCondition OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            ok(2),
            degraded(3),
            failed(4)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Remote Insight/ Integrated Lights-Out condition.

         This represents the overall condition of the
         Remote Insight/ Integrated Lights-Out."

        ::= { cpqSm2MibRev 3 }


-- ****************************************************************************
--   Remote Insight/ Integrated Lights-Out OS Common
--   ==============================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSm2 Group                   (1.3.6.1.4.1.232.9)
--       cpqSm2Component Group         (1.3.6.1.4.1.232.9.2)
--        cpqSm2Interface Group        (1.3.6.1.4.1.232.9.2.1)
--         cpqSm2OsCommon Group        (1.3.6.1.4.1.232.9.2.1.4)
--
--
--  Implementation of the cpqSm2OsCommon group is mandatory for all
--  agents that support the Remote Insight/ Integrated Lights-Out MIB.
--
-- ****************************************************************************

    cpqSm2OsCommonPollFreq OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "The Insight Agent's polling frequency.

            The frequency, in seconds, at which the Insight Agent requests
            information from the device driver.  A frequency of zero (0)
            indicates that the Insight Agent retrieves the information upon
            request of a management station, it does not poll the device
            driver at a specific interval.

            If the poll frequency is zero (0) all attempts to write to this
            object will fail.  If the poll frequency is non-zero,
            setting this value will change the polling frequency of the
            Insight Agent.  Setting the poll frequency to zero (0) will
            always fail.  An agent may choose to fail any request to change
            the poll frequency to a value that would severely impact system
            performance."
        ::= { cpqSm2OsCommon 1 }


-- ****************************************************************************
--   Remote Insight/ Integrated Lights-Out OS Common Module Table
--   ===========================================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSm2 Group                   (1.3.6.1.4.1.232.9)
--       cpqSm2Component Group         (1.3.6.1.4.1.232.9.2)
--        cpqSm2Interface Group        (1.3.6.1.4.1.232.9.2.1)
--         cpqSm2OsCommon Group        (1.3.6.1.4.1.232.9.2.1.4)
--          cpqSm2OsCommonModuleTable  (1.3.6.1.4.1.232.9.2.1.4.2) deprecated
--
-- ****************************************************************************

    cpqSm2OsCommonModuleTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSm2OsCommonModuleEntry
        ACCESS  not-accessible
        STATUS  deprecated
        DESCRIPTION
            "A table of software modules that provide an interface to the
            device this MIB describes."
        ::= { cpqSm2OsCommon 2 }

    cpqSm2OsCommonModuleEntry OBJECT-TYPE
        SYNTAX  CpqSm2OsCommonModuleEntry
        ACCESS  not-accessible
        STATUS  deprecated
        DESCRIPTION
            "A description of a software module that provides an interface
            to the device this MIB describes."
        INDEX   { cpqSm2OsCommonModuleIndex }
        ::= { cpqSm2OsCommonModuleTable 1 }

        CpqSm2OsCommonModuleEntry ::= SEQUENCE {
            cpqSm2OsCommonModuleIndex       INTEGER,
            cpqSm2OsCommonModuleName        DisplayString,
            cpqSm2OsCommonModuleVersion     DisplayString,
            cpqSm2OsCommonModuleDate        OCTET STRING,
            cpqSm2OsCommonModulePurpose     DisplayString
        }

    cpqSm2OsCommonModuleIndex OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "A unique index for this module description."
        ::= { cpqSm2OsCommonModuleEntry 1 }

    cpqSm2OsCommonModuleName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The module name."
        ::= { cpqSm2OsCommonModuleEntry 2 }

    cpqSm2OsCommonModuleVersion OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..5))
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The module version in XX.YY format.

            Where XX is the major version number and YY is the minor version
            number.  This field will be null (size 0) string if the agent
            cannot provide the module version."
        ::= { cpqSm2OsCommonModuleEntry 3 }

    cpqSm2OsCommonModuleDate OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (7))
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The module date.

             field  octets  contents                  range
             =====  ======  =======                  =====
               1      1-2   year                      0..65536
               2       3    month                     1..12
               3       4    day                       1..31
               4       5    hour                      0..23
               5       6    minute                    0..59
               6       7    second                    0..60
                            (use 60 for leap-second)


            This field will be set to year = 0 if the agent cannot provide
            the module date.  The hour, minute, and second field will be set
            to zero (0) if they are not relevant.  The year field is set
            with the most significant octet first."
        ::= { cpqSm2OsCommonModuleEntry 4 }

    cpqSm2OsCommonModulePurpose OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The purpose of the module described in this entry."
        ::= { cpqSm2OsCommonModuleEntry 5 }


-- ****************************************************************************
--   Remote Insight/ Integrated Lights-Out Controller Group
--   ======================================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSm2 Group                   (1.3.6.1.4.1.232.9)
--       cpqSm2Component Group         (1.3.6.1.4.1.232.9.2)
--        cpqSm2Cntrl Group            (1.3.6.1.4.1.232.9.2.2)
--
--      The cpqSm2Cntlr group contains the configuration and statistical
--      information of the Remote Insight/ Integrated Lights-Out.
--
--      Implementation of the cpqSm2Cntlr group is mandatory for all agents
--      that support the Remote Insight/ Integrated Lights-Out MIB.
--
-- ****************************************************************************

    cpqSm2CntlrRomDate OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..10))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out ROM Date.

            The firmware date format is mm/dd/yyyy format."
        ::= { cpqSm2Cntlr 1 }

    cpqSm2CntlrRomRevision OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..5))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out ROM Revision.

            The revision of the firmware on the
            Remote Insight/ Integrated Lights-Out."
        ::= { cpqSm2Cntlr 2 }

    cpqSm2CntlrVideoStatus OBJECT-TYPE
        SYNTAX  INTEGER {
                other(1),
                enabled(2),
                disabled(3)
                }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Video Hardware Status.

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine the status of
              the Remote Insight/ Integrated Lights-Out video.

            enabled(2)
              The Remote Insight/ Integrated Lights-Out video is enabled.

            disabled(3)
              The Remote Insight/ Integrated Lights-Out video is disabled."
        ::= { cpqSm2Cntlr 3 }

    cpqSm2CntlrBatteryEnabled OBJECT-TYPE
        SYNTAX  INTEGER {
                other(1),
                enabled(2),
                disabled(3),
                noBattery(4)
                }
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight Battery Enabled.

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine the status of the
              Remote Insight battery.

            enabled(2)
              The Remote Insight battery is present and is enabled.

            disabled(3)
              The Remote Insight battery is present and is disabled.

            noBattery(4)
              This Remote Insight model does not use a battery."
        ::= { cpqSm2Cntlr 4 }

    cpqSm2CntlrBatteryStatus OBJECT-TYPE
        SYNTAX  INTEGER {
                other(1),
                batteryOk(2),
                batteryFailed(3),
                batteryDisconnected(4)
                }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight Battery Status.

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine if the battery
              needs replacement.

            batteryOk(2)
              The Remote Insight battery is OK.

            batteryFailed(3)
              The Remote Insight battery needs replacement.

            batteryDisconnected(4)
              The Remote Insight battery is disconnected."
        ::= { cpqSm2Cntlr 5 }

    cpqSm2CntlrBatteryPercentCharged OBJECT-TYPE
        SYNTAX  INTEGER (0..100)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight Battery Percent Charged.

            The Remote Insight battery recharge level."

        ::= { cpqSm2Cntlr 6 }

    cpqSm2CntlrAlertStatus OBJECT-TYPE
        SYNTAX  INTEGER {
                other(1),
                enabled(2),
                disabled(3)
                }
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Alerting Status.

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine the status of Remote
              Insight alerting.

            enabled(2)
              Remote Insight/ Integrated Lights-Out alerting is enabled.

            disabled(3)
              Remote Insight/ Integrated Lights-Out alerting is disabled."
        ::= { cpqSm2Cntlr 7 }

    cpqSm2CntlrPendingAlerts OBJECT-TYPE
        SYNTAX  INTEGER {
                other(1),
                noAlertsPending(2),
                alertsPending(3),
                clearPendingAlerts(4)
                }
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "Pending Remote Insight/ Integrated Lights-Out alerts.

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine the state of Remote
              Insight pending alerts.

            noAlertsPending(2)
              No Remote Insight/ Integrated Lights-Out alerts are pending.
              All alerts have been delivered.

            alertsPending(3)
              Remote Insight/ Integrated Lights-Out alerts are pending.
              There are alerts remaining to be sent.

            clearPendingAlerts(4)
              This value is set to clear any Remote Insight/ Integrated Lights-Out
              alerts that have not been sent."
        ::= { cpqSm2Cntlr 8 }

    cpqSm2CntlrSelfTestErrors OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Self Test Errors.

            This is a collection of post error flags.  Each bit has the
            following meaning when it is on (1):

                Bit 17-31: RESERVED: Always 0.
                Bit 16:    I2C error.
                Bit 15:    EEPROM error.
                Bit 14:    SRAM error.
                Bit 13:    CPLD error.
                Bit 12:    Mouse interface error.
                Bit 11:    NIC Error
                Bit 10:    PCMCIA Error
                Bit 9:     Video Error
                Bit 8:     NVRAM write / read / verify error.
                Bit 7:     NVRAM interface error.
                Bit 6:     Battery interface error.
                Bit 5:     Keyboard interface error.
                Bit 4:     Serial port UART error.
                Bit 3:     Modem UART error.
                Bit 2:     Modem firmware error.
                Bit 1:     Memory test error.
                Bit 0:     Busmaster I/O read error.

            NOTE:   bit 31 is the most significant bit, bit 0 is the least
                    significant.

            A value of 0 means no errors have occurred."
        ::= { cpqSm2Cntlr 9 }

    cpqSm2CntlrAgentLocation OBJECT-TYPE
        SYNTAX  INTEGER {
                hostOsAgent(1),
                firmwareAgent(2),
                remoteInsightPciFirmwareAgent(3),
                enclosureFirmwareAgent(4)
                }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Agent Location.

            The following values are defined:

            hostOsAgent(1)
              The Remote Insight/ Integrated Lights-Out MIB information
              is provided by the host OS agents.

            firmwareAgent(2)
              The Remote Insight/ Integrated Lights-Out MIB information is
              provided by the EISA Remote Insight/ Integrated Lights-Out firmware.

            remoteInsightPciFirmwareAgent(3)
              The Remote Insight/ Integrated Lights-Out MIB information is provided
              by the PCI Remote Insight/ Integrated Lights-Out firmware.

            enclosureFirmwareAgent(4)
              The Remote Insight/ Integrated Lights-Out MIB information is provided
              by a rack enclosure firmware agent."
        ::= { cpqSm2Cntlr 10 }

    cpqSm2CntlrLastDataUpdate OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (7))
        ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
            "The date and time that the Remote Insight/ Integrated Lights-Out
            offline data was last updated.

             field  octets  contents                  range
             =====  ======  =======                  =====
               1      1-2   year                      0..65536
               2       3    month                     1..12
               3       4    day                       1..31
               4       5    hour                      0..23
               5       6    minute                    0..59
               6       7    second                    0..60
                            (use 60 for leap-second)


            This field will be set to year = 0 if the agent cannot provide
            the date and time.  The hour, minute, and second field will be set
            to zero (0) if they are not relevant.  The year field is set
            with the most significant octet first."
        ::= { cpqSm2Cntlr 11}

    cpqSm2CntlrDataStatus OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            noData(2),
            onlineData(3),
            offlineData(4)
        }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Host OS Data Status.

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine the status of the
              host OS data.

            noData(2)
              There is no data available for the host system OS.

            onlineData(3)
              Data is available from the host OS Insight Agent.

            offlineData(4)
              A backup copy of data is available from the
              Remote Insight/ Integrated Lights-Out firmware agent."
        ::= { cpqSm2Cntlr 12 }

    cpqSm2CntlrColdReboot OBJECT-TYPE
        SYNTAX  INTEGER {
                notAvailable(1),
                available(2),
                doColdReboot(3)
        }
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Server Cold Reboot

            The following values are defined:

            notAvailable(1)
              Cold reboot of the system is not available.

            available(2)
              Cold reboot of the system is available.

            doColdReboot(3)
              This value is set to cause a cold reboot of the system."
        ::= { cpqSm2Cntlr 13 }

    cpqSm2CntlrBadLoginAttemptsThresh OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Maximum Unauthorized Login Attempts Threshold.

            This is the threshold for consecutive unsuccessful login attempts.
            When this threshold is exceeded, a trap is sent."

        ::= { cpqSm2Cntlr 14 }

    cpqSm2CntlrBoardSerialNumber OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..40))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Serial Number.

            The Serial Number of this Remote Insight/ Integrated Lights-Out."
        ::= { cpqSm2Cntlr 15 }

    cpqSm2CntlrRemoteSessionStatus OBJECT-TYPE
        SYNTAX  INTEGER {
                other(1),
                active(2),
                inactive(3)
                }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Session Status.

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine the status of a Remote
              Insight session.

            active(2)
              A Remote Insight/ Integrated Lights-Out session is active.

            inactive(3)
              There is no active Remote Insight/ Integrated Lights-Out session."
        ::= { cpqSm2Cntlr 16 }

    cpqSm2CntlrInterfaceStatus OBJECT-TYPE
        SYNTAX  INTEGER {
                other(1),
                ok(2),
                notResponding(3)
                }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Interface Status.

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine the status of the
              Remote Insight/ Integrated Lights-Out interface.

            ok(2)
              The Remote Insight/ Integrated Lights-Out firmware is
              responding to commands.

            notResponding(3)
              The Remote Insight/ Integrated Lights-Out firmware is not
              responding to commands."
        ::= { cpqSm2Cntlr 17 }

    cpqSm2CntlrSystemId OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..9))
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out System ID.

            A number used to identify this system in
            Remote Insight/ Integrated Lights-Out pager alerts."
        ::= { cpqSm2Cntlr 18 }

    cpqSm2CntlrKeyboardCableStatus OBJECT-TYPE
        SYNTAX  INTEGER {
                other(1),
                connected(2),
                disconnected(3)
                }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight Keyboard Cable Status.

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine if the keyboard
              cable is connected to the Remote Insight.

            connected(2)
              The keyboard cable is connected to the Remote Insight.

            disconnected(3)
              The keyboard cable is not connected to the Remote Insight."
        ::= { cpqSm2Cntlr 19 }

    cpqSm2ServerIpAddress OBJECT-TYPE
        SYNTAX  IpAddress
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The IP address for this servers connection to the
            Remote Insight/ Integrated Lights-Out. This address is
            used to communicate remotely to the host server via the
            Remote Insight/ Integrated Lights-Out."

        ::= { cpqSm2Cntlr 20 }

    cpqSm2CntlrModel OBJECT-TYPE
        SYNTAX  INTEGER {
                other(1),
                eisaRemoteInsightBoard(2),
                pciRemoteInsightBoard(3),
                pciLightsOutRemoteInsightBoard(4),
                pciIntegratedLightsOutRemoteInsight(5),
                pciLightsOutRemoteInsightBoardII(6)
                }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Model.

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine the model of
              the Remote Insight/ Integrated Lights-Out.

            eisaRemoteInsightBoard(2)
              This is the EISA Remote Insight.

            pciRemoteInsightBoard(3)
              This is the PCI Remote Insight.

            pciLightsOutRemoteInsightBoard(4)
              This is the Remote Insight Lights-Out Edition.

            pciIntegratedLightsOutRemoteInsight(5)
              This is Integrated Remote Insight Lights-Out Edition.

            pciLightsOutRemoteInsightBoardII(6)
              This is the Remote Insight Lights-Out Edition version II."

        ::= { cpqSm2Cntlr 21 }

    cpqSm2CntlrSelfTestErrorMask OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Self Test Error Mask.

            Each bit in this mask corresponds to a bit in the MIB variable
            cpqSm2CntlrSelfTestErrors.  If the mask bit is a 1, then the
            corresponding bit in cpqSm2CntlrSelfTestErrors is relevant to
            the particular version of the Remote Insight/ Integrated Lights-Out.
            This variable is necessary since the different versions of the
            Remote Insight/ Integrated Lights-Out hardware have different
            subsets of tests that are performed."
        ::= { cpqSm2Cntlr 22 }

    cpqSm2CntlrMouseCableStatus OBJECT-TYPE
        SYNTAX  INTEGER {
                other(1),
                connected(2),
                disconnected(3)
                }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight Mouse Cable Status.

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine if the mouse
              cable is connected to the Remote Insight.

            connected(2)
              The mouse cable is connected to the Remote Insight.

            disconnected(3)
              The mouse cable is not connected to the Remote Insight."
        ::= { cpqSm2Cntlr 23 }

    cpqSm2CntlrVirtualPowerCableStatus OBJECT-TYPE
        SYNTAX  INTEGER {
                other(1),
                connected(2),
                disconnected(3),
                notApplicable(4)
                }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight Virtual Power Cable Status.

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine if the virtual power
              cable is connected to the Remote Insight.

            connected(2)
              The virtual power cable is connected to the Remote Insight.

            disconnected(3)
              The virtual power cable is not connected to the Remote Insight.

            notApplicable(4)
              Not Applicable."
        ::= { cpqSm2Cntlr 24 }

    cpqSm2CntlrExternalPowerCableStatus OBJECT-TYPE
        SYNTAX  INTEGER {
                other(1),
                externallyConnected(2),
                disconnected(3),
                internallyConnected(4),
                externallyAndInternallyConnected(5),
                notApplicable(6)
                }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight External Power Cable Status.

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine if the External or
              Internal power cable connections to the Remote Insight.

            externallyConnected(2)
              Just External power cable is connected to the Remote Insight.

            disconnected(3)
              Both External and Internal power cables are disconnected from
              the Remote Insight.

            internallyConnected(4)
              Just Internal power cable is connected to the Remote Insight.

            externallyAndInternallyConnected(5)
              Both External and Internal power cables are connected to the
              Remote Insight.

            notApplicable(6)
              Not Applicable."
        ::= { cpqSm2Cntlr 25 }

    cpqSm2CntlrHostGUID OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (16))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The globally unique identifier of this server.

             This variable can by used by management stations to correlate
             the Remote Insight/ Integrated Lights-Out controller to the server
             containing the controller.  This variable is identical to the variable
             'cpqHoGUID' which is returned from the CPQHOST.MIB."
        ::= { cpqSm2Cntlr 26 }

    cpqSm2CntlriLOSecurityOverrideSwitchState OBJECT-TYPE
        SYNTAX  INTEGER {
                notSupported(1),
                set(2),
                notSet(3)
                }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Integrated Lights-Out Security Override Switch State.

            The following values are defined:

            notSupported(1)
              The iLO Security Override Switch state is not supported on this
              model of Integrated Lights-Out.

            set(2)
              The iLO Security Override Switch is set, which implies security
              is disabled.

            notSet(3)
              The iLO Security Override Switch is not set, which implies normal
              secure operation."
        ::= { cpqSm2Cntlr 27 }

    cpqSm2CntlrHardwareVer OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Hardware Version of Remote Insight/ Integrated Lights-Out."
        ::= { cpqSm2Cntlr 28}

    cpqSm2CntlrAction OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Action Flags.

            This is a collection of flags used to indicate the various
            options available.

            ResetSupportBit:
            If bit-0 is set to 1, the option is available.
            If bit-0 is set to 0, the option is NOT available.

            iLOAlerts
            If bit-1 is set to 1, iLO alerts are enabled.
            If bit-2 is set to 1, iLO alerts are disabled.
            These two bits should never have the same value.

            HostAlerts
            If bit-3 is set to 1, Host alerts are enabled.
            If bit-4 is set to 1, Host alerts are disabled.
            These two bits should never have the same value.

            Bit-31 is used to execute the set operation.

            NOTE:   bit 31 is the most significant bit, bit 0 is the least
                    significant.

            Status   This is a collection of flags.  Each bit has the
                     following meaning when it is on (1):

                     Bit 0:      Reset Supported
                     Bit 1:      iLO Alerts Enabled
                     Bit 2:      iLO Alerts Disabled
                     Bit 3:      Host Alerts Enabled
                     Bit 4:      Host Alerts Disabled
                     Bit 5-30:   RESERVED
                     Bit 31:     Execute Set
            "

        ::= { cpqSm2Cntlr 29}


-- ****************************************************************************
--   Remote Insight/ Integrated Lights-Out Event Log Group
--   =====================================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSm2 Group                   (1.3.6.1.4.1.232.9)
--       cpqSm2Component Group         (1.3.6.1.4.1.232.9.2)
--        cpqSm2EventLog Group         (1.3.6.1.4.1.232.9.2.3)
--
--      The cpqSm2EventLog group contains ...
--
--      Implementation of the cpqSm2EventLog group is mandatory for all agents
--      that support the Remote Insight/Integrated Lights-Out MIB.
--
-- ****************************************************************************

    cpqSm2EventTotalEntries OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "The number of entries in the Remote Insight/ Integrated Lights-Out
            event log.  Setting the number of entries to 0 clears the Remote
            Insight/ Integrated Lights-Out event log. Setting the number of
            entries to something other than 0 will always fail."
        ::= { cpqSm2EventLog 1 }

-- ****************************************************************************
--   Remote Insight/ Integrated Lights-Out Event Log Table
--   =====================================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSm2 Group                   (1.3.6.1.4.1.232.9)
--       cpqSm2Component Group         (1.3.6.1.4.1.232.9.2)
--        cpqSm2EventLog Group         (1.3.6.1.4.1.232.9.2.3)
--         cpqSm2EventLogTable         (1.3.6.1.4.1.232.9.2.3.2)
--
-- ****************************************************************************

    cpqSm2EventLogTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSm2EventLogEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A table of event log descriptions."
        ::= { cpqSm2EventLog 2 }

    cpqSm2EventLogEntry OBJECT-TYPE
        SYNTAX  CpqSm2EventLogEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "An event log description."
        INDEX   { cpqSm2EventLogIndex }
        ::= { cpqSm2EventLogTable 1 }

    CpqSm2EventLogEntry ::= SEQUENCE {
        cpqSm2EventLogIndex           INTEGER,
        cpqSm2EventLogNumber          INTEGER,
        cpqSm2EventLogDate            OCTET STRING,
        cpqSm2EventLogMessage         DisplayString
        }

    cpqSm2EventLogIndex OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "An index that uniquely specifies this entry."
        ::= { cpqSm2EventLogEntry 1 }

    cpqSm2EventLogNumber OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number assigned by the Remote Insight/ Integrated Lights-Out
            firmware."
        ::= { cpqSm2EventLogEntry 2 }

    cpqSm2EventLogDate OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE (7))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The time and date for this event log entry.

             field  octets  contents                  range
             =====  ======  =======                  =====
               1      1-2   year                      0..65536
               2       3    month                     1..12
               3       4    day                       1..31
               4       5    hour                      0..23
               5       6    minute                    0..59
               6       7    second                    0..60
                            (use 60 for leap-second)


            This field will be set to year = 0 if the agent cannot provide
            the time and date.  The hour, minute, and second field will be set
            to zero (0) if they are not relevant.  The year field is set
            with the most significant octet first."
        ::= { cpqSm2EventLogEntry 3 }

    cpqSm2EventLogMessage OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..100))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The message text for this event log entry."
        ::= { cpqSm2EventLogEntry 4 }


-- ****************************************************************************
--   Remote Insight Asynchronous Communications Group
--   ================================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSm2 Group                   (1.3.6.1.4.1.232.9)
--       cpqSm2Component Group         (1.3.6.1.4.1.232.9.2)
--        cpqSm2AsyncComm Group        (1.3.6.1.4.1.232.9.2.4)
--
--      The cpqSm2AsyncComm group contains the configuration and status of
--      the Remote Insight asynchronous communication ports.
--
--      Implementation of the cpqSm2AsyncComm group is mandatory for all agents
--      that support the Remote Insight/Integrated Lights-Out MIB.
--
-- ****************************************************************************

-- ****************************************************************************
--   Remote Insight Communications Settings Table
--   ============================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSm2 Group                   (1.3.6.1.4.1.232.9)
--       cpqSm2Component Group         (1.3.6.1.4.1.232.9.2)
--        cpqSm2AsyncComm Group        (1.3.6.1.4.1.232.9.2.4)
--         cpqSm2CommSettingsTable     (1.3.6.1.4.1.232.9.2.4.1)
--
-- ****************************************************************************

    cpqSm2CommSettingsTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSm2CommSettingsEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "The list of communication settings for the Remote Insight."
        ::= { cpqSm2AsyncComm 1 }

    cpqSm2CommSettingsEntry OBJECT-TYPE
        SYNTAX  CpqSm2CommSettingsEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A defined port's communication settings for the Remote Insight."
        INDEX   { cpqSm2CommPort }
        ::= { cpqSm2CommSettingsTable 1 }

    CpqSm2CommSettingsEntry ::= SEQUENCE {
        cpqSm2CommPort                INTEGER,
        cpqSm2CommType                INTEGER,
        cpqSm2CommBaudRate            INTEGER,
        cpqSm2CommParity              INTEGER,
        cpqSm2CommDataBits            INTEGER,
        cpqSm2CommStopBits            INTEGER,
        cpqSm2CommModemReset          DisplayString,
        cpqSm2CommModemInit           DisplayString,
        cpqSm2CommModemDialPrefix     DisplayString,
        cpqSm2CommPortInit            DisplayString,
        cpqSm2CommDialin              INTEGER,
        cpqSm2CommDialbackRequired    INTEGER,
        cpqSm2CommNonPppConnections   INTEGER,
        cpqSm2CommSnmpTrapDelivery    INTEGER,
        cpqSm2CommPageDelivery        INTEGER,
        cpqSm2CommPagerBaudRate       INTEGER,
        cpqSm2CommPagerParity         INTEGER,
        cpqSm2CommPagerDataBits       INTEGER,
        cpqSm2CommPagerStopBits       INTEGER,
        cpqSm2CommPcmciaModel         DisplayString
        }


    cpqSm2CommPort OBJECT-TYPE
        SYNTAX  INTEGER {
            internal(1),
            auxiliary(2)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight Communications Port.

            The following values are defined:

            internal(1)
              This is the Remote Insight internal modem port.

            auxiliary(2)
              This is the Remote Insight auxiliary port."
        ::= { cpqSm2CommSettingsEntry 1 }

    cpqSm2CommType OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            none(2),
            modem(3),
            nulModemCable(4),
            xonXoff(5)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight Communications Type.

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine the communications
              type.

            none(2)
              There is nothing configured on this port.

            modem(3)
              A modem is configured on this port.

            nulModem(4)
              A Null Modem cable is configured on this port.  This type of
              connection is only supported on the Remote Insight auxiliary
              port.

            xonXoff(5)
              An XON/XOFF 3-wire interface is configured on this port.  This
              type of connection is only supported on the Remote Insight
              auxiliary port."
        ::= { cpqSm2CommSettingsEntry 2 }

    cpqSm2CommBaudRate OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The baud rate to be used over this communication medium by the
            Remote Insight."
        ::= { cpqSm2CommSettingsEntry 3 }

    cpqSm2CommParity OBJECT-TYPE
        SYNTAX  INTEGER {
                other(1),
                none(2),
                odd(3),
                even(4)
                }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight Communications Parity.

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine the parity setting.

            none(2)
              This port is set for no parity.

            odd(3)
              This port is set for odd parity.

            even(4)
              This port is set for even parity."
        ::= { cpqSm2CommSettingsEntry 4 }

    cpqSm2CommDataBits OBJECT-TYPE
        SYNTAX  INTEGER {
                other(1),
                sevenBits(2),
                eightBits(3)
                }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight Communications Data Bits.

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine the data bits setting.

            sevenBit(2)
              This port is set for seven data bits.

            eight(3)
              This port is set for eight data bits."
        ::= { cpqSm2CommSettingsEntry 5 }

    cpqSm2CommStopBits OBJECT-TYPE
        SYNTAX  INTEGER {
                other(1),
                oneBit(2),
                twoBits(3)
                }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight Communications Stop Bits.

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine the stop bits setting.

            oneBit(2)
              This port is set for one stop data bit.

            twoBits(3)
              This port is set for two stop bits."
        ::= { cpqSm2CommSettingsEntry 6 }

    cpqSm2CommModemReset OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..42))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The string that is sent to reset the modem."
        ::= { cpqSm2CommSettingsEntry 7 }

    cpqSm2CommModemInit OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..42))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The string that is sent to initialize the modem."
        ::= { cpqSm2CommSettingsEntry 8 }

    cpqSm2CommModemDialPrefix OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..42))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The string that is prepended to phone numbers before dialing."
        ::= { cpqSm2CommSettingsEntry 9 }

    cpqSm2CommPortInit OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..42))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The string that is sent to the auxiliary port before the modem
            is reset."
        ::= { cpqSm2CommSettingsEntry 10 }

    cpqSm2CommDialin OBJECT-TYPE
        SYNTAX  INTEGER {
                other(1),
                enabled(2),
                disabled(3)
                }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Comm Dial-in.

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine the status of dialin.

            enabled(2)
              Dialing in to this modem is enabled.

            disabled(3)
              Dialing in to this modem is disabled."
        ::= { cpqSm2CommSettingsEntry 11 }

    cpqSm2CommDialbackRequired OBJECT-TYPE
        SYNTAX  INTEGER {
                other(1),
                required(2),
                notRequired(3)
                }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight Dialback Required.

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine the dialback required
              setting.

            required(2)
              Dialback is required for all users.

            notRequired(3)
              Dialback is not required.  It is optional on a per user basis."
        ::= { cpqSm2CommSettingsEntry 12 }

    cpqSm2CommNonPppConnections OBJECT-TYPE
        SYNTAX  INTEGER {
                other(1),
                enabled(2),
                disabled(3)
                }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Non-PPP connections.

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine the status of the
              non-PPP connections variable.

            enabled(2)
              Non-PPP connections are allowed on this port.

            disabled(3)
              Non-PPP connections are not allowed on this port.  Only PPP
              sessions are accepted."
        ::= { cpqSm2CommSettingsEntry 13 }

    cpqSm2CommSnmpTrapDelivery OBJECT-TYPE
        SYNTAX  INTEGER {
                other(1),
                enabled(2),
                disabled(3)
                }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "SNMP Trap Delivery.

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine the status of SNMP Trap
              delivery.

            enabled(2)
              SNMP trap delivery is enabled.  The Remote Insight firmware
              will use this port to deliver SNMP traps.

            disabled(3)
              SNMP Trap delivery is disabled.  The Remote Insight firmware
              will not use this port to deliver SNMP traps."
        ::= { cpqSm2CommSettingsEntry 14 }

    cpqSm2CommPageDelivery OBJECT-TYPE
        SYNTAX  INTEGER {
                other(1),
                enabled(2),
                disabled(3)
                }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Page Delivery.

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine the status of page
              delivery.

            enabled(2)
              Page delivery is enabled.  The Remote Insight firmware will use
              this port to deliver pages.

            disabled(3)
              Page delivery is disabled.  The Remote Insight firmware will not
              use this port to deliver pages."
        ::= { cpqSm2CommSettingsEntry 15 }

    cpqSm2CommPagerBaudRate OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The baud rate to be used for pager communications over this medium
            by the Remote Insight."
        ::= { cpqSm2CommSettingsEntry 16 }

    cpqSm2CommPagerParity OBJECT-TYPE
        SYNTAX  INTEGER {
                other(1),
                none(2),
                odd(3),
                even(4)
                }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight Communications Pager Parity.

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine the pager parity
              setting.

            none(2)
              This port is set for no parity when paging.

            odd(3)
              This port is set for odd parity when paging.

            even(4)
              This port is set for even parity when paging."
        ::= { cpqSm2CommSettingsEntry 17 }

    cpqSm2CommPagerDataBits OBJECT-TYPE
        SYNTAX  INTEGER {
                other(1),
                sevenBits(2),
                eightBits(3)
                }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight Communications Pager Data Bits.

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine the data bits setting.

            sevenBit(2)
              This port is set for seven data bits when paging.

            eight(3)
              This port is set for eight data bits when paging."
        ::= { cpqSm2CommSettingsEntry 18 }

    cpqSm2CommPagerStopBits OBJECT-TYPE
        SYNTAX  INTEGER {
                other(1),
                oneBit(2),
                twoBits(3)
                }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight Communications Pager Stop Bits.

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine the stop bits setting.

            oneBit(2)
              This port is set for one stop data bit when paging.

            twoBits(3)
              This port is set for two stop bits when paging."
        ::= { cpqSm2CommSettingsEntry 19 }

    cpqSm2CommPcmciaModel OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..80))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight Network PCMCIA Card Model.

             This is a NULL terminated ASCII string.  If the agent
             cannot determine the model name, it should return a NULL
             string."
        ::= { cpqSm2CommSettingsEntry 20 }

-- ****************************************************************************
--   Remote Insight/ Integrated Lights-Out Network Interface Group
--   =============================================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSm2 Group                   (1.3.6.1.4.1.232.9)
--       cpqSm2Component Group         (1.3.6.1.4.1.232.9.2)
--        cpqSm2Nic Group              (1.3.6.1.4.1.232.9.2.5)
--
--      The cpqSm2Nic group contains the configuration and statistics for
--      the network interface card associated with the
--      Remote Insight/ Integrated Lights-Out.
--
--      Implementation of the cpqSm2Nic group is mandatory for all agents
--      that support the Remote Insight/Integrated Lights-Out MIB.
--
-- ****************************************************************************

-- ****************************************************************************
--   Remote Insight/ Integrated Lights-Out Network Interface Configuration Table
--   ===========================================================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSm2 Group                   (1.3.6.1.4.1.232.9)
--       cpqSm2Component Group         (1.3.6.1.4.1.232.9.2)
--        cpqSm2Nic Group              (1.3.6.1.4.1.232.9.2.5)
--         cpqSm2NicConfigTable        (1.3.6.1.4.1.232.9.2.5.1)
--
-- ****************************************************************************

    cpqSm2NicConfigTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSm2NicConfigEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "The list of network interface configuration settings for the
            Remote Insight/ Integrated Lights-Out."
        ::= { cpqSm2Nic 1 }

    cpqSm2NicConfigEntry OBJECT-TYPE
        SYNTAX  CpqSm2NicConfigEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A defined nic's configuration settings for the
            Remote Insight/ Integrated Lights-Out."
        INDEX   { cpqSm2NicLocation }
        ::= { cpqSm2NicConfigTable 1 }

    CpqSm2NicConfigEntry ::= SEQUENCE {
        cpqSm2NicLocation             INTEGER,
        cpqSm2NicModel                DisplayString,
        cpqSm2NicType                 INTEGER,
        cpqSm2NicMacAddress           OCTET STRING,
        cpqSm2NicIpAddress            IpAddress,
        cpqSm2NicIpSubnetMask         IpAddress,
        cpqSm2NicEnabledStatus        INTEGER,
        cpqSm2NicDuplexState          INTEGER,
        cpqSm2NicSpeed                INTEGER,
        cpqSm2NicDhcpUse              INTEGER,
        cpqSm2NicCondition            INTEGER,
        cpqSm2NicMtu                  INTEGER,
        cpqSm2NicGatewayIpAddress     IpAddress,
        cpqSm2NicRibFullQualDnsName   DisplayString
        }


    cpqSm2NicLocation OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            embedded(2),
            pcmcia(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Location of the Network Interface Controller associated with
            the Remote Insight/ Integrated Lights-Out.

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine type of network
              interface controller.

            embedded(2)
              This is an embedded network interface controller.

            pcmcia(3)
              This is a PCMCIA network interface controller."

        ::= { cpqSm2NicConfigEntry 1 }

    cpqSm2NicModel OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..80))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Network Interface Controller
            Model.

             This is a NULL terminated ASCII string.  If the agent
             cannot determine the model name, it should return a NULL
             string."
        ::= { cpqSm2NicConfigEntry 2 }

    cpqSm2NicType OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            ethernet(2),
            tokenRing(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Network Interface
            Controller Type.

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine type of network
              interface controller.

            ethernet(2)
              This is an ethernet network interface controller.

            tokenRing(3)
              This is a token ring network interface controller."
        ::= { cpqSm2NicConfigEntry 3 }

    cpqSm2NicMacAddress OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE(6))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The MAC Address of the Network Interface Controller associated
             with the Remote Insight/ Integrated Lights-Out.

              This is a 6 octet address in the 'canonical' order
              defined by IEEE 802.1a, i.e., as if it were transmitted
              least significant bit first, even though 802.5 (in
              contrast to other 802.x protocols) requires MAC addresses
              to be transmitted most significant bit first.

              16-bit addresses, if needed, are represented by setting
              their upper 4 octets to all 0's, i.e., AAFF would be
              represented as 00000000AAFF."
        ::= { cpqSm2NicConfigEntry 4 }

    cpqSm2NicIpAddress OBJECT-TYPE
        SYNTAX  IpAddress
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Network Interface
            Controller IP Address.

            The IP address for the network interface controller associated
            with the Remote Insight/ Integrated Lights-Out.  All octets should
            be set to 0xff if there is not an IP address associated with the
            NIC. The order will be in network byte order (i.e. MSB first.)"
        ::= { cpqSm2NicConfigEntry 5 }

    cpqSm2NicIpSubnetMask OBJECT-TYPE
        SYNTAX  IpAddress
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Network Interface Controller
            Subnet Mask."
        ::= { cpqSm2NicConfigEntry 6 }

    cpqSm2NicEnabledStatus OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            enabled(2),
            disabled(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Network Interface Controller
            Enabled Status

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine type of network
              interface controller enabled status

            enabled(2)
              This network interface controller is enabled.

            disabled(3)
              This network interface controller is disabled."
        ::= { cpqSm2NicConfigEntry 7 }

    cpqSm2NicDuplexState OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            halfDuplex(2),
            fullDuplex(3),
            notSupported(4)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Network Interface Controller
            Enabled Status.

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine type of network
              interface controller duplex state.

            halfDuplex(2)
              This network interface controller is half duplex.

            fullDuplex(3)
              This network interface controller is full duplex.

            notSupported(4)
              This network interface controller is does not support duplex
              state."
        ::= { cpqSm2NicConfigEntry 8 }

    cpqSm2NicSpeed OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Network Interface Controller
             Speed.

             The speed of the network interface controller in megabits per
             second."
        ::= { cpqSm2NicConfigEntry 9 }

    cpqSm2NicDhcpUse OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            enabled(2),
            disabled(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Network Interface Controller
            DHCP Usage

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine if DHCP is supported
              for this network interface controller.

            enabled(2)
              DHCP usage is enabled for this network interface controller.

            disabled(3)
              DHCP usage is disabled for this network interface controller."
        ::= { cpqSm2NicConfigEntry 10 }

    cpqSm2NicCondition OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            ok(2),
            degraded(3),
            failed(4)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
        "Remote Insight/ Integrated Lights-Out Network Interface Controller
        condition.

        This represents the overall condition of the
        Remote Insight/ Integrated Lights-Out Network
        Interface Controller (NIC)."
        ::= { cpqSm2NicConfigEntry 11 }

    cpqSm2NicMtu OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Network Interface Maximum
            Transfer Unit.

            The maximum packet size (in bytes) of the network interface
            controller."
        ::= { cpqSm2NicConfigEntry 12 }

    cpqSm2NicGatewayIpAddress OBJECT-TYPE
        SYNTAX  IpAddress
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Network Interface Controller Default
            Gateway IP Address.

            The Default Gateway IP address for the network interface controller
            associated with the Remote Insight/ Integrated Lights-Out.
            If cpqSm2NicDhcpUse is enabled(2), this is the DHCP supplied gateway.
            If cpqSm2NicDhcpUse is disabled(3), this is the static gateway.
            The order will be in network byte order (i.e. MSB first.)"
        ::= { cpqSm2NicConfigEntry 13 }

    cpqSm2NicRibFullQualDnsName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..180))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Fully Qualified DNS Name.

            The Fully Qualified DNS Name assigned to this
            Remote Insight/ Integrated Lights-Out.

            This is composed of the DNS name and the Domain name associated
            with the Remote Insight/ Integrated Lights-Out."
        ::= { cpqSm2NicConfigEntry 14 }


-- ****************************************************************************
--   Remote Insight/ Integrated Lights-Out Network Interface Statistics Table
--   ========================================================================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqSm2 Group                   (1.3.6.1.4.1.232.9)
--       cpqSm2Component Group         (1.3.6.1.4.1.232.9.2)
--        cpqSm2Nic Group              (1.3.6.1.4.1.232.9.2.5)
--         cpqSm2NicStatsTable         (1.3.6.1.4.1.232.9.2.5.2)
--
-- ****************************************************************************

    cpqSm2NicStatsTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqSm2NicStatsEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "The list of network interface configuration settings for the
            Remote Insight/ Integrated Lights-Out."
        ::= { cpqSm2Nic 2 }

    cpqSm2NicStatsEntry OBJECT-TYPE
        SYNTAX  CpqSm2NicStatsEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A defined nic's configuration settings for the
            Remote Insight/ Integrated Lights-Out."
        INDEX   { cpqSm2NicStatsLocation }
        ::= { cpqSm2NicStatsTable 1 }

    CpqSm2NicStatsEntry ::= SEQUENCE {
        cpqSm2NicStatsLocation        INTEGER,
        cpqSm2NicXmitBytes            Counter,
        cpqSm2NicXmitTotalPackets     Counter,
        cpqSm2NicXmitUnicastPackets   Counter,
        cpqSm2NicXmitNonUniPackets    Counter,
        cpqSm2NicXmitDiscardPackets   Counter,
        cpqSm2NicXmitErrorPackets     Counter,
        cpqSm2NicXmitQueueLength      Counter,
        cpqSm2NicRecvBytes            Counter,
        cpqSm2NicRecvTotalPackets     Counter,
        cpqSm2NicRecvUnicastPackets   Counter,
        cpqSm2NicRecvNonUniPackets    Counter,
        cpqSm2NicRecvDiscardPackets   Counter,
        cpqSm2NicRecvErrorPackets     Counter,
        cpqSm2NicRecvUnknownPackets   Counter
        }


    cpqSm2NicStatsLocation OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            embedded(2),
            pcmcia(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Location of the Network Interface Controller associated with
            the Remote Insight/ Integrated Lights-Out.

            The following values are defined:

            other(1)
              The Insight Agent is unable to determine type of network
              interface controller.

            embedded(2)
              This is an embedded network interface controller.

            pcmcia(3)
              This is a PCMCIA network interface controller."
        ::= { cpqSm2NicStatsEntry 1 }

    cpqSm2NicXmitBytes OBJECT-TYPE
        SYNTAX  Counter
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Network Interface Controller
            Bytes Transmitted."
        ::= { cpqSm2NicStatsEntry 2 }


    cpqSm2NicXmitTotalPackets OBJECT-TYPE
        SYNTAX  Counter
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Network Interface Controller
            Total Transmit Packets."
        ::= { cpqSm2NicStatsEntry 3 }

    cpqSm2NicXmitUnicastPackets OBJECT-TYPE
        SYNTAX  Counter
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Network Interface Controller
            Unicast Transmit Packets."
        ::= { cpqSm2NicStatsEntry 4 }

    cpqSm2NicXmitNonUniPackets OBJECT-TYPE
        SYNTAX  Counter
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Network Interface Controller
            Non-Unicast Transmit Packets."
        ::= { cpqSm2NicStatsEntry 5 }

    cpqSm2NicXmitDiscardPackets OBJECT-TYPE
        SYNTAX  Counter
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Network Interface Controller Total
            Transmit Discarded Packets."
        ::= { cpqSm2NicStatsEntry 6 }

    cpqSm2NicXmitErrorPackets OBJECT-TYPE
        SYNTAX  Counter
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Network Interface Controller Total
            Error Transmit Packets."
        ::= { cpqSm2NicStatsEntry 7 }

    cpqSm2NicXmitQueueLength OBJECT-TYPE
        SYNTAX  Counter
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Network Interface Controller Number
            of Outstanding Packets in Transmit Queue."
        ::= { cpqSm2NicStatsEntry 8 }


    cpqSm2NicRecvBytes OBJECT-TYPE
        SYNTAX  Counter
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Network Interface Controller
            Bytes Received."
        ::= { cpqSm2NicStatsEntry 9 }

    cpqSm2NicRecvTotalPackets OBJECT-TYPE
        SYNTAX  Counter
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Network Interface Controller
            Total Receive Packets."
        ::= { cpqSm2NicStatsEntry 10}

    cpqSm2NicRecvUnicastPackets OBJECT-TYPE
        SYNTAX  Counter
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Network Interface Controller Unicast
            Receive Packets."
        ::= { cpqSm2NicStatsEntry 11}

    cpqSm2NicRecvNonUniPackets OBJECT-TYPE
        SYNTAX  Counter
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Network Interface Controller Non-Unicast
            Receive Packets."
        ::= { cpqSm2NicStatsEntry 12}

    cpqSm2NicRecvDiscardPackets OBJECT-TYPE
        SYNTAX  Counter
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Network Interface Controller Total Receive
            Discarded Packets."
        ::= { cpqSm2NicStatsEntry 13 }

    cpqSm2NicRecvErrorPackets OBJECT-TYPE
        SYNTAX  Counter
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Network Interface Controller Total Receive
            Error Packets."
        ::= { cpqSm2NicStatsEntry 14 }

    cpqSm2NicRecvUnknownPackets OBJECT-TYPE
        SYNTAX  Counter
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Network Interface Controller Number of Unknown
            Protocol Packets."
        ::= { cpqSm2NicStatsEntry 15 }


-- ****************************************************************************
--   Remote Insight/ Integrated Lights-Out Trap Definition
--   =====================================================
--
--  The compaq enterprise               (1.3.6.1.4.1.232)
--
--  The SNMP trap messages must not be bigger than 484 octets (bytes).
--
--  Trap support in an SNMP agent implementation is optional.  An SNMP
--  agent implementation may support all, some, or none of the traps.
--  If traps are supported, the user should be provided with the option of
--  disabling traps.
--
-- ****************************************************************************

    cpqSm2ServerReset TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags }
        DESCRIPTION
            "Server Reset Detected.

            The Remote Insight/ Integrated Lights-Out firmware has detected a server reset."

              --#TYPE "Server Reset Detected (9001)"
              --#SUMMARY "Server reset detected."
              --#ARGUMENTS {}
              --#SEVERITY CRITICAL
              --#TIMEINDEX 99
              --#STATE   DEGRADED

        ::= 9001

    cpqSm2ServerPowerOutage TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags }
        DESCRIPTION
            "Server Power Outage.

            The Remote Insight/ Integrated Lights-Out firmware has detected server
            power failure."

              --#TYPE "Server Power Outage (9002)"
              --#SUMMARY "Server power outage detected."
              --#ARGUMENTS {}
              --#SEVERITY CRITICAL
              --#TIMEINDEX 99
              --#STATE   DEGRADED

        ::= 9002

    cpqSm2UnauthorizedLoginAttempts TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSm2CntlrBadLoginAttemptsThresh}
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Unauthorized Login Attempts.

            The Remote Insight/ Integrated Lights-Out firmware has detected
            unauthorized login attempts."

              --#TYPE "Remote Insight/ Integrated Lights-Out Unauthorized Login Attempts (9003)"
              --#SUMMARY "More than %d unauthorized login attempts detected."
              --#ARGUMENTS {2}
              --#SEVERITY INFORMATIONAL
              --#TIMEINDEX 99
              --#STATE   OPERATIONAL

        ::= 9003

    cpqSm2BatteryFailed TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags }
        DESCRIPTION
            "Remote Insight Battery Failed.

            The Remote Insight battery has failed and needs to be replaced."

              --#TYPE "Remote Insight Battery Failed (9004)"
              --#SUMMARY "Remote Insight battery failed."
              --#ARGUMENTS {}
              --#SEVERITY CRITICAL
              --#TIMEINDEX 99
              --#STATE   FAILED

        ::= 9004

    cpqSm2SelfTestError TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags, cpqSm2CntlrSelfTestErrors }
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Self Test Error.

            The Remote Insight/ Integrated Lights-Out firmware has detected a Remote
            Insight self test error."

              --#TYPE "Remote Insight/ Integrated Lights-Out Self Test Error (9005)"
              --#SUMMARY "Remote Insight/ Integrated Lights-Out self test error %d."
              --#ARGUMENTS {2}
              --#SEVERITY CRITICAL
              --#TIMEINDEX 99
              --#STATE   FAILED

        ::= 9005

    cpqSm2InterfaceError TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags }
        DESCRIPTION
            "Remote Insight/ Integrated Lights-Out Interface Error.

            The host OS has detected an error in the Remote Insight/ Integrated Lights-Out
            interface.  The firmware is not responding."

              --#TYPE "Remote Insight/ Integrated Lights-Out Interface Error (9006)"
              --#SUMMARY "Server %s, Remote Insight/ Integrated Lights-Out interface error."
              --#ARGUMENTS {0}
              --#SEVERITY MAJOR
              --#TIMEINDEX 99
              --#STATE   DEGRADED

        ::= 9006

    cpqSm2BatteryDisconnected TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags }
        DESCRIPTION
            "Remote Insight Battery Disconnected.

            The Remote Insight battery cable has been disconnected."

              --#TYPE "Remote Insight Battery Disconnected (9007)"
              --#SUMMARY "Remote Insight battery disconnected."
              --#ARGUMENTS {}
              --#SEVERITY MAJOR
              --#TIMEINDEX 99
              --#STATE   DEGRADED

        ::= 9007

    cpqSm2KeyboardCableDisconnected TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags }
        DESCRIPTION
            "Keyboard Cable Disconnected.

            The Remote Insight keyboard cable has been disconnected."

              --#TYPE "Remote Insight keyboard cable disconnected (9008)"
              --#SUMMARY "Remote Insight keyboard cable disconnected."
              --#ARGUMENTS {}
              --#SEVERITY MAJOR
              --#TIMEINDEX 99
              --#STATE   DEGRADED

        ::= 9008

    cpqSm2MouseCableDisconnected TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags }
        DESCRIPTION
            "Mouse Cable Disconnected.

            The Remote Insight mouse cable has been disconnected."

              --#TYPE "Remote Insight mouse cable disconnected (9009)"
              --#SUMMARY "Remote Insight mouse cable disconnected."
              --#ARGUMENTS {}
              --#SEVERITY MAJOR
              --#TIMEINDEX 99
              --#STATE   DEGRADED

        ::= 9009

    cpqSm2ExternalPowerCableDisconnected TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags }
        DESCRIPTION
            "External Power Cable Disconnected.

            The Remote Insight external power cable has been disconnected."

              --#TYPE "Remote Insight external power cable disconnected (9010)"
              --#SUMMARY "Remote Insight external power cable disconnected."
              --#ARGUMENTS {}
              --#SEVERITY MAJOR
              --#TIMEINDEX 99
              --#STATE   DEGRADED

        ::= 9010

-- New for 5.30.0.0
    cpqSm2LogsFull TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags  }
        DESCRIPTION
            "Logs Full.

            The Remote Insight/ Integrated Lights-Out firmware has detected the logs are full."

              --#TYPE "Remote Insight/ Integrated Lights-Out Logs Full. (9011)"
              --#SUMMARY "Remote Insight/ Integrated Lights-Out Logs Full"
              --#ARGUMENTS {}
              --#SEVERITY MINOR
              --#TIMEINDEX 99
              --#STATE   OPERATIONAL

        ::= 9011

-- New for 5.30.0.0
    cpqSm2SecurityOverrideEngaged TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags }
        DESCRIPTION
            "Security Override Engaged.

            The Remote Insight/ Integrated Lights-Out firmware has detected the security override jumper
            has been toggled to the engaged position."

              --#TYPE "Security override engaged. (9012)"
              --#SUMMARY "Remote Insight/ Integrated Lights-Out firmware has detected the security override jumper has been engaged."
              --#ARGUMENTS {}
              --#SEVERITY INFORMATIONAL
              --#TIMEINDEX 99
              --#STATE   OPERATIONAL

        ::= 9012

-- New for 5.30.0.0
    cpqSm2SecurityOverrideDisengaged TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName, cpqHoTrapFlags }
        DESCRIPTION
            "Security Override Disengaged.

            The Remote Insight/ Integrated Lights-Out firmware has detected the security override jumper
            has been toggled to the disengaged position."

              --#TYPE "Security override disengaged. (9013)"
              --#SUMMARY "Remote Insight/ Integrated Lights-Out firmware has detected the security override jumper has been disengaged."
              --#ARGUMENTS {}
              --#SEVERITY INFORMATIONAL
              --#TIMEINDEX 99
              --#STATE   OPERATIONAL

        ::= 9013

END

