State Event Messages defined in INSIGHTMANAGER.DAT:

HostMibCond:\$event:\$oldState:\$newState:$hostName $reason
ThermalCondition:\$event:\$oldState:\$newState:$hostName $reason
HealthStatFSM:\$event:\$oldState:\$newState:$hostName $reason
cpqCorrectableMemory:\$event:\$oldState:\$newState:$hostName $reason
CriticalErrorLog_FSM:\$event:\$oldState:\$newState:$hostName $reason
EquipmentCondition:\$event:\$oldState:\$newState:$hostName $reason
cpu_fsm:\$event:\$oldState:\$newState:$hostName:$cpqSeCpuUnitIndex $reason
SystemInfoMibCondition:\$event:\$oldState:\$newState:$hostName $reason
ThresholdCondition:\$event:\$oldState:\$newState:$hostName $reason
UPSCondition:\$event:\$oldState:\$newState:$hostName $reason
UPSLineStatus:\$event:\$oldState:\$newState:$hostName $reason
cpqScsiMibCnd_FSM:\$event:\$oldState:\$newState:$hostName $reason
ScsiCntrl_FSM:\$event:\$oldState:\$newState:$hostName:$cpqScsiCntrlIndex $reason
ScsiLogicalDrive_fsm:\$event:\$oldState:\$newState:$hostName:$cpqScsiLogDrvIndex $reason
ScsiPhysicalDrive_fsm:\$event:\$oldState:\$newState:$hostName:$cpqScsiPhyDrvIndex $reason
cpqDaMibCnd_FSM:\$event:\$oldState:\$newState:$hostName $reason
DACntrlEnt_fsm:\$event:\$oldState:\$newState:$hostName:$cpqDACntrlIndex $reason
Accelerator_fsm:\$event:\$oldState:\$newState:$hostName:$cpqDAccIndex $reason
IdaLogicalDrive_fsm:\$event:\$oldState:\$newState:$hostName:$cpqIdaLogDrvIndex $reason
IdaPhysicalDrive_fsm:\$event:\$oldState:\$newState:$hostName:$cpqDaPhyDrvIndex $reason
CPQ_ClusterFSM:\$event:\$oldState:\$newState:$hostName $reason
CPQ_RemoteInsight_FSM:\$event:\$oldState:\$newState:$hostName $reason
CPQ_FibreChannelFSM:\$event:\$oldState:\$newState:$hostName $reason
CPQ_NIC_FSM:\$event:\$oldState:\$newState:$hostName $reason
CPQ_RACKENCLOSURE_FSM:\$event:\$oldState:\$newState:$hostName $reason


DSM State Change polling messages (oldState and newState will vary):

161 ( ClassName = HostMibCond oldState = ?? newState = ?? )
161 ( ClassName = ThermalCondition oldState = ?? newState = ?? )
161 ( ClassName = HealthStatFSM oldState = ?? newState = ?? )
161 ( ClassName = cpqCorrectableMemory oldState = ?? newState = ?? )
161 ( ClassName = CriticalErrorLog_FSM oldState = ?? newState = ?? )
161 ( ClassName = EquipmentCondition oldState = ?? newState = ?? )
161 ( ClassName = cpu_fsm oldState = ?? newState = ?? )
161 ( ClassName = SystemInfoMibCondition oldState = ?? newState = ?? )
161 ( ClassName = ThresholdCondition oldState = ?? newState = ?? )
161 ( ClassName = UPSCondition oldState = ?? newState = ?? )
161 ( ClassName = UPSLineStatus oldState = ?? newState = ?? )
161 ( ClassName = cpqScsiMibCnd_FSM oldState = ?? newState = ?? )
161 ( ClassName = ScsiCntrl_FSM oldState = ?? newState = ?? )
161 ( ClassName = ScsiLogicalDrive_fsm oldState = ?? newState = ?? )
161 ( ClassName = ScsiPhysicalDrive_fsm oldState = ?? newState = ?? )
161 ( ClassName = cpqDaMibCnd_FSM oldState = ?? newState = ?? )
161 ( ClassName = DACntrlEnt_fsm oldState = ?? newState = ?? )
161 ( ClassName = Accelerator_fsm oldState = ?? newState = ?? )
161 ( ClassName = IdaLogicalDrive_fsm oldState = ?? newState = ?? )
161 ( ClassName = IdaPhysicalDrive_fsm oldState = ?? newState = ?? )
161 ( ClassName = CPQ_ClusterFSM oldState = ?? newState = ?? )
161 ( ClassName = CPQ_RemoteInsight_FSM oldState = ?? newState = ?? )
161 ( ClassName = CPQ_FibreChannelFSM oldState = ?? newState = ?? )
161 ( ClassName = CPQ_NIC_FSM oldState = ?? newState = ?? )
161 ( ClassName = CPQ_RACKENCLOSURE_FSM oldState = ?? newState = ?? )


Possible State Change values for oldState and newState:

Result of Acknowledgement by User:
oldState = Broken               newState = CriticalAcknowledged
oldState = Warning              newState = WarningAcknowledged
oldState = Repaired             newState = Up

Result of Polling by DSM:
oldState = CriticalAcknowledged newState = Repaired
oldState = CriticalAcknowledged newState = Warning
oldState = WarningAcknowledged  newState = Repaired
oldState = WarningAcknowledged  newState = Broken
oldState = Down                 newState = Repaired
oldState = Down                 newState = Warning
oldState = Down                 newState = Broken
oldState = Broken               newState = Repaired
oldState = Broken               newState = Warning
oldState = Unknown              newState = Up
oldState = Unknown              newState = Warning
oldState = Unknown              newState = Broken
oldState = Repaired             newState = Warning
oldState = Repaired             newState = Broken
oldState = Up                   newState = Warning
oldState = Up                   newState = Broken
oldState = Warning              newState = Repaired
oldState = Warning              newState = Broken


Polling State Change Message examples:

161 ( ClassName = cpqScsiMibCnd_FSM oldState = Up newState = Broken )
161 ( ClassName = ScsiCntrl_FSM oldState = Up newState = Broken )
161 ( ClassName = cpqScsiMibCnd_FSM oldState = Broken newState = Repaired )
161 ( ClassName = ScsiCntrl_FSM oldState = Broken newState = Repaired )

Acknowledged State Change examples:

( ClassName = HealthStatFSM oldState = Broken newState = CriticalAcknowledged )
( ClassName = HealthStatFSM oldState = Warning newState = WarningAcknowledged )
( ClassName = ScsiCntrl_FSM oldState = Repaired newState = Up )


